### Bug Summary

File: | epan/dissectors/packet-oran.c
Warning: | line 2123, column 17 Value stored to 'cPRB' is never read

### Annotated Source Code

Press '?' to see keyboard shortcuts

Show analyzer invocation
clang -cc1 -cc1 -triple x86_64-pc-linux-gnu -analyze -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name packet-oran.c -analyzer-checker=core -analyzer-checker=apiModeling -analyzer-checker=unix -analyzer-checker=deadcode -analyzer-checker=security.insecureAPI.UncheckedReturn -analyzer-checker=security.insecureAPI.getpw -analyzer-checker=security.insecureAPI.gets -analyzer-checker=security.insecureAPI.mktemp -analyzer-checker=security.insecureAPI.mkstemp -analyzer-checker=security.insecureAPI.vfork -analyzer-checker=nullability.NullPassedToNonnull -analyzer-checker=nullability.NullReturnedFromNonnull -analyzer-output plist -w -setup-static-analyzer -mrelocation-model pic -pic-level 2 -fhalf-no-semantic-interposition -fno-delete-null-pointer-checks -mframe-pointer=all -relaxed-aliasing -fmath-errno -ffp-contract=on -fno-rounding-math -ffloat16-excess-precision=fast -fbfloat16-excess-precision=fast -mconstructor-aliases -funwind-tables=2 -target-cpu x86-64 -tune-cpu generic -debugger-tuning=gdb -fdebug-compilation-dir=/builds/wireshark/wireshark/build -fcoverage-compilation-dir=/builds/wireshark/wireshark/build -resource-dir /usr/lib/llvm-21/lib/clang/21 -isystem /usr/include/glib-2.0 -isystem /usr/lib/x86_64-linux-gnu/glib-2.0/include -isystem /builds/wireshark/wireshark/epan/dissectors -isystem /builds/wireshark/wireshark/build/epan/dissectors -isystem /usr/include/mit-krb5 -isystem /usr/include/libxml2 -isystem /builds/wireshark/wireshark/epan -D G_DISABLE_DEPRECATED -D G_DISABLE_SINGLE_INCLUDES -D WS_BUILD_DLL -D WS_DEBUG -D WS_DEBUG_UTF_8 -I /builds/wireshark/wireshark/build -I /builds/wireshark/wireshark -I /builds/wireshark/wireshark/include -D _GLIBCXX_ASSERTIONS -internal-isystem /usr/lib/llvm-21/lib/clang/21/include -internal-isystem /usr/local/include -internal-isystem /usr/lib/gcc/x86_64-linux-gnu/14/../../../../x86_64-linux-gnu/include -internal-externc-isystem /usr/include/x86_64-linux-gnu -internal-externc-isystem /include -internal-externc-isystem /usr/include -fmacro-prefix-map=/builds/wireshark/wireshark/= -fmacro-prefix-map=/builds/wireshark/wireshark/build/= -fmacro-prefix-map=../= -Wno-format-truncation -Wno-format-nonliteral -Wno-pointer-sign -std=gnu11 -ferror-limit 19 -fvisibility=hidden -fwrapv -fwrapv-pointer -fstrict-flex-arrays=3 -stack-protector 2 -fstack-clash-protection -fcf-protection=full -fgnuc-version=4.2.1 -fskip-odr-check-in-gmf -fexceptions -fcolor-diagnostics -analyzer-output=html -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -o /builds/wireshark/wireshark/sbout/2025-10-20-100319-3623-1 -x c /builds/wireshark/wireshark/epan/dissectors/packet-oran.c

Keyboard shortcuts:

- Use 'j/k' keys for keyboard navigation
- Use 'Shift+S' to show/hide relevant lines
- Use '?' to toggle this window

Close
Show only relevant lines Show control flow arrows

1 | /* packet-oran.c
2 | * Routines for O-RAN fronthaul UC-plane dissection
3 | * Copyright 2020, Jan Schiefer, Keysight Technologies, Inc.
4 | * Copyright 2020- Martin Mathieson
5 | *
6 | * Wireshark - Network traffic analyzer
7 | * By Gerald Combs <gerald@wireshark.org>
8 | * Copyright 1998 Gerald Combs
9 | *
10 | * SPDX-License-Identifier: GPL-2.0-or-later
11 | */
12 |
13 | /*
14 | * Dissector for the O-RAN Fronthaul CUS protocol specification.
15 | * See https://specifications.o-ran.org/specifications, WG4, Fronthaul Interfaces Workgroup
16 | * The current implementation is based on the ORAN-WG4.CUS.0-v17.01 specification.
17 | * - haven't spotted any differences in v18.00
18 | * Note that other eCPRI message types are handled in packet-ecpri.c
19 | */
20 |
21 | #include <config.h>
22 |
23 | #include <math.h>
24 |
25 | #include <epan/packet.h>
26 | #include <epan/expert.h>
27 | #include <epan/prefs.h>
28 | #include <epan/tap.h>
29 |
30 | #include <epan/tfs.h>
31 |
32 | #include <wsutil/ws_roundup.h>
33 | #include <wsutil/ws_padding_to.h>
34 |
35 | #include "epan/dissectors/packet-oran.h"
36 |
37 | /* N.B. dissector preferences are taking the place of (some) M-plane parameters, so unfortunately it can be
38 | * fiddly to get the preferences into a good state to decode a given capture..
39 | * TODO:
40 | * - for U-Plane, track back to last C-Plane frame for that eAxC
41 | * - use udCompHdr values from C-Plane if not overridden by U-Plane?
42 | * N.B. this matching is tricky see 7.8.1 Coupling of C-Plane and U-Plane
43 | * - Radio transport layer (eCPRI) fragmentation / reassembly
44 | * - Detect/indicate signs of application layer fragmentation?
45 | * - Not handling M-plane setting for "little endian byte order" as applied to IQ samples and beam weights
46 | * - for section extensions, check more constraints (which other extension types appear with them, order)
47 | * - when some section extensions are present, some section header fields are effectively ignored - flag any remaining ("ignored, "shall")?
48 | * - re-order items (decl and hf definitions) to match spec order?
49 | * - track energy-saving status, and identify TRX or ASM commands as 'Sleep extension'
50 | */
51 |
52 | /* Prototypes */
53 | void proto_reg_handoff_oran(void);
54 | void proto_register_oran(void);
55 |
56 | /* Initialize the protocol and registered fields */
57 | static int proto_oran;
58 |
59 | static int oran_tap = -1;
60 |
61 | static int hf_oran_du_port_id;
62 | static int hf_oran_bandsector_id;
63 | static int hf_oran_cc_id;
64 | static int hf_oran_ru_port_id;
65 | static int hf_oran_sequence_id;
66 | static int hf_oran_e_bit;
67 | static int hf_oran_subsequence_id;
68 | static int hf_oran_previous_frame;
69 |
70 |
71 | static int hf_oran_data_direction;
72 | static int hf_oran_payload_version;
73 | static int hf_oran_filter_index;
74 | static int hf_oran_frame_id;
75 | static int hf_oran_subframe_id;
76 | static int hf_oran_slot_id;
77 | static int hf_oran_slot_within_frame;
78 | static int hf_oran_start_symbol_id;
79 | static int hf_oran_numberOfSections;
80 | static int hf_oran_sectionType;
81 |
82 | static int hf_oran_udCompHdr;
83 | static int hf_oran_udCompHdrIqWidth;
84 | static int hf_oran_udCompHdrIqWidth_pref;
85 | static int hf_oran_udCompHdrMeth;
86 | static int hf_oran_udCompHdrMeth_pref;
87 | static int hf_oran_udCompLen;
88 | static int hf_oran_numberOfUEs;
89 | static int hf_oran_timeOffset;
90 | static int hf_oran_frameStructure_fft;
91 | static int hf_oran_frameStructure_subcarrier_spacing;
92 | static int hf_oran_cpLength;
93 | static int hf_oran_timing_header;
94 | static int hf_oran_section_id;
95 | static int hf_oran_rb;
96 | static int hf_oran_symInc;
97 | static int hf_oran_startPrbc;
98 | static int hf_oran_reMask_re1;
99 | static int hf_oran_reMask_re2;
100 | static int hf_oran_reMask_re3;
101 | static int hf_oran_reMask_re4;
102 | static int hf_oran_reMask_re5;
103 | static int hf_oran_reMask_re6;
104 | static int hf_oran_reMask_re7;
105 | static int hf_oran_reMask_re8;
106 | static int hf_oran_reMask_re9;
107 | static int hf_oran_reMask_re10;
108 | static int hf_oran_reMask_re11;
109 | static int hf_oran_reMask_re12;
110 | static int hf_oran_reMask;
111 | static int hf_oran_numPrbc;
112 | static int hf_oran_numSymbol;
113 | static int hf_oran_ef;
114 | static int hf_oran_beamId;
115 |
116 | static int hf_oran_sinrCompHdrIqWidth_pref;
117 | static int hf_oran_sinrCompHdrMeth_pref;
118 |
119 | static int hf_oran_ciCompHdr;
120 | static int hf_oran_ciCompHdrIqWidth;
121 | static int hf_oran_ciCompHdrMeth;
122 | static int hf_oran_ciCompOpt;
123 |
124 | static int hf_oran_extension;
125 | static int hf_oran_exttype;
126 | static int hf_oran_extlen;
127 |
128 | static int hf_oran_bfw_bundle;
129 | static int hf_oran_bfw_bundle_id;
130 | static int hf_oran_bfw;
131 | static int hf_oran_bfw_i;
132 | static int hf_oran_bfw_q;
133 |
134 | static int hf_oran_ueId;
135 | static int hf_oran_freqOffset;
136 | static int hf_oran_regularizationFactor;
137 | static int hf_oran_laaMsgType;
138 | static int hf_oran_laaMsgLen;
139 | static int hf_oran_lbtHandle;
140 | static int hf_oran_lbtDeferFactor;
141 | static int hf_oran_lbtBackoffCounter;
142 | static int hf_oran_lbtOffset;
143 | static int hf_oran_MCOT;
144 | static int hf_oran_lbtMode;
145 | static int hf_oran_sfnSfEnd;
146 | static int hf_oran_lbtPdschRes;
147 | static int hf_oran_sfStatus;
148 | static int hf_oran_initialPartialSF;
149 | static int hf_oran_lbtDrsRes;
150 | static int hf_oran_lbtBufErr;
151 | static int hf_oran_lbtTrafficClass;
152 | static int hf_oran_lbtCWConfig_H;
153 | static int hf_oran_lbtCWConfig_T;
154 | static int hf_oran_lbtCWR_Rst;
155 |
156 | static int hf_oran_reserved;
157 | static int hf_oran_reserved_1bit;
158 | static int hf_oran_reserved_2bits;
159 | static int hf_oran_reserved_3bits;
160 | static int hf_oran_reserved_4bits;
161 | static int hf_oran_reserved_last_4bits;
162 | static int hf_oran_reserved_last_5bits;
163 | static int hf_oran_reserved_6bits;
164 | static int hf_oran_reserved_last_6bits;
165 | static int hf_oran_reserved_7bits;
166 | static int hf_oran_reserved_last_7bits;
167 | static int hf_oran_reserved_8bits;
168 | static int hf_oran_reserved_16bits;
169 | static int hf_oran_reserved_15bits;
170 | static int hf_oran_reserved_bit1;
171 | static int hf_oran_reserved_bit2;
172 | static int hf_oran_reserved_bit4;
173 | static int hf_oran_reserved_bit5;
174 | static int hf_oran_reserved_bits123;
175 | static int hf_oran_reserved_bits456;
176 |
177 | static int hf_oran_bundle_offset;
178 | static int hf_oran_cont_ind;
179 |
180 | static int hf_oran_bfwCompHdr;
181 | static int hf_oran_bfwCompHdr_iqWidth;
182 | static int hf_oran_bfwCompHdr_compMeth;
183 | static int hf_oran_symbolId;
184 | static int hf_oran_startPrbu;
185 | static int hf_oran_numPrbu;
186 |
187 | static int hf_oran_udCompParam;
188 | static int hf_oran_sReSMask;
189 | static int hf_oran_sReSMask_re12;
190 | static int hf_oran_sReSMask_re11;
191 | static int hf_oran_sReSMask_re10;
192 | static int hf_oran_sReSMask_re9;
193 | static int hf_oran_sReSMask_re8;
194 | static int hf_oran_sReSMask_re7;
195 | static int hf_oran_sReSMask_re6;
196 | static int hf_oran_sReSMask_re5;
197 | static int hf_oran_sReSMask_re4;
198 | static int hf_oran_sReSMask_re3;
199 | static int hf_oran_sReSMask_re2;
200 | static int hf_oran_sReSMask_re1;
201 |
202 | static int hf_oran_sReSMask1;
203 | static int hf_oran_sReSMask2;
204 | static int hf_oran_sReSMask1_2_re12;
205 | static int hf_oran_sReSMask1_2_re11;
206 | static int hf_oran_sReSMask1_2_re10;
207 | static int hf_oran_sReSMask1_2_re9;
208 |
209 | static int hf_oran_bfwCompParam;
210 |
211 | static int hf_oran_iSample;
212 | static int hf_oran_qSample;
213 |
214 | static int hf_oran_ciCompParam;
215 |
216 | static int hf_oran_blockScaler;
217 | static int hf_oran_compBitWidth;
218 | static int hf_oran_compShift;
219 |
220 | static int hf_oran_active_beamspace_coefficient_n1;
221 | static int hf_oran_active_beamspace_coefficient_n2;
222 | static int hf_oran_active_beamspace_coefficient_n3;
223 | static int hf_oran_active_beamspace_coefficient_n4;
224 | static int hf_oran_active_beamspace_coefficient_n5;
225 | static int hf_oran_active_beamspace_coefficient_n6;
226 | static int hf_oran_active_beamspace_coefficient_n7;
227 | static int hf_oran_active_beamspace_coefficient_n8;
228 | static int hf_oran_activeBeamspaceCoefficientMask;
229 | static int hf_oran_activeBeamspaceCoefficientMask_bits_set;
230 |
231 | static int hf_oran_se6_repetition;
232 |
233 | static int hf_oran_rbgSize;
234 | static int hf_oran_rbgMask;
235 | static int hf_oran_noncontig_priority;
236 |
237 | static int hf_oran_symbol_mask;
238 | static int hf_oran_symbol_mask_s13;
239 | static int hf_oran_symbol_mask_s12;
240 | static int hf_oran_symbol_mask_s11;
241 | static int hf_oran_symbol_mask_s10;
242 | static int hf_oran_symbol_mask_s9;
243 | static int hf_oran_symbol_mask_s8;
244 | static int hf_oran_symbol_mask_s7;
245 | static int hf_oran_symbol_mask_s6;
246 | static int hf_oran_symbol_mask_s5;
247 | static int hf_oran_symbol_mask_s4;
248 | static int hf_oran_symbol_mask_s3;
249 | static int hf_oran_symbol_mask_s2;
250 | static int hf_oran_symbol_mask_s1;
251 | static int hf_oran_symbol_mask_s0;
252 |
253 | static int hf_oran_exponent;
254 | static int hf_oran_iq_user_data;
255 |
256 | static int hf_oran_disable_bfws;
257 | static int hf_oran_rad;
258 | static int hf_oran_num_bund_prbs;
259 | static int hf_oran_beam_id;
260 | static int hf_oran_num_weights_per_bundle;
261 |
262 | static int hf_oran_ack_nack_req_id;
263 |
264 | static int hf_oran_frequency_range;
265 | static int hf_oran_off_start_prb;
266 | static int hf_oran_num_prb;
267 |
268 | static int hf_oran_samples_prb;
269 | static int hf_oran_ciSample;
270 | static int hf_oran_ciIsample;
271 | static int hf_oran_ciQsample;
272 |
273 | static int hf_oran_beamGroupType;
274 | static int hf_oran_numPortc;
275 |
276 | static int hf_oran_csf;
277 | static int hf_oran_modcompscaler;
278 |
279 | static int hf_oran_modcomp_param_set;
280 | static int hf_oran_mc_scale_re_mask_re1;
281 | static int hf_oran_mc_scale_re_mask_re2;
282 | static int hf_oran_mc_scale_re_mask_re3;
283 | static int hf_oran_mc_scale_re_mask_re4;
284 | static int hf_oran_mc_scale_re_mask_re5;
285 | static int hf_oran_mc_scale_re_mask_re6;
286 | static int hf_oran_mc_scale_re_mask_re7;
287 | static int hf_oran_mc_scale_re_mask_re8;
288 | static int hf_oran_mc_scale_re_mask_re9;
289 | static int hf_oran_mc_scale_re_mask_re10;
290 | static int hf_oran_mc_scale_re_mask_re11;
291 | static int hf_oran_mc_scale_re_mask_re12;
292 | static int hf_oran_mc_scale_re_mask_re1_even;
293 | static int hf_oran_mc_scale_re_mask_re2_even;
294 | static int hf_oran_mc_scale_re_mask_re3_even;
295 | static int hf_oran_mc_scale_re_mask_re4_even;
296 | static int hf_oran_mc_scale_re_mask_re5_even;
297 | static int hf_oran_mc_scale_re_mask_re6_even;
298 | static int hf_oran_mc_scale_re_mask_re7_even;
299 | static int hf_oran_mc_scale_re_mask_re8_even;
300 | static int hf_oran_mc_scale_re_mask_re9_even;
301 | static int hf_oran_mc_scale_re_mask_re10_even;
302 | static int hf_oran_mc_scale_re_mask_re11_even;
303 | static int hf_oran_mc_scale_re_mask_re12_even;
304 |
305 | static int hf_oran_mc_scale_re_mask;
306 | static int hf_oran_mc_scale_re_mask_even;
307 |
308 | static int hf_oran_mc_scale_offset;
309 |
310 | static int hf_oran_eAxC_mask;
311 | static int hf_oran_technology;
312 | static int hf_oran_nullLayerInd;
313 |
314 | static int hf_oran_se19_repetition;
315 | static int hf_oran_portReMask;
316 | static int hf_oran_portSymbolMask;
317 |
318 | static int hf_oran_ext19_port;
319 |
320 | static int hf_oran_prb_allocation;
321 | static int hf_oran_nextSymbolId;
322 | static int hf_oran_nextStartPrbc;
323 |
324 | static int hf_oran_puncPattern;
325 | static int hf_oran_numPuncPatterns;
326 | static int hf_oran_symbolMask_ext20;
327 | static int hf_oran_startPuncPrb;
328 | static int hf_oran_numPuncPrb;
329 | static int hf_oran_puncReMask;
330 | static int hf_oran_multiSDScope;
331 | static int hf_oran_RbgIncl;
332 |
333 | static int hf_oran_ci_prb_group_size;
334 | static int hf_oran_prg_size_st5;
335 | static int hf_oran_prg_size_st6;
336 |
337 | static int hf_oran_num_ueid;
338 |
339 | static int hf_oran_antMask;
340 |
341 | static int hf_oran_transmissionWindowOffset;
342 | static int hf_oran_transmissionWindowSize;
343 | static int hf_oran_toT;
344 |
345 | static int hf_oran_bfaCompHdr;
346 | static int hf_oran_bfAzPtWidth;
347 | static int hf_oran_bfZePtWidth;
348 | static int hf_oran_bfAz3ddWidth;
349 | static int hf_oran_bfZe3ddWidth;
350 | static int hf_oran_bfAzPt;
351 | static int hf_oran_bfZePt;
352 | static int hf_oran_bfAz3dd;
353 | static int hf_oran_bfZe3dd;
354 | static int hf_oran_bfAzSl;
355 | static int hf_oran_bfZeSl;
356 |
357 | static int hf_oran_cmd_scope;
358 | static int hf_oran_number_of_st4_cmds;
359 |
360 | static int hf_oran_st4_cmd_header;
361 | static int hf_oran_st4_cmd_type;
362 | static int hf_oran_st4_cmd_len;
363 | static int hf_oran_st4_cmd_num_slots;
364 | static int hf_oran_st4_cmd_ack_nack_req_id;
365 |
366 | static int hf_oran_st4_cmd;
367 |
368 | static int hf_oran_sleepmode_trx;
369 | static int hf_oran_sleepmode_asm;
370 | static int hf_oran_log2maskbits;
371 | static int hf_oran_num_slots_ext;
372 | static int hf_oran_antMask_trx_control;
373 |
374 | static int hf_oran_ready;
375 | static int hf_oran_number_of_acks;
376 | static int hf_oran_number_of_nacks;
377 | static int hf_oran_ackid;
378 | static int hf_oran_nackid;
379 |
380 | static int hf_oran_acknack_request_frame;
381 | static int hf_oran_acknack_request_time;
382 | static int hf_oran_acknack_request_type;
383 | static int hf_oran_acknack_response_frame;
384 | static int hf_oran_acknack_response_time;
385 |
386 | static int hf_oran_disable_tdbfns;
387 | static int hf_oran_td_beam_group;
388 | static int hf_oran_disable_tdbfws;
389 | static int hf_oran_td_beam_num;
390 |
391 | static int hf_oran_dir_pattern;
392 | static int hf_oran_guard_pattern;
393 |
394 | static int hf_oran_ecpri_pcid;
395 | static int hf_oran_ecpri_rtcid;
396 | static int hf_oran_ecpri_seqid;
397 |
398 | static int hf_oran_num_sym_prb_pattern;
399 | static int hf_oran_prb_mode;
400 | static int hf_oran_sym_prb_pattern;
401 | static int hf_oran_sym_mask;
402 | static int hf_oran_num_mc_scale_offset;
403 | static int hf_oran_prb_pattern;
404 | static int hf_oran_prb_block_offset;
405 | static int hf_oran_prb_block_size;
406 |
407 | static int hf_oran_codebook_index;
408 | static int hf_oran_layerid;
409 | static int hf_oran_numlayers;
410 | static int hf_oran_txscheme;
411 | static int hf_oran_crs_remask;
412 | static int hf_oran_crs_shift;
413 | static int hf_oran_crs_symnum;
414 | static int hf_oran_beamid_ap1;
415 | static int hf_oran_beamid_ap2;
416 | static int hf_oran_beamid_ap3;
417 |
418 | static int hf_oran_port_list_index;
419 | static int hf_oran_alpn_per_sym;
420 | static int hf_oran_ant_dmrs_snr;
421 | static int hf_oran_user_group_size;
422 | static int hf_oran_user_group_id;
423 | static int hf_oran_entry_type;
424 | static int hf_oran_dmrs_port_number;
425 | static int hf_oran_ueid_reset;
426 |
427 | static int hf_oran_dmrs_symbol_mask;
428 | static int hf_oran_dmrs_symbol_mask_s13;
429 | static int hf_oran_dmrs_symbol_mask_s12;
430 | static int hf_oran_dmrs_symbol_mask_s11;
431 | static int hf_oran_dmrs_symbol_mask_s10;
432 | static int hf_oran_dmrs_symbol_mask_s9;
433 | static int hf_oran_dmrs_symbol_mask_s8;
434 | static int hf_oran_dmrs_symbol_mask_s7;
435 | static int hf_oran_dmrs_symbol_mask_s6;
436 | static int hf_oran_dmrs_symbol_mask_s5;
437 | static int hf_oran_dmrs_symbol_mask_s4;
438 | static int hf_oran_dmrs_symbol_mask_s3;
439 | static int hf_oran_dmrs_symbol_mask_s2;
440 | static int hf_oran_dmrs_symbol_mask_s1;
441 | static int hf_oran_dmrs_symbol_mask_s0;
442 |
443 | static int hf_oran_scrambling;
444 | static int hf_oran_nscid;
445 | static int hf_oran_dtype;
446 | static int hf_oran_cmd_without_data;
447 | static int hf_oran_lambda;
448 | static int hf_oran_first_prb;
449 | static int hf_oran_last_prb;
450 | static int hf_oran_low_papr_type;
451 | static int hf_oran_hopping_mode;
452 |
453 | static int hf_oran_tx_win_for_on_air_symbol_l;
454 | static int hf_oran_tx_win_for_on_air_symbol_r;
455 |
456 | static int hf_oran_num_fo_fb;
457 | static int hf_oran_freq_offset_fb;
458 |
459 | static int hf_oran_num_ue_sinr_rpt;
460 | static int hf_oran_num_sinr_per_prb;
461 | static int hf_oran_num_sinr_per_prb_right;
462 |
463 | static int hf_oran_sinr_value;
464 |
465 | static int hf_oran_measurement_report;
466 | static int hf_oran_mf;
467 | static int hf_oran_meas_data_size;
468 | static int hf_oran_meas_type_id;
469 | static int hf_oran_ipn_power;
470 | static int hf_oran_ue_tae;
471 | static int hf_oran_ue_layer_power;
472 | static int hf_oran_num_elements;
473 | static int hf_oran_ant_dmrs_snr_val;
474 | static int hf_oran_ue_freq_offset;
475 |
476 | static int hf_oran_measurement_command;
477 |
478 | static int hf_oran_beam_type;
479 | static int hf_oran_meas_cmd_size;
480 |
481 | static int hf_oran_symbol_reordering_layer;
482 | static int hf_oran_dmrs_entry;
483 |
484 | static int hf_oran_c_section_common;
485 | static int hf_oran_c_section;
486 | static int hf_oran_u_section;
487 |
488 | static int hf_oran_u_section_ul_symbol_time;
489 | static int hf_oran_u_section_ul_symbol_frames;
490 | static int hf_oran_u_section_ul_symbol_first_frame;
491 | static int hf_oran_u_section_ul_symbol_last_frame;
492 |
493 | /* Computed fields */
494 | static int hf_oran_c_eAxC_ID;
495 | static int hf_oran_refa;
496 |
497 | /* Convenient fields for filtering, mostly shown as hidden */
498 | static int hf_oran_cplane;
499 | static int hf_oran_uplane;
500 | static int hf_oran_bf; /* to match frames that configure beamforming in any way */
501 | static int hf_oran_zero_prb;
502 |
503 | static int hf_oran_ul_cplane_ud_comp_hdr_frame;
504 |
505 | /* Initialize the subtree pointers */
506 | static int ett_oran;
507 | static int ett_oran_ecpri_rtcid;
508 | static int ett_oran_ecpri_pcid;
509 | static int ett_oran_ecpri_seqid;
510 | static int ett_oran_section;
511 | static int ett_oran_section_type;
512 | static int ett_oran_u_timing;
513 | static int ett_oran_u_section;
514 | static int ett_oran_u_prb;
515 | static int ett_oran_iq;
516 | static int ett_oran_bfw_bundle;
517 | static int ett_oran_bfw;
518 | static int ett_oran_frequency_range;
519 | static int ett_oran_prb_cisamples;
520 | static int ett_oran_cisample;
521 | static int ett_oran_udcomphdr;
522 | static int ett_oran_udcompparam;
523 | static int ett_oran_cicomphdr;
524 | static int ett_oran_cicompparam;
525 | static int ett_oran_bfwcomphdr;
526 | static int ett_oran_bfwcompparam;
527 | static int ett_oran_ext19_port;
528 | static int ett_oran_prb_allocation;
529 | static int ett_oran_punc_pattern;
530 | static int ett_oran_bfacomphdr;
531 | static int ett_oran_modcomp_param_set;
532 | static int ett_oran_st4_cmd_header;
533 | static int ett_oran_st4_cmd;
534 | static int ett_oran_sym_prb_pattern;
535 | static int ett_oran_measurement_report;
536 | static int ett_oran_measurement_command;
537 | static int ett_oran_sresmask;
538 | static int ett_oran_c_section_common;
539 | static int ett_oran_c_section;
540 | static int ett_oran_remask;
541 | static int ett_oran_mc_scale_remask;
542 | static int ett_oran_symbol_reordering_layer;
543 | static int ett_oran_dmrs_entry;
544 | static int ett_oran_dmrs_symbol_mask;
545 | static int ett_oran_symbol_mask;
546 | static int ett_active_beamspace_coefficient_mask;
547 |
548 |
549 | /* Don't want all extensions to open and close together. Use extType-1 entry */
550 | static int ett_oran_c_section_extension[HIGHEST_EXTTYPE28];
551 |
552 | /* Expert info */
553 | static expert_field ei_oran_unsupported_bfw_compression_method;
554 | static expert_field ei_oran_invalid_sample_bit_width;
555 | static expert_field ei_oran_reserved_numBundPrb;
556 | static expert_field ei_oran_extlen_wrong;
557 | static expert_field ei_oran_invalid_eaxc_bit_width;
558 | static expert_field ei_oran_extlen_zero;
559 | static expert_field ei_oran_rbg_size_reserved;
560 | static expert_field ei_oran_frame_length;
561 | static expert_field ei_oran_numprbc_ext21_zero;
562 | static expert_field ei_oran_ci_prb_group_size_reserved;
563 | static expert_field ei_oran_st8_nackid;
564 | static expert_field ei_oran_st4_no_cmds;
565 | static expert_field ei_oran_st4_zero_len_cmd;
566 | static expert_field ei_oran_st4_wrong_len_cmd;
567 | static expert_field ei_oran_st4_unknown_cmd;
568 | static expert_field ei_oran_mcot_out_of_range;
569 | static expert_field ei_oran_se10_unknown_beamgrouptype;
570 | static expert_field ei_oran_se10_not_allowed;
571 | static expert_field ei_oran_start_symbol_id_not_zero;
572 | static expert_field ei_oran_trx_control_cmd_scope;
573 | static expert_field ei_oran_unhandled_se;
574 | static expert_field ei_oran_bad_symbolmask;
575 | static expert_field ei_oran_numslots_not_zero;
576 | static expert_field ei_oran_version_unsupported;
577 | static expert_field ei_oran_laa_msg_type_unsupported;
578 | static expert_field ei_oran_se_on_unsupported_st;
579 | static expert_field ei_oran_cplane_unexpected_sequence_number_ul;
580 | static expert_field ei_oran_cplane_unexpected_sequence_number_dl;
581 | static expert_field ei_oran_uplane_unexpected_sequence_number_ul;
582 | static expert_field ei_oran_uplane_unexpected_sequence_number_dl;
583 | static expert_field ei_oran_acknack_no_request;
584 | static expert_field ei_oran_udpcomphdr_should_be_zero;
585 | static expert_field ei_oran_radio_fragmentation_c_plane;
586 | static expert_field ei_oran_radio_fragmentation_u_plane;
587 | static expert_field ei_oran_lastRbdid_out_of_range;
588 | static expert_field ei_oran_rbgMask_beyond_last_rbdid;
589 | static expert_field ei_oran_unexpected_measTypeId;
590 | static expert_field ei_oran_unsupported_compression_method;
591 | static expert_field ei_oran_ud_comp_len_wrong_size;
592 | static expert_field ei_oran_sresmask2_not_zero_with_rb;
593 | static expert_field ei_oran_st6_rb_shall_be_0;
594 | static expert_field ei_oran_st9_not_ul;
595 | static expert_field ei_oran_st10_numsymbol_not_14;
596 | static expert_field ei_oran_st10_startsymbolid_not_0;
597 | static expert_field ei_oran_st10_not_ul;
598 | static expert_field ei_oran_se24_nothing_to_inherit;
599 | static expert_field ei_oran_num_sinr_per_prb_unknown;
600 | static expert_field ei_oran_start_symbol_id_bits_ignored;
601 | static expert_field ei_oran_user_group_id_reserved_value;
602 | static expert_field ei_oran_port_list_index_zero;
603 | static expert_field ei_oran_ul_uplane_symbol_too_long;
604 |
605 |
606 | /* These are the message types handled by this dissector */
607 | #define ECPRI_MT_IQ_DATA0 0
608 | #define ECPRI_MT_RT_CTRL_DATA2 2
609 |
610 |
611 | /* Preference settings - try to set reasonable defaults */
612 | static unsigned pref_du_port_id_bits = 4;
613 | static unsigned pref_bandsector_id_bits = 4;
614 | static unsigned pref_cc_id_bits = 4;
615 | static unsigned pref_ru_port_id_bits = 4;
616 |
617 | /* TODO: ideally should be per-flow */
618 | static unsigned pref_sample_bit_width_uplink = 14;
619 | static unsigned pref_sample_bit_width_downlink = 14;
620 | static unsigned pref_sample_bit_width_sinr = 14;
621 |
622 | /* 8.3.3.15 Compression schemes */
623 | #define COMP_NONE0 0
624 | #define COMP_BLOCK_FP1 1
625 | #define COMP_BLOCK_SCALE2 2
626 | #define COMP_U_LAW3 3
627 | #define COMP_MODULATION4 4
628 | #define BFP_AND_SELECTIVE_RE5 5
629 | #define MOD_COMPR_AND_SELECTIVE_RE6 6
630 | #define BFP_AND_SELECTIVE_RE_WITH_MASKS7 7
631 | #define MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8 8
632 |
633 | /* TODO: these ideally should be per-flow too */
634 | static int pref_iqCompressionUplink = COMP_BLOCK_FP1;
635 | static int pref_iqCompressionDownlink = COMP_BLOCK_FP1;
636 |
637 | static int pref_iqCompressionSINR = COMP_BLOCK_FP1;
638 |
639 |
640 | /* Is udCompHeader present (both directions) */
641 | static int pref_includeUdCompHeaderUplink = 2; /* start heuristic */
642 | static int pref_includeUdCompHeaderDownlink = 2; /* start heuristic */
643 |
644 | static unsigned pref_data_plane_section_total_rbs = 273;
645 | static unsigned pref_num_bf_antennas = 32;
646 | static bool_Bool pref_showIQSampleValues = true1;
647 |
648 | /* Based upon m-plane param, so will be system-wide */
649 | static int pref_support_udcompLen = 2; /* start heuristic, can force other settings if necessary */
650 | static bool_Bool udcomplen_heuristic_result_set = false0;
651 | static bool_Bool udcomplen_heuristic_result = false0;
652 |
653 | /* st6-4byte-alignment-required */
654 | static bool_Bool st6_4byte_alignment = false0;
655 |
656 | /* Requested, allows I/Q to be stored as integers.. */
657 | static bool_Bool show_unscaled_values = false0;
658 |
659 | /* Initialized off. Timing is in microseconds. */
660 | static unsigned us_allowed_for_ul_in_symbol = 0;
661 |
662 | static const enum_val_t dl_compression_options[] = {
663 | { "COMP_NONE", "No Compression", COMP_NONE0 },
664 | { "COMP_BLOCK_FP", "Block Floating Point Compression", COMP_BLOCK_FP1 },
665 | { "COMP_BLOCK_SCALE", "Block Scaling Compression", COMP_BLOCK_SCALE2 },
666 | { "COMP_U_LAW", "u-Law Compression", COMP_U_LAW3 },
667 | { "COMP_MODULATION", "Modulation Compression", COMP_MODULATION4 },
668 | { "BFP_AND_SELECTIVE_RE", "Block Floating Point + selective RE sending", BFP_AND_SELECTIVE_RE5 },
669 | { "MOD_COMPR_AND_SELECTIVE_RE", "Modulation Compression + selective RE sending", MOD_COMPR_AND_SELECTIVE_RE6 },
670 | { "BFP_AND_SELECTIVE_RE_WITH_MASKS", "Block Floating Point + selective RE sending with masks in section header", BFP_AND_SELECTIVE_RE_WITH_MASKS7 },
671 | { "MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS", "Modulation Compression + selective RE sending with masks in section header", MOD_COMPR_AND_SELECTIVE_RE6 },
672 | { NULL((void*)0), NULL((void*)0), 0 }
673 | };
674 |
675 | static const enum_val_t ul_compression_options[] = {
676 | { "COMP_NONE", "No Compression", COMP_NONE0 },
677 | { "COMP_BLOCK_FP", "Block Floating Point Compression", COMP_BLOCK_FP1 },
678 | { "COMP_BLOCK_SCALE", "Block Scaling Compression", COMP_BLOCK_SCALE2 },
679 | { "COMP_U_LAW", "u-Law Compression", COMP_U_LAW3 },
680 | { "BFP_AND_SELECTIVE_RE", "Block Floating Point + selective RE sending", BFP_AND_SELECTIVE_RE5 },
681 | { "BFP_AND_SELECTIVE_RE_WITH_MASKS", "Block Floating Point + selective RE sending with masks in section header", BFP_AND_SELECTIVE_RE_WITH_MASKS7 },
682 | { NULL((void*)0), NULL((void*)0), 0 }
683 | };
684 |
685 | static const enum_val_t udcomplen_support_options[] = {
686 | { "NOT_SUPPORTED", "Not Supported", 0 },
687 | { "SUPPORTED", "Supported", 1 },
688 | { "HEURISTIC", "Attempt Heuristic", 2 },
689 | { NULL((void*)0), NULL((void*)0), 0 }
690 | };
691 |
692 | static const enum_val_t udcomphdr_present_options[] = {
693 | { "NOT_PRESENT", "Not Present", 0 },
694 | { "PRESENT", "Present", 1 },
695 | { "HEURISTIC", "Attempt Heuristic", 2 },
696 | { NULL((void*)0), NULL((void*)0), 0 }
697 | };
698 |
699 |
700 |
701 | static const value_string e_bit[] = {
702 | { 0, "More fragments follow" },
703 | { 1, "Last fragment" },
704 | { 0, NULL((void*)0)}
705 | };
706 |
707 | #define DIR_UPLINK0 0
708 | #define DIR_DOWNLINK1 1
709 |
710 |
711 | static const value_string data_direction_vals[] = {
712 | { DIR_UPLINK0, "Uplink" }, /* gNB Rx */
713 | { DIR_DOWNLINK1, "Downlink" }, /* gNB Tx */
714 | { 0, NULL((void*)0)}
715 | };
716 |
717 | static const value_string rb_vals[] = {
718 | { 0, "Every RB used" },
719 | { 1, "Every other RB used" },
720 | { 0, NULL((void*)0)}
721 | };
722 |
723 | static const value_string sym_inc_vals[] = {
724 | { 0, "Use the current symbol number" },
725 | { 1, "Increment the current symbol number" },
726 | { 0, NULL((void*)0)}
727 | };
728 |
729 | static const value_string lbtMode_vals[] = {
730 | { 0, "Full LBT (regular LBT, sending reservation signal until the beginning of the SF/slot)" },
731 | { 1, "Partial LBT (looking back 25 usec prior to transmission" },
732 | { 2, "Partial LBT (looking back 34 usec prior to transmission" },
733 | { 3, "Full LBT and stop (regular LBT, without sending reservation signal" },
734 | { 0, NULL((void*)0)}
735 | };
736 |
737 | static const range_string filter_indices[] = {
738 | {0, 0, "standard channel filter"},
739 | {1, 1, "UL filter for PRACH preamble formats 0, 1, 2; min. passband 839 x 1.25kHz = 1048.75 kHz"},
740 | {2, 2, "UL filter for PRACH preamble format 3, min. passband 839 x 5 kHz = 4195 kHz"},
741 | {3, 3, "UL filter for PRACH preamble formats A1, A2, A3, B1, B2, B3, B4, C0, C2; min. passband 139 x \u0394fRA"},
742 | {4, 4, "UL filter for NPRACH 0, 1; min. passband 48 x 3.75KHz = 180 KHz"},
743 | {5, 5, "UL filter for PRACH preamble formats"},
744 | {8, 8, "UL filter NPUSCH"},
745 | {9, 9, "Mixed numerology and other channels except PRACH and NB-IoT"},
746 | {9, 15, "Reserved"},
747 | {0, 0, NULL((void*)0)}
748 | };
749 |
750 | static const range_string section_types[] = {
751 | { SEC_C_UNUSED_RB, SEC_C_UNUSED_RB, "Unused Resource Blocks or symbols in Downlink or Uplink" },
752 | { SEC_C_NORMAL, SEC_C_NORMAL, "Most DL/UL radio channels" },
753 | { SEC_C_RSVD2, SEC_C_RSVD2, "Reserved for future use" },
754 | { SEC_C_PRACH, SEC_C_PRACH, "PRACH and mixed-numerology channels" },
755 | { SEC_C_SLOT_CONTROL, SEC_C_SLOT_CONTROL, "Slot Configuration Control" },
756 | { SEC_C_UE_SCHED, SEC_C_UE_SCHED, "UE scheduling information (UE-ID assignment to section)" },
757 | { SEC_C_CH_INFO, SEC_C_CH_INFO, "Channel information" },
758 | { SEC_C_LAA, SEC_C_LAA, "LAA (License Assisted Access)" },
759 | { SEC_C_ACK_NACK_FEEDBACK, SEC_C_ACK_NACK_FEEDBACK, "ACK/NACK Feedback" },
760 | { SEC_C_SINR_REPORTING, SEC_C_SINR_REPORTING, "SINR Reporting" },
761 | { SEC_C_RRM_MEAS_REPORTS, SEC_C_RRM_MEAS_REPORTS, "RRM Measurement Reports" },
762 | { SEC_C_REQUEST_RRM_MEAS, SEC_C_REQUEST_RRM_MEAS, "Request RRM Measurements" },
763 | { 12, 255, "Reserved for future use" },
764 | { 0, 0, NULL((void*)0)} };
765 |
766 | static const range_string section_types_short[] = {
767 | { SEC_C_UNUSED_RB, SEC_C_UNUSED_RB, "(Unused RBs) " },
768 | { SEC_C_NORMAL, SEC_C_NORMAL, "(Most channels) " },
769 | { SEC_C_RSVD2, SEC_C_RSVD2, "(reserved) " },
770 | { SEC_C_PRACH, SEC_C_PRACH, "(PRACH/mixed-\u03bc)" },
771 | { SEC_C_SLOT_CONTROL, SEC_C_SLOT_CONTROL, "(Slot info) " },
772 | { SEC_C_UE_SCHED, SEC_C_UE_SCHED, "(UE scheduling info)" },
773 | { SEC_C_CH_INFO, SEC_C_CH_INFO, "(Channel info) " },
774 | { SEC_C_LAA, SEC_C_LAA, "(LAA) " },
775 | { SEC_C_ACK_NACK_FEEDBACK, SEC_C_ACK_NACK_FEEDBACK, "(ACK/NACK) " },
776 | { SEC_C_SINR_REPORTING, SEC_C_SINR_REPORTING, "(SINR Reporting) " },
777 | { SEC_C_RRM_MEAS_REPORTS, SEC_C_RRM_MEAS_REPORTS, "(RRM Meas Reports) " },
778 | { SEC_C_REQUEST_RRM_MEAS, SEC_C_REQUEST_RRM_MEAS, "(Req RRM Meas) " },
779 | { 12, 255, "Reserved for future use" },
780 | { 0, 0, NULL((void*)0) }
781 | };
782 |
783 | static const range_string ud_comp_header_width[] = {
784 | {0, 0, "I and Q are each 16 bits wide"},
785 | {1, 15, "Bit width of I and Q"},
786 | {0, 0, NULL((void*)0)} };
787 |
788 | /* Table 8.3.3.13-3 */
789 | static const range_string ud_comp_header_meth[] = {
790 | {COMP_NONE0, COMP_NONE0, "No compression" },
791 | {COMP_BLOCK_FP1, COMP_BLOCK_FP1, "Block floating point compression" },
792 | {COMP_BLOCK_SCALE2, COMP_BLOCK_SCALE2, "Block scaling" },
793 | {COMP_U_LAW3, COMP_U_LAW3, "Mu - law" },
794 | {COMP_MODULATION4, COMP_MODULATION4, "Modulation compression" },
795 | {BFP_AND_SELECTIVE_RE5, BFP_AND_SELECTIVE_RE5, "BFP + selective RE sending" },
796 | {MOD_COMPR_AND_SELECTIVE_RE6, MOD_COMPR_AND_SELECTIVE_RE6, "mod-compr + selective RE sending" },
797 | {BFP_AND_SELECTIVE_RE_WITH_MASKS7, BFP_AND_SELECTIVE_RE_WITH_MASKS7, "BFP + selective RE sending with masks in section header" },
798 | {MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8, MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8, "mod-compr + selective RE sending with masks in section header"},
799 | {9, 15, "Reserved"},
800 | {0, 0, NULL((void*)0)}
801 | };
802 |
803 | /* Table 7.5.2.13-2 */
804 | static const range_string frame_structure_fft[] = {
805 | {0, 0, "Reserved (no FFT/iFFT processing)"},
806 | {1, 3, "Reserved"},
807 | {4, 4, "FFT size 16"},
808 | {5, 5, "FFT size 32"},
809 | {6, 6, "FFT size 64"},
810 | {7, 7, "FFT size 128"},
811 | {8, 8, "FFT size 256"},
812 | {9, 9, "FFT size 512"},
813 | {10, 10, "FFT size 1024"},
814 | {11, 11, "FFT size 2048"},
815 | {12, 12, "FFT size 4096"},
816 | {13, 13, "FFT size 1536"},
817 | {14, 14, "FFT size 3072"},
818 | {15, 15, "Reserved"},
819 | {0, 0, NULL((void*)0)}
820 | };
821 |
822 | /* Table 7.5.2.13-3 */
823 | static const range_string subcarrier_spacings[] = {
824 | { 0, 0, "SCS 15 kHz, 1 slot/subframe, slot length 1 ms" },
825 | { 1, 1, "SCS 30 kHz, 2 slots/subframe, slot length 500 \u03bcs" },
826 | { 2, 2, "SCS 60 kHz, 4 slots/subframe, slot length 250 \u03bcs" },
827 | { 3, 3, "SCS 120 kHz, 8 slots/subframe, slot length 125 \u03bcs" },
828 | { 4, 4, "SCS 240 kHz, 16 slots/subframe, slot length 62.5 \u03bcs" },
829 | { 5, 11, "Reserved" }, /* N.B., 5 was 480kHz in early spec versions */
830 | { 12, 12, "SCS 1.25 kHz, 1 slot/subframe, slot length 1 ms" },
831 | { 13, 13, "SCS 3.75 kHz(LTE - specific), 1 slot/subframe, slot length 1 ms" },
832 | { 14, 14, "SCS 5 kHz, 1 slot/subframe, slot length 1 ms" },
833 | { 15, 15, "SCS 7.5 kHz(LTE - specific), 1 slot/subframe, slot length 1 ms" },
834 | { 0, 0, NULL((void*)0) }
835 | };
836 |
837 | /* Table 7.5.3.14-1 laaMsgType definition */
838 | static const range_string laaMsgTypes[] = {
839 | {0, 0, "LBT_PDSCH_REQ - lls - O-DU to O-RU request to obtain a PDSCH channel"},
840 | {1, 1, "LBT_DRS_REQ - lls - O-DU to O-RU request to obtain the channel and send DRS"},
841 | {2, 2, "LBT_PDSCH_RSP - O-RU to O-DU response, channel acq success or failure"},
842 | {3, 3, "LBT_DRS_RSP - O-RU to O-DU response, DRS sending success or failure"},
843 | {4, 4, "LBT_Buffer_Error - O-RU to O-DU response, reporting buffer overflow"},
844 | {5, 5, "LBT_CWCONFIG_REQ - O-DU to O-RU request, congestion window configuration"},
845 | {6, 6, "LBT_CWCONFIG_RST - O-RU to O-DU request, congestion window config, response"},
846 | {7, 15, "reserved for future methods"},
847 | {0, 0, NULL((void*)0)}
848 | };
849 |
850 | static const range_string freq_offset_fb_values[] = {
851 | {0, 0, "no frequency offset"},
852 | {8000, 8000, "value not provided"},
853 | {1, 30000, "positive frequency offset, (0, +0.5] subcarrier"},
854 | {0x8ad0, 0xffff, "negative frequency offset, [-0.5, 0) subcarrier"},
855 | {0x0, 0xffff, "reserved"},
856 | {0, 0, NULL((void*)0)}
857 | };
858 |
859 | static const value_string num_sinr_per_prb_vals[] = {
860 | { 0, "1" },
861 | { 1, "2" },
862 | { 2, "3" },
863 | { 3, "4" },
864 | { 4, "6" },
865 | { 5, "12" },
866 | { 6, "reserved" },
867 | { 7, "reserved" },
868 | { 0, NULL((void*)0)}
869 | };
870 |
871 | static const value_string meas_type_id_vals[] = {
872 | { 1, "UE Timing Advance Error" },
873 | { 2, "UE Layer power" },
874 | { 3, "UE frequency offset" },
875 | { 4, "Interference plus Noise for allocated PRBs" },
876 | { 5, "Interference plus Noise for unallocated PRBs" },
877 | { 6, "DMRS SNR per antenna" },
878 | { 0, NULL((void*)0)}
879 | };
880 |
881 | static const value_string beam_type_vals[] = {
882 | { 0, "List of beamId values" },
883 | { 1, "Range of beamId values" },
884 | { 0, NULL((void*)0)}
885 | };
886 |
887 | /* 7.7.24.3 */
888 | static const value_string entry_type_vals[] = {
889 | { 0, "inherit config from preceding entry (2 or 3) ueIdReset=0" },
890 | { 1, "inherit config from preceding entry (2 or 3) ueIdReset=1" },
891 | { 2, "related parameters if have transform precoding disabled " },
892 | { 3, "related parameters if have transform precoding enabled " },
893 | { 0, NULL((void*)0)}
894 | };
895 |
896 |
897 | /* Table 7.6.1-1 */
898 | static const value_string exttype_vals[] = {
899 | {0, "Reserved"},
900 | {1, "Beamforming weights"},
901 | {2, "Beamforming attributes"},
902 | {3, "DL Precoding configuration parameters and indications"},
903 | {4, "Modulation compr. params"},
904 | {5, "Modulation compression additional scaling parameters"},
905 | {6, "Non-contiguous PRB allocation"},
906 | {7, "Multiple-eAxC designation"},
907 | {8, "Regularization factor"},
908 | {9, "Dynamic Spectrum Sharing parameters"},
909 | {10, "Multiple ports grouping"},
910 | {11, "Flexible BF weights"},
911 | {12, "Non-Contiguous PRB Allocation with Frequency Ranges"},
912 | {13, "PRB Allocation with Frequency Hopping"},
913 | {14, "Nulling-layer Info. for ueId-based beamforming"},
914 | {15, "Mixed-numerology Info. for ueId-based beamforming"},
915 | {16, "Section description for antenna mapping in UE channel information based UL beamforming"},
916 | {17, "Section description for indication of user port group"},
917 | {18, "Section description for Uplink Transmission Management"},
918 | {19, "Compact beamforming information for multiple port"},
919 | {20, "Puncturing extension"},
920 | {21, "Variable PRB group size for channel information"},
921 | {22, "ACK/NACK request"},
922 | {23, "Multiple symbol modulation compression parameters"},
923 | {24, "PUSCH DMRS configuration"},
924 | {25, "Symbol reordering for DMRS-BF"},
925 | {26, "Frequency offset feedback"},
926 | {27, "O-DU controlled dimensionality reduction"},
927 | {28, "O-DU controlled frequency resolution for SINR reporting"},
928 | {0, NULL((void*)0)}
929 | };
930 |
931 | /**************************************************************************************/
932 | /* Keep track for each Section Extension, which section types are allowed to carry it */
933 | typedef struct {
934 | bool_Bool ST0;
935 | bool_Bool ST1;
936 | bool_Bool ST3;
937 | bool_Bool ST5;
938 | bool_Bool ST6;
939 | bool_Bool ST10;
940 | bool_Bool ST11;
941 | } AllowedCTs_t;
942 |
943 |
944 | static AllowedCTs_t ext_cts[HIGHEST_EXTTYPE28] = {
945 | /* ST0 ST1 ST3 ST5 ST6 ST10 ST11 */
946 | { false0, true1, true1, false0, false0, false0, false0}, // SE 1 (1,3)
947 | { false0, true1, true1, false0, false0, false0, false0}, // SE 2 (1,3)
948 | { false0, true1, true1, false0, false0, false0, false0}, // SE 3 (1,3)
949 | { false0, true1, true1, true1, false0, false0, false0}, // SE 4 (1,3,5)
950 | { false0, true1, true1, true1, false0, false0, false0}, // SE 5 (1,3,5)
951 | { false0, true1, true1, true1, false0, true1, true1 }, // SE 6 (1,3,5,10,11)
952 | { true1, false0, false0, false0, false0, false0, false0}, // SE 7 (0)
953 | { false0, false0, false0, true1, false0, false0, false0}, // SE 8 (5)
954 | { true1, true1, true1, true1, true1, true1, true1 }, // SE 9 (all)
955 | { false0, true1, true1, true1, false0, false0, false0}, // SE 10 (1,3,5)
956 | { false0, true1, true1, false0, false0, false0, false0}, // SE 11 (1,3)
957 | { false0, true1, true1, true1, false0, true1, true1 }, // SE 12 (1,3,5,10,11)
958 | { false0, true1, true1, true1, false0, false0, false0}, // SE 13 (1,3,5)
959 | { false0, false0, false0, true1, false0, false0, false0}, // SE 14 (5)
960 | { false0, false0, false0, true1, true1, false0, false0}, // SE 15 (5,6)
961 | { false0, false0, false0, true1, false0, false0, false0}, // SE 16 (5)
962 | { false0, false0, false0, true1, false0, false0, false0}, // SE 17 (5)
963 | { false0, true1, true1, true1, false0, false0, false0}, // SE 18 (1,3,5)
964 | { false0, true1, true1, false0, false0, false0, false0}, // SE 19 (1,3)
965 | { true1, true1, true1, true1, true1, true1, true1 }, // SE 20 (0,1,3,5,10,11)
966 | { false0, false0, false0, true1, true1, false0, false0}, // SE 21 (5,6)
967 | { true1, true1, true1, true1, true1, true1, true1 }, // SE 22 (all)
968 | { false0, true1, true1, true1, false0, false0, false0}, // SE 23 (1,3,5)
969 | { false0, false0, false0, true1, false0, false0, false0}, // SE 24 (5)
970 | { false0, false0, false0, true1, false0, false0, false0}, // SE 25 (5)
971 | { false0, false0, false0, true1, false0, false0, false0}, // SE 26 (5)
972 | { false0, false0, false0, true1, false0, false0, false0}, // SE 27 (5)
973 | { false0, false0, false0, true1, false0, false0, false0}, // SE 28 (5)
974 | };
975 |
976 | static bool_Bool se_allowed_in_st(unsigned se, unsigned ct)
977 | {
978 | if (se==0 || se>HIGHEST_EXTTYPE28) {
979 | /* Don't know about new SE, so don't complain.. */
980 | return true1;
981 | }
982 |
983 | switch (ct) {
984 | case 1:
985 | return ext_cts[se-1].ST1;
986 | case 3:
987 | return ext_cts[se-1].ST3;
988 | case 5:
989 | return ext_cts[se-1].ST5;
990 | case 6:
991 | return ext_cts[se-1].ST6;
992 | case 10:
993 | return ext_cts[se-1].ST10;
994 | case 11:
995 | return ext_cts[se-1].ST11;
996 | default:
997 | /* New/unknown section type that includes 'ef'.. assume ok */
998 | return true1;
999 | }
1000 | }
1001 |
1002 | /************************************************************************************/
1003 |
1004 | /* Table 7.7.1.2-2 */
1005 | static const value_string bfw_comp_headers_iq_width[] = {
1006 | {0, "I and Q are 16 bits wide"},
1007 | {1, "I and Q are 1 bit wide"},
1008 | {2, "I and Q are 2 bits wide"},
1009 | {3, "I and Q are 3 bits wide"},
1010 | {4, "I and Q are 4 bits wide"},
1011 | {5, "I and Q are 5 bits wide"},
1012 | {6, "I and Q are 6 bits wide"},
1013 | {7, "I and Q are 7 bits wide"},
1014 | {8, "I and Q are 8 bits wide"},
1015 | {9, "I and Q are 9 bits wide"},
1016 | {10, "I and Q are 10 bits wide"},
1017 | {11, "I and Q are 11 bits wide"},
1018 | {12, "I and Q are 12 bits wide"},
1019 | {13, "I and Q are 13 bits wide"},
1020 | {14, "I and Q are 14 bits wide"},
1021 | {15, "I and Q are 15 bits wide"},
1022 | {0, NULL((void*)0)}
1023 | };
1024 |
1025 | /* Table 7.7.1.2-3 */
1026 | static const value_string bfw_comp_headers_comp_meth[] = {
1027 | {COMP_NONE0, "no compression"},
1028 | {COMP_BLOCK_FP1, "block floating point"},
1029 | {COMP_BLOCK_SCALE2, "block scaling"},
1030 | {COMP_U_LAW3, "u-law"},
1031 | {4, "beamspace compression type I"},
1032 | {5, "beamspace compression type II"},
1033 | {0, NULL((void*)0)}
1034 | };
1035 |
1036 | /* 7.7.6.2 rbgSize (resource block group size) */
1037 | static const value_string rbg_size_vals[] = {
1038 | {0, "reserved"},
1039 | {1, "1"},
1040 | {2, "2"},
1041 | {3, "3"},
1042 | {4, "4"},
1043 | {5, "6"},
1044 | {6, "8"},
1045 | {7, "16"},
1046 | {0, NULL((void*)0)}
1047 | };
1048 |
1049 | /* 7.7.6.5 */
1050 | static const value_string priority_vals[] = {
1051 | {0, "0"},
1052 | {1, "+1"},
1053 | {2, "-2 (reserved, should not be used)"},
1054 | {3, "-1"},
1055 | {0, NULL((void*)0)}
1056 | };
1057 |
1058 | /* 7.7.10.2 beamGroupType */
1059 | static const value_string beam_group_type_vals[] = {
1060 | {0x0, "common beam"},
1061 | {0x1, "beam matrix indication"},
1062 | {0x2, "beam vector listing"},
1063 | {0x3, "beamId/ueId listing with associated port-list index"},
1064 | {0, NULL((void*)0)}
1065 | };
1066 |
1067 | /* 7.7.9.2 technology (interface name) */
1068 | static const value_string interface_name_vals[] = {
1069 | {0x0, "LTE"},
1070 | {0x1, "NR"},
1071 | {0, NULL((void*)0)}
1072 | };
1073 |
1074 | /* 7.7.18.4 toT (type of transmission) */
1075 | static const value_string type_of_transmission_vals[] = {
1076 | {0x0, "normal transmission mode, data can be distributed in any way the O-RU is implemented to transmit data"},
1077 | {0x1, "uniformly distributed over the transmission window"},
1078 | {0x2, "Reserved"},
1079 | {0x3, "Reserved"},
1080 | {0, NULL((void*)0)}
1081 | };
1082 |
1083 | /* 7.7.2.2 (width of bfa parameters) */
1084 | static const value_string bfa_bw_vals[] = {
1085 | {0, "no bits, the field is not applicable (e.g., O-RU does not support it) or the default value shall be used"},
1086 | {1, "2-bit bitwidth"},
1087 | {2, "3-bit bitwidth"},
1088 | {3, "4-bit bitwidth"},
1089 | {4, "5-bit bitwidth"},
1090 | {5, "6-bit bitwidth"},
1091 | {6, "7-bit bitwidth"},
1092 | {7, "8-bit bitwidth"},
1093 | {0, NULL((void*)0)}
1094 | };
1095 |
1096 | /* 7.7.2.7 & 7.7.2.8 */
1097 | static const value_string sidelobe_suppression_vals[] = {
1098 | {0, "10 dB"},
1099 | {1, "15 dB"},
1100 | {2, "20 dB"},
1101 | {3, "25 dB"},
1102 | {4, "30 dB"},
1103 | {5, "35 dB"},
1104 | {6, "40 dB"},
1105 | {7, ">= 45 dB"},
1106 | {0, NULL((void*)0)}
1107 | };
1108 |
1109 | static const value_string lbtTrafficClass_vals[] = {
1110 | {1, "Priority 1"},
1111 | {2, "Priority 2"},
1112 | {3, "Priority 3"},
1113 | {4, "Priority 4"},
1114 | {0, NULL((void*)0)}
1115 | };
1116 |
1117 | /* 7.5.3.22 */
1118 | static const value_string lbtPdschRes_vals[] = {
1119 | {0, "not sensing – indicates that the O-RU is transmitting data"},
1120 | {1, "currently sensing – indicates the O-RU has not yet acquired the channel"},
1121 | {2, "success – indicates that the channel was successfully acquired"},
1122 | {3, "Failure – indicates expiration of the LBT timer. The LBT process should be reset"},
1123 | {0, NULL((void*)0)}
1124 | };
1125 |
1126 | /* Table 7.5.2.15-3 */
1127 | static const value_string ci_comp_opt_vals[] = {
1128 | {0, "compression per UE, one ciCompParam exists before the I/Q value of each UE"},
1129 | {1, "compression per PRB, one ciCompParam exists before the I/Q value of each PRB"},
1130 | {0, NULL((void*)0)}
1131 | };
1132 |
1133 | /* 7.5.2.17 */
1134 | static const range_string cmd_scope_vals[] = {
1135 | {0, 0, "ARRAY-COMMAND"},
1136 | {1, 1, "CARRIER-COMMAND"},
1137 | {2, 2, "O-RU-COMMAND"},
1138 | {3, 15, "reserved"},
1139 | {0, 0, NULL((void*)0)}
1140 | };
1141 |
1142 | /* N.B., table in 7.5.3.38 is truncated.. */
1143 | static const range_string st4_cmd_type_vals[] = {
1144 | {0, 0, "reserved for future command types"},
1145 | {1, 1, "TIME_DOMAIN_BEAM_CONFIG"},
1146 | {2, 2, "TDD_CONFIG_PATTERN"},
1147 | {3, 3, "TRX_CONTROL"},
1148 | {4, 4, "ASM"},
1149 | {5, 255, "reserved for future command types"},
1150 | {0, 0, NULL((void*)0)}
1151 | };
1152 |
1153 | /* Table 7.5.3.51-1 */
1154 | static const value_string log2maskbits_vals[] = {
1155 | {0, "reserved"},
1156 | {1, "min antMask size is 16 bits.."},
1157 | {2, "min antMask size is 16 bits.."},
1158 | {3, "min antMask size is 16 bits.."},
1159 | {4, "16 bits"},
1160 | {5, "32 bits"},
1161 | {6, "64 bits"},
1162 | {7, "128 bits"},
1163 | {8, "256 bits"},
1164 | {9, "512 bits"},
1165 | {10, "1024 bits"},
1166 | {11, "2048 bits"},
1167 | {12, "4096 bits"},
1168 | {13, "8192 bits"},
1169 | {14, "16384 bits"},
1170 | {15, "reserved"},
1171 | {0, NULL((void*)0)}
1172 | };
1173 |
1174 | /* Table 16.1-1 Sleep modes */
1175 | static const value_string sleep_mode_trx_vals[] = {
1176 | { 0, "TRXC-mode0-wake-up-duration (symbol)"},
1177 | { 1, "TRXC-mode1-wake-up-duration (L)"},
1178 | { 2, "TRXC-mode2-wake-up-duration (M)"},
1179 | { 3, "TRXC-mode3-wake-up-duration (N)"},
1180 | { 0, NULL((void*)0)}
1181 | };
1182 |
1183 | static const value_string sleep_mode_asm_vals[] = {
1184 | { 0, "ASM-mode0-wake-up-duration (symbol)"},
1185 | { 1, "ASM-mode1-wake-up-duration (L)"},
1186 | { 2, "ASM-mode2-wake-up-duration (M)"},
1187 | { 3, "ASM-mode3-wake-up-duration (N)"},
1188 | { 0, NULL((void*)0)}
1189 | };
1190 |
1191 | /* 7.7.21.3.1 */
1192 | static const value_string prg_size_st5_vals[] = {
1193 | { 0, "reserved"},
1194 | { 1, "Precoding resource block group size as WIDEBAND"},
1195 | { 2, "Precoding resource block group size 2"},
1196 | { 3, "Precoding resource block group size 4"},
1197 | { 0, NULL((void*)0)}
1198 | };
1199 |
1200 | /* 7.7.21.3.2 */
1201 | static const value_string prg_size_st6_vals[] = {
1202 | { 0, "if ciPrbGroupSize is 2 or 4, then ciPrbGroupSize, else WIDEBAND"},
1203 | { 1, "Precoding resource block group size as WIDEBAND"},
1204 | { 2, "Precoding resource block group size 2"},
1205 | { 3, "Precoding resource block group size 4"},
1206 | { 0, NULL((void*)0)}
1207 | };
1208 |
1209 | /* 7.7.24.4 */
1210 | static const value_string alpn_per_sym_vals[] = {
1211 | { 0, "report one allocated IPN value per all allocated symbols with DMRS"},
1212 | { 1, "report one allocated IPN value per group of consecutive DMRS symbols"},
1213 | { 0, NULL((void*)0)}
1214 | };
1215 |
1216 | /* 7.7.24.5 */
1217 | static const value_string ant_dmrs_snr_vals[] = {
1218 | { 0, "O-RU shall not report the MEAS_ANT_DMRS_SNR"},
1219 | { 1, "O-RU shall report the MEAS_ANT_DMRS_SNR"},
1220 | { 0, NULL((void*)0)}
1221 | };
1222 |
1223 | /* 7.7.24.14 */
1224 | static const value_string dtype_vals[] = {
1225 | { 0, "assume DMRS configuration type 1"},
1226 | { 1, "assume DMRS configuration type 2"},
1227 | { 0, NULL((void*)0)}
1228 | };
1229 |
1230 | /* 7.7.24.17 */
1231 | static const value_string papr_type_vals[] = {
1232 | { 0, "sequence generator type 1 for short sequence lengths"},
1233 | { 1, "sequence generator type 1 for long sequence lengths"},
1234 | { 2, "sequence generator type 2 for short sequence lengths"},
1235 | { 3, "sequence generator type 2 for long sequence lengths"},
1236 | { 0, NULL((void*)0)}
1237 | };
1238 |
1239 | /* 7.7.24.18 */
1240 | static const value_string hopping_mode_vals[] = {
1241 | { 0, "neither group, nor sequence hopping is enabled"},
1242 | { 1, "group hopping is enabled and sequence hopping is disabled"},
1243 | { 2, "sequence hopping is enabled and group hopping is disabled"},
1244 | { 3, "reserved"},
1245 | { 0, NULL((void*)0)}
1246 | };
1247 |
1248 |
1249 | static const true_false_string tfs_sfStatus =
1250 | {
1251 | "subframe was transmitted",
1252 | "subframe was dropped"
1253 | };
1254 |
1255 | static const true_false_string tfs_lbtBufErr =
1256 | {
1257 | "buffer overflow – data received at O-RU is larger than the available buffer size",
1258 | "reserved"
1259 | };
1260 |
1261 | static const true_false_string tfs_partial_full_sf = {
1262 | "partial SF",
1263 | "full SF"
1264 | };
1265 |
1266 | static const true_false_string disable_tdbfns_tfs = {
1267 | "beam numbers excluded",
1268 | "beam numbers included"
1269 | };
1270 |
1271 | static const true_false_string continuity_indication_tfs = {
1272 | "continuity between current and next bundle",
1273 | "discontinuity between current and next bundle"
1274 | };
1275 |
1276 | static const true_false_string prb_mode_tfs = {
1277 | "PRB-BLOCK mode",
1278 | "PRB-MASK mode"
1279 | };
1280 |
1281 | static const true_false_string symbol_direction_tfs = {
1282 | "DL symbol",
1283 | "UL symbol"
1284 | };
1285 |
1286 | static const true_false_string symbol_guard_tfs = {
1287 | "guard symbol",
1288 | "non-guard symbol"
1289 | };
1290 |
1291 | static const true_false_string beam_numbers_included_tfs = {
1292 | "time-domain beam numbers excluded in this command",
1293 | "time-domain beam numbers included in this command"
1294 | };
1295 |
1296 | static const true_false_string measurement_flag_tfs = {
1297 | "at least one additional measurement report or command after the current one",
1298 | "no additional measurement report or command"
1299 | };
1300 |
1301 | static const true_false_string repetition_se6_tfs = {
1302 | "repeated highest priority data section in the C-Plane message",
1303 | "no repetition"
1304 | };
1305 |
1306 | static const true_false_string repetition_se19_tfs = {
1307 | "per port information not present in the extension",
1308 | "per port info present in the extension"
1309 | };
1310 |
1311 |
1312 |
1313 | /* Forward declaration */
1314 | static int dissect_udcompparam(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree, unsigned offset,
1315 | unsigned comp_meth,
1316 | uint32_t *exponent, uint16_t *sReSMask, bool_Bool for_sinr);
1317 |
1318 |
1319 | static const true_false_string ready_tfs = {
1320 | "message is a \"ready\" message",
1321 | "message is a ACK message"
1322 | };
1323 |
1324 | static const true_false_string multi_sd_scope_tfs = {
1325 | "Puncturing pattern applies to current and following sections",
1326 | "Puncturing pattern applies to current section"
1327 | };
1328 |
1329 | static const true_false_string tfs_ueid_reset = {
1330 | "cannot assume same UE as in preceding slot",
1331 | "can assume same UE as in preceding slot"
1332 | };
1333 |
1334 |
1335 | /* Config for (and later, worked-out allocations) bundles for ext11 (dynamic BFW) */
1336 | typedef struct {
1337 | /* Ext 6 config */
1338 | bool_Bool ext6_set;
1339 | uint8_t ext6_rbg_size; /* number of PRBs allocated by bitmask */
1340 |
1341 | uint8_t ext6_num_bits_set;
1342 | uint8_t ext6_bits_set[28]; /* Which bit position this entry has */
1343 | /* TODO: store an f value for each bit position? */
1344 |
1345 | /* Ext 12 config */
1346 | bool_Bool ext12_set;
1347 | unsigned ext12_num_pairs;
1348 | #define MAX_BFW_EXT12_PAIRS128 128
1349 | struct {
1350 | uint8_t off_start_prb;
1351 | uint8_t num_prb;
1352 | } ext12_pairs[MAX_BFW_EXT12_PAIRS128];
1353 |
1354 | /* Ext 13 config */
1355 | bool_Bool ext13_set;
1356 | unsigned ext13_num_start_prbs;
1357 | #define MAX_BFW_EXT13_ALLOCATIONS128 128
1358 | unsigned ext13_start_prbs[MAX_BFW_EXT13_ALLOCATIONS128];
1359 | /* TODO: store nextSymbolId here too? */
1360 |
1361 | /* Ext 21 config */
1362 | bool_Bool ext21_set;
1363 | uint8_t ext21_ci_prb_group_size;
1364 |
1365 | /* Results/settings (after calling ext11_work_out_bundles()) */
1366 | uint32_t num_bundles;
1367 | #define MAX_BFW_BUNDLES512 512
1368 | struct {
1369 | uint32_t start; /* first prb of bundle */
1370 | uint32_t end; /* last prb of bundle*/
1371 | bool_Bool is_orphan; /* true if not complete (i.e., end-start < numBundPrb) */
1372 | } bundles[MAX_BFW_BUNDLES512];
1373 | } ext11_settings_t;
1374 |
1375 |
1376 | /* Work out bundle allocation for ext 11. Take into account ext6/ext21, ext12 or ext13 in this section before ext 11. */
1377 | /* Won't be called with numBundPrb=0 */
1378 | static void ext11_work_out_bundles(unsigned startPrbc,
1379 | unsigned numPrbc,
1380 | unsigned numBundPrb, /* number of PRBs pre (full) bundle */
1381 | ext11_settings_t *settings)
1382 | {
1383 | /* Allocation configured by ext 6 */
1384 | if (settings->ext6_set) {
1385 | unsigned bundles_per_entry = (settings->ext6_rbg_size / numBundPrb);
1386 |
1387 | /* Need to cope with these not dividing exactly, or even having more PRbs in a bundle that
1388 | rbg size. i.e. each bundle gets the correct number of PRBs until
1389 | all rbg entries are consumed... */
1390 |
1391 | /* TODO: need to check 7.9.4.2. Different cases depending upon value of RAD */
1392 |
1393 | if (bundles_per_entry == 0) {
1394 | bundles_per_entry = 1;
1395 | }
1396 |
1397 | /* Maybe also be affected by ext 21 */
1398 | if (settings->ext21_set) {
1399 | /* N.B., have already checked that numPrbc is not 0 */
1400 |
1401 | /* ciPrbGroupSize overrides number of contiguous PRBs in group */
1402 | bundles_per_entry = (settings->ext6_rbg_size / settings->ext21_ci_prb_group_size);
1403 |
1404 | /* numPrbc is the number of PRB groups per antenna - handled in call to dissect_bfw_bundle() */
1405 | }
1406 |
1407 | unsigned bundles_set = 0;
1408 | for (unsigned n=0;
1409 | n < (settings->ext6_num_bits_set * settings->ext6_rbg_size) / numBundPrb;
1410 | n++) {
1411 |
1412 | /* Watch out for array bound */
1413 | if (n >= 28) {
1414 | break;
1415 | }
1416 |
1417 | /* For each bundle... */
1418 |
1419 | /* TODO: Work out where first PRB is */
1420 | /* May not be the start of an rbg block... */
1421 | uint32_t prb_start = (settings->ext6_bits_set[n] * settings->ext6_rbg_size);
1422 |
1423 | /* For each bundle within identified rbgSize block */
1424 | for (unsigned m=0; m < bundles_per_entry; m++) {
1425 | settings->bundles[bundles_set].start = startPrbc+prb_start+(m*numBundPrb);
1426 | /* Start already beyond end, so doesn't count. */
1427 | if (settings->bundles[bundles_set].start > (startPrbc+numPrbc-1)) {
1428 | break;
1429 | }
1430 | /* Bundle consists of numBundPrb bundles */
1431 | /* TODO: may involve PRBs from >1 rbg blocks.. */
1432 | settings->bundles[bundles_set].end = startPrbc+prb_start+((m+1)*numBundPrb)-1;
1433 | if (settings->bundles[bundles_set].end > (startPrbc+numPrbc-1)) {
1434 | /* Extends beyond end, so counts but is an orphan bundle */
1435 | settings->bundles[bundles_set].end = numPrbc;
1436 | settings->bundles[bundles_set].is_orphan = true1;
1437 | }
1438 |
1439 | /* Get out if have reached array bound */
1440 | if (++bundles_set == MAX_BFW_BUNDLES512) {
1441 | return;
1442 | }
1443 | }
1444 | }
1445 | settings->num_bundles = bundles_set;
1446 | }
1447 |
1448 | /* Allocation configured by ext 12 */
1449 | else if (settings->ext12_set) {
1450 | /* First, allocate normally from startPrbc, numPrbc */
1451 | settings->num_bundles = (numPrbc+numBundPrb-1) / numBundPrb;
1452 |
1453 | /* Don't overflow settings->bundles[] ! */
1454 | settings->num_bundles = MIN(MAX_BFW_BUNDLES, settings->num_bundles)(((512) < (settings->num_bundles)) ? (512) : (settings-> num_bundles));
1455 |
1456 | for (uint32_t n=0; n < settings->num_bundles; n++) {
1457 | settings->bundles[n].start = startPrbc + n*numBundPrb;
1458 | settings->bundles[n].end = settings->bundles[n].start + numBundPrb-1;
1459 | /* Does it go beyond the end? */
1460 | if (settings->bundles[n].end > startPrbc+numPrbc) {
1461 | settings->bundles[n].end = numPrbc+numPrbc;
1462 | settings->bundles[n].is_orphan = true1;
1463 | }
1464 | }
1465 | if (settings->num_bundles == MAX_BFW_BUNDLES512) {
1466 | return;
1467 | }
1468 |
1469 | unsigned prb_offset = startPrbc + numPrbc;
1470 |
1471 | /* Loop over pairs, adding bundles for each */
1472 | for (unsigned p=0; p < settings->ext12_num_pairs; p++) {
1473 | prb_offset += settings->ext12_pairs[p].off_start_prb;
1474 | unsigned pair_bundles = (settings->ext12_pairs[p].num_prb+numBundPrb-1) / numBundPrb;
1475 |
1476 | for (uint32_t n=0; n < pair_bundles; n++) {
1477 | unsigned idx = settings->num_bundles;
1478 |
1479 | settings->bundles[idx].start = prb_offset + n*numBundPrb;
1480 | settings->bundles[idx].end = settings->bundles[idx].start + numBundPrb-1;
1481 | /* Does it go beyond the end? */
1482 | if (settings->bundles[idx].end > prb_offset + settings->ext12_pairs[p].num_prb) {
1483 | settings->bundles[idx].end = prb_offset + settings->ext12_pairs[p].num_prb;
1484 | settings->bundles[idx].is_orphan = true1;
1485 | }
1486 | /* Range check / return */
1487 | settings->num_bundles++;
1488 | if (settings->num_bundles == MAX_BFW_BUNDLES512) {
1489 | return;
1490 | }
1491 | }
1492 |
1493 | prb_offset += settings->ext12_pairs[p].num_prb;
1494 | }
1495 | }
1496 |
1497 | /* Allocation configured by ext 13 */
1498 | else if (settings->ext13_set) {
1499 | unsigned alloc_size = (numPrbc+numBundPrb-1) / numBundPrb;
1500 | settings->num_bundles = alloc_size * settings->ext13_num_start_prbs;
1501 |
1502 | /* Don't overflow settings->bundles[] ! */
1503 | settings->num_bundles = MIN(MAX_BFW_BUNDLES, settings->num_bundles)(((512) < (settings->num_bundles)) ? (512) : (settings-> num_bundles));
1504 |
1505 | for (unsigned alloc=0; alloc < settings->ext13_num_start_prbs; alloc++) {
1506 | unsigned alloc_start = alloc * alloc_size;
1507 | for (uint32_t n=0; n < alloc_size; n++) {
1508 | if ((alloc_start+n) >= MAX_BFW_BUNDLES512) {
1509 | /* ERROR */
1510 | return;
1511 | }
1512 | settings->bundles[alloc_start+n].start = settings->ext13_start_prbs[alloc] + startPrbc + n*numBundPrb;
1513 | settings->bundles[alloc_start+n].end = settings->bundles[alloc_start+n].start + numBundPrb-1;
1514 | if (settings->bundles[alloc_start+n].end > settings->ext13_start_prbs[alloc] + numPrbc) {
1515 | settings->bundles[alloc_start+n].end = settings->ext13_start_prbs[alloc] + numPrbc;
1516 | settings->bundles[alloc_start+n].is_orphan = true1;
1517 | }
1518 | }
1519 | }
1520 | }
1521 |
1522 | /* Case where bundles are not controlled by other extensions - just divide up range into bundles we have */
1523 | else {
1524 | settings->num_bundles = (numPrbc+numBundPrb-1) / numBundPrb; /* rounded up */
1525 |
1526 | /* Don't overflow settings->bundles[] */
1527 | settings->num_bundles = MIN(MAX_BFW_BUNDLES, settings->num_bundles)(((512) < (settings->num_bundles)) ? (512) : (settings-> num_bundles));
1528 |
1529 | /* For each bundle.. */
1530 | for (uint32_t n=0; n < settings->num_bundles; n++) {
1531 | /* Allocate start and end */
1532 | settings->bundles[n].start = startPrbc + n*numBundPrb;
1533 | settings->bundles[n].end = settings->bundles[n].start + numBundPrb - 1;
1534 | /* If would go beyond end of PRBs, limit and identify as orphan */
1535 | if (settings->bundles[n].end > startPrbc+numPrbc) {
1536 | settings->bundles[n].end = startPrbc+numPrbc;
1537 | settings->bundles[n].is_orphan = true1;
1538 | }
1539 | }
1540 | }
1541 | }
1542 |
1543 | typedef struct {
1544 | #define MAX_MOD_COMPR_CONFIGS16 16
1545 | struct {
1546 | /* Application of each entry is filtered by RE.
1547 | * TODO: should also be filtering by PRB + symbol... */
1548 | uint16_t mod_compr_re_mask;
1549 |
1550 | /* Settings to apply */
1551 | bool_Bool mod_compr_csf;
1552 | double mod_compr_scaler;
1553 | } configs[MAX_MOD_COMPR_CONFIGS16];
1554 | uint32_t num_configs;
1555 | } mod_compr_params_t;
1556 |
1557 | /*******************************************************/
1558 | /* Overall state of a flow (eAxC/plane) */
1559 | typedef struct {
1560 | /* State for sequence analysis [each direction] */
1561 | bool_Bool last_frame_seen[2];
1562 | uint32_t last_frame[2];
1563 | uint8_t next_expected_sequence_number[2];
1564 |
1565 | /* Table recording ackNack requests (ackNackId -> ack_nack_request_t*)
1566 | Note that this assumes that the same ackNackId will not be reused within a state,
1567 | which may well not be valid */
1568 | wmem_tree_t *ack_nack_requests;
1569 |
1570 | /* Store udCompHdr seen in C-Plane for UL - can be looked up and used by U-PLane.
1571 | Note that this appears in the common section header parts of ST1, ST3, ST5,
1572 | so can still be over-written per sectionId in the U-Plane */
1573 | unsigned ul_ud_comp_hdr_frame;
1574 | bool_Bool ul_ud_comp_hdr_set;
1575 | unsigned ul_ud_comp_hdr_bit_width;
1576 | int ul_ud_comp_hdr_compression;
1577 |
1578 | bool_Bool udcomphdrDownlink_heuristic_result_set;
1579 | bool_Bool udcomphdrDownlink_heuristic_result;
1580 | bool_Bool udcomphdrUplink_heuristic_result_set;
1581 | bool_Bool udcomphdrUplink_heuristic_result;
1582 |
1583 | /* Modulation compression params */
1584 | /* This probably needs to be per section!? */
1585 | mod_compr_params_t mod_comp_params;
1586 | } flow_state_t;
1587 |
1588 | typedef struct {
1589 | uint32_t request_frame_number;
1590 | nstime_t request_frame_time;
1591 | enum {
1592 | SE22,
1593 | ST4Cmd1,
1594 | ST4Cmd2,
1595 | ST4Cmd3,
1596 | ST4Cmd4
1597 | } requestType;
1598 |
1599 | uint32_t response_frame_number;
1600 | nstime_t response_frame_time;
1601 | } ack_nack_request_t;
1602 |
1603 | static const value_string acknack_type_vals[] = {
1604 | { SE22, "SE 22" },
1605 | { ST4Cmd1, "ST4 (TIME_DOMAIN_BEAM_CONFIG)" },
1606 | { ST4Cmd2, "ST4 (TDD_CONFIG_PATTERN)" },
1607 | { ST4Cmd3, "ST4 (TRX_CONTROL)" },
1608 | { ST4Cmd4, "ST4 (ASM)" },
1609 | { 0, NULL((void*)0)}
1610 | };
1611 |
1612 | #define ORAN_C_PLANE0 0
1613 | #define ORAN_U_PLANE1 1
1614 |
1615 | /* Using parts of src/dst MAC address, so don't confuse UL messages with DL messages configuring UL.. */
1616 | static uint32_t make_flow_key(packet_info *pinfo, uint16_t eaxc_id, uint8_t plane, bool_Bool opposite_dir)
1617 | {
1618 | uint16_t eth_bits = 0;
1619 | if (pinfo->dl_src.len == 6 && pinfo->dl_dst.len == 6) {
1620 | /* Only using (most of) 2 bytes from addresses for now, but reluctant to make key longer.. */
1621 | uint8_t *src_eth = (uint8_t*)pinfo->dl_src.data;
1622 | uint8_t *dst_eth = (uint8_t*)pinfo->dl_dst.data;
1623 | if (!opposite_dir) {
1624 | eth_bits = (src_eth[0]<<8) | dst_eth[5];
1625 | }
1626 | else {
1627 | eth_bits = (dst_eth[0]<<8) | src_eth[5];
1628 | }
1629 | }
1630 | return eaxc_id | (plane << 16) | (eth_bits << 17);
1631 | }
1632 |
1633 |
1634 | /* Table maintained on first pass from flow_key(uint32_t) -> flow_state_t* */
1635 | static wmem_tree_t *flow_states_table;
1636 |
1637 | /* Table consulted on subsequent passes: frame_num -> flow_result_t* */
1638 | static wmem_tree_t *flow_results_table;
1639 |
1640 | typedef struct {
1641 | /* Sequence analysis */
1642 | bool_Bool unexpected_seq_number;
1643 | uint8_t expected_sequence_number;
1644 | uint32_t previous_frame;
1645 | } flow_result_t;
1646 |
1647 |
1648 | /* Uplink timing */
1649 | /* For a given symbol, track first to last UL frame to find out first-last time */
1650 | /* frameId (8) + subframeId (4) + slotId (6) + symbolId (6) = 24 bits */
1651 | /* N.B. if a capture lasts > 2.5s, may see same timing come around again... */
1652 | static uint32_t get_timing_key(uint8_t frameId, uint8_t subframeId, uint8_t slotId, uint8_t symbolId)
1653 | {
1654 | return symbolId + (slotId<<8) + (subframeId<<14) + (frameId<<18);
1655 | }
1656 |
1657 | typedef struct {
1658 | uint32_t first_frame;
1659 | nstime_t first_frame_time;
1660 | uint32_t frames_seen_in_symbol;
1661 | uint32_t last_frame_in_symbol;
1662 | } ul_timing_for_slot;
1663 |
1664 | /* Set during first pass. timing_key -> ul_timing_for_slot* */
1665 | static wmem_tree_t *ul_symbol_timing;
1666 |
1667 |
1668 | static void show_link_to_acknack_response(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo,
1669 | ack_nack_request_t *response);
1670 |
1671 |
1672 |
1673 |
1674 | static void write_pdu_label_and_info(proto_item *ti1, proto_item *ti2,
1675 | packet_info *pinfo, const char *format, ...) G_GNUC_PRINTF(4, 5)__attribute__((__format__ (__printf__, 4, 5)));
1676 |
1677 | /* Write the given formatted text to:
1678 | - the info column (if pinfo != NULL)
1679 | - 1 or 2 other labels (optional)
1680 | */
1681 | static void write_pdu_label_and_info(proto_item *ti1, proto_item *ti2,
1682 | packet_info *pinfo, const char *format, ...)
1683 | {
1684 | #define MAX_INFO_BUFFER256 256
1685 | char info_buffer[MAX_INFO_BUFFER256];
1686 | va_list ap;
1687 |
1688 | if ((ti1 == NULL((void*)0)) && (ti2 == NULL((void*)0)) && (pinfo == NULL((void*)0))) {
1689 | return;
1690 | }
1691 |
1692 | va_start(ap, format)__builtin_va_start(ap, format);
1693 | vsnprintf(info_buffer, MAX_INFO_BUFFER256, format, ap);
1694 | va_end(ap)__builtin_va_end(ap);
1695 |
1696 | /* Add to indicated places */
1697 | if (pinfo != NULL((void*)0)) {
1698 | col_append_str(pinfo->cinfo, COL_INFO, info_buffer);
1699 | }
1700 | if (ti1 != NULL((void*)0)) {
1701 | proto_item_append_text(ti1, "%s", info_buffer);
1702 | }
1703 | if (ti2 != NULL((void*)0)) {
1704 | proto_item_append_text(ti2, "%s", info_buffer);
1705 | }
1706 | }
1707 |
1708 | /* Add section labels (type + PRB range) for C-Plane, U-Plane */
1709 | static void
1710 | write_section_info(proto_item *section_heading, packet_info *pinfo, proto_item *protocol_item,
1711 | uint32_t section_id, uint32_t start_prbx, uint32_t num_prbx, uint32_t rb)
1712 | {
1713 | switch (num_prbx) {
1714 | case 0:
1715 | /* None -> all */
1716 | write_pdu_label_and_info(section_heading, protocol_item, pinfo, ", Id: %4d (all PRBs)", section_id);
1717 | break;
1718 | case 1:
1719 | /* Single PRB */
1720 | write_pdu_label_and_info(section_heading, protocol_item, pinfo, ", Id: %4d (PRB: %7u)", section_id, start_prbx);
1721 | break;
1722 | default:
1723 | /* Range */
1724 | write_pdu_label_and_info(section_heading, protocol_item, pinfo, ", Id: %4d (PRB: %3u-%3u%s)", section_id, start_prbx,
1725 | start_prbx + (num_prbx-1)*(1+rb), rb ? " (every-other)" : "");
1726 | }
1727 | }
1728 |
1729 | static void
1730 | write_channel_section_info(proto_item *section_heading, packet_info *pinfo,
1731 | uint32_t section_id, uint32_t ueId, uint32_t start_prbx, uint32_t num_prbx,
1732 | uint32_t num_trx)
1733 | {
1734 | switch (num_prbx) {
1735 | case 0:
1736 | /* TODO: ?? */
1737 | break;
1738 | case 1:
1739 | /* Single PRB */
1740 | write_pdu_label_and_info(section_heading, NULL((void*)0), pinfo,
1741 | ", Id: %4d (UEId=%5u PRB %7u, %2u antennas)",
1742 | section_id, ueId, start_prbx, num_trx);
1743 | break;
1744 | default:
1745 | /* Range */
1746 | write_pdu_label_and_info(section_heading, NULL((void*)0), pinfo,
1747 | ", Id: %4d (UEId=%5u PRBs %3u-%3u, %2u antennas)",
1748 | section_id, ueId, start_prbx, start_prbx+num_prbx-1, num_trx);
1749 | }
1750 | }
1751 |
1752 |
1753 | /* 5.1.3.2.7 (real time control data / IQ data transfer message series identifier) */
1754 | static void
1755 | addPcOrRtcid(tvbuff_t *tvb, proto_tree *tree, int *offset, int hf, uint16_t *eAxC)
1756 | {
1757 | /* Subtree */
1758 | proto_item *oran_pcid_ti = proto_tree_add_item(tree, hf,
1759 | tvb, *offset, 2, ENC_NA0x00000000);
1760 | proto_tree *oran_pcid_tree = proto_item_add_subtree(oran_pcid_ti, ett_oran_ecpri_pcid);
1761 |
1762 | uint64_t duPortId, bandSectorId, ccId, ruPortId = 0;
1763 | int id_offset = *offset;
1764 |
1765 | /* All parts of eAxC should be above 0, and should total 16 bits (breakdown controlled by preferences) */
1766 | if (!((pref_du_port_id_bits > 0) && (pref_bandsector_id_bits > 0) && (pref_cc_id_bits > 0) && (pref_ru_port_id_bits > 0) &&
1767 | ((pref_du_port_id_bits + pref_bandsector_id_bits + pref_cc_id_bits + pref_ru_port_id_bits) == 16))) {
1768 | expert_add_info(NULL((void*)0), tree, &ei_oran_invalid_eaxc_bit_width);
1769 | *eAxC = 0;
1770 | *offset += 2;
1771 | return;
1772 | }
1773 |
1774 | unsigned bit_offset = *offset * 8;
1775 |
1776 | /* N.B. For sequence analysis / tapping, just interpret these 2 bytes as eAxC ID... */
1777 | *eAxC = tvb_get_uint16(tvb, *offset, ENC_BIG_ENDIAN0x00000000);
1778 |
1779 | /* DU Port ID */
1780 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_du_port_id, tvb, bit_offset, pref_du_port_id_bits, &duPortId, ENC_BIG_ENDIAN0x00000000);
1781 | bit_offset += pref_du_port_id_bits;
1782 | /* BandSector ID */
1783 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_bandsector_id, tvb, bit_offset, pref_bandsector_id_bits, &bandSectorId, ENC_BIG_ENDIAN0x00000000);
1784 | bit_offset += pref_bandsector_id_bits;
1785 | /* CC ID */
1786 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_cc_id, tvb, bit_offset, pref_cc_id_bits, &ccId, ENC_BIG_ENDIAN0x00000000);
1787 | bit_offset += pref_cc_id_bits;
1788 | /* RU Port ID */
1789 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_ru_port_id, tvb, bit_offset, pref_ru_port_id_bits, &ruPortId, ENC_BIG_ENDIAN0x00000000);
1790 | *offset += 2;
1791 |
1792 | proto_item_append_text(oran_pcid_ti, " (DU_Port_ID: %d, BandSector_ID: %d, CC_ID: %d, RU_Port_ID: %d)",
1793 | (int)duPortId, (int)bandSectorId, (int)ccId, (int)ruPortId);
1794 | char id[16];
1795 | snprintf(id, 16, "%x:%x:%x:%x", (int)duPortId, (int)bandSectorId, (int)ccId, (int)ruPortId);
1796 | proto_item *pi = proto_tree_add_string(oran_pcid_tree, hf_oran_c_eAxC_ID, tvb, id_offset, 2, id);
1797 | proto_item_set_generated(pi);
1798 | }
1799 |
1800 | /* 5.1.3.2.8 ecpriSeqid (message identifier) */
1801 | static int
1802 | addSeqid(tvbuff_t *tvb, proto_tree *oran_tree, int offset, int plane, uint8_t *seq_id, proto_item **seq_id_ti, packet_info *pinfo)
1803 | {
1804 | /* Subtree */
1805 | proto_item *seqIdItem = proto_tree_add_item(oran_tree, hf_oran_ecpri_seqid, tvb, offset, 2, ENC_NA0x00000000);
1806 | proto_tree *oran_seqid_tree = proto_item_add_subtree(seqIdItem, ett_oran_ecpri_seqid);
1807 | uint32_t seqId, subSeqId, e = 0;
1808 |
1809 | /* Sequence ID (8 bits) */
1810 | *seq_id_ti = proto_tree_add_item_ret_uint(oran_seqid_tree, hf_oran_sequence_id, tvb, offset, 1, ENC_NA0x00000000, &seqId);
1811 | *seq_id = seqId;
1812 | offset += 1;
1813 |
1814 | /* Show link back to previous sequence ID, if set */
1815 | flow_result_t *result = wmem_tree_lookup32(flow_results_table, pinfo->num);
1816 | if (result) {
1817 | proto_item *prev_ti = proto_tree_add_uint(oran_seqid_tree, hf_oran_previous_frame, tvb, 0, 0, result->previous_frame);
1818 | proto_item_set_generated(prev_ti);
1819 | }
1820 |
1821 | /* E bit */
1822 | proto_tree_add_item_ret_uint(oran_seqid_tree, hf_oran_e_bit, tvb, offset, 1, ENC_NA0x00000000, &e);
1823 | /* Subsequence ID (7 bits) */
1824 | proto_tree_add_item_ret_uint(oran_seqid_tree, hf_oran_subsequence_id, tvb, offset, 1, ENC_NA0x00000000, &subSeqId);
1825 | offset += 1;
1826 |
1827 | /* radio-transport fragmentation not allowed for C-Plane messages */
1828 | if (plane == ORAN_C_PLANE0) {
1829 | if (e !=1 || subSeqId != 0) {
1830 | expert_add_info(NULL((void*)0), seqIdItem, &ei_oran_radio_fragmentation_c_plane);
1831 | }
1832 | }
1833 | else {
1834 | if (e !=1 || subSeqId != 0) {
1835 | /* TODO: Re-assembly of any radio-fragmentation on U-Plane */
1836 | expert_add_info(NULL((void*)0), seqIdItem, &ei_oran_radio_fragmentation_u_plane);
1837 | }
1838 | }
1839 |
1840 | /* Summary */
1841 | proto_item_append_text(seqIdItem, " (SeqId: %3d, E: %d, SubSeqId: %d)", seqId, e, subSeqId);
1842 | return offset;
1843 | }
1844 |
1845 | static int dissect_symbolmask(tvbuff_t *tvb, proto_tree *tree, int offset, uint32_t *symbol_mask, proto_item **ti)
1846 | {
1847 | uint64_t temp_val;
1848 |
1849 | static int * const symbol_mask_flags[] = {
1850 | &hf_oran_symbol_mask_s13,
1851 | &hf_oran_symbol_mask_s12,
1852 | &hf_oran_symbol_mask_s11,
1853 | &hf_oran_symbol_mask_s10,
1854 | &hf_oran_symbol_mask_s9,
1855 | &hf_oran_symbol_mask_s8,
1856 | &hf_oran_symbol_mask_s7,
1857 | &hf_oran_symbol_mask_s6,
1858 | &hf_oran_symbol_mask_s5,
1859 | &hf_oran_symbol_mask_s4,
1860 | &hf_oran_symbol_mask_s3,
1861 | &hf_oran_symbol_mask_s2,
1862 | &hf_oran_symbol_mask_s1,
1863 | &hf_oran_symbol_mask_s0,
1864 | NULL((void*)0)
1865 | };
1866 |
1867 | proto_item *temp_ti = proto_tree_add_bitmask_ret_uint64(tree, tvb, offset,
1868 | hf_oran_symbol_mask,
1869 | ett_oran_symbol_mask, symbol_mask_flags,
1870 | ENC_BIG_ENDIAN0x00000000, &temp_val);
1871 | /* Set out parameters */
1872 | if (symbol_mask) {
1873 | *symbol_mask = (uint32_t)temp_val;
1874 | }
1875 | if (ti) {
1876 | *ti = temp_ti;
1877 | }
1878 | return offset+2;
1879 | }
1880 |
1881 | /* 7.7.1.2 bfwCompHdr (beamforming weight compression header) */
1882 | static int dissect_bfwCompHdr(tvbuff_t *tvb, proto_tree *tree, int offset,
1883 | uint32_t *iq_width, uint32_t *comp_meth, proto_item **comp_meth_ti)
1884 | {
1885 | /* Subtree */
1886 | proto_item *bfwcomphdr_ti = proto_tree_add_string_format(tree, hf_oran_bfwCompHdr,
1887 | tvb, offset, 1, "",
1888 | "bfwCompHdr");
1889 | proto_tree *bfwcomphdr_tree = proto_item_add_subtree(bfwcomphdr_ti, ett_oran_bfwcomphdr);
1890 |
1891 | /* Width and method */
1892 | proto_tree_add_item_ret_uint(bfwcomphdr_tree, hf_oran_bfwCompHdr_iqWidth,
1893 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, iq_width);
1894 | /* Special case: 0 -> 16 */
1895 | *iq_width = (*iq_width==0) ? 16 : *iq_width;
1896 | *comp_meth_ti = proto_tree_add_item_ret_uint(bfwcomphdr_tree, hf_oran_bfwCompHdr_compMeth,
1897 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, comp_meth);
1898 | offset++;
1899 |
1900 | /* Summary */
1901 | proto_item_append_text(bfwcomphdr_ti, " (IqWidth=%u, compMeth=%s)",
1902 | *iq_width,
1903 | val_to_str_const(*comp_meth, bfw_comp_headers_comp_meth, "reserved"));
1904 |
1905 | return offset;
1906 | }
1907 |
1908 | /* Return offset */
1909 | /* Returning number of entries set - would be good to also return an array of set TRX# so could show which array element
1910 | each BFW is actually for.. */
1911 | static int dissect_active_beamspace_coefficient_mask(tvbuff_t *tvb, proto_tree *tree, int offset, unsigned *num_trx_entries, uint16_t **trx_entries)
1912 | {
1913 | /* activeBeamspaceCoefficientMask - ceil(K/8) octets */
1914 | /* K is the number of elements in uncompressed beamforming weight vector.
1915 | * Calculated from parameters describing tx-array or tx-array */
1916 | unsigned k_octets = (pref_data_plane_section_total_rbs + 7) / 8;
1917 |
1918 | static uint16_t trx_enabled[1024];
1919 |
1920 | /* TODO: could use a bigger bitmask array, but for now just uses this bytes-worth for each byte */
1921 | static int * const mask_bits[] = {
1922 | &hf_oran_active_beamspace_coefficient_n1,
1923 | &hf_oran_active_beamspace_coefficient_n2,
1924 | &hf_oran_active_beamspace_coefficient_n3,
1925 | &hf_oran_active_beamspace_coefficient_n4,
1926 | &hf_oran_active_beamspace_coefficient_n5,
1927 | &hf_oran_active_beamspace_coefficient_n6,
1928 | &hf_oran_active_beamspace_coefficient_n7,
1929 | &hf_oran_active_beamspace_coefficient_n8,
1930 | NULL((void*)0)
1931 | };
1932 |
1933 | *num_trx_entries = 0;
1934 | guint64 val;
1935 | for (unsigned n=0; n < k_octets; n++) {
1936 | proto_tree_add_bitmask_ret_uint64(tree, tvb, offset,
1937 | hf_oran_activeBeamspaceCoefficientMask,
1938 | ett_active_beamspace_coefficient_mask, mask_bits,
1939 | ENC_BIG_ENDIAN0x00000000, &val);
1940 | offset++;
1941 | /* Add up the set bits for this byte (but be careful not to count beyond last real K bit..) */
1942 | for (unsigned b=0; b < 8; b++) {
1943 | if ((1 << b) & (unsigned)val) {
1944 | if (((n*8)+b) < pref_data_plane_section_total_rbs) {
1945 | if (*num_trx_entries < 1024-1) { /* Don't write beyond array (which should be plenty big) */
1946 | trx_enabled[(*num_trx_entries)++] = (n*8) + b + 1;
1947 | }
1948 | }
1949 | }
1950 | }
1951 | }
1952 | /* Set pointer to static array */
1953 | *trx_entries = trx_enabled;
1954 |
1955 | /* Show how many bits set */
1956 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_activeBeamspaceCoefficientMask_bits_set, tvb,
1957 | offset-k_octets, k_octets, *num_trx_entries);
1958 | proto_item_set_generated(ti);
1959 |
1960 | return offset;
1961 | }
1962 |
1963 | /* 7.7.1.3 bfwCompParam (beamforming weight compression parameter).
1964 | * Depends upon passed-in bfwCompMeth (field may be empty) */
1965 | static int dissect_bfwCompParam(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo, int offset,
1966 | proto_item *meth_ti, uint32_t *bfw_comp_method,
1967 | uint32_t *exponent, bool_Bool *supported, unsigned *num_trx_entries, uint16_t **trx_entries)
1968 | {
1969 | if (*bfw_comp_method == COMP_NONE0) {
1970 | /* Absent! */
1971 | *num_trx_entries = 0;
1972 | *supported = true1;
1973 | return offset;
1974 | }
1975 |
1976 | /* Subtree */
1977 | proto_item *bfwcompparam_ti = proto_tree_add_string_format(tree, hf_oran_bfwCompParam,
1978 | tvb, offset, 1, "",
1979 | "bfwCompParam");
1980 | proto_tree *bfwcompparam_tree = proto_item_add_subtree(bfwcompparam_ti, ett_oran_bfwcompparam);
1981 |
1982 | proto_item_append_text(bfwcompparam_ti,
1983 | " (meth=%s)", val_to_str_const(*bfw_comp_method, bfw_comp_headers_comp_meth, "reserved"));
1984 |
1985 | *num_trx_entries = 0;
1986 | *supported = false0;
1987 | switch (*bfw_comp_method) {
1988 | case COMP_BLOCK_FP1: /* block floating point */
1989 | /* 4 reserved bits + exponent */
1990 | proto_tree_add_item_ret_uint(bfwcompparam_tree, hf_oran_exponent,
1991 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, exponent);
1992 | proto_item_append_text(bfwcompparam_ti, " exponent=%u", *exponent);
1993 | *supported = true1;
1994 | offset++;
1995 | break;
1996 | case COMP_BLOCK_SCALE2: /* block scaling */
1997 | /* Separate into integer and fractional bits? */
1998 | proto_tree_add_item(bfwcompparam_tree, hf_oran_blockScaler,
1999 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2000 | offset++;
2001 | break;
2002 | case COMP_U_LAW3: /* u-law */
2003 | /* compBitWidth, compShift */
2004 | proto_tree_add_item(bfwcompparam_tree, hf_oran_compBitWidth,
2005 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2006 | proto_tree_add_item(bfwcompparam_tree, hf_oran_compShift,
2007 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2008 | offset++;
2009 | break;
2010 | case 4: /* beamspace I (BLOCK SCALING) */
2011 | /* activeBeamspaceCoefficientMask */
2012 | offset = dissect_active_beamspace_coefficient_mask(tvb, bfwcompparam_tree, offset, num_trx_entries, trx_entries);
2013 | *bfw_comp_method = COMP_BLOCK_SCALE2;
2014 | *supported = false0; /* TODO: true once BLOCK SCALE is supported */
2015 | break;
2016 | case 5: /* beamspace II (BLOCK FLOATING POINT) */
2017 | /* activeBeamspaceCoefficientMask */
2018 | offset = dissect_active_beamspace_coefficient_mask(tvb, bfwcompparam_tree, offset, num_trx_entries, trx_entries);
2019 | /* reserved (4 bits) + exponent (4 bits) */
2020 | proto_tree_add_item(bfwcompparam_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
2021 | proto_tree_add_item_ret_uint(bfwcompparam_tree, hf_oran_exponent, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, exponent);
2022 | offset += 1;
2023 | *bfw_comp_method = COMP_BLOCK_FP1;
2024 | *supported = true1;
2025 | break;
2026 |
2027 | default:
2028 | /* Not handled */
2029 | break;
2030 | }
2031 |
2032 | /* Can't go on if compression scheme not supported */
2033 | if (!(*supported) && meth_ti) {
2034 | expert_add_info_format(pinfo, meth_ti, &ei_oran_unsupported_bfw_compression_method,
2035 | "BFW Compression method %u (%s) not decompressed by dissector",
2036 | *bfw_comp_method,
2037 | val_to_str_const(*bfw_comp_method, bfw_comp_headers_comp_meth, "reserved"));
2038 | }
2039 | return offset;
2040 | }
2041 |
2042 |
2043 | /* Special case for uncompressed/16-bit value */
2044 | static float uncompressed_to_float(uint32_t h)
2045 | {
2046 | int16_t i16 = h & 0x0000ffff;
2047 | if (show_unscaled_values) {
2048 | return (float)i16;
2049 | }
2050 | return ((float)i16) / 0x7fff;
2051 | }
2052 |
2053 | /* Decompress I/Q value, taking into account method, width, exponent, other input-specific methods */
2054 | static float decompress_value(uint32_t bits, uint32_t comp_method, uint8_t iq_width,
2055 | uint32_t exponent,
2056 | /* Modulation compression settings. N.B. should also pass in PRB + symbol? */
2057 | mod_compr_params_t *m_c_p, uint8_t re)
2058 | {
2059 | switch (comp_method) {
2060 | case COMP_NONE0: /* no compression */
2061 | return uncompressed_to_float(bits);
2062 |
2063 | case COMP_BLOCK_FP1: /* block floating point */
2064 | case BFP_AND_SELECTIVE_RE5:
2065 | {
2066 | /* A.1.3 Block Floating Point Decompression Algorithm */
2067 | int32_t cPRB = bits;
2068 | uint32_t scaler = 1 << exponent; /* i.e. 2^exponent */
2069 |
2070 | /* Check last bit, in case we need to flip to -ve */
2071 | if (cPRB >= (1<<(iq_width-1))) {
2072 | cPRB -= (1<<iq_width);
2073 | }
2074 |
2075 | /* Unscale (8.1.3.1) */
2076 | cPRB *= scaler;
2077 | if (show_unscaled_values) {
2078 | return (float)cPRB;
2079 | }
2080 |
2081 | uint32_t mantissa_scale_factor = 1 << (iq_width-1); /* 2^(mantissabits-1) */
2082 | uint32_t exp_scale_factor = 1 << 15; /* 2^(2^exponentbits - 1 ) The exponent bit width is fixed to 4, so the maximum exponent is 15 */
2083 |
2084 | float ret = cPRB / ((float)(mantissa_scale_factor*exp_scale_factor));
2085 | return ret;
2086 | }
2087 |
2088 | case COMP_BLOCK_SCALE2:
2089 | case COMP_U_LAW3:
2090 | /* Not supported! But will be reported as expert info outside of this function! */
2091 | return 0.0;
2092 |
2093 | case COMP_MODULATION4:
2094 | case MOD_COMPR_AND_SELECTIVE_RE6:
2095 | {
2096 | /* Described in A.5 (with pseudo code) */
2097 | /* N.B., Applies to downlink data only - is not used for BFW */
2098 |
2099 | /* Defaults if not overridden. TODO: what should these be? */
2100 | bool_Bool csf = false0;
2101 | //double mcScaler = (double)(1 << 11);
2102 |
2103 |
2104 | /* Find csf + mcScaler to use. Non-default configs gleaned from SE 4,5,23 */
2105 | /* TODO: should ideally be filtering by symbol and PRB too (at least from SE23) */
2106 | if (re > 0 && m_c_p && m_c_p->num_configs > 0) {
2107 | for (unsigned c=0; c<m_c_p->num_configs; c++) {
2108 | if (m_c_p->configs[c].mod_compr_re_mask & (1 << (12-re))) {
2109 | /* Return first (should be only) found */
2110 | csf = m_c_p->configs[c].mod_compr_csf;
2111 | //mcScaler = m_c_p->configs[c].mod_compr_scaler;
2112 | break;
2113 | }
2114 | }
2115 | }
2116 |
2117 |
2118 | int32_t cPRB = bits;
2119 | //uint32_t scaler = 1 << exponent; /* i.e. 2^exponent */
2120 |
2121 | /* Check last bit, in case we need to flip to -ve */
2122 | if (cPRB >= (1<<(iq_width-1))) {
2123 | cPRB -= (1<<iq_width);
| Value stored to 'cPRB' is never read
2124 | }
2125 |
2126 | if (csf) {
2127 | /* TODO: unshift the constellation point */
2128 | }
2129 |
2130 | /* TODO: scale the constellation point */
2131 |
2132 | /* Not returning a calculated value yet */
2133 | return 0.0;
2134 | }
2135 |
2136 | default:
2137 | /* Not supported! But will be reported as expert info outside of this function! */
2138 | return 0.0;
2139 | }
2140 | }
2141 |
2142 | /* Out-of-range value used for special case */
2143 | #define ORPHAN_BUNDLE_NUMBER999 999
2144 |
2145 | /* Bundle of PRBs/TRX I/Q samples (ext 11) */
2146 | static uint32_t dissect_bfw_bundle(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo, unsigned offset,
2147 | proto_item *comp_meth_ti, uint32_t bfwcomphdr_comp_meth,
2148 | mod_compr_params_t *mod_compr_params,
2149 | uint32_t num_weights_per_bundle,
2150 | uint8_t iq_width,
2151 | unsigned bundle_number,
2152 | unsigned first_prb, unsigned last_prb, bool_Bool is_orphan)
2153 | {
2154 | /* Set bundle name */
2155 | char bundle_name[32];
2156 | if (!is_orphan) {
2157 | snprintf(bundle_name, 32, "Bundle %3u", bundle_number);
2158 | }
2159 | else {
2160 | g_strlcpy(bundle_name, "Orphaned ", 32);
2161 | }
2162 |
2163 | /* Create Bundle root */
2164 | proto_item *bundle_ti;
2165 | if (first_prb != last_prb) {
2166 | bundle_ti = proto_tree_add_string_format(tree, hf_oran_bfw_bundle,
2167 | tvb, offset, 0, "",
2168 | "%s: (PRBs %3u-%3u)",
2169 | bundle_name,
2170 | first_prb, last_prb);
2171 | }
2172 | else {
2173 | bundle_ti = proto_tree_add_string_format(tree, hf_oran_bfw_bundle,
2174 | tvb, offset, 0, "",
2175 | "%s: (PRB %3u)",
2176 | bundle_name,
2177 | first_prb);
2178 | }
2179 | proto_tree *bundle_tree = proto_item_add_subtree(bundle_ti, ett_oran_bfw_bundle);
2180 |
2181 | /* Generated bundle id */
2182 | proto_item *bundleid_ti = proto_tree_add_uint(bundle_tree, hf_oran_bfw_bundle_id, tvb, 0, 0,
2183 | bundle_number);
2184 | proto_item_set_generated(bundleid_ti);
2185 | proto_item_set_hidden(bundleid_ti);
2186 |
2187 | /* bfwCompParam */
2188 | bool_Bool compression_method_supported = false0;
2189 | unsigned exponent = 0;
2190 | unsigned num_trx_entries = 0;
2191 | uint16_t *trx_entries;
2192 | offset = dissect_bfwCompParam(tvb, bundle_tree, pinfo, offset, comp_meth_ti,
2193 | &bfwcomphdr_comp_meth, &exponent, &compression_method_supported,
2194 | &num_trx_entries, &trx_entries);
2195 |
2196 | /* Can't show details of unsupported compression method */
2197 | if (!compression_method_supported) {
2198 | /* Don't know how to show, so give up */
2199 | return offset;
2200 | }
2201 |
2202 | /* Create Bundle subtree */
2203 | int bit_offset = offset*8;
2204 | int bfw_offset;
2205 | int prb_offset = offset;
2206 |
2207 | /* contInd */
2208 | proto_tree_add_item(bundle_tree, hf_oran_cont_ind,
2209 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2210 | /* beamId */
2211 | uint32_t beam_id;
2212 | proto_tree_add_item_ret_uint(bundle_tree, hf_oran_beam_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &beam_id);
2213 | proto_item_append_text(bundle_ti, " (beamId:%u) ", beam_id);
2214 | bit_offset += 16;
2215 |
2216 | /* Number of weights per bundle (from preference) */
2217 | proto_item *wpb_ti = proto_tree_add_uint(bundle_tree, hf_oran_num_weights_per_bundle, tvb, 0, 0,
2218 | num_weights_per_bundle);
2219 | proto_item_set_generated(wpb_ti);
2220 |
2221 | /* Add the weights for this bundle. Overwrite with what was seen in bfwCompParam if beamspace */
2222 | if (num_trx_entries != 0) {
2223 | num_weights_per_bundle = num_trx_entries;
2224 | }
2225 |
2226 | for (unsigned w=0; w < num_weights_per_bundle; w++) {
2227 |
2228 | uint16_t trx_index = (num_trx_entries) ? trx_entries[w] : w+1;
2229 |
2230 | /* Create subtree */
2231 | bfw_offset = bit_offset / 8;
2232 | uint8_t bfw_extent = ((bit_offset + (iq_width*2)) / 8) - bfw_offset;
2233 | proto_item *bfw_ti = proto_tree_add_string_format(bundle_tree, hf_oran_bfw,
2234 | tvb, bfw_offset, bfw_extent,
2235 | "", "TRX %3u: (", trx_index);
2236 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
2237 |
2238 | /* I */
2239 | /* Get bits, and convert to float. */
2240 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, iq_width, ENC_BIG_ENDIAN0x00000000);
2241 | float value = decompress_value(bits, bfwcomphdr_comp_meth, iq_width,
2242 | exponent, mod_compr_params, 0 /* RE */);
2243 | /* Add to tree. */
2244 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8, (iq_width+7)/8, value, "#%u=%f", w, value);
2245 | bit_offset += iq_width;
2246 | proto_item_append_text(bfw_ti, "I%u=%f ", w, value);
2247 |
2248 | /* Q */
2249 | /* Get bits, and convert to float. */
2250 | bits = tvb_get_bits32(tvb, bit_offset, iq_width, ENC_BIG_ENDIAN0x00000000);
2251 | value = decompress_value(bits, bfwcomphdr_comp_meth, iq_width,
2252 | exponent, mod_compr_params, 0 /* RE */);
2253 | /* Add to tree. */
2254 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8, (iq_width+7)/8, value, "#%u=%f", w, value);
2255 | bit_offset += iq_width;
2256 | proto_item_append_text(bfw_ti, "Q%u=%f)", w, value);
2257 | }
2258 |
2259 | /* Set extent of bundle */
2260 | proto_item_set_len(bundle_ti, (bit_offset+7)/8 - prb_offset);
2261 |
2262 | return (bit_offset+7)/8;
2263 | }
2264 |
2265 | /* Return new bit offset. in/out will always be byte-aligned.. */
2266 | static int dissect_ciCompParam(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo _U___attribute__((unused)), unsigned bit_offset,
2267 | unsigned comp_meth, uint8_t *exponent)
2268 | {
2269 | if (comp_meth == COMP_NONE0) {
2270 | /* Nothing in frame so don't even create subtree */
2271 | return bit_offset;
2272 | }
2273 |
2274 | /* Subtree */
2275 | proto_item *cicompparam_ti = proto_tree_add_string_format(tree, hf_oran_ciCompParam,
2276 | tvb, bit_offset/8, 1, "",
2277 | "ciCompParam");
2278 | proto_tree *cicompparam_tree = proto_item_add_subtree(cicompparam_ti, ett_oran_cicompparam);
2279 | uint32_t ci_exponent;
2280 |
2281 | /* Contents differ by compression method */
2282 | switch (comp_meth) {
2283 | case COMP_BLOCK_FP1:
2284 | proto_tree_add_item(cicompparam_tree, hf_oran_reserved_4bits, tvb, bit_offset/8, 1, ENC_NA0x00000000);
2285 | proto_tree_add_item_ret_uint(cicompparam_tree, hf_oran_exponent,
2286 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000, &ci_exponent);
2287 | *exponent = ci_exponent;
2288 | proto_item_append_text(cicompparam_ti, " (Exponent=%u)", ci_exponent);
2289 | bit_offset += 8; /* one byte */
2290 | break;
2291 | case COMP_BLOCK_SCALE2:
2292 | /* Separate into integer (1) and fractional (7) bits? */
2293 | proto_tree_add_item(cicompparam_tree, hf_oran_blockScaler,
2294 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000);
2295 | bit_offset += 8;
2296 | break;
2297 | case COMP_U_LAW3:
2298 | /* compBitWidth, compShift (4 bits each) */
2299 | proto_tree_add_item(cicompparam_tree, hf_oran_compBitWidth,
2300 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000);
2301 | proto_tree_add_item(cicompparam_tree, hf_oran_compShift,
2302 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000);
2303 | bit_offset += 8;
2304 | break;
2305 |
2306 | default:
2307 | /* reserved, ? bytes of zeros.. */
2308 | break;
2309 | }
2310 |
2311 | return bit_offset;
2312 | }
2313 |
2314 | /* frameStructure (7.5.2.13) */
2315 | static unsigned dissect_frame_structure(proto_item *tree, tvbuff_t *tvb, unsigned offset,
2316 | uint32_t subframeId, uint32_t slotId)
2317 | {
2318 | uint32_t scs;
2319 | /* FFT Size (4 bits) */
2320 | proto_tree_add_item(tree, hf_oran_frameStructure_fft, tvb, offset, 1, ENC_NA0x00000000);
2321 | /* Subcarrier spacing (SCS) */
2322 | proto_tree_add_item_ret_uint(tree, hf_oran_frameStructure_subcarrier_spacing, tvb, offset, 1, ENC_NA0x00000000, &scs);
2323 |
2324 | /* Show slot within frame as a generated field. See table 7.5.13-3 */
2325 | uint32_t slots_per_subframe = 1;
2326 | if (scs <= 4) {
2327 | slots_per_subframe = 1 << scs;
2328 | }
2329 | if (scs <= 4 || scs >= 12) {
2330 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_slot_within_frame, tvb, 0, 0,
2331 | (slots_per_subframe*subframeId) + slotId);
2332 | proto_item_set_generated(ti);
2333 | }
2334 | return offset + 1;
2335 | }
2336 |
2337 | static unsigned dissect_csf(proto_item *tree, tvbuff_t *tvb, unsigned bit_offset,
2338 | unsigned iq_width, bool_Bool *p_csf)
2339 | {
2340 | proto_item *csf_ti;
2341 | uint64_t csf;
2342 | csf_ti = proto_tree_add_bits_ret_val(tree, hf_oran_csf, tvb, bit_offset, 1, &csf, ENC_BIG_ENDIAN0x00000000);
2343 | if (csf) {
2344 | /* Table 7.7.4.2-1 Constellation shift definition (index is udIqWidth) */
2345 | const char* shift_value[] = { "n/a", "1/2", "1/4", "1/8", "1/16", "1/32" };
2346 | if (iq_width >=1 && iq_width <= 5) {
2347 | proto_item_append_text(csf_ti, " (Shift Value is %s)", shift_value[iq_width]);
2348 | }
2349 | }
2350 |
2351 | /* Set out parameter */
2352 | if (p_csf != NULL((void*)0)) {
2353 | *p_csf = (csf!=0);
2354 | }
2355 | return bit_offset+1;
2356 | }
2357 |
2358 |
2359 | /* Section 7.
2360 | * N.B. these are the green parts of the tables showing Section Types, differing by section Type */
2361 | static int dissect_oran_c_section(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo,
2362 | flow_state_t* state,
2363 | uint32_t sectionType, oran_tap_info *tap_info, proto_item *protocol_item,
2364 | uint32_t subframeId, uint32_t slotId,
2365 | uint8_t ci_iq_width, uint8_t ci_comp_meth, unsigned ci_comp_opt,
2366 | unsigned num_sinr_per_prb)
2367 | {
2368 | unsigned offset = 0;
2369 | proto_tree *c_section_tree = NULL((void*)0);
2370 | proto_item *sectionHeading = NULL((void*)0);
2371 |
2372 | /* Section subtree */
2373 | sectionHeading = proto_tree_add_string_format(tree, hf_oran_c_section,
2374 | tvb, offset, 0, "", "Section");
2375 | c_section_tree = proto_item_add_subtree(sectionHeading, ett_oran_c_section);
2376 |
2377 | uint32_t sectionId = 0;
2378 |
2379 | uint32_t startPrbc=0, startPrbu=0;
2380 | uint32_t numPrbc=0, numPrbu=0;
2381 | uint32_t ueId = 0;
2382 | proto_item *ueId_ti = NULL((void*)0);
2383 | uint32_t beamId = 0;
2384 | proto_item *beamId_ti = NULL((void*)0);
2385 | bool_Bool beamId_ignored = false0;
2386 |
2387 | proto_item *numsymbol_ti = NULL((void*)0);
2388 | bool_Bool numsymbol_ignored = false0;
2389 |
2390 | proto_item *numprbc_ti = NULL((void*)0);
2391 |
2392 | /* Config affecting ext11 bundles (initially unset) */
2393 | ext11_settings_t ext11_settings;
2394 | memset(&ext11_settings, 0, sizeof(ext11_settings));
2395 |
2396 | /* Section Type 10 needs to keep track of PRB range that should be reported
2397 | for msgTypeId=5 (Interference plus Noise for unallocated PRBs) */
2398 | /* All PRBs start as false */
2399 | #define MAX_PRBS273 273
2400 | bool_Bool prbs_for_st10_type5[MAX_PRBS273];
2401 | memset(&prbs_for_st10_type5, 0, sizeof(prbs_for_st10_type5));
2402 |
2403 |
2404 | #define MAX_UEIDS16 16
2405 | uint32_t ueids[MAX_UEIDS16];
2406 | uint32_t number_of_ueids = 0;
2407 |
2408 | bool_Bool extension_flag = false0;
2409 |
2410 | /* These sections (ST0, ST1, ST2, ST3, ST5, ST9, ST10, ST11) are similar, so handle as common with per-type differences */
2411 | if (((sectionType <= SEC_C_UE_SCHED) || (sectionType >= SEC_C_SINR_REPORTING)) &&
2412 | (sectionType != SEC_C_SLOT_CONTROL)) {
2413 |
2414 | /* sectionID */
2415 | proto_item *ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_section_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &sectionId);
2416 | if (sectionId == 4095) {
2417 | proto_item_append_text(ti, " (not default coupling C/U planes using sectionId)");
2418 | }
2419 | offset++;
2420 |
2421 | if (tap_info->num_section_ids < MAX_SECTION_IDs32) {
2422 | tap_info->section_ids[tap_info->num_section_ids++] = sectionId;
2423 | }
2424 |
2425 | /* rb */
2426 | uint32_t rb;
2427 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_rb, tvb, offset, 1, ENC_NA0x00000000, &rb);
2428 | /* symInc (1 bit) */
2429 | if (sectionType != SEC_C_RRM_MEAS_REPORTS && /* Section Type 10 */
2430 | sectionType != SEC_C_REQUEST_RRM_MEAS) { /* Section Type 11 */
2431 | unsigned int sym_inc;
2432 | proto_item *sym_inc_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_symInc, tvb, offset, 1, ENC_NA0x00000000, &sym_inc);
2433 | if (sym_inc !=0 && (sectionType == SEC_C_SINR_REPORTING)) { /* Section Type 9 */
2434 | /* "0 shall be used" */
2435 | proto_item_append_text(sym_inc_ti, " (should be 0)");
2436 | }
2437 | }
2438 | else {
2439 | /* reserved (1 bit) */
2440 | proto_tree_add_item(c_section_tree, hf_oran_reserved_bit5, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2441 | }
2442 |
2443 | /* startPrbx and numPrbx */
2444 | if (sectionType == SEC_C_SINR_REPORTING) {
2445 | /* startPrbu (10 bits) */
2446 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_startPrbu, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbu);
2447 | offset += 2;
2448 | /* numPrbu */
2449 | numprbc_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numPrbu, tvb, offset, 1, ENC_NA0x00000000, &numPrbu);
2450 | if (numPrbu == 0) {
2451 | proto_item_append_text(numprbc_ti, " (all PRBs - configured as %u)", pref_data_plane_section_total_rbs);
2452 | numPrbu = pref_data_plane_section_total_rbs;
2453 | }
2454 | offset += 1;
2455 | }
2456 | else {
2457 | /* startPrbc (10 bits) */
2458 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_startPrbc, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbc);
2459 | offset += 2;
2460 | /* numPrbc */
2461 | numprbc_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numPrbc, tvb, offset, 1, ENC_NA0x00000000, &numPrbc);
2462 | if (numPrbc == 0) {
2463 | proto_item_append_text(numprbc_ti, " (all PRBs - configured as %u)", pref_data_plane_section_total_rbs);
2464 | /* TODO: should probably set to pref_data_plane_section_total_rbs, and define MAX_PRBS to > 273 ? */
2465 | numPrbc = MAX_PRBS273;
2466 | }
2467 | offset += 1;
2468 | }
2469 |
2470 | /* Start with range from section. May get changed by SE6, SE12, SE20 */
2471 | for (unsigned n=startPrbc; n < startPrbc+numPrbc; n++) {
2472 | if (n < MAX_PRBS273) {
2473 | prbs_for_st10_type5[n] = true1;
2474 | }
2475 | }
2476 |
2477 | if (sectionType != SEC_C_SINR_REPORTING) { /* Section Type 9 */
2478 | static int * const remask_flags[] = {
2479 | &hf_oran_reMask_re1,
2480 | &hf_oran_reMask_re2,
2481 | &hf_oran_reMask_re3,
2482 | &hf_oran_reMask_re4,
2483 | &hf_oran_reMask_re5,
2484 | &hf_oran_reMask_re6,
2485 | &hf_oran_reMask_re7,
2486 | &hf_oran_reMask_re8,
2487 | &hf_oran_reMask_re9,
2488 | &hf_oran_reMask_re10,
2489 | &hf_oran_reMask_re11,
2490 | &hf_oran_reMask_re12,
2491 | NULL((void*)0)
2492 | };
2493 |
2494 | /* reMask */
2495 | uint64_t remask;
2496 | proto_tree_add_bitmask_ret_uint64(c_section_tree, tvb, offset,
2497 | hf_oran_reMask, ett_oran_remask, remask_flags, ENC_BIG_ENDIAN0x00000000, &remask);
2498 | offset++;
2499 | /* numSymbol */
2500 | /* TODO: should warn if startSymbol + numSymbol would be > 14? */
2501 | uint32_t numSymbol;
2502 | numsymbol_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numSymbol, tvb, offset, 1, ENC_NA0x00000000, &numSymbol);
2503 | if ((sectionType == SEC_C_RRM_MEAS_REPORTS) && (numSymbol != 14)) { /* Section type 10 */
2504 | proto_item_append_text(numsymbol_ti, " (for ST10, should be 14!)");
2505 | expert_add_info_format(pinfo, numsymbol_ti, &ei_oran_st10_numsymbol_not_14,
2506 | "numSymbol should be 14 for ST10 - found %u", numSymbol);
2507 | }
2508 | offset++;
2509 |
2510 | /* [ef] (extension flag) */
2511 | switch (sectionType) {
2512 | case SEC_C_UNUSED_RB: /* Section Type 0 */
2513 | case SEC_C_NORMAL: /* Section Type 1 */
2514 | case SEC_C_PRACH: /* Section Type 3 */
2515 | case SEC_C_UE_SCHED: /* Section Type 5 */
2516 | case SEC_C_RRM_MEAS_REPORTS: /* Section Type 10 */
2517 | case SEC_C_REQUEST_RRM_MEAS: /* Section Type 11 */
2518 | proto_tree_add_item_ret_boolean(c_section_tree, hf_oran_ef, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &extension_flag);
2519 | break;
2520 | default:
2521 | /* Other section types don't support extensions */
2522 | break;
2523 | }
2524 |
2525 | write_section_info(sectionHeading, pinfo, protocol_item, sectionId, startPrbc, numPrbc, rb);
2526 | proto_item_append_text(sectionHeading, ", Symbols: %2u", numSymbol);
2527 |
2528 | if (numPrbc == 0) {
2529 | /* Special case for all PRBs */
2530 | numPrbc = pref_data_plane_section_total_rbs;
2531 | startPrbc = 0; /* may already be 0... */
2532 | }
2533 | }
2534 | else {
2535 | /* Section Type 9 */
2536 | write_section_info(sectionHeading, pinfo, protocol_item, sectionId, startPrbu, numPrbu, rb);
2537 | proto_item_append_text(sectionHeading, ", numSinrPerPrb: %2u", num_sinr_per_prb);
2538 | }
2539 |
2540 | /* Section type specific fields (after 'numSymbol') */
2541 | switch (sectionType) {
2542 | case SEC_C_UNUSED_RB: /* Section Type 0 - Table 7.4.2-1 */
2543 | /* reserved (15 bits) */
2544 | proto_tree_add_item(c_section_tree, hf_oran_reserved_15bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2545 | offset += 2;
2546 | break;
2547 |
2548 | case SEC_C_NORMAL: /* Section Type 1 - Table 7.4.3-1 */
2549 | /* beamId */
2550 | beamId_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &beamId);
2551 | offset += 2;
2552 |
2553 | proto_item_append_text(sectionHeading, ", BeamId: %d", beamId);
2554 | break;
2555 |
2556 | case SEC_C_PRACH: /* Section Type 3 - Table 7.4.5-1 */
2557 | {
2558 | /* beamId */
2559 | beamId_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &beamId);
2560 | offset += 2;
2561 |
2562 | /* freqOffset */
2563 | int32_t freqOffset; /* Yes, this is signed, so the implicit cast is intentional. */
2564 | proto_item *freq_offset_item = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_freqOffset, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000, &freqOffset);
2565 | freqOffset |= 0xff000000; /* Must sign-extend */
2566 | proto_item_set_text(freq_offset_item, "Frequency offset: %d \u0394f", freqOffset);
2567 | offset += 3;
2568 |
2569 | /* reserved */
2570 | proto_tree_add_item(c_section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
2571 | offset += 1;
2572 |
2573 | proto_item_append_text(sectionHeading, ", BeamId: %d, FreqOffset: %d \u0394f", beamId, freqOffset);
2574 | break;
2575 | }
2576 |
2577 | case SEC_C_UE_SCHED: /* Section Type 5 - Table 7.4.7-1 */
2578 | case SEC_C_RRM_MEAS_REPORTS: /* Section Type 10 - Table 7.4.12-1 */
2579 | /* ueId */
2580 | ueId_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_ueId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ueId);
2581 | offset += 2;
2582 | if (ueId == 0x7fff) {
2583 | proto_item_append_text(ueId_ti, " (PRBs not scheduled for eAxC ID in transport header)");
2584 | }
2585 | else {
2586 | ueids[number_of_ueids++] = ueId;
2587 | }
2588 |
2589 | proto_item_append_text(sectionHeading, ", UEId: %d", ueId);
2590 | break;
2591 |
2592 | case SEC_C_SINR_REPORTING: /* Section Type 9 - SINR Reporting */
2593 | {
2594 | /* Hidden filter for bf (DMFS-BF) */
2595 | proto_item *bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
2596 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
2597 |
2598 | unsigned bit_offset = offset*8;
2599 |
2600 | /* sinr iqWidth */
2601 | proto_item *iq_width_item = proto_tree_add_uint(c_section_tree, hf_oran_sinrCompHdrIqWidth_pref, tvb, 0, 0, pref_sample_bit_width_sinr);
2602 | proto_item_append_text(iq_width_item, " (from preferences)");
2603 | proto_item_set_generated(iq_width_item);
2604 |
2605 | /* sinr compMethod */
2606 | proto_item *sinr_comp_meth_item = proto_tree_add_uint(c_section_tree, hf_oran_sinrCompHdrMeth_pref, tvb, 0, 0, pref_iqCompressionSINR);
2607 | proto_item_append_text(sinr_comp_meth_item, " (from preferences)");
2608 | proto_item_set_generated(sinr_comp_meth_item);
2609 |
2610 | /* Add SINR entries for each PRB */
2611 | for (unsigned prb=0; prb < numPrbu; prb++) {
2612 | /* TODO: create a subtree for each PRB entry with good summary? */
2613 |
2614 | /* Each prb starts byte-aligned */
2615 | bit_offset = ((bit_offset+7)/8) * 8;
2616 |
2617 | /* N.B., using width/method from UL U-plane preferences, not certain that this is correct.. */
2618 |
2619 | /* sinrCompParam (udCompParam format, may be empty) */
2620 | uint32_t exponent = 0; /* N.B. init to silence warnings, but will always be set if read in COMP_BLOCK_FP case */
2621 | uint16_t sReSMask;
2622 | bit_offset = dissect_udcompparam(tvb, pinfo, c_section_tree, bit_offset/8,
2623 | pref_iqCompressionSINR, &exponent, &sReSMask,
2624 | true1) * 8; /* last param is for_sinr */
2625 |
2626 | /* sinrValues for this PRB. */
2627 | /* TODO: not sure how numSinrPerPrb interacts with rb==1... */
2628 | for (unsigned n=0; n < num_sinr_per_prb; n++) {
2629 | unsigned sinr_bits = tvb_get_bits32(tvb, bit_offset, pref_sample_bit_width_sinr, ENC_BIG_ENDIAN0x00000000);
2630 |
2631 | /* Using SINR compression settings from preferences */
2632 | float value = decompress_value(sinr_bits,
2633 | pref_iqCompressionSINR, pref_sample_bit_width_sinr,
2634 | exponent,
2635 | (state) ? &state->mod_comp_params : NULL((void*)0), 0 /* RE */);
2636 | unsigned sample_len_in_bytes = ((bit_offset%8)+pref_sample_bit_width_sinr+7)/8;
2637 | proto_item *val_ti = proto_tree_add_float(c_section_tree, hf_oran_sinr_value, tvb,
2638 | bit_offset/8, sample_len_in_bytes, value);
2639 |
2640 | /* Show here which subcarriers share which values (they all divide 12..) */
2641 | if (num_sinr_per_prb == 12) {
2642 | proto_item_append_text(val_ti, " (PRB=%u, subcarrier %u)",
2643 | startPrbu+(prb*(rb+1)),
2644 | n*(12/num_sinr_per_prb));
2645 | }
2646 | else {
2647 | proto_item_append_text(val_ti, " (PRB=%u, subcarriers %u-%u)",
2648 | startPrbu+(prb*(rb+1)),
2649 | n*(12/num_sinr_per_prb), (n+1)*(12/num_sinr_per_prb)-1);
2650 | }
2651 | bit_offset += pref_sample_bit_width_sinr;
2652 | }
2653 |
2654 | /* 1-byte alignment per PRB (7.2.11) */
2655 | offset = (bit_offset+7)/8;
2656 | bit_offset = offset*8;
2657 | }
2658 | break;
2659 | }
2660 | case SEC_C_REQUEST_RRM_MEAS: /* Section Type 11 - Request RRM Measurements */
2661 | /* Reserved (15 bits) */
2662 | proto_tree_add_item(c_section_tree, hf_oran_reserved_15bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2663 | offset += 2;
2664 | break;
2665 |
2666 | default:
2667 | break;
2668 | }
2669 | }
2670 | else if (sectionType == SEC_C_CH_INFO) { /* Section Type 6 */
2671 | /* ef */
2672 | proto_tree_add_item_ret_boolean(c_section_tree, hf_oran_ef, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &extension_flag);
2673 | /* ueId */
2674 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_ueId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ueId);
2675 | offset += 2;
2676 | /* regularizationFactor */
2677 | proto_tree_add_item(c_section_tree, hf_oran_regularizationFactor, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
2678 | offset += 2;
2679 | /* reserved (4 bits) */
2680 | proto_tree_add_item(c_section_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
2681 | /* rb ("Value=0 shall be set") */
2682 | uint32_t rb;
2683 | proto_item *rb_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_rb, tvb, offset, 1, ENC_NA0x00000000, &rb);
2684 | if (rb != 0) {
2685 | proto_item_append_text(rb_ti, " (should be set to 0)");
2686 | expert_add_info(pinfo, rb_ti, &ei_oran_st6_rb_shall_be_0);
2687 | }
2688 | /* symInc */
2689 | proto_tree_add_item(c_section_tree, hf_oran_symInc, tvb, offset, 1, ENC_NA0x00000000);
2690 | /* startPrbc */
2691 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_startPrbc, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbc);
2692 | offset += 2;
2693 | /* numPrbc */
2694 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numPrbc, tvb, offset, 1, ENC_NA0x00000000, &numPrbc);
2695 | offset += 1;
2696 |
2697 | /* Hidden filter for bf */
2698 | proto_item *bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
2699 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
2700 |
2701 | /* ciIsample,ciQsample pairs */
2702 | unsigned m;
2703 | unsigned prb;
2704 | uint32_t bit_offset = offset*8;
2705 |
2706 | /* Antenna count from preference */
2707 | unsigned num_trx = pref_num_bf_antennas;
2708 |
2709 | write_channel_section_info(sectionHeading, pinfo,
2710 | sectionId, ueId, startPrbc, numPrbc, num_trx);
2711 |
2712 | bool_Bool first_prb = true1;
2713 | uint8_t exponent = 0;
2714 | for (prb=startPrbc; prb < startPrbc+numPrbc; prb++) {
2715 |
2716 | /* PRB subtree */
2717 | unsigned prb_start_offset = bit_offset;
2718 | proto_item *prb_ti = proto_tree_add_string_format(c_section_tree, hf_oran_samples_prb,
2719 | tvb, bit_offset/8, 0,
2720 | "", "PRB=%u", prb);
2721 | proto_tree *prb_tree = proto_item_add_subtree(prb_ti, ett_oran_prb_cisamples);
2722 |
2723 | /* There may be a ciCompParam here.. */
2724 | if (first_prb || ci_comp_opt==1) {
2725 | bit_offset = dissect_ciCompParam(tvb, prb_tree, pinfo, bit_offset, ci_comp_meth, &exponent);
2726 | }
2727 | first_prb = false0;
2728 |
2729 | /* Antennas */
2730 | for (m=0; m < num_trx; m++) {
2731 |
2732 | unsigned sample_offset = bit_offset / 8;
2733 | uint8_t sample_extent = ((bit_offset + (ci_iq_width*2)) / 8) - sample_offset;
2734 |
2735 | /* Create subtree for antenna */
2736 | proto_item *sample_ti = proto_tree_add_string_format(prb_tree, hf_oran_ciSample,
2737 | tvb, sample_offset, sample_extent,
2738 | "", "TRX=%2u: ", m);
2739 | proto_tree *sample_tree = proto_item_add_subtree(sample_ti, ett_oran_cisample);
2740 |
2741 | /* I */
2742 | /* Get bits, and convert to float. */
2743 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, ci_iq_width, ENC_BIG_ENDIAN0x00000000);
2744 | float value = decompress_value(bits, ci_comp_meth, ci_iq_width, exponent, (state) ? &state->mod_comp_params : NULL((void*)0), 0 /* RE */);
2745 |
2746 | /* Add to tree. */
2747 | proto_tree_add_float_format_value(sample_tree, hf_oran_ciIsample, tvb, bit_offset/8, (ci_iq_width+7)/8, value, "#%u=%f", m, value);
2748 | bit_offset += ci_iq_width;
2749 | proto_item_append_text(sample_ti, "I%u=%f ", m, value);
2750 |
2751 | /* Q */
2752 | /* Get bits, and convert to float. */
2753 | bits = tvb_get_bits32(tvb, bit_offset, ci_iq_width, ENC_BIG_ENDIAN0x00000000);
2754 | value = decompress_value(bits, ci_comp_meth, ci_iq_width, exponent, (state) ? &state->mod_comp_params : NULL((void*)0), 0 /* RE */);
2755 |
2756 | /* Add to tree. */
2757 | proto_tree_add_float_format_value(sample_tree, hf_oran_ciQsample, tvb, bit_offset/8, (ci_iq_width+7)/8, value, "#%u=%f", m, value);
2758 | bit_offset += ci_iq_width;
2759 | proto_item_append_text(sample_ti, "Q%u=%f ", m, value);
2760 | }
2761 | proto_item_set_len(prb_ti, (bit_offset-prb_start_offset+7)/8);
2762 | }
2763 |
2764 | /* Pad out by 1 or 4 bytes, according to preference */
2765 | if (!st6_4byte_alignment) {
2766 | offset = (bit_offset + 7) / 8;
2767 | }
2768 | else {
2769 | int mode = bit_offset % 32;
2770 | if (mode != 0) {
2771 | offset = (bit_offset + (32-mode))/8;
2772 | }
2773 | else {
2774 | offset = bit_offset/8;
2775 | }
2776 | }
2777 | proto_item_set_end(c_section_tree, tvb, offset);
2778 | }
2779 |
2780 | bool_Bool seen_se10 = false0;
2781 | uint32_t numPortc = 0;
2782 | proto_item *bf_ti = NULL((void*)0);
2783 |
2784 | /* Section extension commands */
2785 | while (extension_flag) {
2786 | int extension_start_offset = offset;
2787 |
2788 | /* Prefetch extType so can use specific extension type ett */
2789 | uint32_t exttype = tvb_get_uint8(tvb, offset) & 0x7f;
2790 | uint32_t exttype_ett_index = exttype;
2791 | if (exttype == 0 || exttype > HIGHEST_EXTTYPE28) {
2792 | /* Just use first one if out of range */
2793 | exttype_ett_index = 1;
2794 | }
2795 |
2796 | /* Create subtree for each extension (with summary) */
2797 | proto_item *extension_ti = proto_tree_add_string_format(c_section_tree, hf_oran_extension,
2798 | tvb, offset, 0, "", "Extension");
2799 | proto_tree *extension_tree = proto_item_add_subtree(extension_ti, ett_oran_c_section_extension[exttype_ett_index-1]);
2800 |
2801 | /* ef (i.e. another extension after this one?) */
2802 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_ef, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &extension_flag);
2803 |
2804 | /* extType */
2805 | proto_item *exttype_ti;
2806 | exttype_ti = proto_tree_add_item(extension_tree, hf_oran_exttype, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2807 | offset++;
2808 | proto_item_append_text(sectionHeading, " (ext-%u)", exttype);
2809 |
2810 | proto_item_append_text(extension_ti, " (ext-%u: %s)", exttype, val_to_str_const(exttype, exttype_vals, "Reserved"));
2811 |
2812 | /* Don't tap if out of range. */
2813 | if (exttype > 0 && exttype <= HIGHEST_EXTTYPE28) {
2814 | tap_info->extensions[exttype] = true1;
2815 | }
2816 |
2817 | /* Is this SE allowed for this section type? */
2818 | if (!se_allowed_in_st(exttype, sectionType)) {
2819 | expert_add_info_format(pinfo, extension_tree, &ei_oran_se_on_unsupported_st,
2820 | "SE %u (%s) should not appear in ST %u (%s)!",
2821 | exttype, val_to_str_const(exttype, exttype_vals, "Reserved"),
2822 | sectionType, rval_to_str_const(sectionType, section_types, "Unknown"));
2823 | }
2824 |
2825 |
2826 | /* extLen (number of 32-bit words) */
2827 | uint32_t extlen_len = ((exttype==11)||(exttype==19)||(exttype==20)) ? 2 : 1; /* Extensions 11/19/20 are special */
2828 | uint32_t extlen;
2829 | proto_item *extlen_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_extlen, tvb,
2830 | offset, extlen_len, ENC_BIG_ENDIAN0x00000000, &extlen);
2831 | proto_item_append_text(extlen_ti, " (%u bytes)", extlen*4);
2832 | offset += extlen_len;
2833 | if (extlen == 0) {
2834 | expert_add_info_format(pinfo, extlen_ti, &ei_oran_extlen_zero,
2835 | "extlen value of 0 is reserved");
2836 | /* Break out to avoid infinitely looping! */
2837 | break;
2838 | }
2839 |
2840 | bool_Bool ext_unhandled = false0;
2841 |
2842 | switch (exttype) {
2843 |
2844 | case 1: /* SE 1: Beamforming Weights */
2845 | {
2846 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
2847 | proto_item *comp_meth_ti = NULL((void*)0);
2848 |
2849 | /* Hidden filter for bf */
2850 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
2851 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
2852 |
2853 | /* bfwCompHdr (2 subheaders - bfwIqWidth and bfwCompMeth)*/
2854 | offset = dissect_bfwCompHdr(tvb, extension_tree, offset,
2855 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
2856 |
2857 | /* bfwCompParam */
2858 | uint32_t exponent = 0;
2859 | bool_Bool compression_method_supported = false0;
2860 | unsigned num_trx = 0;
2861 | uint16_t *trx; /* ptr to array */
2862 | offset = dissect_bfwCompParam(tvb, extension_tree, pinfo, offset, comp_meth_ti,
2863 | &bfwcomphdr_comp_meth, &exponent, &compression_method_supported,
2864 | &num_trx, &trx);
2865 |
2866 | /* Can't show details of unsupported compression method */
2867 | if (!compression_method_supported) {
2868 | break;
2869 | }
2870 |
2871 | /* We know:
2872 | - iq_width (above)
2873 | - numBfWeights (taken from preference)
2874 | - remaining bytes in extension
2875 | We can therefore derive TRX (number of antennas).
2876 | */
2877 |
2878 | bool_Bool using_array = false0;
2879 |
2880 | /* I & Q samples
2881 | May know how many entries from activeBeamspaceCoefficientMask. */
2882 | if (num_trx == 0) {
2883 | /* Don't know how many there will be, so just fill available bytes... */
2884 | unsigned weights_bytes = (extlen*4)-3;
2885 | unsigned num_weights_pairs = (weights_bytes*8) / (bfwcomphdr_iq_width*2);
2886 | num_trx = num_weights_pairs;
2887 | }
2888 | else {
2889 | using_array = true1;
2890 | num_trx = pref_num_bf_antennas;
2891 | }
2892 |
2893 | int bit_offset = offset*8;
2894 |
2895 | for (unsigned n=0; n < num_trx; n++) {
2896 | /* Create antenna subtree */
2897 | int bfw_offset = bit_offset / 8;
2898 |
2899 | uint16_t trx_index = (using_array) ? trx[n] : n+1;
2900 |
2901 | proto_item *bfw_ti = proto_tree_add_string_format(extension_tree, hf_oran_bfw,
2902 | tvb, bfw_offset, 0, "", "TRX %3u: (", trx_index);
2903 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
2904 |
2905 | /* I value */
2906 | /* Get bits, and convert to float. */
2907 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
2908 | float value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent, (state) ? &state->mod_comp_params : NULL((void*)0), 0 /* RE */);
2909 | /* Add to tree. */
2910 | proto_tree_add_float(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8,
2911 | (bfwcomphdr_iq_width+7)/8, value);
2912 | bit_offset += bfwcomphdr_iq_width;
2913 | proto_item_append_text(bfw_ti, "I=%f ", value);
2914 |
2915 | /* Leave a gap between I and Q values */
2916 | proto_item_append_text(bfw_ti, " ");
2917 |
2918 | /* Q value */
2919 | /* Get bits, and convert to float. */
2920 | bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
2921 | value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent, (state) ? &state->mod_comp_params : NULL((void*)0), 0 /* RE */);
2922 | /* Add to tree. */
2923 | proto_tree_add_float(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8,
2924 | (bfwcomphdr_iq_width+7)/8, value);
2925 | bit_offset += bfwcomphdr_iq_width;
2926 | proto_item_append_text(bfw_ti, "Q=%f", value);
2927 |
2928 | proto_item_append_text(bfw_ti, ")");
2929 | proto_item_set_len(bfw_ti, (bit_offset+7)/8 - bfw_offset);
2930 | }
2931 | /* Need to round to next byte */
2932 | offset = (bit_offset+7)/8;
2933 |
2934 | break;
2935 | }
2936 |
2937 | case 2: /* SE 2: Beamforming attributes */
2938 | {
2939 | /* Hidden filter for bf */
2940 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
2941 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
2942 |
2943 | /* bfaCompHdr (get widths of fields to follow) */
2944 | uint32_t bfAzPtWidth, bfZePtWidth, bfAz3ddWidth, bfZe3ddWidth;
2945 | /* subtree */
2946 | proto_item *bfa_ti = proto_tree_add_string_format(extension_tree, hf_oran_bfaCompHdr,
2947 | tvb, offset, 2, "", "bfaCompHdr");
2948 | proto_tree *bfa_tree = proto_item_add_subtree(bfa_ti, ett_oran_bfacomphdr);
2949 |
2950 | /* reserved (2 bits) */
2951 | proto_tree_add_item(bfa_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2952 | /* bfAzPtWidth (3 bits) */
2953 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfAzPtWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfAzPtWidth);
2954 | /* bfZePtWidth (3 bits) */
2955 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfZePtWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfZePtWidth);
2956 | offset += 1;
2957 |
2958 | /* reserved (2 bits) */
2959 | proto_tree_add_item(bfa_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2960 | /* bfAz3ddWidth (3 bits) */
2961 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfAz3ddWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfAz3ddWidth);
2962 | /* bfZe3ddWidth (3 bits) */
2963 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfZe3ddWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfZe3ddWidth);
2964 | offset += 1;
2965 |
2966 | unsigned bit_offset = offset*8;
2967 |
2968 | /* bfAzPt */
2969 | if (bfAzPtWidth > 0) {
2970 | proto_tree_add_bits_item(extension_tree, hf_oran_bfAzPt, tvb, bit_offset, bfAzPtWidth+1, ENC_BIG_ENDIAN0x00000000);
2971 | bit_offset += (bfAzPtWidth+1);
2972 | }
2973 | /* bfZePt */
2974 | if (bfZePtWidth > 0) {
2975 | proto_tree_add_bits_item(extension_tree, hf_oran_bfZePt, tvb, bit_offset, bfZePtWidth+1, ENC_BIG_ENDIAN0x00000000);
2976 | bit_offset += (bfZePtWidth+1);
2977 | }
2978 | /* bfAz3dd */
2979 | if (bfAz3ddWidth > 0) {
2980 | proto_tree_add_bits_item(extension_tree, hf_oran_bfAz3dd, tvb, bit_offset, bfAz3ddWidth+1, ENC_BIG_ENDIAN0x00000000);
2981 | bit_offset += (bfAz3ddWidth+1);
2982 | }
2983 | /* bfZe3dd */
2984 | if (bfZe3ddWidth > 0) {
2985 | proto_tree_add_bits_item(extension_tree, hf_oran_bfZe3dd, tvb, bit_offset, bfZe3ddWidth+1, ENC_BIG_ENDIAN0x00000000);
2986 | bit_offset += (bfZe3ddWidth+1);
2987 | }
2988 |
2989 | /* Pad to next byte (unless last 2 fields already fit in this one) */
2990 | if ((bit_offset % 8) > 2) {
2991 | offset = (bit_offset+7) / 8;
2992 | }
2993 | else {
2994 | offset = bit_offset / 8;
2995 | }
2996 |
2997 | /* bfAzSl (3 bits) */
2998 | proto_tree_add_item(extension_tree, hf_oran_bfAzSl, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2999 | /* bfZeSl (3 bits) */
3000 | proto_tree_add_item(extension_tree, hf_oran_bfZeSl, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3001 | offset += 1;
3002 | break;
3003 | }
3004 |
3005 | case 3: /* SE 3: DL precoding parameters */
3006 | {
3007 | /* codebookindex (8 bits) */
3008 | /* "This parameter is not used and shall be set to zero." */
3009 | proto_tree_add_item(extension_tree, hf_oran_codebook_index, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3010 | offset += 1;
3011 | /* layerid */
3012 | uint32_t layerid;
3013 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_layerid, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &layerid);
3014 | /* numLayers */
3015 | proto_tree_add_item(extension_tree, hf_oran_numlayers, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3016 | offset += 1;
3017 |
3018 | /* Stop here for non-first data layer */
3019 | if (layerid != 0 && layerid != 0xf) {
3020 | break;
3021 | }
3022 |
3023 | /* First data layer case */
3024 | /* txScheme */
3025 | proto_tree_add_item(extension_tree, hf_oran_txscheme, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3026 | /* crsReMask */
3027 | proto_tree_add_item(extension_tree, hf_oran_crs_remask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3028 | offset += 2;
3029 |
3030 | /* crsShift (1 bit) */
3031 | proto_tree_add_item(extension_tree, hf_oran_crs_shift, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3032 | /* reserved (3 bits) */
3033 | proto_tree_add_item(extension_tree, hf_oran_reserved_bits123, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3034 | /* crsSymNum (4 bits) */
3035 | proto_tree_add_item(extension_tree, hf_oran_crs_symnum, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3036 | offset += 1;
3037 | /* reserved */
3038 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3039 | offset += 1;
3040 |
3041 | /* reserved (1 bit) */
3042 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3043 | /* beamIdAP1 (15 bits) */
3044 | proto_tree_add_item(extension_tree, hf_oran_beamid_ap1, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3045 | offset += 2;
3046 | /* reserved (1 bit) */
3047 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3048 | /* beamIdAP2 (15 bits) */
3049 | proto_tree_add_item(extension_tree, hf_oran_beamid_ap2, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3050 | offset += 2;
3051 | /* reserved (1 bit) */
3052 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3053 | /* beamIdAP3 (15 bits) */
3054 | proto_tree_add_item(extension_tree, hf_oran_beamid_ap3, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3055 | offset += 2;
3056 | break;
3057 | }
3058 |
3059 | case 4: /* SE 4: Modulation compression params (5.4.7.4) (single sets) */
3060 | {
3061 | /* csf */
3062 | bool_Bool csf;
3063 | dissect_csf(extension_tree, tvb, offset*8, ci_iq_width, &csf);
3064 |
3065 | /* modCompScaler */
3066 | uint32_t modCompScaler;
3067 | proto_item *ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_modcompscaler,
3068 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &modCompScaler);
3069 | offset += 2;
3070 |
3071 | /* Work out and show floating point value too. exponent and mantissa are both unsigned */
3072 | uint16_t exponent = (modCompScaler >> 11) & 0x000f; /* m.s. 4 bits */
3073 | uint16_t mantissa = modCompScaler & 0x07ff; /* l.s. 11 bits */
3074 | double value = ((double)mantissa/(1<<11)) * (1.0 / (1 << exponent));
3075 | proto_item_append_text(ti, " (%f)", value);
3076 |
3077 | /* Store these params in this flow's state */
3078 | if (state && state->mod_comp_params.num_configs < MAX_MOD_COMPR_CONFIGS16) {
3079 | unsigned i = state->mod_comp_params.num_configs;
3080 | state->mod_comp_params.configs[i].mod_compr_re_mask = 0xfff; /* Covers all REs */
3081 | state->mod_comp_params.configs[i].mod_compr_csf = csf;
3082 | state->mod_comp_params.configs[i].mod_compr_scaler = value;
3083 | state->mod_comp_params.num_configs++;
3084 | }
3085 | break;
3086 | }
3087 |
3088 | case 5: /* SE 5: Modulation Compression Additional Parameters (7.7.5) (multiple sets) */
3089 | {
3090 | /* Applies only to section types 1,3 and 5 */
3091 | /* N.B. there may be multiple instances of this SE in the same frame */
3092 |
3093 | /* There may be one or 2 entries, depending upon extlen */
3094 | int sets = 1, reserved_bits = 0;
3095 | switch (extlen) {
3096 | case 2:
3097 | sets = 1;
3098 | reserved_bits = 20;
3099 | break;
3100 | case 3:
3101 | sets = 2;
3102 | reserved_bits = 24;
3103 | break;
3104 | case 4:
3105 | /* sets can be 3 or 4, depending upon whether last 28 bits are 0.. */
3106 | if ((tvb_get_ntohl(tvb, offset+10) & 0x0fffffff) == 0) {
3107 | sets = 3;
3108 | reserved_bits = 28;
3109 | }
3110 | else {
3111 | sets = 4;
3112 | reserved_bits = 0;
3113 | }
3114 | break;
3115 |
3116 | default:
3117 | /* Malformed error!!! */
3118 | expert_add_info_format(pinfo, extlen_ti, &ei_oran_extlen_wrong,
3119 | "For section 5, extlen must be 2, 3 or 4, but %u was dissected",
3120 | extlen);
3121 | break;
3122 | }
3123 |
3124 | unsigned bit_offset = offset*8;
3125 | /* Dissect each set */
3126 | for (int n=0; n < sets; n++) {
3127 | /* Subtree for each set */
3128 | unsigned set_start_offset = bit_offset/8;
3129 | proto_item *set_ti = proto_tree_add_string(extension_tree, hf_oran_modcomp_param_set,
3130 | tvb, set_start_offset, 0, "");
3131 | proto_tree *set_tree = proto_item_add_subtree(set_ti, ett_oran_modcomp_param_set);
3132 |
3133 | uint64_t mcScaleReMask, mcScaleOffset;
3134 | bool_Bool csf;
3135 |
3136 | /* mcScaleReMask (12 bits). Defines which REs the following csf and mcScaleOffset apply to */
3137 | static int * const remask_flags[] = {
3138 | &hf_oran_mc_scale_re_mask_re1,
3139 | &hf_oran_mc_scale_re_mask_re2,
3140 | &hf_oran_mc_scale_re_mask_re3,
3141 | &hf_oran_mc_scale_re_mask_re4,
3142 | &hf_oran_mc_scale_re_mask_re5,
3143 | &hf_oran_mc_scale_re_mask_re6,
3144 | &hf_oran_mc_scale_re_mask_re7,
3145 | &hf_oran_mc_scale_re_mask_re8,
3146 | &hf_oran_mc_scale_re_mask_re9,
3147 | &hf_oran_mc_scale_re_mask_re10,
3148 | &hf_oran_mc_scale_re_mask_re11,
3149 | &hf_oran_mc_scale_re_mask_re12,
3150 | NULL((void*)0)
3151 | };
3152 | /* Same as above, but offset by 4 bits */
3153 | static int * const remask_flags_even[] = {
3154 | &hf_oran_mc_scale_re_mask_re1_even,
3155 | &hf_oran_mc_scale_re_mask_re2_even,
3156 | &hf_oran_mc_scale_re_mask_re3_even,
3157 | &hf_oran_mc_scale_re_mask_re4_even,
3158 | &hf_oran_mc_scale_re_mask_re5_even,
3159 | &hf_oran_mc_scale_re_mask_re6_even,
3160 | &hf_oran_mc_scale_re_mask_re7_even,
3161 | &hf_oran_mc_scale_re_mask_re8_even,
3162 | &hf_oran_mc_scale_re_mask_re9_even,
3163 | &hf_oran_mc_scale_re_mask_re10_even,
3164 | &hf_oran_mc_scale_re_mask_re11_even,
3165 | &hf_oran_mc_scale_re_mask_re12_even,
3166 | NULL((void*)0)
3167 | };
3168 |
3169 | /* RE Mask (12 bits) */
3170 | proto_tree_add_bitmask_ret_uint64(set_tree, tvb, bit_offset / 8,
3171 | (n % 2) ? hf_oran_mc_scale_re_mask_even : hf_oran_mc_scale_re_mask,
3172 | ett_oran_mc_scale_remask,
3173 | (n % 2) ? remask_flags_even : remask_flags, ENC_BIG_ENDIAN0x00000000, &mcScaleReMask);
3174 | bit_offset += 12;
3175 |
3176 | /* csf (1 bit) */
3177 | bit_offset = dissect_csf(set_tree, tvb, bit_offset, ci_iq_width, &csf);
3178 | /* mcScaleOffset (15 bits) */
3179 | proto_item *ti = proto_tree_add_bits_ret_val(set_tree, hf_oran_mc_scale_offset, tvb, bit_offset, 15, &mcScaleOffset, ENC_BIG_ENDIAN0x00000000);
3180 | uint16_t exponent = (mcScaleOffset >> 11) & 0x000f; /* m.s. 4 bits */
3181 | uint16_t mantissa = mcScaleOffset & 0x07ff; /* l.s. 11 bits */
3182 | double mcScaleOffset_value = ((double)mantissa/(1<<11)) * (1.0 / (1 << exponent));
3183 | proto_item_append_text(ti, " (%f)", mcScaleOffset_value);
3184 | bit_offset += 15;
3185 |
3186 | /* Record this config */
3187 | if (state && state->mod_comp_params.num_configs < MAX_MOD_COMPR_CONFIGS16) {
3188 | unsigned i = state->mod_comp_params.num_configs;
3189 | state->mod_comp_params.configs[i].mod_compr_re_mask = (uint16_t)mcScaleReMask;
3190 | state->mod_comp_params.configs[i].mod_compr_csf = csf;
3191 | state->mod_comp_params.configs[i].mod_compr_scaler = mcScaleOffset_value;
3192 | state->mod_comp_params.num_configs++;
3193 | }
3194 |
3195 | /* Summary */
3196 | proto_item_set_len(set_ti, (bit_offset+7)/8 - set_start_offset);
3197 | proto_item_append_text(set_ti, " (mcScaleReMask=0x%03x csf=%5s mcScaleOffset=%f)",
3198 | (unsigned)mcScaleReMask, tfs_get_true_false(csf)tfs_get_string(csf, ((void*)0)), mcScaleOffset_value);
3199 | }
3200 |
3201 | proto_item_append_text(extension_ti, " (%u sets)", sets);
3202 |
3203 | /* Reserved (variable-length) */
3204 | if (reserved_bits) {
3205 | proto_tree_add_bits_item(extension_tree, hf_oran_reserved, tvb, bit_offset, reserved_bits, ENC_BIG_ENDIAN0x00000000);
3206 | bit_offset += reserved_bits;
3207 | }
3208 |
3209 | offset = bit_offset/8;
3210 | break;
3211 | }
3212 |
3213 | case 6: /* SE 6: Non-contiguous PRB allocation in time and frequency domain */
3214 | {
3215 | /* numSymbol not used in this case */
3216 | if (numsymbol_ti && !numsymbol_ignored) {
3217 | proto_item_append_text(numsymbol_ti, " (ignored)");
3218 | numsymbol_ignored = true1;
3219 | }
3220 |
3221 | /* Will update ext6 recorded info */
3222 | ext11_settings.ext6_set = true1;
3223 |
3224 | /* repetition */
3225 | proto_tree_add_bits_item(extension_tree, hf_oran_se6_repetition, tvb, offset*8, 1, ENC_BIG_ENDIAN0x00000000);
3226 | /* rbgSize (PRBs per bit set in rbgMask) */
3227 | uint32_t rbgSize;
3228 | proto_item *rbg_size_ti;
3229 | rbg_size_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_rbgSize, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &rbgSize);
3230 | if (rbgSize == 0) {
3231 | /* N.B. this is only true if "se6-rb-bit-supported" is set... */
3232 | expert_add_info_format(pinfo, rbg_size_ti, &ei_oran_rbg_size_reserved,
3233 | "rbgSize value of 0 is reserved");
3234 | }
3235 | /* rbgMask (28 bits) */
3236 | uint32_t rbgMask;
3237 | proto_item *rbgmask_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_rbgMask, tvb, offset, 4, ENC_BIG_ENDIAN0x00000000, &rbgMask);
3238 | if (rbgSize == 0) {
3239 | proto_item_append_text(rbgmask_ti, " (value ignored since rbgSize is 0)");
3240 | }
3241 |
3242 | /* TODO: if receiver detects non-zero bits outside the valid range, those shall be ignored. */
3243 | offset += 4;
3244 | /* priority */
3245 | proto_tree_add_item(extension_tree, hf_oran_noncontig_priority, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3246 | /* symbolMask */
3247 | offset = dissect_symbolmask(tvb, extension_tree, offset, NULL((void*)0), NULL((void*)0));
3248 |
3249 | /* Look up rbg_size enum -> value */
3250 | switch (rbgSize) {
3251 | case 0:
3252 | /* N.B. reserved, but covered above with expert info (would remain 0) */
3253 | break;
3254 | case 1:
3255 | ext11_settings.ext6_rbg_size = 1; break;
3256 | case 2:
3257 | ext11_settings.ext6_rbg_size = 2; break;
3258 | case 3:
3259 | ext11_settings.ext6_rbg_size = 3; break;
3260 | case 4:
3261 | ext11_settings.ext6_rbg_size = 4; break;
3262 | case 5:
3263 | ext11_settings.ext6_rbg_size = 6; break;
3264 | case 6:
3265 | ext11_settings.ext6_rbg_size = 8; break;
3266 | case 7:
3267 | ext11_settings.ext6_rbg_size = 16; break;
3268 | /* N.B., encoded in 3 bits, so no other values are possible */
3269 | }
3270 |
3271 | /* Set to looked-up value */
3272 | rbgSize = ext11_settings.ext6_rbg_size;
3273 |
3274 | uint32_t lastRbgid = 0;
3275 | if (rbgSize != 0) {
3276 | /* The O-DU shall not use combinations of startPrbc, numPrbc and rbgSize leading to a value of lastRbgid larger than 27 */
3277 | /* i.e., leftmost bit used should not need to go off left end of rbgMask! */
3278 | lastRbgid = (uint32_t)ceil((numPrbc + (startPrbc % rbgSize)) / (float)rbgSize) - 1;
3279 | if (lastRbgid > 27) {
3280 | expert_add_info_format(pinfo, rbg_size_ti, &ei_oran_lastRbdid_out_of_range,
3281 | "SE6: rbgSize (%u) not compatible with startPrbc(%u) and numPrbc(%u)",
3282 | rbgSize, startPrbc, numPrbc);
3283 | break;
3284 | }
3285 | }
3286 |
3287 | /* Record (and count) which bits are set in rbgMask */
3288 | bool_Bool first_seen = false0;
3289 | unsigned first_seen_pos=0, last_seen_pos=0;
3290 | for (unsigned n=0; n < 28 && ext11_settings.ext6_num_bits_set < 28; n++) {
3291 | if ((rbgMask >> n) & 0x01) {
3292 | ext11_settings.ext6_bits_set[ext11_settings.ext6_num_bits_set++] = n;
3293 | if (!first_seen) {
3294 | first_seen = true1;
3295 | first_seen_pos = n;
3296 | }
3297 | last_seen_pos = n;
3298 | }
3299 | }
3300 |
3301 | /* Show how many bits were set in rbgMask */
3302 | proto_item_append_text(rbgmask_ti, " (%u bits set)", ext11_settings.ext6_num_bits_set);
3303 | /* Also, that is the range of bits */
3304 | if (first_seen) {
3305 | proto_item_append_text(rbgmask_ti, " (%u bits spread)", last_seen_pos-first_seen_pos+1);
3306 | }
3307 |
3308 | /* Complain if last set bit is beyond lastRbgid */
3309 | if (first_seen) {
3310 | if (last_seen_pos > lastRbgid) {
3311 | expert_add_info_format(pinfo, rbgmask_ti, &ei_oran_rbgMask_beyond_last_rbdid,
3312 | "SE6: rbgMask (0x%07x) has bit %u set, but lastRbgId is %u",
3313 | rbgMask, last_seen_pos, lastRbgid);
3314 | }
3315 | }
3316 |
3317 | /* Also update prbs_for_st10_type5[] */
3318 | if (sectionType == 10 && rbgSize != 0) {
3319 | /* Unset all entries */
3320 | memset(&prbs_for_st10_type5, 0, sizeof(prbs_for_st10_type5));
3321 |
3322 | /* Work out which PRB first bit corresponds to */
3323 | unsigned firstPrbStart = (startPrbc/rbgSize) * rbgSize;
3324 |
3325 | /* Add PRBs corresponding to each bit set */
3326 | for (unsigned n=0; n < 28 ; n++) {
3327 | if ((rbgMask >> n) & 0x01) {
3328 | /* Lazy way to clip any values that lie outside of range for section */
3329 | for (unsigned p=0; p < rbgSize; p++) {
3330 | unsigned start = firstPrbStart + (n*rbgSize);
3331 | if ((start+p < MAX_PRBS273) && (start+p >= startPrbc) && (start+p <= startPrbc+numPrbc-1)) {
3332 | prbs_for_st10_type5[start+p] = true1;
3333 | }
3334 | }
3335 | }
3336 | }
3337 | }
3338 |
3339 | break;
3340 | }
3341 |
3342 | case 7: /* SE 7: eAxC mask */
3343 | /* Allow ST0 to address multiple eAxC_ID values for transmission blanking */
3344 | proto_tree_add_item(extension_tree, hf_oran_eAxC_mask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3345 | offset += 2;
3346 | break;
3347 |
3348 | case 8: /* SE 8: Regularization factor */
3349 | proto_tree_add_item(extension_tree, hf_oran_regularizationFactor, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3350 | offset += 2;
3351 | break;
3352 |
3353 | case 9: /* SE 9: Dynamic Spectrum Sharing parameters */
3354 | proto_tree_add_item(extension_tree, hf_oran_technology, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3355 | offset += 1;
3356 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3357 | offset += 1;
3358 | break;
3359 |
3360 | case 10: /* SE 10: Group configuration of multiple ports */
3361 | {
3362 | seen_se10 = true1;
3363 |
3364 | /* beamGroupType */
3365 | uint32_t beam_group_type = 0;
3366 | proto_item *bgt_ti;
3367 | bgt_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_beamGroupType,
3368 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &beam_group_type);
3369 | proto_item_append_text(extension_ti, " (%s)", val_to_str_const(beam_group_type, beam_group_type_vals, "Unknown"));
3370 |
3371 | /* numPortc */
3372 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_numPortc,
3373 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPortc);
3374 | offset++;
3375 |
3376 | /* Will append all beamId values to extension_ti, regardless of beamGroupType */
3377 | unsigned n;
3378 |
3379 | switch (beam_group_type) {
3380 | case 0x0: /* common beam */
3381 | case 0x1: /* beam matrix indication */
3382 | /* Reserved byte */
3383 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
3384 | offset++;
3385 |
3386 | /* Explain how entries are allocated */
3387 | if (beam_group_type == 0x0) {
3388 | proto_item_append_text(extension_ti, " (all %u ueid/Beam entries are %u)", numPortc, ueId);
3389 | }
3390 | else {
3391 | /* 'numPortc' consecutive BeamIds from section header */
3392 | proto_item_append_text(extension_ti, " (ueId/beam entries are %u -> %u)", ueId, ueId+numPortc);
3393 | }
3394 |
3395 | if (sectionType == 5) {
3396 | /* These types are not allowed */
3397 | expert_add_info_format(pinfo, bgt_ti, &ei_oran_se10_not_allowed,
3398 | "SE10: beamGroupType %u is not allowed for section type 5", beam_group_type);
3399 | }
3400 | break;
3401 |
3402 | case 0x2: /* beam vector listing */
3403 | {
3404 | proto_item_append_text(extension_ti, " [ ");
3405 |
3406 | /* Beam listing vector case */
3407 | /* Work out how many port beam entries there is room for */
3408 | /* Using numPortC as visible in issue 18116 */
3409 | for (n=0; n < numPortc; n++) {
3410 | /* 1 reserved bit */
3411 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3412 |
3413 | /* port beam ID (or UEID) (15 bits) */
3414 | uint32_t id;
3415 | proto_item *beamid_or_ueid_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_beamId,
3416 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &id);
3417 | proto_item_append_text(beamid_or_ueid_ti, " port #%u beam ID (or UEId) %u", n, id);
3418 | offset += 2;
3419 |
3420 | if (id != 0x7fff) {
3421 | if (number_of_ueids < MAX_UEIDS16) {
3422 | ueids[number_of_ueids++] = id;
3423 | }
3424 | }
3425 |
3426 | proto_item_append_text(extension_ti, "%u ", id);
3427 | }
3428 |
3429 | proto_item_append_text(extension_ti, "]");
3430 | break;
3431 | }
3432 | case 0x3: /* beamId/ueId listing with associated port-list index */
3433 | {
3434 | proto_item_append_text(extension_ti, " [ ");
3435 |
3436 | if (numPortc > 0) {
3437 | /* first portListIndex is outside loop */
3438 | uint32_t port_list_index;
3439 | proto_item *pli_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_port_list_index, tvb,
3440 | offset, 1, ENC_BIG_ENDIAN0x00000000, &port_list_index);
3441 | if (port_list_index == 0) {
3442 | /* Value 0 is reserved */
3443 | expert_add_info(pinfo, pli_ti, &ei_oran_port_list_index_zero);
3444 | }
3445 | offset += 1;
3446 |
3447 | for (n=0; n < numPortc-1; n++) {
3448 | /* 1 reserved bit */
3449 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3450 |
3451 | /* port beam ID (or UEID) */
3452 | uint32_t id;
3453 | proto_item *beamid_or_ueid_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_beamId,
3454 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &id);
3455 | proto_item_append_text(beamid_or_ueid_ti, " port #%u beam ID (or UEId) %u", n, id);
3456 | offset += 2;
3457 |
3458 | if (id != 0x7fff) {
3459 | if (number_of_ueids < MAX_UEIDS16) {
3460 | ueids[number_of_ueids++] = id;
3461 | }
3462 | }
3463 |
3464 | /* subsequent portListIndex */
3465 | pli_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_port_list_index, tvb,
3466 | offset, 1, ENC_BIG_ENDIAN0x00000000, &port_list_index);
3467 | if (port_list_index == 0) {
3468 | /* Value 0 is reserved */
3469 | expert_add_info(pinfo, pli_ti, &ei_oran_port_list_index_zero);
3470 | }
3471 | offset += 1;
3472 |
3473 | proto_item_append_text(extension_ti, "%u:%u ", port_list_index, id);
3474 | }
3475 | }
3476 |
3477 | proto_item_append_text(extension_ti, "]");
3478 | break;
3479 | }
3480 |
3481 |
3482 | default:
3483 | /* Warning for unsupported/reserved value */
3484 | expert_add_info(NULL((void*)0), bgt_ti, &ei_oran_se10_unknown_beamgrouptype);
3485 | break;
3486 | }
3487 | break;
3488 | }
3489 |
3490 | case 11: /* SE 11: Flexible Weights Extension Type */
3491 | {
3492 | /* Hidden filter for bf */
3493 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
3494 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
3495 |
3496 | /* beamId in section header should be ignored. Guard against appending multiple times.. */
3497 | if (beamId_ti && !beamId_ignored) {
3498 | proto_item_append_text(beamId_ti, " (ignored)");
3499 | beamId_ignored = true1;
3500 | }
3501 |
3502 | bool_Bool disableBFWs;
3503 | uint32_t numBundPrb;
3504 | bool_Bool rad;
3505 |
3506 | /* disableBFWs */
3507 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_disable_bfws,
3508 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disableBFWs);
3509 | if (disableBFWs) {
3510 | proto_item_append_text(extension_ti, " (disableBFWs)");
3511 | }
3512 |
3513 | /* RAD */
3514 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_rad,
3515 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &rad);
3516 | /* bundleOffset (6 bits) */
3517 | proto_tree_add_item(extension_tree, hf_oran_bundle_offset, tvb,
3518 | offset, 1, ENC_BIG_ENDIAN0x00000000);
3519 | offset++;
3520 |
3521 | /* numBundPrb (number of prbs in each bundle) */
3522 | proto_item *num_bund_prb_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_bund_prbs,
3523 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numBundPrb);
3524 | offset++;
3525 | /* value zero is reserved.. */
3526 | if (numBundPrb == 0) {
3527 | expert_add_info_format(pinfo, num_bund_prb_ti, &ei_oran_reserved_numBundPrb,
3528 | "Reserved value 0 for numBundPrb seen - not valid");
3529 | }
3530 |
3531 | uint32_t num_bundles;
3532 | bool_Bool orphaned_prbs = false0;
3533 |
3534 | if (!disableBFWs) {
3535 | /********************************************/
3536 | /* Table 7.7.1.1-1 */
3537 | /********************************************/
3538 |
3539 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
3540 | proto_item *comp_meth_ti = NULL((void*)0);
3541 |
3542 | /* bfwCompHdr (2 subheaders - bfwIqWidth and bfwCompMeth)*/
3543 | offset = dissect_bfwCompHdr(tvb, extension_tree, offset,
3544 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
3545 |
3546 | /* Work out number of bundles, but take care not to divide by zero. */
3547 | if (numBundPrb == 0) {
3548 | break;
3549 | }
3550 |
3551 | /* Work out bundles! */
3552 | ext11_work_out_bundles(startPrbc, numPrbc, numBundPrb, &ext11_settings);
3553 | num_bundles = ext11_settings.num_bundles;
3554 |
3555 | /* Add (complete) bundles */
3556 | for (unsigned b=0; b < num_bundles; b++) {
3557 |
3558 | offset = dissect_bfw_bundle(tvb, extension_tree, pinfo, offset,
3559 | comp_meth_ti, bfwcomphdr_comp_meth,
3560 | (state) ? &state->mod_comp_params : NULL((void*)0),
3561 | (ext11_settings.ext21_set) ?
3562 | numPrbc :
3563 | pref_num_bf_antennas,
3564 | bfwcomphdr_iq_width,
3565 | b, /* bundle number */
3566 | ext11_settings.bundles[b].start,
3567 | ext11_settings.bundles[b].end,
3568 | ext11_settings.bundles[b].is_orphan);
3569 | if (!offset) {
3570 | break;
3571 | }
3572 | }
3573 | if (num_bundles > 0) {
3574 | /* Set flag from last bundle entry */
3575 | orphaned_prbs = ext11_settings.bundles[num_bundles-1].is_orphan;
3576 | }
3577 | }
3578 | else {
3579 | /********************************************/
3580 | /* Table 7.7.1.1-2 */
3581 | /* No weights in this case */
3582 | /********************************************/
3583 |
3584 | /* Work out number of bundles, but take care not to divide by zero. */
3585 | if (numBundPrb == 0) {
3586 | break;
3587 | }
3588 |
3589 | ext11_work_out_bundles(startPrbc, numPrbc, numBundPrb, &ext11_settings);
3590 | num_bundles = ext11_settings.num_bundles;
3591 |
3592 | for (unsigned n=0; n < num_bundles; n++) {
3593 | /* contInd */
3594 | proto_tree_add_item(extension_tree, hf_oran_cont_ind,
3595 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3596 | /* beamId */
3597 | proto_item *ti = proto_tree_add_item(extension_tree, hf_oran_beam_id,
3598 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3599 | if (!ext11_settings.bundles[n].is_orphan) {
3600 | proto_item_append_text(ti, " (PRBs %3u-%3u) (Bundle %2u)",
3601 | ext11_settings.bundles[n].start,
3602 | ext11_settings.bundles[n].end,
3603 | n);
3604 | }
3605 | else {
3606 | orphaned_prbs = true1;
3607 | proto_item_append_text(ti, " (PRBs %3u-%3u) (Orphaned PRBs)",
3608 | ext11_settings.bundles[n].start,
3609 | ext11_settings.bundles[n].end);
3610 | }
3611 | offset += 2;
3612 | }
3613 | }
3614 |
3615 | /* Add summary to extension root */
3616 | if (orphaned_prbs) {
3617 | proto_item_append_text(extension_ti, " (%u full bundles + orphaned)", num_bundles-1);
3618 | }
3619 | else {
3620 | proto_item_append_text(extension_ti, " (%u bundles)", num_bundles);
3621 | }
3622 | }
3623 |
3624 | break;
3625 |
3626 | case 12: /* SE 12: Non-Contiguous PRB Allocation with Frequency Ranges */
3627 | {
3628 | /* numSymbol not used in this case */
3629 | if (numsymbol_ti && !numsymbol_ignored) {
3630 | proto_item_append_text(numsymbol_ti, " (ignored)");
3631 | numsymbol_ignored = true1;
3632 | }
3633 |
3634 | ext11_settings.ext12_set = true1;
3635 |
3636 | /* priority */
3637 | proto_tree_add_item(extension_tree, hf_oran_noncontig_priority, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3638 |
3639 | /* symbolMask */
3640 | offset = dissect_symbolmask(tvb, extension_tree, offset, NULL((void*)0), NULL((void*)0));
3641 |
3642 | /* There are now 'R' pairs of (offStartPrb, numPrb) values. Fill extlen bytes with values. If last one is not set,
3643 | should be populated with 0s. */
3644 | uint32_t extlen_remaining_bytes = (extlen*4) - 4;
3645 | uint8_t prb_index;
3646 |
3647 | /* This is for ST10/ST11. First pair starts after frames signalled there */
3648 | uint16_t st10_st11_offset = startPrbc + numPrbc;
3649 |
3650 | for (prb_index = 1; extlen_remaining_bytes > 0; prb_index++)
3651 | {
3652 | /* Create a subtree for each pair */
3653 | proto_item *pair_ti = proto_tree_add_string(extension_tree, hf_oran_frequency_range,
3654 | tvb, offset, 2, "");
3655 | proto_tree *pair_tree = proto_item_add_subtree(pair_ti, ett_oran_frequency_range);
3656 |
3657 | /* offStartPrb */
3658 | uint32_t off_start_prb;
3659 | proto_tree_add_item_ret_uint(pair_tree, hf_oran_off_start_prb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &off_start_prb);
3660 | offset++;
3661 |
3662 | /* numPrb */
3663 | uint32_t num_prb;
3664 | proto_tree_add_item_ret_uint(pair_tree, hf_oran_num_prb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_prb);
3665 | offset++;
3666 |
3667 | extlen_remaining_bytes -= 2;
3668 |
3669 | /* Last pair may be 0,0 if not used. Check for this */
3670 | if ((extlen_remaining_bytes == 0) && (off_start_prb == 0) && (num_prb == 0)) {
3671 | proto_item_append_text(pair_ti, " (not used)");
3672 | }
3673 | /* Add summary to pair root item, and configure details in ext11_settings */
3674 | else {
3675 | proto_item_append_text(pair_ti, "(%u) [%u : %u]",
3676 | prb_index, off_start_prb, num_prb);
3677 | proto_item_append_text(extension_ti, "[%u : %u]",
3678 | off_start_prb, num_prb);
3679 | if (ext11_settings.ext12_num_pairs < MAX_BFW_EXT12_PAIRS128) {
3680 | ext11_settings.ext12_pairs[ext11_settings.ext12_num_pairs].off_start_prb = off_start_prb;
3681 | ext11_settings.ext12_pairs[ext11_settings.ext12_num_pairs++].num_prb = num_prb;
3682 | }
3683 |
3684 | /* Also update PRBs to be covered for ST10 type 5 */
3685 | /* Original range from section is added to.. */
3686 | /* TODO: I don't think this is quite right.. */
3687 | for (unsigned prb=st10_st11_offset+off_start_prb; prb < st10_st11_offset+off_start_prb+num_prb; prb++) {
3688 | if (prb < MAX_PRBS273) {
3689 | prbs_for_st10_type5[prb] = true1;
3690 | }
3691 | }
3692 |
3693 | /* Any next pair will begin after this one */
3694 | st10_st11_offset += (off_start_prb + num_prb);
3695 | }
3696 | }
3697 | break;
3698 | }
3699 |
3700 | case 13: /* SE 13: PRB Allocation with Frequency Hopping */
3701 | {
3702 | /* Will update settings for ext11 */
3703 | ext11_settings.ext13_set = true1;
3704 |
3705 | uint32_t extlen_remaining_bytes = (extlen*4) - 2;
3706 | uint8_t allocation_index;
3707 |
3708 | unsigned prev_next_symbol_id = 0, prev_next_start_prbc = 0;
3709 |
3710 | for (allocation_index = 1; extlen_remaining_bytes > 0; allocation_index++)
3711 | {
3712 | /* Subtree for allocation */
3713 | proto_item *allocation_ti = proto_tree_add_string(extension_tree, hf_oran_prb_allocation,
3714 | tvb, offset, 2, "");
3715 | proto_tree *allocation_tree = proto_item_add_subtree(allocation_ti, ett_oran_prb_allocation);
3716 |
3717 | /* Reserved (2 bits) */
3718 | proto_tree_add_item(allocation_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3719 |
3720 | /* nextSymbolId (4 bits) */
3721 | uint32_t next_symbol_id;
3722 | proto_tree_add_item_ret_uint(allocation_tree, hf_oran_nextSymbolId, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &next_symbol_id);
3723 |
3724 | /* nextStartPrbc (10 bits) */
3725 | uint32_t next_start_prbc;
3726 | proto_tree_add_item_ret_uint(allocation_tree, hf_oran_nextStartPrbc, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &next_start_prbc);
3727 | offset += 2;
3728 |
3729 | /* Add summary to allocation root item */
3730 | proto_item_append_text(allocation_ti, "(%u) nextSymbolId=%3u, nextStartPrbc=%u",
3731 | allocation_index, next_symbol_id, next_start_prbc);
3732 |
3733 | /* Checking for duplicates (expected if e.g. had only 2 entries but extlen bytes still to fill */
3734 | if ((allocation_index > 1) && (next_symbol_id == prev_next_symbol_id) && (next_start_prbc == prev_next_start_prbc)) {
3735 | proto_item_append_text(allocation_ti, " (repeated - to fill up extlen)");
3736 | }
3737 | else {
3738 | /* Add entry for configuring ext11. don't store out of range */
3739 | if (ext11_settings.ext13_num_start_prbs < MAX_BFW_EXT13_ALLOCATIONS128) {
3740 | ext11_settings.ext13_start_prbs[ext11_settings.ext13_num_start_prbs++] = next_start_prbc;
3741 | }
3742 | }
3743 | prev_next_symbol_id = next_symbol_id;
3744 | prev_next_start_prbc = next_start_prbc;
3745 |
3746 | extlen_remaining_bytes -= 2;
3747 | }
3748 | break;
3749 | }
3750 |
3751 | case 14: /* SE 14: Nulling-layer Info. for ueId-based beamforming */
3752 | /* Hidden filter for bf (DMRS BF) */
3753 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
3754 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
3755 |
3756 | if (!seen_se10) {
3757 | proto_tree_add_item(extension_tree, hf_oran_nullLayerInd, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3758 | offset += 1;
3759 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3760 | offset += 1;
3761 | }
3762 | else {
3763 | /* Loop over numPortc++1 (from SE 10) nullLayerInd fields */
3764 | for (unsigned port=0; port < numPortc+1; port++) {
3765 | proto_tree_add_item(extension_tree, hf_oran_nullLayerInd, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3766 | offset += 1;
3767 | }
3768 | }
3769 | break;
3770 |
3771 | case 15: /* SE 15: Mixed-numerology Info. for ueId-based beamforming */
3772 | {
3773 | /* frameStructure */
3774 | offset = dissect_frame_structure(extension_tree, tvb, offset,
3775 | subframeId, slotId);
3776 | /* freqOffset */
3777 | proto_tree_add_item(extension_tree, hf_oran_freqOffset, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
3778 | offset += 3;
3779 | /* cpLength */
3780 | proto_item *cplength_ti = proto_tree_add_item(extension_tree, hf_oran_cpLength, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3781 | if (sectionType != 0 && sectionType != 3) {
3782 | proto_item_append_text(cplength_ti, " (ignored - used only with ST0 and ST3)");
3783 | }
3784 | offset += 2;
3785 | break;
3786 | }
3787 |
3788 | case 16: /* SE 16: Antenna mapping in UE channel information based UL beamforming */
3789 | {
3790 | /* Just filling available bytes with antMask entries.
3791 | N.B., if SE 10 also used, could associate each antMask with (beamId or UEId) RX eAxC */
3792 | uint32_t extlen_remaining_bytes = (extlen*4) - 2;
3793 | unsigned num_ant_masks = extlen_remaining_bytes / 8;
3794 | for (unsigned n=0; n < num_ant_masks; n++) {
3795 | proto_item *ti = proto_tree_add_item(extension_tree, hf_oran_antMask, tvb, offset, 8, ENC_BIG_ENDIAN0x00000000);
3796 | proto_item_append_text(ti, " (RX eAxC #%u)", n+1);
3797 | offset += 8;
3798 | }
3799 | break;
3800 | }
3801 |
3802 | case 17: /* SE 17: Indication of user port group */
3803 | {
3804 | uint32_t extlen_remaining_bytes = (extlen*4) - 2;
3805 | uint32_t end_bit = (offset+extlen_remaining_bytes) * 8;
3806 | uint32_t ueid_index = 1;
3807 | /* TODO: just filling up all available bytes - some may actually be padding.. */
3808 | /* "the preceding Section Type and extension messages implicitly provide the number of scheduled users" */
3809 | for (uint32_t bit_offset=offset*8; bit_offset < end_bit; bit_offset+=4, ueid_index++) {
3810 | proto_item *ti = proto_tree_add_bits_item(extension_tree, hf_oran_num_ueid, tvb, bit_offset, 4, ENC_BIG_ENDIAN0x00000000);
3811 | proto_item_append_text(ti, " (user #%u)", ueid_index);
3812 | }
3813 | break;
3814 | }
3815 |
3816 | case 18: /* SE 18: Uplink transmission management */
3817 | /* transmissionWindowOffset */
3818 | proto_tree_add_item(extension_tree, hf_oran_transmissionWindowOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3819 | offset += 2;
3820 | /* reserved (2 bits) */
3821 | proto_tree_add_item(extension_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3822 | /* transmissionWindowSize (14 bits) */
3823 | proto_tree_add_item(extension_tree, hf_oran_transmissionWindowSize, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3824 | offset += 2;
3825 |
3826 | /* reserved (6 bits) */
3827 | proto_tree_add_item(extension_tree, hf_oran_reserved_6bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3828 | /* toT (2 bits) */
3829 | proto_tree_add_item(extension_tree, hf_oran_toT, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3830 | offset += 1;
3831 | break;
3832 |
3833 | case 19: /* SE 19: Compact beamforming information for multiple port */
3834 | {
3835 | /* beamId in section header should be ignored. Guard against appending multiple times.. */
3836 | if (beamId_ti && !beamId_ignored) {
3837 | proto_item_append_text(beamId_ti, " (ignored)");
3838 | beamId_ignored = true1;
3839 | }
3840 |
3841 | /* numSymbol not used in this case */
3842 | if (numsymbol_ti && !numsymbol_ignored) {
3843 | proto_item_append_text(numsymbol_ti, " (ignored)");
3844 | numsymbol_ignored = true1;
3845 | }
3846 |
3847 | /* disableBFWs */
3848 | bool_Bool disableBFWs;
3849 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_disable_bfws,
3850 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disableBFWs);
3851 | if (disableBFWs) {
3852 | proto_item_append_text(extension_ti, " (disableBFWs)");
3853 | }
3854 | /* repetition (1 bit) */
3855 | uint64_t repetition;
3856 | proto_tree_add_bits_ret_val(extension_tree, hf_oran_se19_repetition, tvb, (offset*8)+1, 1, &repetition, ENC_BIG_ENDIAN0x00000000);
3857 | /* numPortc (6 bits) */
3858 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_numPortc,
3859 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPortc);
3860 | offset++;
3861 |
3862 | /* priority (2 bits) */
3863 | proto_tree_add_item(extension_tree, hf_oran_noncontig_priority, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3864 | /* symbolMask (14 bits) */
3865 | offset = dissect_symbolmask(tvb, extension_tree, offset, NULL((void*)0), NULL((void*)0));
3866 |
3867 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
3868 | proto_item *comp_meth_ti = NULL((void*)0);
3869 |
3870 | if (!repetition) {
3871 |
3872 | if (!disableBFWs) {
3873 | /* bfwCompHdr */
3874 | offset = dissect_bfwCompHdr(tvb, extension_tree, offset,
3875 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
3876 | }
3877 |
3878 | /* Add entries for each port */
3879 | for (unsigned port=0; port < numPortc; port++) {
3880 |
3881 | /* Create subtree for port entry*/
3882 | int port_start_offset = offset;
3883 | proto_item *port_ti = proto_tree_add_string_format(extension_tree, hf_oran_ext19_port,
3884 | tvb, offset, 0,
3885 | "", "Port %u: ", port);
3886 | proto_tree *port_tree = proto_item_add_subtree(port_ti, ett_oran_ext19_port);
3887 |
3888 | /* Reserved (4 bits) */
3889 | proto_tree_add_item(port_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3890 | /* portReMask (12 bits) */
3891 | proto_tree_add_item(port_tree, hf_oran_portReMask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3892 | offset += 2;
3893 |
3894 | /* Reserved (2 bits) */
3895 | proto_tree_add_item(port_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3896 | /* portSymbolMask (14 bits) */
3897 | proto_tree_add_item(port_tree, hf_oran_portSymbolMask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3898 | offset += 2;
3899 |
3900 | /* Reserved (1 bit) */
3901 | proto_tree_add_item(port_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3902 | /* beamID (15 bits) */
3903 | proto_tree_add_item_ret_uint(port_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &beamId);
3904 | proto_item_append_text(port_ti, " (beamId=%u)", beamId);
3905 | offset += 2;
3906 |
3907 | /* No weights present */
3908 | if (!disableBFWs) {
3909 | /*******************************************************************/
3910 | /* Table 7.7.19.1-1 (there is no part -2 for disableBFWs case...), */
3911 | /* but for SE 11, bfwCompParam was only present for !disableBFWs */
3912 | /*******************************************************************/
3913 |
3914 | /* bfwCompParam */
3915 | bool_Bool compression_method_supported = false0;
3916 | uint32_t exponent = 0;
3917 | unsigned num_trx_entries = 0;
3918 | uint16_t *trx;
3919 | offset = dissect_bfwCompParam(tvb, port_tree, pinfo, offset, comp_meth_ti,
3920 | &bfwcomphdr_comp_meth, &exponent, &compression_method_supported,
3921 | &num_trx_entries, &trx);
3922 |
3923 | int bit_offset = offset*8;
3924 | int bfw_offset;
3925 |
3926 | /* Add weights for each TRX */
3927 | unsigned trx_to_add = (num_trx_entries==0) ? pref_num_bf_antennas : num_trx_entries;
3928 | for (unsigned b=0; b < trx_to_add; b++) {
3929 |
3930 | uint16_t trx_index = (num_trx_entries) ? trx[b] : b+1;
3931 |
3932 | /* Create BFW subtree */
3933 | bfw_offset = bit_offset / 8;
3934 | uint8_t bfw_extent = ((bit_offset + (bfwcomphdr_iq_width*2)) / 8) - bfw_offset;
3935 | proto_item *bfw_ti = proto_tree_add_string_format(port_tree, hf_oran_bfw,
3936 | tvb, bfw_offset, bfw_extent,
3937 | "", "TRX %u: (", trx_index);
3938 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
3939 |
3940 | /* I */
3941 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
3942 | float value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent, (state) ? &state->mod_comp_params : NULL((void*)0), 0 /* RE */);
3943 | /* Add to tree. */
3944 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8,
3945 | (bfwcomphdr_iq_width+7)/8, value, "#%u=%f", b, value);
3946 | bit_offset += bfwcomphdr_iq_width;
3947 | proto_item_append_text(bfw_ti, "I%u=%f ", b, value);
3948 |
3949 | /* Q */
3950 | bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
3951 | value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent, (state) ? &state->mod_comp_params : NULL((void*)0), 0 /* RE */);
3952 | /* Add to tree. */
3953 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8,
3954 | (bfwcomphdr_iq_width+7)/8, value, "#%u=%f", b, value);
3955 | bit_offset += bfwcomphdr_iq_width;
3956 | proto_item_append_text(bfw_ti, "Q%u=%f)", b, value);
3957 | }
3958 |
3959 | offset = (bit_offset+7)/8;
3960 | }
3961 | else {
3962 | /* No weights... */
3963 | }
3964 |
3965 | /* Set length of this port entry */
3966 | proto_item_set_len(port_ti, offset-port_start_offset);
3967 | }
3968 | }
3969 | break;
3970 | }
3971 |
3972 | case 20: /* SE 20: Puncturing extension */
3973 | {
3974 | /* numPuncPatterns */
3975 | uint32_t numPuncPatterns;
3976 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_numPuncPatterns, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPuncPatterns);
3977 | offset += 1;
3978 |
3979 | /* Add each puncturing pattern */
3980 | for (uint32_t n=0; n < numPuncPatterns; n++) {
3981 | unsigned pattern_start_offset = offset;
3982 |
3983 | /* Subtree for this puncturing pattern */
3984 | proto_item *pattern_ti = proto_tree_add_string_format(extension_tree, hf_oran_puncPattern,
3985 | tvb, offset, 0,
3986 | "", "Puncturing Pattern: %u/%u", n+1, numPuncPatterns);
3987 | proto_tree *pattern_tree = proto_item_add_subtree(pattern_ti, ett_oran_punc_pattern);
3988 |
3989 | /* SymbolMask (14 bits) */
3990 | proto_tree_add_item(pattern_tree, hf_oran_symbolMask_ext20, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3991 | offset += 1;
3992 |
3993 | uint32_t startPuncPrb, numPuncPrb;
3994 |
3995 | /* startPuncPrb (10 bits) */
3996 | proto_tree_add_item_ret_uint(pattern_tree, hf_oran_startPuncPrb, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPuncPrb);
3997 | offset += 2;
3998 | /* numPuncPrb (8 bits) */
3999 | proto_tree_add_item_ret_uint(pattern_tree, hf_oran_numPuncPrb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPuncPrb);
4000 | offset += 1;
4001 |
4002 | proto_item_append_text(pattern_ti, " [%u->%u]", startPuncPrb, startPuncPrb+numPuncPrb-1);
4003 |
4004 | /* Make a hole in range of PRBs to report */
4005 | for (unsigned p=startPuncPrb; p < startPuncPrb+numPuncPrb; p++) {
4006 | if (p < MAX_PRBS273) {
4007 | prbs_for_st10_type5[p] = false0;
4008 | }
4009 | }
4010 |
4011 | /* puncReMask (12 bits) */
4012 | proto_tree_add_item(pattern_tree, hf_oran_puncReMask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4013 | offset += 1;
4014 | /* rb (1 bit) */
4015 | proto_item *rb_ti = proto_tree_add_item(pattern_tree, hf_oran_rb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4016 | /* reserved (1 bit) */
4017 | proto_tree_add_item(pattern_tree, hf_oran_reserved_bit5, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4018 | /* multiSDScope (1 bit) */
4019 | proto_tree_add_item(pattern_tree, hf_oran_multiSDScope, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4020 | /* rbgIncl (1 bit) */
4021 | bool_Bool rbgIncl;
4022 | proto_tree_add_item_ret_boolean(pattern_tree, hf_oran_RbgIncl, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &rbgIncl);
4023 | offset += 1;
4024 |
4025 | if (rbgIncl) {
4026 | /* reserved (1 bit) */
4027 | proto_tree_add_item(pattern_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4028 | /* rbgSize(3 bits) */
4029 | proto_tree_add_item(pattern_tree, hf_oran_rbgSize, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4030 | /* rbgMask (28 bits) */
4031 | proto_tree_add_item(pattern_tree, hf_oran_rbgMask, tvb, offset, 4, ENC_BIG_ENDIAN0x00000000);
4032 | offset += 4;
4033 |
4034 | proto_item_append_text(rb_ti, " (ignored)");
4035 | }
4036 |
4037 | proto_item_set_len(pattern_ti, offset-pattern_start_offset);
4038 | }
4039 |
4040 | break;
4041 | }
4042 | case 21: /* SE 21: Variable PRB group size for channel information */
4043 | {
4044 | /* ciPrbGroupSize */
4045 | uint32_t ci_prb_group_size;
4046 | proto_item *prb_group_size_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_ci_prb_group_size, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &ci_prb_group_size);
4047 | offset += 1;
4048 |
4049 | switch (ci_prb_group_size) {
4050 | case 0:
4051 | case 1:
4052 | case 255:
4053 | /* Reserved value */
4054 | expert_add_info_format(pinfo, prb_group_size_ti, &ei_oran_ci_prb_group_size_reserved,
4055 | "SE 11 ciPrbGroupSize is reserved value %u - must be 2-254",
4056 | ci_prb_group_size);
4057 | break;
4058 | default:
4059 | /* This value affects how SE 11 is interpreted */
4060 | ext11_settings.ext21_set = true1;
4061 | ext11_settings.ext21_ci_prb_group_size = ci_prb_group_size;
4062 |
4063 | if (numPrbc == 0) {
4064 | expert_add_info(pinfo, numprbc_ti, &ei_oran_numprbc_ext21_zero);
4065 | }
4066 | break;
4067 | }
4068 |
4069 | /* reserved (6 bits) */
4070 | proto_tree_add_item(extension_tree, hf_oran_reserved_6bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4071 |
4072 | /* prgSize (2 bits). Interpretation depends upon section type (5 or 6), but also mplane parameters? */
4073 | if (sectionType == SEC_C_UE_SCHED) { /* Section Type 5 */
4074 | proto_tree_add_item(extension_tree, hf_oran_prg_size_st5, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4075 | }
4076 | else if (sectionType == SEC_C_CH_INFO) { /* Section Type 6 */
4077 | proto_tree_add_item(extension_tree, hf_oran_prg_size_st6, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4078 | }
4079 | offset += 1;
4080 | break;
4081 | }
4082 |
4083 | case 22: /* SE 22: ACK/NACK request */
4084 | {
4085 | uint32_t ack_nack_req_id;
4086 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_ack_nack_req_id, tvb, offset, 2,
4087 | ENC_BIG_ENDIAN0x00000000, &ack_nack_req_id);
4088 | offset += 2;
4089 |
4090 | if (state) {
4091 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
4092 | /* Add this request into conversation state on first pass */
4093 | ack_nack_request_t *request_details = wmem_new0(wmem_file_scope(), ack_nack_request_t)((ack_nack_request_t*)wmem_alloc0((wmem_file_scope()), sizeof (ack_nack_request_t)));
4094 | request_details->request_frame_number = pinfo->num;
4095 | request_details->request_frame_time = pinfo->abs_ts;
4096 | request_details->requestType = SE22;
4097 | /* Insert into flow's tree */
4098 | wmem_tree_insert32(state->ack_nack_requests, ack_nack_req_id, request_details);
4099 | }
4100 | else {
4101 | /* Try to link forward to ST8 response */
4102 | ack_nack_request_t *response = wmem_tree_lookup32(state->ack_nack_requests,
4103 | ack_nack_req_id);
4104 | if (response) {
4105 | show_link_to_acknack_response(extension_tree, tvb, pinfo, response);
4106 | }
4107 | }
4108 | }
4109 | break;
4110 | }
4111 |
4112 | case 23: /* SE 23: Arbitrary symbol pattern modulation compression parameters */
4113 | {
4114 | /* Green common header */
4115 |
4116 | /* numSymPrbPattern (4 bits) */
4117 | uint32_t num_sym_prb_pattern;
4118 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_sym_prb_pattern, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_sym_prb_pattern);
4119 | /* reserved (3 bits) */
4120 | proto_tree_add_item(extension_tree, hf_oran_reserved_bits456, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4121 | /* prbMode (1 bit) */
4122 | bool_Bool prb_mode;
4123 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_prb_mode, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &prb_mode);
4124 | offset += 1;
4125 |
4126 | /* reserved (8 bits) */
4127 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4128 | offset += 1;
4129 |
4130 | /* Dissect each SymPrbPattern */
4131 | for (uint32_t n=0; n < num_sym_prb_pattern; n++) {
4132 |
4133 | /* Subtree */
4134 | proto_item *pattern_ti = proto_tree_add_string_format(extension_tree, hf_oran_sym_prb_pattern,
4135 | tvb, offset, 1, "",
4136 | prb_mode ? "PRB-BLOCK" : "PRB-MASK");
4137 | proto_tree *pattern_tree = proto_item_add_subtree(pattern_ti, ett_oran_sym_prb_pattern);
4138 |
4139 |
4140 | /* Orange part */
4141 |
4142 | /* Reserved (2 bits) */
4143 | proto_tree_add_item(pattern_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4144 | /* symMask (14 bits) */
4145 | proto_tree_add_item(pattern_tree, hf_oran_sym_mask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4146 | offset += 2;
4147 | /* numMcScaleOffset (4 bits) */
4148 | uint32_t numMcScaleOffset;
4149 | proto_tree_add_item_ret_uint(pattern_tree, hf_oran_num_mc_scale_offset, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numMcScaleOffset);
4150 |
4151 | if (!prb_mode) { /* PRB-MASK */
4152 | /* prbPattern (4 bits) */
4153 | proto_tree_add_item(pattern_tree, hf_oran_prb_pattern, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4154 | offset += 1;
4155 | /* reserved (8 bits) */
4156 | proto_tree_add_item(pattern_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4157 | offset += 1;
4158 | }
4159 | else { /* PRB-BLOCK */
4160 | /* prbBlkOffset (8 bits) */
4161 | proto_tree_add_item(pattern_tree, hf_oran_prb_block_offset, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4162 | offset += 1;
4163 | /* prbBlkSize (4 bits) */
4164 | proto_tree_add_item(pattern_tree, hf_oran_prb_block_size, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4165 | offset += 1;
4166 | }
4167 |
4168 | /* Yellowish part */
4169 | if (prb_mode) { /* PRB-BLOCK */
4170 | /* prbBlkSize (4 bits) */
4171 | proto_tree_add_item(pattern_tree, hf_oran_prb_block_size, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4172 | }
4173 | else {
4174 | /* reserved (4 bits) */
4175 | proto_tree_add_item(pattern_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4176 | }
4177 |
4178 | for (unsigned c=0; c < numMcScaleOffset; c++) {
4179 |
4180 | if (c > 0) {
4181 | /* reserved (4 bits) */
4182 | proto_tree_add_item(pattern_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4183 | }
4184 |
4185 | static int * const remask_flags_even[] = {
4186 | &hf_oran_mc_scale_re_mask_re1_even,
4187 | &hf_oran_mc_scale_re_mask_re2_even,
4188 | &hf_oran_mc_scale_re_mask_re3_even,
4189 | &hf_oran_mc_scale_re_mask_re4_even,
4190 | &hf_oran_mc_scale_re_mask_re5_even,
4191 | &hf_oran_mc_scale_re_mask_re6_even,
4192 | &hf_oran_mc_scale_re_mask_re7_even,
4193 | &hf_oran_mc_scale_re_mask_re8_even,
4194 | &hf_oran_mc_scale_re_mask_re9_even,
4195 | &hf_oran_mc_scale_re_mask_re10_even,
4196 | &hf_oran_mc_scale_re_mask_re11_even,
4197 | &hf_oran_mc_scale_re_mask_re12_even,
4198 | NULL((void*)0)
4199 | };
4200 |
4201 | /* mcScaleReMask (12 bits). Defines which REs the following csf and mcScaleOffset apply to */
4202 | uint64_t mcScaleReMask, mcScaleOffset;
4203 | proto_tree_add_bitmask_ret_uint64(pattern_tree, tvb, offset,
4204 | hf_oran_mc_scale_re_mask_even,
4205 | ett_oran_mc_scale_remask,
4206 | remask_flags_even, ENC_BIG_ENDIAN0x00000000, &mcScaleReMask);
4207 |
4208 | offset += 2;
4209 | /* csf (1 bit) */
4210 | bool_Bool csf;
4211 | dissect_csf(pattern_tree, tvb, offset*8, ci_iq_width, &csf);
4212 | /* mcScaleOffset (15 bits) */
4213 | proto_item *ti = proto_tree_add_bits_ret_val(pattern_tree, hf_oran_mc_scale_offset, tvb, offset*8 + 1, 15, &mcScaleOffset, ENC_BIG_ENDIAN0x00000000);
4214 | uint16_t exponent = (mcScaleOffset >> 11) & 0x000f; /* m.s. 4 bits */
4215 | uint16_t mantissa = mcScaleOffset & 0x07ff; /* l.s. 11 bits */
4216 | double mcScaleOffset_value = ((double)mantissa/(1<<11)) * (1.0 / (1 << exponent));
4217 | proto_item_append_text(ti, " (%f)", mcScaleOffset_value);
4218 |
4219 | offset += 2;
4220 |
4221 | /* Record this config. */
4222 | if (state && state->mod_comp_params.num_configs < MAX_MOD_COMPR_CONFIGS16) {
4223 | unsigned i = state->mod_comp_params.num_configs;
4224 | state->mod_comp_params.configs[i].mod_compr_re_mask = (uint16_t)mcScaleReMask;
4225 | state->mod_comp_params.configs[i].mod_compr_csf = csf;
4226 | state->mod_comp_params.configs[i].mod_compr_scaler = mcScaleOffset_value;
4227 | state->mod_comp_params.num_configs++;
4228 | }
4229 | }
4230 |
4231 | proto_item_set_end(pattern_ti, tvb, offset);
4232 | }
4233 | break;
4234 | }
4235 |
4236 | case 24: /* SE 24: PUSCH DMRS configuration */
4237 | {
4238 | /* Hidden filter for bf (DMRS BF) */
4239 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
4240 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
4241 |
4242 | /* alpnPerSym (1 bit) */
4243 | proto_tree_add_item(extension_tree, hf_oran_alpn_per_sym, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4244 | /* antDmrsSnr (1 bit) */
4245 | proto_tree_add_item(extension_tree, hf_oran_ant_dmrs_snr, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4246 | /* reserved (1 bit) */
4247 | proto_tree_add_item(extension_tree, hf_oran_reserved_bit2, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4248 | /* userGroupSize (5 bits) */
4249 | uint32_t user_group_size;
4250 | proto_item *ugs_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_user_group_size, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &user_group_size);
4251 | if (user_group_size == 0) {
4252 | proto_item_append_text(ugs_ti, " (not used)");
4253 | }
4254 | else if (user_group_size > 12) {
4255 | proto_item_append_text(ugs_ti, " (reserved)");
4256 | }
4257 | offset += 1;
4258 | /* userGroupId (8 bits)*/
4259 | uint32_t user_group_id;
4260 | proto_item *ugi_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_user_group_id, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &user_group_id);
4261 | if (user_group_id == 0) {
4262 | /* TODO: Value 0 can happen in several cases, described in 7.7.24.7.. */
4263 | }
4264 | if (user_group_id == 255) {
4265 | /* Value 255 is reserved */
4266 | expert_add_info(pinfo, ugi_ti, &ei_oran_user_group_id_reserved_value);
4267 | }
4268 | offset += 1;
4269 |
4270 | bool_Bool seen_value_to_inherit = false0;
4271 | bool_Bool inherited_config_has_transform_precoding = false0;
4272 | int dmrs_configs_seen = 0;
4273 |
4274 | /* Dissect each entry until reach number of configured ueIds (or run out of extlen bytes..) */
4275 | uint32_t ueid_index = 0;
4276 | while ((offset < (extension_start_offset + extlen*4)) && (ueid_index < number_of_ueids)) {
4277 | dmrs_configs_seen++;
4278 |
4279 | /* Subtree */
4280 | proto_item *entry_ti = proto_tree_add_string_format(extension_tree, hf_oran_dmrs_entry,
4281 | tvb, offset, 0, "",
4282 | "Entry");
4283 | proto_tree *entry_tree = proto_item_add_subtree(entry_ti, ett_oran_dmrs_entry);
4284 |
4285 | /* entryType (3 bits) */
4286 | uint32_t entry_type;
4287 | proto_item *entry_type_ti;
4288 | entry_type_ti = proto_tree_add_item_ret_uint(entry_tree, hf_oran_entry_type, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &entry_type);
4289 | if (entry_type > 3) {
4290 | proto_item_append_text(entry_type_ti, " (reserved)");
4291 | }
4292 |
4293 | /* dmrsPortNumber (5 bits). Values 0-11 allowed */
4294 | unsigned int dmrs_port_number;
4295 | proto_item *dpn_ti = proto_tree_add_item_ret_uint(entry_tree, hf_oran_dmrs_port_number, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &dmrs_port_number);
4296 | if (dmrs_port_number > 11) {
4297 | proto_item_append_text(dpn_ti, " (12-31 are reserved)");
4298 | }
4299 | offset += 1;
4300 |
4301 | /* What follows depends upon entryType */
4302 | switch (entry_type) {
4303 | case 0: /* dmrsPortNumber config same as previous, ueId ueIdReset=0 */
4304 | case 1: /* dmrsPortNumber config same as previous, ueId ueIdReset=1 */
4305 | /* No further fields for these */
4306 | /* Error here if no previous values to inherit!! */
4307 | if (!seen_value_to_inherit) {
4308 | expert_add_info_format(pinfo, entry_type_ti, &ei_oran_se24_nothing_to_inherit,
4309 | "SE24: have seen entry type %u, but no previous config (type 2 or 3) to inherit config from", entry_type);
4310 |
4311 | }
4312 | /* TODO: would be useful to repeat whole inherited config here? */
4313 | break;
4314 |
4315 | case 2: /* transform precoding disabled */
4316 | case 3: /* transform precoding enabled */
4317 | {
4318 | /* Type 2/3 are very similar.. */
4319 |
4320 | /* ueIdReset (1 bit) */
4321 | proto_tree_add_item(entry_tree, hf_oran_ueid_reset, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4322 | /* reserved (1 bit) */
4323 | proto_tree_add_item(entry_tree, hf_oran_reserved_bit1, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4324 |
4325 | /* dmrsSymbolMask (14 bits) */
4326 | static int * const dmrs_symbol_mask_flags[] = {
4327 | &hf_oran_dmrs_symbol_mask_s13,
4328 | &hf_oran_dmrs_symbol_mask_s12,
4329 | &hf_oran_dmrs_symbol_mask_s11,
4330 | &hf_oran_dmrs_symbol_mask_s10,
4331 | &hf_oran_dmrs_symbol_mask_s9,
4332 | &hf_oran_dmrs_symbol_mask_s8,
4333 | &hf_oran_dmrs_symbol_mask_s7,
4334 | &hf_oran_dmrs_symbol_mask_s6,
4335 | &hf_oran_dmrs_symbol_mask_s5,
4336 | &hf_oran_dmrs_symbol_mask_s4,
4337 | &hf_oran_dmrs_symbol_mask_s3,
4338 | &hf_oran_dmrs_symbol_mask_s2,
4339 | &hf_oran_dmrs_symbol_mask_s1,
4340 | &hf_oran_dmrs_symbol_mask_s0,
4341 | NULL((void*)0)
4342 | };
4343 | proto_tree_add_bitmask(entry_tree, tvb, offset,
4344 | hf_oran_dmrs_symbol_mask, ett_oran_dmrs_symbol_mask, dmrs_symbol_mask_flags, ENC_BIG_ENDIAN0x00000000);
4345 | offset += 2;
4346 |
4347 | /* scrambling */
4348 | proto_tree_add_item(entry_tree, hf_oran_scrambling, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4349 | offset += 2;
4350 |
4351 | /* nscid (1 bit) */
4352 | proto_tree_add_item(entry_tree, hf_oran_nscid, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4353 |
4354 | /* These 5 bits differ depending upon entry type */
4355 | if (entry_type == 2) { /* type 2 */
4356 | /* dType (1 bit) */
4357 | proto_tree_add_item(entry_tree, hf_oran_dtype, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4358 | /* cdmWithoutData (2 bits) */
4359 | proto_tree_add_item(entry_tree, hf_oran_cmd_without_data, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4360 | /* lambda (2 bits) */
4361 | proto_tree_add_item(entry_tree, hf_oran_lambda, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4362 | }
4363 | else { /* type 3 */
4364 | /* reserved (1 bit) */
4365 | proto_tree_add_item(entry_tree, hf_oran_reserved_bit1, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4366 | /* lowPaprType (2 bits) */
4367 | proto_tree_add_item(entry_tree, hf_oran_low_papr_type, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4368 | /* hoppingMode (2 bits) */
4369 | proto_tree_add_item(entry_tree, hf_oran_hopping_mode, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4370 | }
4371 |
4372 | /* firstPrb (9 bits) */
4373 | proto_tree_add_item(entry_tree, hf_oran_first_prb, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4374 | offset += 1;
4375 | /* lastPrb (9 bits) */
4376 | proto_tree_add_item(entry_tree, hf_oran_last_prb, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4377 | offset += 2;
4378 | /* Reserved (16 bits) */
4379 | proto_tree_add_item(entry_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4380 | offset += 2;
4381 |
4382 | /* Could now see entry types 0 or 1 - they have these values to inherit */
4383 | seen_value_to_inherit = true1;
4384 | inherited_config_has_transform_precoding = (entry_type == 3);
4385 | break;
4386 | }
4387 |
4388 | default:
4389 | /* reserved - expert info */
4390 | break;
4391 | }
4392 |
4393 | proto_item_append_text(entry_ti, " [UEId=%u] (dmrsPortNumber=%2u) (type %u - %s) ",
4394 | ueids[ueid_index++], dmrs_port_number, entry_type, val_to_str_const(entry_type, entry_type_vals, "Unknown"));
4395 | proto_item_set_end(entry_ti, tvb, offset);
4396 |
4397 | if (entry_type <= 1) {
4398 | proto_item_append_text(entry_ti, " [transform-precoding %s]",
4399 | inherited_config_has_transform_precoding ? "enabled" : "disabled");
4400 | }
4401 | }
4402 |
4403 | proto_item_append_text(extension_ti, " (%d DMRS configs seen)", dmrs_configs_seen);
4404 | break;
4405 | }
4406 |
4407 | case 25: /* SE 25: Symbol reordering for DMRS-BF */
4408 | /* Just dissect each available block of 7 bytes as the 14 symbols for a layer,
4409 | where each layer could be one or apply to all layers. */
4410 | {
4411 | /* TODO: should only appear in one section of a message - check? */
4412 | unsigned layer = 0;
4413 | proto_item *layer_ti;
4414 | while (offset+7 <= (extension_start_offset + extlen*4)) {
4415 | /* Layer subtree */
4416 | layer_ti = proto_tree_add_string_format(extension_tree, hf_oran_symbol_reordering_layer,
4417 | tvb, offset, 7, "",
4418 | "Layer");
4419 | proto_tree *layer_tree = proto_item_add_subtree(layer_ti, ett_oran_symbol_reordering_layer);
4420 |
4421 | /* All 14 symbols for a layer (or all layers) */
4422 | for (unsigned s=0; s < 14; s++) {
4423 | proto_item *sym_ti;
4424 | /* txWinForOnAirSymbol */
4425 | unsigned int tx_win_for_on_air_symbol;
4426 | sym_ti = proto_tree_add_item_ret_uint(layer_tree,
4427 | (s % 2) ? hf_oran_tx_win_for_on_air_symbol_r : hf_oran_tx_win_for_on_air_symbol_l,
4428 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &tx_win_for_on_air_symbol);
4429 | if (tx_win_for_on_air_symbol == 0x0F) {
4430 | /* Ordering not affected */
4431 | proto_item_append_text(sym_ti, " (sym %u - no info)", s);
4432 | }
4433 | else {
4434 | proto_item_append_text(sym_ti, " (sym %u)", s);
4435 | }
4436 | if (s % 2) {
4437 | offset += 1;
4438 | }
4439 | }
4440 |
4441 | proto_item_append_text(layer_ti, " (layer %u)", ++layer);
4442 | proto_item_append_text(extension_ti, " (layer %u)", layer);
4443 | }
4444 | /* Set layer subtree label */
4445 | if (layer == 1) {
4446 | proto_item_append_text(layer_ti, " (all)");
4447 | proto_item_append_text(extension_ti, " (all)");
4448 | }
4449 | if (layer == 0) {
4450 | /* TODO: are no layers valid? What does it mean? */
4451 | proto_item_append_text(extension_ti, " (none)");
4452 | }
4453 | break;
4454 | }
4455 |
4456 | case 26: /* SE 26: Frequency offset feedback */
4457 | /* Reserved (8 bits). N.B., added after draft? */
4458 | proto_tree_add_item(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4459 | offset += 1;
4460 | /* Reserved (1 bit) */
4461 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4462 | /* numFoFb (7 bits) */
4463 | unsigned num_fo_fb;
4464 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_fo_fb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_fo_fb);
4465 | offset += 1;
4466 |
4467 | /* Add each freqOffsetFb value */
4468 | for (unsigned n=0; n < num_fo_fb; n++) {
4469 | unsigned freq_offset_fb;
4470 | /* freqOffsetFb (16 bits) */
4471 | proto_item *offset_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_freq_offset_fb,
4472 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &freq_offset_fb);
4473 | /* Show if maps onto a -ve number */
4474 | if ((freq_offset_fb >= 0x8ad0) && (freq_offset_fb <= 0xffff)) {
4475 | proto_item_append_text(offset_ti, "(value %d)", -1 - (0xffff-freq_offset_fb));
4476 | }
4477 | proto_item_append_text(offset_ti, " [#%u]", n+1);
4478 | offset += 2;
4479 | }
4480 | break;
4481 |
4482 | case 27: /* SE 27: O-DU controlled dimensionality reduction */
4483 | {
4484 | /* Hidden filter for bf (DMRS BF) */
4485 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
4486 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
4487 |
4488 | /* beamType (2 bits) */
4489 | unsigned beam_type;
4490 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_beam_type, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &beam_type);
4491 | /* reserved (6 bits) */
4492 | proto_tree_add_item(extension_tree, hf_oran_reserved_last_6bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4493 | offset += 1;
4494 |
4495 | /* numElements */
4496 | unsigned num_elements;
4497 | proto_item *num_elements_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_elements, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_elements);
4498 | if (num_elements == 0) {
4499 | num_elements = 256;
4500 | proto_item_append_text(num_elements_ti, " (256");
4501 | }
4502 |
4503 | offset += 1;
4504 |
4505 | /* beamId value(s) */
4506 | switch (beam_type) {
4507 | case 0:
4508 | for (unsigned n=0; n < num_elements; n++) {
4509 | /* reserved (1 bit) + beamId */
4510 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4511 | proto_tree_add_item(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4512 | offset += 2;
4513 | }
4514 | break;
4515 | case 1:
4516 | /* reserved (1 bit) + beamId */
4517 | proto_tree_add_item(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4518 | proto_tree_add_item(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4519 | offset += 2;
4520 | break;
4521 | default:
4522 | /* Unknown type... */
4523 | break;
4524 | }
4525 | break;
4526 | }
4527 |
4528 | case 28: /* SE 28: O-DU controlled frequency resolution for SINR reporting */
4529 | {
4530 | /* reserved (3 bits) */
4531 | proto_tree_add_item(extension_tree, hf_oran_reserved_3bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4532 | /* numUeSinrRpt */
4533 | uint32_t num_ue_sinr_rpt;
4534 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_ue_sinr_rpt, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_ue_sinr_rpt);
4535 | offset += 1;
4536 |
4537 | for (uint32_t n=0; n < num_ue_sinr_rpt; n++) {
4538 | /* reserved (1 bit) */
4539 | proto_tree_add_item(extension_tree, (n % 2) ? hf_oran_reserved_bit4 : hf_oran_reserved_1bit,
4540 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4541 |
4542 | /* numSinrPerPrb (3 bits). Taken from alternate nibbles within byte. */
4543 | proto_tree_add_item(extension_tree, (n % 2) ? hf_oran_num_sinr_per_prb_right : hf_oran_num_sinr_per_prb,
4544 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4545 | if (n % 2) {
4546 | offset += 1;
4547 | }
4548 | }
4549 |
4550 | /* May need to skip beyond half-used byte */
4551 | if (num_ue_sinr_rpt % 2) {
4552 | offset += 1;
4553 | }
4554 | break;
4555 | }
4556 |
4557 |
4558 | default:
4559 | /* Other/unexpected extension types */
4560 | expert_add_info_format(pinfo, exttype_ti, &ei_oran_unhandled_se,
4561 | "SE %u (%s) not supported by dissector",
4562 | exttype, val_to_str_const(exttype, exttype_vals, "Reserved"));
4563 | ext_unhandled = true1;
4564 | break;
4565 | }
4566 |
4567 | /* Check offset compared with extlen. There should be 0-3 bytes of padding */
4568 | int num_padding_bytes = (extension_start_offset + (extlen*4) - offset);
4569 | if (!ext_unhandled && ((num_padding_bytes<0) || (num_padding_bytes>3))) {
4570 | expert_add_info_format(pinfo, extlen_ti, &ei_oran_extlen_wrong,
4571 | "extlen signalled %u bytes (+ 0-3 bytes padding), but %u were dissected",
4572 | extlen*4, offset-extension_start_offset);
4573 | }
4574 |
4575 | /* Move offset to beyond signalled length of extension */
4576 | offset = extension_start_offset + (extlen*4);
4577 |
4578 | /* Set length of extension header. */
4579 | proto_item_set_len(extension_ti, extlen*4);
4580 | }
4581 | /* End of section extension handling */
4582 |
4583 |
4584 |
4585 | /* RRM measurement reports have measurement reports *after* extensions */
4586 | if (sectionType == SEC_C_RRM_MEAS_REPORTS) /* Section Type 10 */
4587 | {
4588 | /* Hidden filter for bf (DMFS-BF). No BF weights though.. */
4589 | bf_ti = proto_tree_add_item(c_section_tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
4590 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
4591 |
4592 | bool_Bool mf;
4593 | do {
4594 | /* Measurement report subtree */
4595 | proto_item *mr_ti = proto_tree_add_string_format(c_section_tree, hf_oran_measurement_report,
4596 | tvb, offset, 1, "", "Measurement Report");
4597 | proto_tree *mr_tree = proto_item_add_subtree(mr_ti, ett_oran_measurement_report);
4598 | unsigned report_start_offset = offset;
4599 |
4600 | /* more fragments (after this one) (1 bit) */
4601 | proto_tree_add_item_ret_boolean(mr_tree, hf_oran_mf, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &mf);
4602 |
4603 | /* measTypeId (7 bits) */
4604 | uint32_t meas_type_id;
4605 | proto_item *meas_type_id_ti;
4606 | meas_type_id_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_meas_type_id, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &meas_type_id);
4607 | offset += 1;
4608 |
4609 | /* Common to all measurement types */
4610 | unsigned num_elements = 0;
4611 | if (meas_type_id == 6) {
4612 | /* numElements */
4613 | proto_tree_add_item_ret_uint(mr_tree, hf_oran_num_elements, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_elements);
4614 | }
4615 | else {
4616 | /* All other meas ids have a reserved byte */
4617 | proto_tree_add_item(mr_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4618 | }
4619 | offset += 1;
4620 |
4621 | /* measDataSize (16 bits). N.B. begins at mf field, i.e. 2 bytes before this one */
4622 | unsigned meas_data_size;
4623 | proto_item *meas_data_size_ti;
4624 | meas_data_size_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_meas_data_size, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &meas_data_size);
4625 | meas_data_size *= 4;
4626 | proto_item_append_text(meas_data_size_ti, " (%u bytes)", meas_data_size);
4627 | offset += 2;
4628 |
4629 | /* Summary for measurement report root */
4630 | proto_item_append_text(mr_ti, " (measTypeId=%u - %s)",
4631 | meas_type_id, val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
4632 | /* And section header */
4633 | proto_item_append_text(tree, " (%s)", val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
4634 | /* And Info column */
4635 | col_append_fstr(pinfo->cinfo, COL_INFO, " (%s)", val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
4636 |
4637 | /* Handle specific message type fields */
4638 | switch (meas_type_id) {
4639 | case 1:
4640 | {
4641 | /* ueTae */
4642 | unsigned ue_tae;
4643 | proto_item *ue_tae_ti;
4644 | ue_tae_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_tae, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_tae);
4645 | /* Show if maps onto a -ve number */
4646 | if ((ue_tae >= 0x8ad0) && (ue_tae <= 0xffff)) {
4647 | proto_item_append_text(ue_tae_ti, "(value %d)", -1 - (0xffff-ue_tae));
4648 | }
4649 | offset += 2;
4650 |
4651 | /* Reserved (16 bits) */
4652 | proto_tree_add_item(mr_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4653 | offset += 2;
4654 | break;
4655 | }
4656 | case 2:
4657 | /* ueLayerPower entries (how many? for now just use up meas_data_size..) */
4658 | /* TODO: add number of distinct dmrsPortNumber entries seen in SE24 and save in state? */
4659 | /* Or would it make sense to use the preference 'pref_num_bf_antennas' ? */
4660 | for (unsigned n=0; n < (meas_data_size-4)/2; n++) {
4661 | unsigned ue_layer_power;
4662 | proto_item *ue_layer_power_ti;
4663 | ue_layer_power_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_layer_power, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_layer_power);
4664 | /* Show if maps onto a -ve number */
4665 | if ((ue_layer_power >= 0x8ad0) && (ue_layer_power <= 0xffff)) {
4666 | proto_item_append_text(ue_layer_power_ti, "(value %d)", -1 - (0xffff-ue_layer_power));
4667 | }
4668 | offset += 2;
4669 | }
4670 | /* padding out to 4 bytes */
4671 | break;
4672 | case 3:
4673 | {
4674 | /* ueFreqOffset */
4675 | unsigned ue_freq_offset;
4676 | proto_item *ue_freq_offset_ti;
4677 | ue_freq_offset_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_freq_offset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_freq_offset);
4678 | /* Show if maps onto a -ve number */
4679 | if ((ue_freq_offset >= 0x8ad0) && (ue_freq_offset <= 0xffff)) {
4680 | proto_item_append_text(ue_freq_offset_ti, "(value %d)", -1 - (0xffff-ue_freq_offset));
4681 | }
4682 | offset += 2;
4683 |
4684 | /* Reserved (16 bits) */
4685 | proto_tree_add_item(mr_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4686 | offset += 2;
4687 | break;
4688 | }
4689 | case 4:
4690 | case 5:
4691 | /* reserved (2 bits) */
4692 | proto_tree_add_item(mr_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4693 | /* symbolMask (14 bits) */
4694 | offset = dissect_symbolmask(tvb, mr_tree, offset, NULL((void*)0), NULL((void*)0));
4695 |
4696 | /* 2 bytes for each PRB ipnPower */
4697 | for (unsigned prb=0; prb<MAX_PRBS273; prb++) {
4698 | /* Skip if should not be reported */
4699 | if (!prbs_for_st10_type5[prb]) {
4700 | continue;
4701 | }
4702 | unsigned ipn_power;
4703 | proto_item *ipn_power_ti;
4704 | /* ipnPower (2 bytes) */
4705 | ipn_power_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ipn_power, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ipn_power);
4706 | proto_item_append_text(ipn_power_ti, " (PRB %3d)", prb);
4707 | /* Show if maps onto a -ve number */
4708 | if ((ipn_power >= 0x8ad0) && (ipn_power <= 0xffff)) {
4709 | proto_item_append_text(ipn_power_ti, " (value %d)", -1 - (0xffff-ipn_power));
4710 | }
4711 | offset += 2;
4712 | }
4713 | /* padding out to 4 bytes */
4714 | break;
4715 | case 6:
4716 | /* antDmrsSnrVal entries */
4717 | for (unsigned n=0; n < num_elements; n++) {
4718 | unsigned snr_value;
4719 | proto_item *snr_value_ti;
4720 | /* antDmrsSnrVal (2 bytes) */
4721 | snr_value_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ant_dmrs_snr_val, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &snr_value);
4722 | proto_item_append_text(snr_value_ti, " (elem %2u)", n+1);
4723 | /* Show if maps onto a -ve number */
4724 | if ((snr_value >= 0x8ad0) && (snr_value <= 0xffff)) {
4725 | proto_item_append_text(snr_value_ti, " (value %d)", -1 - (0xffff-snr_value));
4726 | }
4727 | offset += 2;
4728 | }
4729 | break;
4730 |
4731 | default:
4732 | /* Anything else is not expected */
4733 | expert_add_info_format(pinfo, meas_type_id_ti, &ei_oran_unexpected_measTypeId,
4734 | "measTypeId %u (%s) not supported - only 1-6 are expected",
4735 | meas_type_id,
4736 | val_to_str_const(meas_type_id, meas_type_id_vals, "reserved"));
4737 | break;
4738 |
4739 | }
4740 |
4741 | /* Pad out to next 4 bytes */
4742 | offset += WS_PADDING_TO_4(offset-report_start_offset)((4U - ((offset-report_start_offset) % 4U)) % 4U);
4743 |
4744 | /* TODO: verify dissected size of report vs meas_data_size? */
4745 |
4746 | /* End of measurement report tree */
4747 | proto_item_set_end(mr_ti, tvb, offset);
4748 | } while (mf);
4749 | }
4750 |
4751 | /* Request for RRM Measurements has measurement commands after extensions */
4752 | else if (sectionType == SEC_C_REQUEST_RRM_MEAS) /* Section Type 11 */
4753 | {
4754 | bool_Bool mf = true1;
4755 | do {
4756 | /* Measurement command subtree */
4757 | proto_item *mc_ti = proto_tree_add_string_format(c_section_tree, hf_oran_measurement_command,
4758 | tvb, offset, 8, "", "Measurement Command");
4759 | proto_tree *mc_tree = proto_item_add_subtree(mc_ti, ett_oran_measurement_command);
4760 |
4761 | /* mf (1 bit). 1st measurement command is always preset */
4762 | proto_tree_add_item_ret_boolean(mc_tree, hf_oran_mf, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &mf);
4763 |
4764 | /* measTypeId (7 bits) */
4765 | uint32_t meas_type_id;
4766 | proto_item *meas_type_id_ti;
4767 | meas_type_id_ti = proto_tree_add_item_ret_uint(mc_tree, hf_oran_meas_type_id, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &meas_type_id);
4768 | offset += 1;
4769 |
4770 | proto_item *meas_command_ti;
4771 | uint32_t meas_command_size;
4772 |
4773 | switch (meas_type_id) {
4774 | case 5: /* command for IpN for unallocated PRBs */
4775 | /* reserved (1 byte) */
4776 | proto_tree_add_item(mc_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4777 | offset += 1;
4778 | /* measCmdSize. Presumably number of words so in future could skip unrecognised command types.. */
4779 | meas_command_ti = proto_tree_add_item_ret_uint(mc_tree, hf_oran_meas_cmd_size, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &meas_command_size);
4780 | proto_item_append_text(meas_command_ti, " (%u bytes)", meas_command_size*4);
4781 | offset += 2;
4782 | /* reserved (2 bits) */
4783 | proto_tree_add_item(mc_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4784 | /* symbolMask (14 bits) */
4785 | offset = dissect_symbolmask(tvb, mc_tree, offset, NULL((void*)0), NULL((void*)0));
4786 | /* reserved (16 bits) */
4787 | proto_tree_add_item(mc_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4788 | offset += 2;
4789 | break;
4790 |
4791 | default:
4792 | /* Anything else is not expected */
4793 | expert_add_info_format(pinfo, meas_type_id_ti, &ei_oran_unexpected_measTypeId,
4794 | "measTypeId %u (%s) not supported - only 5 is expected",
4795 | meas_type_id,
4796 | val_to_str_const(meas_type_id, meas_type_id_vals, "reserved"));
4797 | break;
4798 | }
4799 | proto_item_append_text(mc_ti, " (%s)", val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
4800 |
4801 | } while (mf);
4802 | }
4803 |
4804 | /* Set extent of overall section */
4805 | proto_item_set_len(sectionHeading, offset);
4806 |
4807 | return offset;
4808 | }
4809 |
4810 | /* Dissect udCompHdr (user data compression header, 7.5.2.10) */
4811 | /* bit_width and comp_meth are out params */
4812 | static int dissect_udcomphdr(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, unsigned offset,
4813 | bool_Bool ignore,
4814 | unsigned *bit_width, unsigned *comp_meth, proto_item **comp_meth_ti)
4815 | {
4816 | /* Subtree */
4817 | proto_item *udcomphdr_ti = proto_tree_add_string_format(tree, hf_oran_udCompHdr,
4818 | tvb, offset, 1, "",
4819 | "udCompHdr");
4820 | proto_tree *udcomphdr_tree = proto_item_add_subtree(udcomphdr_ti, ett_oran_udcomphdr);
4821 |
4822 | /* udIqWidth */
4823 | uint32_t hdr_iq_width;
4824 | proto_item *iq_width_item = proto_tree_add_item_ret_uint(udcomphdr_tree, hf_oran_udCompHdrIqWidth , tvb, offset, 1, ENC_NA0x00000000, &hdr_iq_width);
4825 | *bit_width = (hdr_iq_width) ? hdr_iq_width : 16;
4826 | proto_item_append_text(iq_width_item, " (%u bits)", *bit_width);
4827 |
4828 | /* udCompMeth */
4829 | uint32_t ud_comp_meth;
4830 | *comp_meth_ti = proto_tree_add_item_ret_uint(udcomphdr_tree, hf_oran_udCompHdrMeth, tvb, offset, 1, ENC_NA0x00000000, &ud_comp_meth);
4831 | if (comp_meth) {
4832 | *comp_meth = ud_comp_meth;
4833 | }
4834 |
4835 | /* Summary */
4836 | if (!ignore) {
4837 | proto_item_append_text(udcomphdr_ti, " (IqWidth=%u, udCompMeth=%s)",
4838 | *bit_width, rval_to_str_const(ud_comp_meth, ud_comp_header_meth, "Unknown"));
4839 | }
4840 | else {
4841 | proto_item_append_text(udcomphdr_ti, " (ignored)");
4842 | if (hdr_iq_width || ud_comp_meth) {
4843 | expert_add_info_format(pinfo, udcomphdr_ti, &ei_oran_udpcomphdr_should_be_zero,
4844 | "udCompHdr in C-Plane for DL should be 0 - found 0x%02x",
4845 | tvb_get_uint8(tvb, offset));
4846 | }
4847 |
4848 | }
4849 | return offset+1;
4850 | }
4851 |
4852 | /* Dissect udCompParam (user data compression parameter, 8.3.3.15) */
4853 | /* bit_width and comp_meth are out params */
4854 | static int dissect_udcompparam(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree, unsigned offset,
4855 | unsigned comp_meth,
4856 | uint32_t *exponent, uint16_t *sReSMask,
4857 | bool_Bool for_sinr)
4858 | {
4859 | if (for_sinr && (comp_meth != COMP_BLOCK_FP1)) {
4860 | /* sinrCompParam only present when bfp is used */
4861 | return offset;
4862 | }
4863 |
4864 | if (comp_meth == COMP_NONE0 ||
4865 | comp_meth == COMP_MODULATION4 ||
4866 | comp_meth == MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8) {
4867 |
4868 | /* Not even creating a subtree for udCompMeth 0, 4, 8 */
4869 | return offset;
4870 | }
4871 |
4872 | /* Subtree */
4873 | unsigned start_offset = offset;
4874 | proto_item *udcompparam_ti = proto_tree_add_string_format(tree, hf_oran_udCompParam,
4875 | tvb, offset, 1, "",
4876 | (for_sinr) ? "sinrCompParam" : "udCompParam");
4877 | proto_tree *udcompparam_tree = proto_item_add_subtree(udcompparam_ti, ett_oran_udcompparam);
4878 |
4879 | /* Show comp_meth as a generated field */
4880 | proto_item *meth_ti = proto_tree_add_uint(udcompparam_tree, hf_oran_udCompHdrMeth_pref, tvb, 0, 0, comp_meth);
4881 | proto_item_set_generated(meth_ti);
4882 |
4883 | uint32_t param_exponent;
4884 | uint64_t param_sresmask;
4885 |
4886 | static int * const sres_mask_flags[] = {
4887 | &hf_oran_sReSMask_re12,
4888 | &hf_oran_sReSMask_re11,
4889 | &hf_oran_sReSMask_re10,
4890 | &hf_oran_sReSMask_re9,
4891 | &hf_oran_sReSMask_re8,
4892 | &hf_oran_sReSMask_re7,
4893 | &hf_oran_sReSMask_re6,
4894 | &hf_oran_sReSMask_re5,
4895 | &hf_oran_sReSMask_re4,
4896 | &hf_oran_sReSMask_re3,
4897 | &hf_oran_sReSMask_re2,
4898 | &hf_oran_sReSMask_re1,
4899 | NULL((void*)0)
4900 | };
4901 |
4902 | switch (comp_meth) {
4903 | case COMP_BLOCK_FP1: /* 1 */
4904 | case BFP_AND_SELECTIVE_RE_WITH_MASKS7: /* 7 */
4905 | /* reserved (4 bits) */
4906 | proto_tree_add_item(udcompparam_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
4907 | /* exponent (4 bits) */
4908 | proto_tree_add_item_ret_uint(udcompparam_tree, hf_oran_exponent,
4909 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &param_exponent);
4910 | *exponent = param_exponent;
4911 | proto_item_append_text(udcompparam_ti, " (Exponent=%u)", param_exponent);
4912 | offset += 1;
4913 | break;
4914 |
4915 | case COMP_BLOCK_SCALE2: /* 2 */
4916 | /* Separate into integer and fractional bits? */
4917 | proto_tree_add_item(udcompparam_tree, hf_oran_blockScaler,
4918 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4919 | offset++;
4920 | break;
4921 |
4922 | case COMP_U_LAW3: /* 3 */
4923 | /* compBitWidth, compShift */
4924 | proto_tree_add_item(udcompparam_tree, hf_oran_compBitWidth,
4925 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4926 | proto_tree_add_item(udcompparam_tree, hf_oran_compShift,
4927 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4928 | offset += 1;
4929 | break;
4930 |
4931 | case BFP_AND_SELECTIVE_RE5: /* 5 */
4932 | {
4933 | /* sReSMask (exponent in middle!) */
4934 | proto_item *sresmask_ti;
4935 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(udcompparam_tree, tvb, offset,
4936 | hf_oran_sReSMask,
4937 | ett_oran_sresmask,
4938 | sres_mask_flags,
4939 | ENC_NA0x00000000,
4940 | &param_sresmask);
4941 |
4942 | /* Get rid of exponent-shaped gap */
4943 | param_sresmask = ((param_sresmask >> 4) & 0x0f00) | (param_sresmask & 0xff);
4944 | unsigned res = 0;
4945 | for (unsigned n=0; n < 12; n++) {
4946 | if ((param_sresmask >> n) & 0x1) {
4947 | res++;
4948 | }
4949 | }
4950 | proto_item_append_text(sresmask_ti, " (%2u REs)", res);
4951 |
4952 | /* exponent */
4953 | proto_tree_add_item_ret_uint(udcompparam_tree, hf_oran_exponent,
4954 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &param_exponent);
4955 | *sReSMask = (uint16_t)param_sresmask;
4956 | *exponent = param_exponent;
4957 |
4958 | proto_item_append_text(udcompparam_ti, " (exponent=%u, %u REs)", *exponent, res);
4959 | offset += 2;
4960 | break;
4961 | }
4962 |
4963 | case MOD_COMPR_AND_SELECTIVE_RE6: /* 6 */
4964 | {
4965 | /* sReSMask (exponent in middle!) */
4966 | proto_item *sresmask_ti;
4967 |
4968 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(udcompparam_tree, tvb, offset,
4969 | hf_oran_sReSMask,
4970 | ett_oran_sresmask,
4971 | sres_mask_flags,
4972 | ENC_NA0x00000000,
4973 | &param_sresmask);
4974 |
4975 | /* Get rid of reserved-shaped gap */
4976 | param_sresmask = ((param_sresmask >> 4) & 0x0f00) | (param_sresmask & 0xff);
4977 | unsigned res = 0;
4978 | for (unsigned n=0; n < 12; n++) {
4979 | if ((param_sresmask >> n) & 0x1) {
4980 | res++;
4981 | }
4982 | }
4983 | proto_item_append_text(sresmask_ti, " (%u REs)", res);
4984 |
4985 | /* reserved (4 bits) */
4986 | proto_tree_add_item(udcompparam_tree, hf_oran_reserved_last_4bits,
4987 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4988 | *sReSMask = (uint16_t)param_sresmask;
4989 |
4990 | proto_item_append_text(udcompparam_ti, " (%u REs)", res);
4991 | offset += 2;
4992 | break;
4993 | }
4994 |
4995 | default:
4996 | /* reserved (set to all zeros), but how many bytes?? */
4997 | break;
4998 | }
4999 |
5000 | proto_item_set_len(udcompparam_ti, offset-start_offset);
5001 | return offset;
5002 | }
5003 |
5004 |
5005 | /* Dissect ciCompHdr (channel information compression header, 7.5.2.15) */
5006 | /* bit_width and comp_meth are out params */
5007 | static int dissect_cicomphdr(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree, unsigned offset,
5008 | unsigned *bit_width, unsigned *comp_meth, uint8_t *comp_opt)
5009 | {
5010 | /* Subtree */
5011 | proto_item *cicomphdr_ti = proto_tree_add_string_format(tree, hf_oran_ciCompHdr,
5012 | tvb, offset, 1, "",
5013 | "ciCompHdr");
5014 | proto_tree *cicomphdr_tree = proto_item_add_subtree(cicomphdr_ti, ett_oran_cicomphdr);
5015 |
5016 | /* ciIqWidth */
5017 | uint32_t hdr_iq_width;
5018 | proto_item *iq_width_item = proto_tree_add_item_ret_uint(cicomphdr_tree, hf_oran_ciCompHdrIqWidth , tvb, offset, 1, ENC_NA0x00000000, &hdr_iq_width);
5019 | hdr_iq_width = (hdr_iq_width) ? hdr_iq_width : 16;
5020 | if (bit_width) {
5021 | *bit_width = hdr_iq_width;
5022 | }
5023 | proto_item_append_text(iq_width_item, " (%u bits)", hdr_iq_width);
5024 |
5025 | /* ciCompMeth */
5026 | uint32_t ci_comp_meth;
5027 | proto_tree_add_item_ret_uint(cicomphdr_tree, hf_oran_ciCompHdrMeth, tvb, offset, 1, ENC_NA0x00000000, &ci_comp_meth);
5028 | if (comp_meth) {
5029 | *comp_meth = ci_comp_meth;
5030 | }
5031 |
5032 | /* ciCompOpt */
5033 | uint32_t opt;
5034 | proto_tree_add_item_ret_uint(cicomphdr_tree, hf_oran_ciCompOpt, tvb, offset, 1, ENC_NA0x00000000, &opt);
5035 | *comp_opt = opt;
5036 | offset += 1;
5037 |
5038 | /* Summary */
5039 | proto_item_append_text(cicomphdr_ti, " (IqWidth=%u, ciCompMeth=%s, ciCompOpt=%s)",
5040 | hdr_iq_width,
5041 | rval_to_str_const(ci_comp_meth, ud_comp_header_meth, "Unknown"),
5042 | (*comp_opt) ? "compression per PRB" : "compression per UE");
5043 | return offset;
5044 | }
5045 |
5046 | static void dissect_payload_version(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo, unsigned offset)
5047 | {
5048 | unsigned version;
5049 | proto_item *ti = proto_tree_add_item_ret_uint(tree, hf_oran_payload_version, tvb, offset, 1, ENC_NA0x00000000, &version);
5050 | if (version != 1) {
5051 | expert_add_info_format(pinfo, ti, &ei_oran_version_unsupported,
5052 | "PayloadVersion %u not supported by dissector (only 1 is known)",
5053 | version);
5054 | /* TODO: should throw an exception? */
5055 | }
5056 | }
5057 |
5058 | static void show_link_to_acknack_request(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo,
5059 | ack_nack_request_t *request)
5060 | {
5061 | /* Request frame */
5062 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_acknack_request_frame,
5063 | tvb, 0, 0, request->request_frame_number);
5064 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
5065 |
5066 | /* Work out gap between frames (in ms) */
5067 | int seconds_between_packets = (int)
5068 | (pinfo->abs_ts.secs - request->request_frame_time.secs);
5069 | int nseconds_between_packets =
5070 | pinfo->abs_ts.nsecs - request->request_frame_time.nsecs;
5071 |
5072 | int total_gap = (seconds_between_packets*1000) +
5073 | ((nseconds_between_packets+500000) / 1000000);
5074 |
5075 | ti = proto_tree_add_uint(tree, hf_oran_acknack_request_time,
5076 | tvb, 0, 0, total_gap);
5077 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
5078 |
5079 | /* Type of request */
5080 | ti = proto_tree_add_uint(tree, hf_oran_acknack_request_type,
5081 | tvb, 0, 0, request->requestType);
5082 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
5083 | }
5084 |
5085 | static void show_link_to_acknack_response(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo,
5086 | ack_nack_request_t *response)
5087 | {
5088 | if (response->response_frame_number == 0) {
5089 | /* Requests may not get a response, and can't always tell when to expect one */
5090 | return;
5091 | }
5092 |
5093 | /* Response frame */
5094 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_acknack_response_frame,
5095 | tvb, 0, 0, response->response_frame_number);
5096 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
5097 |
5098 | /* Work out gap between frames (in ms) */
5099 | int seconds_between_packets = (int)
5100 | (response->response_frame_time.secs - pinfo->abs_ts.secs);
5101 | int nseconds_between_packets =
5102 | response->response_frame_time.nsecs - pinfo->abs_ts.nsecs;
5103 |
5104 | int total_gap = (seconds_between_packets*1000) +
5105 | ((nseconds_between_packets+500000) / 1000000);
5106 |
5107 | ti = proto_tree_add_uint(tree, hf_oran_acknack_response_time,
5108 | tvb, 0, 0, total_gap);
5109 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
5110 | }
5111 |
5112 |
5113 |
5114 | /* Control plane dissector (section 7). */
5115 | static int dissect_oran_c(tvbuff_t *tvb, packet_info *pinfo,
5116 | proto_tree *tree, oran_tap_info *tap_info, void *data _U___attribute__((unused)))
5117 | {
5118 | /* Hidden filter for plane */
5119 | proto_item *plane_ti = proto_tree_add_item(tree, hf_oran_cplane, tvb, 0, 0, ENC_NA0x00000000);
5120 | PROTO_ITEM_SET_HIDDEN(plane_ti)proto_item_set_hidden((plane_ti));
5121 |
5122 | /* Set up structures needed to add the protocol subtree and manage it */
5123 | unsigned offset = 0;
5124 |
5125 | col_set_str(pinfo->cinfo, COL_PROTOCOL, "O-RAN-FH-C");
5126 | col_set_str(pinfo->cinfo, COL_INFO, "C-Plane");
5127 |
5128 | tap_info->userplane = false0;
5129 |
5130 | /* Create display subtree for the protocol */
5131 | proto_item *protocol_item = proto_tree_add_item(tree, proto_oran, tvb, 0, -1, ENC_NA0x00000000);
5132 | proto_item_append_text(protocol_item, "-C");
5133 | proto_tree *oran_tree = proto_item_add_subtree(protocol_item, ett_oran);
5134 |
5135 | /* ecpriRtcid (eAxC ID) */
5136 | uint16_t eAxC;
5137 | addPcOrRtcid(tvb, oran_tree, &offset, hf_oran_ecpri_rtcid, &eAxC);
5138 | tap_info->eaxc = eAxC;
5139 |
5140 | /* Look up any existing conversation state for eAxC+plane */
5141 | uint32_t key = make_flow_key(pinfo, eAxC, ORAN_C_PLANE0, false0);
5142 | flow_state_t* state = (flow_state_t*)wmem_tree_lookup32(flow_states_table, key);
5143 |
5144 | /* Message identifier */
5145 | uint8_t seq_id;
5146 | proto_item *seq_id_ti;
5147 | offset = addSeqid(tvb, oran_tree, offset, ORAN_C_PLANE0, &seq_id, &seq_id_ti, pinfo);
5148 |
5149 | /* Section common subtree */
5150 | int section_tree_offset = offset;
5151 | proto_item *sectionHeading = proto_tree_add_string_format(oran_tree, hf_oran_c_section_common,
5152 | tvb, offset, 0, "", "C-Plane Section Type ");
5153 | proto_tree *section_tree = proto_item_add_subtree(sectionHeading, ett_oran_c_section_common);
5154 |
5155 | /* Peek ahead at the section type */
5156 | uint32_t sectionType = 0;
5157 | sectionType = tvb_get_uint8(tvb, offset+5);
5158 |
5159 | uint32_t scs = 0;
5160 | proto_item *scs_ti = NULL((void*)0);
5161 |
5162 | /* dataDirection */
5163 | uint32_t direction = 0;
5164 | proto_item *datadir_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_data_direction, tvb, offset, 1, ENC_NA0x00000000, &direction);
5165 | tap_info->uplink = (direction==0);
5166 |
5167 | /* Update/report status of conversation */
5168 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
5169 |
5170 | if (state == NULL((void*)0)) {
5171 | /* Allocate new state */
5172 | state = wmem_new0(wmem_file_scope(), flow_state_t)((flow_state_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_state_t )));
5173 | state->ack_nack_requests = wmem_tree_new(wmem_epan_scope());
5174 | wmem_tree_insert32(flow_states_table, key, state);
5175 | }
5176 |
5177 | /* Check sequence analysis status */
5178 | if (state->last_frame_seen[direction] && (seq_id != state->next_expected_sequence_number[direction])) {
5179 | /* Store this result */
5180 | flow_result_t *result = wmem_new0(wmem_file_scope(), flow_result_t)((flow_result_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_result_t )));
5181 | result->unexpected_seq_number = true1;
5182 | result->expected_sequence_number = state->next_expected_sequence_number[direction];
5183 | result->previous_frame = state->last_frame[direction];
5184 | wmem_tree_insert32(flow_results_table, pinfo->num, result);
5185 | }
5186 | /* Update conversation info */
5187 | state->last_frame[direction] = pinfo->num;
5188 | state->last_frame_seen[direction] = true1;
5189 | state->next_expected_sequence_number[direction] = (seq_id+1) % 256;
5190 | }
5191 |
5192 | /* Show any issues associated with this frame number */
5193 | flow_result_t *result = wmem_tree_lookup32(flow_results_table, pinfo->num);
5194 | if (result!=NULL((void*)0) && result->unexpected_seq_number) {
5195 | expert_add_info_format(pinfo, seq_id_ti,
5196 | (direction == DIR_UPLINK0) ?
5197 | &ei_oran_cplane_unexpected_sequence_number_ul :
5198 | &ei_oran_cplane_unexpected_sequence_number_dl,
5199 | "Sequence number %u expected, but got %u",
5200 | result->expected_sequence_number, seq_id);
5201 |
5202 | /* Update tap info */
5203 | uint32_t missing_sns = (256 + seq_id - result->expected_sequence_number) % 256;
5204 | /* Don't get confused by being slightly out of order.. */
5205 | if (missing_sns < 128) {
5206 | tap_info->missing_sns = missing_sns;
5207 | }
5208 | else {
5209 | tap_info->missing_sns = 0;
5210 | }
5211 |
5212 | /* TODO: could add previous/next frames (in seqId tree?) ? */
5213 | }
5214 |
5215 | /* payloadVersion */
5216 | dissect_payload_version(section_tree, tvb, pinfo, offset);
5217 |
5218 | /* filterIndex */
5219 | if (sectionType == SEC_C_SLOT_CONTROL || sectionType == SEC_C_ACK_NACK_FEEDBACK) {
5220 | /* scs (for ST4 and ST8) */
5221 | scs_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_frameStructure_subcarrier_spacing, tvb, offset, 1, ENC_NA0x00000000, &scs);
5222 | }
5223 | else if (sectionType == SEC_C_RRM_MEAS_REPORTS || sectionType == SEC_C_REQUEST_RRM_MEAS) {
5224 | /* reserved (4 bits) */
5225 | proto_tree_add_item(section_tree, hf_oran_reserved_last_4bits, tvb, offset, 1, ENC_NA0x00000000);
5226 | }
5227 | else if (sectionType != SEC_C_LAA) {
5228 | /* filterIndex (most common case) */
5229 | proto_tree_add_item(section_tree, hf_oran_filter_index, tvb, offset, 1, ENC_NA0x00000000);
5230 | }
5231 | offset += 1;
5232 |
5233 | unsigned ref_a_offset = offset;
5234 | /* frameId */
5235 | uint32_t frameId = 0;
5236 | proto_tree_add_item_ret_uint(section_tree, hf_oran_frame_id, tvb, offset, 1, ENC_NA0x00000000, &frameId);
5237 | tap_info->frame = frameId;
5238 | offset += 1;
5239 |
5240 | /* subframeId */
5241 | uint32_t subframeId = 0;
5242 | proto_tree_add_item_ret_uint(section_tree, hf_oran_subframe_id, tvb, offset, 1, ENC_NA0x00000000, &subframeId);
5243 | /* slotId */
5244 | uint32_t slotId = 0;
5245 | proto_tree_add_item_ret_uint(section_tree, hf_oran_slot_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &slotId);
5246 | tap_info->slot = slotId;
5247 | offset++;
5248 |
5249 | /* startSymbolId */
5250 | uint32_t startSymbolId = 0;
5251 | proto_item *ssid_ti = NULL((void*)0);
5252 | if ((sectionType == SEC_C_ACK_NACK_FEEDBACK) || /* Section Type 8 */
5253 | (sectionType == SEC_C_SINR_REPORTING)) { /* Section Type 9 */
5254 | /* symbolId */
5255 | proto_tree_add_item_ret_uint(section_tree, hf_oran_symbolId, tvb, offset, 1, ENC_NA0x00000000, &startSymbolId);
5256 | }
5257 | else if (sectionType != SEC_C_LAA) {
5258 | /* startSymbolId is in most section types */
5259 | ssid_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_start_symbol_id, tvb, offset, 1, ENC_NA0x00000000, &startSymbolId);
5260 | if (startSymbolId && (sectionType == SEC_C_RRM_MEAS_REPORTS)) { /* Section Type 10 */
5261 | proto_item_append_text(ssid_ti, " (should be 0 for ST10!)");
5262 | expert_add_info_format(pinfo, ssid_ti, &ei_oran_st10_startsymbolid_not_0,
5263 | "startSymbolId should be 0 for ST10 - found %u", startSymbolId);
5264 | }
5265 | }
5266 | else {
5267 | /* reserved (6 bits) */
5268 | proto_tree_add_item(section_tree, hf_oran_reserved_last_6bits, tvb, offset, 1, ENC_NA0x00000000);
5269 | }
5270 | offset++;
5271 |
5272 | char id[16];
5273 | snprintf(id, 16, "%d-%d-%d-%d", frameId, subframeId, slotId, startSymbolId);
5274 | proto_item *pi = proto_tree_add_string(section_tree, hf_oran_refa, tvb, ref_a_offset, 3, id);
5275 | proto_item_set_generated(pi);
5276 |
5277 | uint32_t cmd_scope = 0;
5278 | bool_Bool st8_ready = false0;
5279 |
5280 | /* numberOfSections (or whatever section has instead) */
5281 | uint32_t nSections = 0;
5282 | if (sectionType == SEC_C_SLOT_CONTROL) { /* Section Type 4 */
5283 | /* Slot Control has these fields instead */
5284 | /* reserved (4 bits) */
5285 | proto_tree_add_item(section_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
5286 | /* cmdScope (4 bits) */
5287 | proto_tree_add_item_ret_uint(section_tree, hf_oran_cmd_scope, tvb, offset, 1, ENC_NA0x00000000, &cmd_scope);
5288 | }
5289 | else if (sectionType == SEC_C_ACK_NACK_FEEDBACK) { /* Section Type 8 */
5290 | /* reserved (7 bits) */
5291 | proto_tree_add_item(section_tree, hf_oran_reserved_7bits, tvb, offset, 1, ENC_NA0x00000000);
5292 | /* ready (1 bit) */
5293 | /* TODO: when set, ready in slotId+1.. */
5294 | proto_tree_add_item_ret_boolean(section_tree, hf_oran_ready, tvb, offset, 1, ENC_NA0x00000000, &st8_ready);
5295 | if (!st8_ready) {
5296 | /* SCS value is ignored, and may be set to any value by O-RU */
5297 | proto_item_append_text(scs_ti, " (ignored)");
5298 | }
5299 | }
5300 | else if (sectionType != SEC_C_LAA) {
5301 | /* numberOfSections */
5302 | proto_tree_add_item_ret_uint(section_tree, hf_oran_numberOfSections, tvb, offset, 1, ENC_NA0x00000000, &nSections);
5303 | }
5304 | else {
5305 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
5306 | }
5307 | offset++;
5308 |
5309 | /* sectionType */
5310 | proto_tree_add_item_ret_uint(section_tree, hf_oran_sectionType, tvb, offset, 1, ENC_NA0x00000000, &sectionType);
5311 | offset += 1;
5312 |
5313 | /* Check that dataDirection is consistent with section type */
5314 | if (sectionType == SEC_C_SINR_REPORTING && direction != 0) { /* Section Type 9 */
5315 | expert_add_info(pinfo, datadir_ti, &ei_oran_st9_not_ul);
5316 | }
5317 | if (sectionType == SEC_C_RRM_MEAS_REPORTS && direction != 0) { /* Section Type 10 */
5318 | expert_add_info(pinfo, datadir_ti, &ei_oran_st10_not_ul);
5319 | }
5320 |
5321 | /* Note this section type in stats */
5322 | if (sectionType < SEC_C_MAX_INDEX) {
5323 | tap_info->section_types[sectionType] = true1;
5324 | }
5325 |
5326 | /* Section-type-specific fields following common header (white entries in Section Type diagrams) */
5327 | unsigned bit_width = 0;
5328 | int comp_meth = 0;
5329 | proto_item *comp_meth_ti;
5330 | unsigned ci_comp_method = 0;
5331 | uint8_t ci_comp_opt = 0;
5332 |
5333 | uint32_t num_ues = 0;
5334 | uint32_t number_of_acks = 0, number_of_nacks = 0;
5335 |
5336 | uint32_t num_sinr_per_prb = 0;
5337 |
5338 | switch (sectionType) {
5339 | case SEC_C_UNUSED_RB: /* Section Type 0 */
5340 | /* timeOffset */
5341 | proto_tree_add_item(section_tree, hf_oran_timeOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5342 | offset += 2;
5343 | /* frameStructure */
5344 | offset = dissect_frame_structure(section_tree, tvb, offset,
5345 | subframeId, slotId);
5346 |
5347 | /* cpLength */
5348 | proto_tree_add_item(section_tree, hf_oran_cpLength, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5349 | offset += 2;
5350 | /* reserved */
5351 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
5352 | offset += 1;
5353 | break;
5354 |
5355 | case SEC_C_NORMAL: /* Section Type 1 */
5356 | case SEC_C_UE_SCHED: /* Section Type 5 */
5357 | /* udCompHdr */
5358 | offset = dissect_udcomphdr(tvb, pinfo, section_tree, offset,
5359 | (direction==1), /* ignore for DL */
5360 | &bit_width, &comp_meth, &comp_meth_ti);
5361 | /* reserved */
5362 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
5363 | offset += 1;
5364 | break;
5365 |
5366 | case SEC_C_SLOT_CONTROL: /* Section Type 4 */
5367 | break;
5368 |
5369 | case SEC_C_PRACH: /* Section Type 3 */
5370 | /* timeOffset */
5371 | proto_tree_add_item(section_tree, hf_oran_timeOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5372 | offset += 2;
5373 | /* frameStructure */
5374 | offset = dissect_frame_structure(section_tree, tvb, offset,
5375 | subframeId, slotId);
5376 | /* cpLength */
5377 | proto_tree_add_item(section_tree, hf_oran_cpLength, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5378 | offset += 2;
5379 | /* udCompHdr */
5380 | offset = dissect_udcomphdr(tvb, pinfo, section_tree, offset,
5381 | (direction==1), /* ignore for DL */
5382 | &bit_width, &comp_meth, &comp_meth_ti);
5383 | break;
5384 |
5385 | case SEC_C_CH_INFO: /* Section Type 6 */
5386 | /* numberOfUEs */
5387 | proto_tree_add_item_ret_uint(section_tree, hf_oran_numberOfUEs, tvb, offset, 1, ENC_NA0x00000000, &num_ues);
5388 | offset += 1;
5389 | /* ciCompHdr (was reserved) */
5390 | offset = dissect_cicomphdr(tvb, pinfo, section_tree, offset, &bit_width, &ci_comp_method, &ci_comp_opt);
5391 |
5392 | /* Number of sections may not be filled in (at all, or correctly), so set to the number of UEs.
5393 | The data entries are per-UE... they don't have a sectionID, but they could have section extensions... */
5394 | if (nSections == 0 || num_ues > nSections) {
5395 | nSections = num_ues;
5396 | }
5397 | break;
5398 |
5399 | case SEC_C_RSVD2:
5400 | break;
5401 |
5402 | case SEC_C_LAA: /* Section Type 7 */
5403 | proto_tree_add_item(section_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5404 | offset += 2;
5405 | break;
5406 |
5407 | case SEC_C_ACK_NACK_FEEDBACK: /* Section Type 8 */
5408 | /* numberOfAcks (1 byte) */
5409 | proto_tree_add_item_ret_uint(section_tree, hf_oran_number_of_acks, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &number_of_acks);
5410 | offset += 1;
5411 | /* numberOfNacks (1 byte) */
5412 | proto_tree_add_item_ret_uint(section_tree, hf_oran_number_of_nacks, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &number_of_nacks);
5413 | offset += 1;
5414 |
5415 | /* Show ACKs and NACKs. For both, try to link back to request. */
5416 | for (unsigned int n=1; n <= number_of_acks; n++) {
5417 | uint32_t ackid;
5418 | proto_item *ack_ti;
5419 | ack_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_ackid, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ackid);
5420 | offset += 2;
5421 |
5422 | /* Look up request table in state (which really should be set by now, but test anyway). */
5423 | if (state && state->ack_nack_requests) {
5424 | ack_nack_request_t *request = wmem_tree_lookup32(state->ack_nack_requests, ackid);
5425 | if (request != NULL((void*)0)) {
5426 | /* On first pass, update with this response */
5427 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
5428 | request->response_frame_number = pinfo->num;
5429 | request->response_frame_time = pinfo->abs_ts;
5430 | }
5431 |
5432 | /* Show request details */
5433 | show_link_to_acknack_request(section_tree, tvb, pinfo, request);
5434 | }
5435 | else {
5436 | /* Request not found */
5437 | expert_add_info_format(pinfo, ack_ti, &ei_oran_acknack_no_request,
5438 | "Response for ackId=%u received, but no request found",
5439 | ackid);
5440 | }
5441 | }
5442 | }
5443 | for (unsigned int m=1; m <= number_of_nacks; m++) {
5444 | uint32_t nackid;
5445 | proto_item *nack_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_nackid, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &nackid);
5446 | offset += 2;
5447 |
5448 | expert_add_info_format(pinfo, nack_ti, &ei_oran_st8_nackid,
5449 | "Received Nack for ackNackId=%u",
5450 | nackid);
5451 |
5452 | /* Look up request table in state. */
5453 | if (state && state->ack_nack_requests) {
5454 | ack_nack_request_t *request = wmem_tree_lookup32(state->ack_nack_requests, nackid);
5455 | if (request) {
5456 | /* On first pass, update with this response */
5457 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
5458 | request->response_frame_number = pinfo->num;
5459 | request->response_frame_time = pinfo->abs_ts;
5460 | }
5461 |
5462 | /* Show request details */
5463 | show_link_to_acknack_request(section_tree, tvb, pinfo, request);
5464 | }
5465 | else {
5466 | /* Request not found */
5467 | expert_add_info_format(pinfo, nack_ti, &ei_oran_acknack_no_request,
5468 | "Response for nackId=%u received, but no request found",
5469 | nackid);
5470 | }
5471 | }
5472 | }
5473 | break;
5474 |
5475 | case SEC_C_SINR_REPORTING: /* Section Type 9 */
5476 | {
5477 | /* numSinrPerPrb (3 bits) */
5478 | proto_item *nspp_ti;
5479 | nspp_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_num_sinr_per_prb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_sinr_per_prb);
5480 | switch (num_sinr_per_prb) {
5481 | case 0:
5482 | num_sinr_per_prb = 1; break;
5483 | case 1:
5484 | num_sinr_per_prb = 2; break;
5485 | case 2:
5486 | num_sinr_per_prb = 3; break;
5487 | case 3:
5488 | num_sinr_per_prb = 4; break;
5489 | case 4:
5490 | num_sinr_per_prb = 6; break;
5491 | case 5:
5492 | num_sinr_per_prb = 12; break;
5493 |
5494 | default:
5495 | proto_item_append_text(nspp_ti, " (invalid)");
5496 | num_sinr_per_prb = 1;
5497 | expert_add_info_format(pinfo, nspp_ti, &ei_oran_num_sinr_per_prb_unknown,
5498 | "Invalid numSinrPerPrb value (%u)",
5499 | num_sinr_per_prb);
5500 | }
5501 |
5502 | /* reserved (13 bits) */
5503 | proto_tree_add_item(section_tree, hf_oran_reserved_last_5bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5504 | offset += 1;
5505 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5506 | offset += 1;
5507 | break;
5508 | }
5509 |
5510 | case SEC_C_RRM_MEAS_REPORTS: /* Section Type 10 */
5511 | case SEC_C_REQUEST_RRM_MEAS: /* Section Type 11 */
5512 | /* reserved (16 bits) */
5513 | proto_tree_add_item(section_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5514 | offset += 2;
5515 | break;
5516 | };
5517 |
5518 | /* Update udCompHdr details in state for UL U-Plane */
5519 | if (state && direction==0) {
5520 | switch (sectionType) {
5521 | case SEC_C_NORMAL: /* Section Type 1 */
5522 | case SEC_C_PRACH: /* Section Type 3 */
5523 | case SEC_C_UE_SCHED: /* Section Type 5 */
5524 | state->ul_ud_comp_hdr_set = true1;
5525 | state->ul_ud_comp_hdr_bit_width = bit_width;
5526 | state->ul_ud_comp_hdr_compression = comp_meth;
5527 | state->ul_ud_comp_hdr_frame = pinfo->num;
5528 | break;
5529 | default:
5530 | break;
5531 | }
5532 | }
5533 |
5534 |
5535 | proto_item_append_text(sectionHeading, "%d, %s, frameId: %d, subframeId: %d, slotId: %d, startSymbolId: %d",
5536 | sectionType, val_to_str_const(direction, data_direction_vals, "Unknown"),
5537 | frameId, subframeId, slotId, startSymbolId);
5538 | if (nSections) {
5539 | proto_item_append_text(sectionHeading, ", numberOfSections=%u", nSections);
5540 | }
5541 |
5542 | write_pdu_label_and_info(protocol_item, NULL((void*)0), pinfo, ", Type: %2d %s", sectionType,
5543 | rval_to_str_const(sectionType, section_types_short, "Unknown"));
5544 |
5545 | /* Set actual length of C-Plane section header */
5546 | proto_item_set_len(section_tree, offset - section_tree_offset);
5547 |
5548 | if (sectionType == SEC_C_ACK_NACK_FEEDBACK) {
5549 | write_pdu_label_and_info(oran_tree, section_tree, pinfo,
5550 | (st8_ready) ? " (Ready)" : " (ACK)");
5551 | }
5552 |
5553 |
5554 | /* Section type 4 doesn't have normal sections, so deal with here before normal sections */
5555 | if (sectionType == SEC_C_SLOT_CONTROL) {
5556 | /* numberOfST4Cmds */
5557 | uint32_t no_st4_cmds, st4_cmd_len, num_slots, ack_nack_req_id, st4_cmd_type;
5558 | proto_item *no_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_number_of_st4_cmds,
5559 | tvb, offset, 1, ENC_NA0x00000000, &no_st4_cmds);
5560 | if (no_st4_cmds == 0) {
5561 | expert_add_info_format(pinfo, no_ti, &ei_oran_st4_no_cmds,
5562 | "Not valid for ST4 to carry no commands");
5563 | }
5564 | offset += 1;
5565 |
5566 | /* reserved (1 byte) */
5567 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5568 | offset += 1;
5569 |
5570 | /* Loop over commands. Each has 8-byte common header, followed by cmd-specific payload */
5571 | proto_item *len_ti;
5572 | for (uint32_t n=0; n < no_st4_cmds; n++) {
5573 | /* Table 7.4.6-2: Section Type 4 Command common header format */
5574 | proto_item *hdr_ti = proto_tree_add_string_format(section_tree, hf_oran_st4_cmd_header,
5575 | tvb, offset, 8, "",
5576 | "Type 4 Command common header");
5577 | proto_tree *hdr_tree = proto_item_add_subtree(hdr_ti, ett_oran_st4_cmd_header);
5578 |
5579 | /* st4CmdType */
5580 | proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_type, tvb, offset, 1, ENC_NA0x00000000, &st4_cmd_type);
5581 | offset += 1;
5582 |
5583 | /* st4CmdLen */
5584 | len_ti = proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_len, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &st4_cmd_len);
5585 | if (st4_cmd_len == 0) {
5586 | /* Meaning of 0 not yet defined (v15.00) */
5587 | proto_item_append_text(len_ti, " (reserved)");
5588 | expert_add_info(pinfo, len_ti, &ei_oran_st4_zero_len_cmd);
5589 | }
5590 | else {
5591 | proto_item_append_text(len_ti, " (%u bytes)", st4_cmd_len*4);
5592 | }
5593 | offset += 2;
5594 |
5595 | /* numSlots */
5596 | proto_item *slots_ti = proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_num_slots, tvb, offset, 1, ENC_NA0x00000000, &num_slots);
5597 | if (num_slots == 0) {
5598 | proto_item_append_text(slots_ti, " (until changed)");
5599 | }
5600 | offset += 1;
5601 |
5602 | /* ackNackReqId */
5603 | proto_item *ack_nack_req_id_ti;
5604 | ack_nack_req_id_ti = proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_ack_nack_req_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ack_nack_req_id);
5605 | offset += 2;
5606 | if (ack_nack_req_id == 0) {
5607 | proto_item_append_text(ack_nack_req_id_ti, " (no Section type 8 response expected)");
5608 | }
5609 |
5610 | /* reserved (16 bits) */
5611 | proto_tree_add_item(hdr_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5612 | offset += 2;
5613 |
5614 | /* Set common header summary */
5615 | proto_item_append_text(hdr_ti, " (cmd=%s, len=%u, slots=%u, ackNackReqId=%u)",
5616 | rval_to_str_const(st4_cmd_type, st4_cmd_type_vals, "Unknown"),
5617 | st4_cmd_len, num_slots, ack_nack_req_id);
5618 |
5619 | col_append_fstr(pinfo->cinfo, COL_INFO, " (%s)",
5620 | rval_to_str_const(st4_cmd_type, st4_cmd_type_vals, "Unknown"));
5621 |
5622 |
5623 | /* Subtree for this command body */
5624 | proto_item *command_ti = proto_tree_add_string_format(section_tree, hf_oran_st4_cmd,
5625 | tvb, offset, 0, "",
5626 | "Type 4 Command (%s)", rval_to_str_const(st4_cmd_type, st4_cmd_type_vals, "Unknown"));
5627 | proto_tree *command_tree = proto_item_add_subtree(command_ti, ett_oran_st4_cmd);
5628 |
5629 | unsigned command_start_offset = offset;
5630 |
5631 | /* Check fields compatible with chosen command. */
5632 | if (st4_cmd_type==1) {
5633 | if (num_slots != 0) {
5634 | /* "the value of numSlots should be set to zero for this command type" */
5635 | expert_add_info_format(pinfo, slots_ti, &ei_oran_numslots_not_zero,
5636 | "numSlots should be zero for ST4 command 1 - found %u",
5637 | num_slots);
5638 | }
5639 | }
5640 |
5641 | if (st4_cmd_type==3 || st4_cmd_type==4) {
5642 | if (startSymbolId != 0) {
5643 | /* "expected reception window for the commands is the symbol zero reception window" */
5644 | expert_add_info_format(pinfo, ssid_ti, &ei_oran_start_symbol_id_not_zero,
5645 | "startSymbolId should be zero for ST4 commands 3&4 - found %u",
5646 | startSymbolId);
5647 | }
5648 | }
5649 |
5650 | /* Add format for this command */
5651 | switch (st4_cmd_type) {
5652 | case 1: /* TIME_DOMAIN_BEAM_CONFIG */
5653 | {
5654 | bool_Bool disable_tdbfns;
5655 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
5656 |
5657 | /* Hidden filter for bf */
5658 | proto_item *bf_ti = proto_tree_add_item(command_tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
5659 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
5660 |
5661 | /* reserved (2 bits) */
5662 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5663 | /* symbolMask (14 bits) */
5664 | uint32_t symbol_mask;
5665 | proto_item *symbol_mask_ti;
5666 | offset = dissect_symbolmask(tvb, command_tree, offset, &symbol_mask, &symbol_mask_ti);
5667 | /* Symbol bits before 'startSymbolId' in Section Type 4 common header should be set to 0 by O-DU and shall be ignored by O-RU */
5668 | /* lsb is symbol 0 */
5669 | for (unsigned s=0; s < 14; s++) {
5670 | if ((startSymbolId & (1 << s)) && (startSymbolId > s)) {
5671 | proto_item_append_text(symbol_mask_ti, " (startSymbolId is %u, so some lower symbol bits ignored!)", startSymbolId);
5672 | expert_add_info(pinfo, symbol_mask_ti, &ei_oran_start_symbol_id_bits_ignored);
5673 | break;
5674 | }
5675 | }
5676 |
5677 | /* disableTDBFNs (1 bit) */
5678 | proto_tree_add_item_ret_boolean(command_tree, hf_oran_disable_tdbfns, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disable_tdbfns);
5679 |
5680 | /* tdBeamNum (15 bits) */
5681 | proto_tree_add_item(command_tree, hf_oran_td_beam_num, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5682 | offset += 2;
5683 |
5684 | /* bfwCompHdr (2 subheaders - bfwIqWidth and bfwCompMeth)*/
5685 | offset = dissect_bfwCompHdr(tvb, command_tree, offset,
5686 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
5687 | /* reserved (3 bytes) */
5688 | proto_tree_add_bits_item(command_tree, hf_oran_reserved, tvb, offset*8, 24, ENC_BIG_ENDIAN0x00000000);
5689 | offset += 3;
5690 |
5691 | if (disable_tdbfns) {
5692 | /* No beamnum information to show so get out. */
5693 | break;
5694 | }
5695 |
5696 | /* Read beam entries until reach end of command length */
5697 | while ((offset - command_start_offset) < (st4_cmd_len * 4)) {
5698 |
5699 | /* disableTDBFWs (1 bit) */
5700 | bool_Bool disable_tdbfws;
5701 | proto_tree_add_item_ret_boolean(command_tree, hf_oran_disable_tdbfws, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disable_tdbfws);
5702 |
5703 | /* tdBeamNum (15 bits) */
5704 | proto_tree_add_item(command_tree, hf_oran_td_beam_num, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5705 | offset += 2;
5706 |
5707 | /* Showing BFWs? */
5708 | if (!disable_tdbfws) {
5709 |
5710 | /* bfwCompParam */
5711 | unsigned exponent = 0;
5712 | bool_Bool supported = false0;
5713 | unsigned num_trx_entries;
5714 | uint16_t *trx_entries;
5715 | offset = dissect_bfwCompParam(tvb, command_tree, pinfo, offset, comp_meth_ti,
5716 | &bfwcomphdr_comp_meth, &exponent, &supported,
5717 | &num_trx_entries, &trx_entries);
5718 |
5719 | /* Antenna count from preference */
5720 | unsigned num_trx = pref_num_bf_antennas;
5721 | int bit_offset = offset*8;
5722 |
5723 | for (unsigned trx=0; trx < num_trx; trx++) {
5724 | /* Create antenna subtree */
5725 | int bfw_offset = bit_offset / 8;
5726 | proto_item *bfw_ti = proto_tree_add_string_format(command_tree, hf_oran_bfw,
5727 | tvb, bfw_offset, 0, "", "TRX %3u: (", trx);
5728 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
5729 |
5730 | /* I value */
5731 | /* Get bits, and convert to float. */
5732 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
5733 | float value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent, (state) ? &state->mod_comp_params : NULL((void*)0), 0 /* RE */);
5734 | /* Add to tree. */
5735 | proto_tree_add_float(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8,
5736 | (bfwcomphdr_iq_width+7)/8, value);
5737 | bit_offset += bfwcomphdr_iq_width;
5738 | proto_item_append_text(bfw_ti, "I=%f ", value);
5739 |
5740 | /* Leave a gap between I and Q values */
5741 | proto_item_append_text(bfw_ti, " ");
5742 |
5743 | /* Q value */
5744 | /* Get bits, and convert to float. */
5745 | bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
5746 | value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent, (state) ? &state->mod_comp_params : NULL((void*)0), 0 /* RE */);
5747 | /* Add to tree. */
5748 | proto_tree_add_float(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8,
5749 | (bfwcomphdr_iq_width+7)/8, value);
5750 | bit_offset += bfwcomphdr_iq_width;
5751 | proto_item_append_text(bfw_ti, "Q=%f", value);
5752 |
5753 | proto_item_append_text(bfw_ti, ")");
5754 | proto_item_set_len(bfw_ti, (bit_offset+7)/8 - bfw_offset);
5755 | }
5756 | /* Need to round to next byte */
5757 | offset = (bit_offset+7)/8;
5758 | }
5759 | }
5760 | break;
5761 | }
5762 | case 2: /* TDD_CONFIG_PATTERN */
5763 | /* reserved (2 bits) */
5764 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5765 | /* dirPattern (14 bits) */
5766 | proto_tree_add_item(command_tree, hf_oran_dir_pattern, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5767 | offset += 2;
5768 |
5769 | /* reserved (2 bits) */
5770 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5771 | /* guardPattern (14 bits) */
5772 | proto_tree_add_item(command_tree, hf_oran_guard_pattern, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5773 | offset += 2;
5774 | break;
5775 |
5776 | case 3: /* TRX_CONTROL */
5777 | {
5778 | /* Only allowed cmdScope is ARRAY-COMMAND */
5779 | if (cmd_scope != 0) {
5780 | expert_add_info(pinfo, command_tree, &ei_oran_trx_control_cmd_scope);
5781 | }
5782 |
5783 | /* reserved (2 bits) */
5784 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5785 | /* log2MaskBits (4 bits) */
5786 | unsigned log2maskbits;
5787 | proto_tree_add_item_ret_uint(command_tree, hf_oran_log2maskbits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &log2maskbits);
5788 | /* sleepMode */
5789 | uint32_t sleep_mode;
5790 | proto_tree_add_item_ret_uint(command_tree, hf_oran_sleepmode_trx, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &sleep_mode);
5791 | offset += 1;
5792 |
5793 | /* reserved (4 bits) */
5794 | proto_tree_add_item(command_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5795 | /* numSlotsExt (20 bits) */
5796 | uint32_t num_slots_ext;
5797 | proto_item *num_slots_ext_ti = proto_tree_add_item_ret_uint(command_tree, hf_oran_num_slots_ext, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000, &num_slots_ext);
5798 | if (num_slots==0 && num_slots_ext==0) {
5799 | proto_item_append_text(num_slots_ext_ti, " (undefined sleep period)");
5800 | }
5801 | else {
5802 | /* Time should be rounded up according to SCS */
5803 | float total = (float)(num_slots + num_slots_ext);
5804 | /* From table 7.5.2.13-3 */
5805 | float slot_length_by_scs[16] = { 1000, 500, 250, 125, 62.5, 31.25,
5806 | 0, 0, 0, 0, 0, 0, /* reserved */
5807 | 1000, 1000, 1000, 1000 };
5808 | float slot_length = slot_length_by_scs[scs];
5809 | /* Only using valid SCS. TODO: is this test ok? */
5810 | if (slot_length != 0) {
5811 | /* Round up to next slot */
5812 | total = ((int)(total / slot_length) + 1) * slot_length;
5813 | proto_item_append_text(num_slots_ext_ti, " (defined sleep period of %f us)", total);
5814 | }
5815 | }
5816 | offset += 3;
5817 |
5818 | /* reserved (2 bits) */
5819 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5820 |
5821 | /* symbolMask (14 bits) */
5822 | uint32_t symbol_mask;
5823 | proto_item *sm_ti;
5824 | offset = dissect_symbolmask(tvb, command_tree, offset, &symbol_mask, &sm_ti);
5825 | if (symbol_mask == 0x0) {
5826 | proto_item_append_text(sm_ti, " (wake)");
5827 | col_append_str(pinfo->cinfo, COL_INFO, " (wake)");
5828 | }
5829 | else if (symbol_mask == 0x3fff) {
5830 | proto_item_append_text(sm_ti, " (sleep)");
5831 | col_append_str(pinfo->cinfo, COL_INFO, " (sleep)");
5832 | }
5833 | else {
5834 | expert_add_info_format(pinfo, sm_ti, &ei_oran_bad_symbolmask,
5835 | "For non-zero sleepMode (%u), symbolMask should be 0x0 or 0x3fff - found 0x%05x",
5836 | sleep_mode, symbol_mask);
5837 | }
5838 | offset += 2;
5839 |
5840 | /* antMask (16-2048 bits). Size is lookup from log2MaskBits enum.. */
5841 | unsigned antmask_length = 2;
5842 | if (log2maskbits >= 4) {
5843 | antmask_length = (1 << log2maskbits) / 8;
5844 | }
5845 | proto_item *ant_mask_ti = proto_tree_add_item(command_tree, hf_oran_antMask_trx_control, tvb, offset, antmask_length, ENC_NA0x00000000);
5846 | /* show count */
5847 | unsigned antenna_count = 0;
5848 | for (unsigned b=0; b < antmask_length; b++) {
5849 | uint8_t byte = tvb_get_uint8(tvb, offset+b);
5850 | for (unsigned bit=0; bit < 8; bit++) {
5851 | if ((1 << bit) & byte) {
5852 | antenna_count++;
5853 | }
5854 | }
5855 | }
5856 | proto_item_append_text(ant_mask_ti, " (%u antennas)", antenna_count);
5857 | offset += antmask_length;
5858 |
5859 | /* Pad to next 4-byte boundary */
5860 | offset = WS_ROUNDUP_4(offset)(((offset) + ((unsigned)(4U-1U))) & (~((unsigned)(4U-1U)) ));
5861 | break;
5862 | }
5863 |
5864 | case 4: /* ASM (advanced sleep mode) */
5865 | /* reserved (2+4=6 bits) */
5866 | proto_tree_add_item(command_tree, hf_oran_reserved_6bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5867 | /* sleepMode (2 bits) */
5868 | uint32_t sleep_mode;
5869 | proto_tree_add_item_ret_uint(command_tree, hf_oran_sleepmode_asm, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &sleep_mode);
5870 | offset += 1;
5871 |
5872 | /* reserved (4 bits) */
5873 | proto_tree_add_item(command_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5874 | /* numSlotsExt (20 bits) */
5875 | proto_tree_add_item(command_tree, hf_oran_num_slots_ext, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
5876 | offset += 3;
5877 |
5878 | /* reserved (2 bits) */
5879 | proto_tree_add_item(command_tree, hf_oran_reserved_2bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5880 | /* symbolMask (14 bits) */
5881 | uint32_t symbol_mask;
5882 | proto_item *sm_ti;
5883 | offset = dissect_symbolmask(tvb, command_tree, offset, &symbol_mask, &sm_ti);
5884 | if (symbol_mask == 0x0) {
5885 | proto_item_append_text(sm_ti, " (wake)");
5886 | col_append_str(pinfo->cinfo, COL_INFO, " (wake)");
5887 | }
5888 | else if (symbol_mask == 0x3fff) {
5889 | proto_item_append_text(sm_ti, " (sleep)");
5890 | col_append_str(pinfo->cinfo, COL_INFO, " (sleep)");
5891 | }
5892 | else {
5893 | expert_add_info_format(pinfo, sm_ti, &ei_oran_bad_symbolmask,
5894 | "For non-zero sleepMode (%u), symbolMask should be 0x0 or 0x3fff - found 0x%05x",
5895 | sleep_mode, symbol_mask);
5896 | }
5897 | offset += 2;
5898 |
5899 | /* reserved (2 bytes) */
5900 | proto_tree_add_item(command_tree, hf_oran_reserved_16bits, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5901 | offset += 2;
5902 | break;
5903 |
5904 | default:
5905 | /* Error! */
5906 | expert_add_info_format(pinfo, len_ti, &ei_oran_st4_unknown_cmd,
5907 | "Dissected ST4 command (%u) not recognised",
5908 | st4_cmd_type);
5909 | break;
5910 | }
5911 |
5912 | /* Check apparent size of padding (0-3 bytes ok) */
5913 | long padding_remaining = command_start_offset + (st4_cmd_len * 4) - offset;
5914 | if (padding_remaining < 0 || padding_remaining > 3) {
5915 | expert_add_info_format(pinfo, len_ti, &ei_oran_st4_wrong_len_cmd,
5916 | "Dissected ST4 command does not match signalled st4CmdLen - set to %u (%u bytes) but dissected %u bytes",
5917 | st4_cmd_len, st4_cmd_len*4, offset-command_start_offset);
5918 | }
5919 |
5920 | /* Advance by signalled length (needs to be aligned on 4-byte boundary) */
5921 | offset = command_start_offset + (st4_cmd_len * 4);
5922 |
5923 | /* Set end of command tree */
5924 | proto_item_set_end(command_ti, tvb, offset);
5925 |
5926 | if (ack_nack_req_id != 0 && state && state->ack_nack_requests) {
5927 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
5928 | /* Add this request into conversation state on first pass */
5929 | ack_nack_request_t *request_details = wmem_new0(wmem_file_scope(), ack_nack_request_t)((ack_nack_request_t*)wmem_alloc0((wmem_file_scope()), sizeof (ack_nack_request_t)));
5930 | request_details->request_frame_number = pinfo->num;
5931 | request_details->request_frame_time = pinfo->abs_ts;
5932 | request_details->requestType = ST4Cmd1+st4_cmd_type-1;
5933 |
5934 | wmem_tree_insert32(state->ack_nack_requests,
5935 | ack_nack_req_id,
5936 | request_details);
5937 | }
5938 | else {
5939 | /* On later passes, try to link forward to ST8 response */
5940 | ack_nack_request_t *response = wmem_tree_lookup32(state->ack_nack_requests,
5941 | ack_nack_req_id);
5942 | if (response) {
5943 | show_link_to_acknack_response(section_tree, tvb, pinfo, response);
5944 | }
5945 | }
5946 | }
5947 | }
5948 | }
5949 | /* LAA doesn't have sections either.. */
5950 | else if (sectionType == SEC_C_LAA) { /* Section Type 7 */
5951 | /* 7.2.5 Table 6.4-6 */
5952 | unsigned mcot;
5953 | proto_item *mcot_ti;
5954 |
5955 | /* laaMsgType */
5956 | uint32_t laa_msg_type;
5957 | proto_item *laa_msg_type_ti;
5958 | laa_msg_type_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_laaMsgType, tvb, offset, 1, ENC_NA0x00000000, &laa_msg_type);
5959 | /* laaMsgLen */
5960 | uint32_t laa_msg_len;
5961 | proto_item *len_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_laaMsgLen, tvb, offset, 1, ENC_NA0x00000000, &laa_msg_len);
5962 | proto_item_append_text(len_ti, " (%u bytes)", 4*laa_msg_len);
5963 | if (laa_msg_len == 0) {
5964 | proto_item_append_text(len_ti, " (reserved)");
5965 | }
5966 | offset += 1;
5967 |
5968 | int payload_offset = offset;
5969 |
5970 | /* Payload */
5971 | switch (laa_msg_type) {
5972 | case 0:
5973 | /* LBT_PDSCH_REQ */
5974 | /* lbtHandle (16 bits) */
5975 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5976 | offset += 2;
5977 | /* lbtOffset (10 bits) */
5978 | proto_tree_add_item(section_tree, hf_oran_lbtOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5979 | offset += 1;
5980 | /* lbtMode (2 bits) */
5981 | proto_tree_add_bits_item(section_tree, hf_oran_lbtMode, tvb, offset*8+2, 2, ENC_BIG_ENDIAN0x00000000);
5982 | /* reserved (1 bit) */
5983 | proto_tree_add_item(section_tree, hf_oran_reserved_bit4, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5984 | /* lbtDeferFactor (3 bits) */
5985 | proto_tree_add_item(section_tree, hf_oran_lbtDeferFactor, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5986 | offset += 1;
5987 | /* lbtBackoffCounter (10 bits) */
5988 | proto_tree_add_item(section_tree, hf_oran_lbtBackoffCounter, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5989 | offset += 1;
5990 | /* MCOT (4 bits) */
5991 | mcot_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_MCOT, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &mcot);
5992 | if (mcot<1 || mcot>10) {
5993 | proto_item_append_text(mcot_ti, " (should be in range 1-10!)");
5994 | expert_add_info_format(pinfo, mcot_ti, &ei_oran_mcot_out_of_range,
5995 | "MCOT seen with value %u (must be 1-10)", mcot);
5996 |
5997 | }
5998 | /* reserved (10 bits) */
5999 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8)+6, 10, ENC_BIG_ENDIAN0x00000000);
6000 | break;
6001 | case 1:
6002 | /* LBT_DRS_REQ */
6003 | /* lbtHandle (16 bits) */
6004 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6005 | offset += 2;
6006 | /* lbtOffset (10 bits) */
6007 | proto_tree_add_item(section_tree, hf_oran_lbtOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6008 | offset += 1;
6009 | /* lbtMode (2 bits) */
6010 | proto_tree_add_bits_item(section_tree, hf_oran_lbtMode, tvb, offset*8+2, 2, ENC_BIG_ENDIAN0x00000000);
6011 | /* reserved (28 bits) */
6012 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8)+4, 28, ENC_BIG_ENDIAN0x00000000);
6013 | break;
6014 | case 2:
6015 | /* LBT_PDSCH_RSP */
6016 | /* lbtHandle (16 bits) */
6017 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6018 | offset += 2;
6019 | /* lbtPdschRes (2 bits) */
6020 | proto_tree_add_item(section_tree, hf_oran_lbtPdschRes, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6021 | /* inParSF (1 bit) */
6022 | proto_tree_add_item(section_tree, hf_oran_initialPartialSF, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6023 | /* sfStatus (1 bit) */
6024 | proto_tree_add_item(section_tree, hf_oran_sfStatus, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6025 | /* sfnSf (12 bits) */
6026 | proto_tree_add_item(section_tree, hf_oran_sfnSfEnd, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6027 | offset += 2;
6028 | /* reserved (24 bits) */
6029 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8), 24, ENC_BIG_ENDIAN0x00000000);
6030 | break;
6031 | case 3:
6032 | /* LBT_DRS_RSP */
6033 | /* lbtHandle (16 bits) */
6034 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6035 | offset += 2;
6036 | /* lbtDrsRes (1 bit) */
6037 | proto_tree_add_item(section_tree, hf_oran_lbtDrsRes, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6038 | /* reserved (7 bits) */
6039 | proto_tree_add_item(section_tree, hf_oran_reserved_last_7bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6040 | break;
6041 | case 4:
6042 | /* LBT_Buffer_Error */
6043 | /* lbtHandle (16 bits) */
6044 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6045 | offset += 2;
6046 | /* lbtBufErr (1 bit) */
6047 | proto_tree_add_item(section_tree, hf_oran_lbtBufErr, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6048 | /* reserved (7 bits) */
6049 | proto_tree_add_item(section_tree, hf_oran_reserved_last_7bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6050 | break;
6051 | case 5:
6052 | /* LBT_CWCONFIG_REQ */
6053 | /* lbtHandle (16 bits) */
6054 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6055 | offset += 2;
6056 | /* lbtCWConfig_H (8 bits) */
6057 | proto_tree_add_item(section_tree, hf_oran_lbtCWConfig_H, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6058 | offset += 1;
6059 | /* lbtCWConfig_T (8 bits) */
6060 | proto_tree_add_item(section_tree, hf_oran_lbtCWConfig_T, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6061 | offset += 1;
6062 | /* lbtMode (2 bits) */
6063 | proto_tree_add_bits_item(section_tree, hf_oran_lbtMode, tvb, offset*8, 2, ENC_BIG_ENDIAN0x00000000);
6064 | /* lbtTrafficClass (3 bits) */
6065 | proto_tree_add_item(section_tree, hf_oran_lbtTrafficClass, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6066 | /* reserved (19 bits) */
6067 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8)+5, 19, ENC_BIG_ENDIAN0x00000000);
6068 | break;
6069 | case 6:
6070 | /* LBT_CWCONFIG_RSP */
6071 | /* lbtHandle (16 bits) */
6072 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6073 | offset += 2;
6074 | /* lbtCWR_Rst (1 bit) */
6075 | proto_tree_add_item(section_tree, hf_oran_lbtCWR_Rst, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6076 | /* reserved (7 bits) */
6077 | proto_tree_add_item(section_tree, hf_oran_reserved_last_7bits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6078 | break;
6079 |
6080 | default:
6081 | /* Unhandled! */
6082 | expert_add_info_format(pinfo, laa_msg_type_ti, &ei_oran_laa_msg_type_unsupported,
6083 | "laaMsgType %u not supported by dissector",
6084 | laa_msg_type);
6085 |
6086 | break;
6087 | }
6088 | /* For now just skip indicated length of bytes */
6089 | offset = payload_offset + 4*(laa_msg_len+1);
6090 | }
6091 |
6092 |
6093 | /* Dissect each C section */
6094 | for (uint32_t i = 0; i < nSections; ++i) {
6095 | tvbuff_t *section_tvb = tvb_new_subset_length_caplen(tvb, offset, -1, -1);
6096 | offset += dissect_oran_c_section(section_tvb, oran_tree, pinfo, state, sectionType, tap_info,
6097 | protocol_item,
6098 | subframeId, slotId,
6099 | bit_width, ci_comp_method, ci_comp_opt,
6100 | num_sinr_per_prb);
6101 | }
6102 |
6103 | /* Expert error if we are short of tvb by > 3 bytes */
6104 | if (tvb_reported_length_remaining(tvb, offset) > 3) {
6105 | expert_add_info_format(pinfo, protocol_item, &ei_oran_frame_length,
6106 | "%u bytes remain at end of frame - should be 0-3",
6107 | tvb_reported_length_remaining(tvb, offset));
6108 | }
6109 |
6110 | return tvb_captured_length(tvb);
6111 | }
6112 |
6113 | static int dissect_oran_u_re(tvbuff_t *tvb, proto_tree *tree,
6114 | unsigned sample_number, int samples_offset,
6115 | oran_tap_info *tap_info,
6116 | unsigned sample_bit_width,
6117 | int comp_meth,
6118 | uint32_t exponent,
6119 | mod_compr_params_t *mod_compr_params,
6120 | uint8_t re)
6121 | {
6122 | /* I */
6123 | unsigned i_bits = tvb_get_bits32(tvb, samples_offset, sample_bit_width, ENC_BIG_ENDIAN0x00000000);
6124 | float i_value = decompress_value(i_bits, comp_meth, sample_bit_width, exponent, mod_compr_params, re);
6125 | unsigned sample_len_in_bytes = ((samples_offset%8)+sample_bit_width+7)/8;
6126 | proto_item *i_ti = proto_tree_add_float(tree, hf_oran_iSample, tvb, samples_offset/8, sample_len_in_bytes, i_value);
6127 | proto_item_set_text(i_ti, "iSample: % 0.7f 0x%04x (RE-%2u in the PRB)", i_value, i_bits, sample_number);
6128 | samples_offset += sample_bit_width;
6129 | /* Q */
6130 | unsigned q_bits = tvb_get_bits32(tvb, samples_offset, sample_bit_width, ENC_BIG_ENDIAN0x00000000);
6131 | float q_value = decompress_value(q_bits, comp_meth, sample_bit_width, exponent, mod_compr_params, re);
6132 | sample_len_in_bytes = ((samples_offset%8)+sample_bit_width+7)/8;
6133 | proto_item *q_ti = proto_tree_add_float(tree, hf_oran_qSample, tvb, samples_offset/8, sample_len_in_bytes, q_value);
6134 | proto_item_set_text(q_ti, "qSample: % 0.7f 0x%04x (RE-%2u in the PRB)", q_value, q_bits, sample_number);
6135 | samples_offset += sample_bit_width;
6136 |
6137 | /* Update RE stats */
6138 | tap_info->num_res++;
6139 | /* if (i_value == 0.0 && q_value == 0.0) { */
6140 | /* TODO: is just checking bits from frame good enough - assuming this always corresponds to a zero value? */
6141 | if (i_bits == 0 && q_bits == 0) {
6142 | tap_info->num_res_zero++;
6143 | }
6144 | else {
6145 | tap_info->non_zero_re_in_current_prb = true1;
6146 | }
6147 | return samples_offset;
6148 | }
6149 |
6150 |
6151 | static bool_Bool udcomplen_appears_present(bool_Bool udcomphdr_present, tvbuff_t *tvb, int offset)
6152 | {
6153 | if (!udcomplen_heuristic_result_set) {
6154 | /* All sections will start the same way */
6155 | unsigned int section_bytes_before_field = (udcomphdr_present) ? 6 : 4;
6156 |
6157 | /* Move offset back to the start of the section */
6158 | offset -= section_bytes_before_field;
6159 |
6160 | do {
6161 | /* This field appears several bytes into the U-plane section */
6162 | uint32_t length_remaining = tvb_reported_length_remaining(tvb, offset);
6163 | /* Are there enough bytes to still read the length field? */
6164 | if (section_bytes_before_field+2 > length_remaining) {
6165 | udcomplen_heuristic_result = false0;
6166 | udcomplen_heuristic_result_set = true1;
6167 | break;
6168 | }
6169 |
6170 | /* Read the length field */
6171 | uint16_t udcomplen = tvb_get_ntohs(tvb, offset+section_bytes_before_field);
6172 |
6173 | /* Is this less than a valid section? Realistic minimal section will be bigger than this..
6174 | * Could take into account numPrbU, etc */
6175 | if (udcomplen < section_bytes_before_field+2) {
6176 | udcomplen_heuristic_result = false0;
6177 | udcomplen_heuristic_result_set = true1;
6178 | break;
6179 | }
6180 |
6181 | /* Does this section fit into the frame? */
6182 | if (udcomplen > length_remaining) {
6183 | udcomplen_heuristic_result = false0;
6184 | udcomplen_heuristic_result_set = true1;
6185 | break;
6186 | }
6187 |
6188 | /* Move past this section */
6189 | offset += udcomplen;
6190 |
6191 | /* Are we at the end of the frame? */
6192 | /* TODO: if frame is less than 60 bytes, there may be > 4 bytes, likely zeros.. */
6193 | if (tvb_reported_length_remaining(tvb, offset) < 4) {
6194 | udcomplen_heuristic_result = true1;
6195 | udcomplen_heuristic_result_set = true1;
6196 | }
6197 | } while (!udcomplen_heuristic_result_set);
6198 | }
6199 | return udcomplen_heuristic_result;
6200 | }
6201 |
6202 | static bool_Bool at_udcomphdr(tvbuff_t *tvb, int offset)
6203 | {
6204 | if (tvb_captured_length_remaining(tvb, offset) < 2) {
6205 | return false0;
6206 | }
6207 | uint8_t first_byte = tvb_get_uint8(tvb, offset);
6208 | uint8_t reserved_byte = tvb_get_uint8(tvb, offset+1);
6209 |
6210 | /* - iq width could be anything, though unlikely to be signalled as (say) < 1-3? */
6211 | /* - meth should be 0-8 */
6212 | /* - reserved byte should be 0 */
6213 | return (((first_byte & 0x0f) <= MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8) && (reserved_byte == 0));
6214 | }
6215 |
6216 | static bool_Bool udcomphdr_appears_present(flow_state_t *flow, uint32_t direction, tvbuff_t *tvb, int offset)
6217 | {
6218 | /* Should really not happen, but guard against this anyway. */
6219 | if (flow == NULL((void*)0)) {
6220 | /* No state to update. */
6221 | return false0;
6222 | }
6223 |
6224 | if (direction == DIR_UPLINK0) {
6225 | if (flow->udcomphdrUplink_heuristic_result_set) {
6226 | /* Return cached value */
6227 | return flow->udcomphdrUplink_heuristic_result;
6228 | }
6229 | else {
6230 | /* Work it out, and save answer for next time */
6231 | flow->udcomphdrUplink_heuristic_result_set = true1;
6232 | flow->udcomphdrUplink_heuristic_result = at_udcomphdr(tvb, offset);
6233 | return flow->udcomphdrUplink_heuristic_result;
6234 | }
6235 | }
6236 | else {
6237 | /* Downlink */
6238 | if (flow->udcomphdrDownlink_heuristic_result_set) {
6239 | /* Return cached value */
6240 | return flow->udcomphdrDownlink_heuristic_result;
6241 | }
6242 | else {
6243 | /* Work it out, and save answer for next time */
6244 | flow->udcomphdrDownlink_heuristic_result_set = true1;
6245 | flow->udcomphdrDownlink_heuristic_result = at_udcomphdr(tvb, offset);
6246 | return flow->udcomphdrDownlink_heuristic_result;
6247 | }
6248 | }
6249 | }
6250 |
6251 | /* User plane dissector (section 8) */
6252 | static int
6253 | dissect_oran_u(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree,
6254 | oran_tap_info *tap_info, void *data _U___attribute__((unused)))
6255 | {
6256 | /* Hidden filter for plane */
6257 | proto_item *plane_ti = proto_tree_add_item(tree, hf_oran_uplane, tvb, 0, 0, ENC_NA0x00000000);
6258 | PROTO_ITEM_SET_HIDDEN(plane_ti)proto_item_set_hidden((plane_ti));
6259 |
6260 | /* Set up structures needed to add the protocol subtree and manage it */
6261 | int offset = 0;
6262 |
6263 | col_set_str(pinfo->cinfo, COL_PROTOCOL, "O-RAN-FH-U");
6264 | col_set_str(pinfo->cinfo, COL_INFO, "U-Plane");
6265 |
6266 | tap_info->userplane = true1;
6267 |
6268 | /* Create display subtree for the protocol */
6269 | proto_item *protocol_item = proto_tree_add_item(tree, proto_oran, tvb, 0, -1, ENC_NA0x00000000);
6270 | proto_item_append_text(protocol_item, "-U");
6271 | proto_tree *oran_tree = proto_item_add_subtree(protocol_item, ett_oran);
6272 |
6273 | /* Transport header */
6274 | /* Real-time control data / IQ data transfer message series identifier */
6275 | uint16_t eAxC;
6276 | addPcOrRtcid(tvb, oran_tree, &offset, hf_oran_ecpri_pcid, &eAxC);
6277 | tap_info->eaxc = eAxC;
6278 |
6279 | /* Update/report status of conversation */
6280 | uint32_t key = make_flow_key(pinfo, eAxC, ORAN_U_PLANE1, false0);
6281 | flow_state_t* state = (flow_state_t*)wmem_tree_lookup32(flow_states_table, key);
6282 |
6283 | /* Message identifier */
6284 | uint8_t seq_id;
6285 | proto_item *seq_id_ti;
6286 | offset = addSeqid(tvb, oran_tree, offset, ORAN_U_PLANE1, &seq_id, &seq_id_ti, pinfo);
6287 |
6288 | /* Common header for time reference */
6289 | proto_item *timingHeader = proto_tree_add_string_format(oran_tree, hf_oran_timing_header,
6290 | tvb, offset, 4, "", "Timing Header (");
6291 | proto_tree *timing_header_tree = proto_item_add_subtree(timingHeader, ett_oran_u_timing);
6292 |
6293 | /* dataDirection */
6294 | uint32_t direction;
6295 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_data_direction, tvb, offset, 1, ENC_NA0x00000000, &direction);
6296 | tap_info->uplink = (direction==0);
6297 | /* payloadVersion */
6298 | dissect_payload_version(timing_header_tree, tvb, pinfo, offset);
6299 | /* filterIndex */
6300 | proto_tree_add_item(timing_header_tree, hf_oran_filter_index, tvb, offset, 1, ENC_NA0x00000000);
6301 | offset += 1;
6302 |
6303 | int ref_a_offset = offset;
6304 |
6305 | /* frameId */
6306 | uint32_t frameId = 0;
6307 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_frame_id, tvb, offset, 1, ENC_NA0x00000000, &frameId);
6308 | tap_info->frame = frameId;
6309 | offset += 1;
6310 |
6311 | /* subframeId */
6312 | uint32_t subframeId = 0;
6313 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_subframe_id, tvb, offset, 1, ENC_NA0x00000000, &subframeId);
6314 | /* slotId */
6315 | uint32_t slotId = 0;
6316 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_slot_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &slotId);
6317 | tap_info->slot = slotId;
6318 | offset++;
6319 | /* symbolId */
6320 | uint32_t symbolId = 0;
6321 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_symbolId, tvb, offset, 1, ENC_NA0x00000000, &symbolId);
6322 | offset++;
6323 |
6324 | char id[16];
6325 | snprintf(id, 16, "%d-%d-%d-%d", frameId, subframeId, slotId, symbolId);
6326 | proto_item *pi = proto_tree_add_string(timing_header_tree, hf_oran_refa, tvb, ref_a_offset, 3, id);
6327 | proto_item_set_generated(pi);
6328 |
6329 | proto_item_append_text(timingHeader, "%s, frameId: %d, subframeId: %d, slotId: %d, symbolId: %d)",
6330 | val_to_str_const(direction, data_direction_vals, "Unknown"), frameId, subframeId, slotId, symbolId);
6331 |
6332 | unsigned sample_bit_width;
6333 | int compression;
6334 | int includeUdCompHeader;
6335 |
6336 | /* Also look up C-PLANE state (sent in opposite direction) so may check current compression settings */
6337 | uint32_t cplane_key = make_flow_key(pinfo, eAxC, ORAN_C_PLANE0, true1);
6338 | flow_state_t* cplane_state = (flow_state_t*)wmem_tree_lookup32(flow_states_table, cplane_key);
6339 |
6340 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
6341 | /* Create conversation if doesn't exist yet */
6342 | if (!state) {
6343 | /* Allocate new state */
6344 | state = wmem_new0(wmem_file_scope(), flow_state_t)((flow_state_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_state_t )));
6345 | state->ack_nack_requests = wmem_tree_new(wmem_epan_scope());
6346 | wmem_tree_insert32(flow_states_table, key, state);
6347 | }
6348 |
6349 | /* Check sequence analysis status */
6350 | if (state->last_frame_seen[direction] && (seq_id != state->next_expected_sequence_number[direction])) {
6351 | /* Store this result */
6352 | flow_result_t *result = wmem_new0(wmem_file_scope(), flow_result_t)((flow_result_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_result_t )));
6353 | result->unexpected_seq_number = true1;
6354 | result->expected_sequence_number = state->next_expected_sequence_number[direction];
6355 | result->previous_frame = state->last_frame[direction];
6356 | wmem_tree_insert32(flow_results_table, pinfo->num, result);
6357 | }
6358 | /* Update sequence analysis state */
6359 | state->last_frame[direction] = pinfo->num;
6360 | state->last_frame_seen[direction] = true1;
6361 | state->next_expected_sequence_number[direction] = (seq_id+1) % 256;
6362 | }
6363 |
6364 | /* Show any issues associated with this frame number */
6365 | flow_result_t *result = wmem_tree_lookup32(flow_results_table, pinfo->num);
6366 | if (result) {
6367 | if (result->unexpected_seq_number) {
6368 | expert_add_info_format(pinfo, seq_id_ti,
6369 | (direction == DIR_UPLINK0) ?
6370 | &ei_oran_uplane_unexpected_sequence_number_ul :
6371 | &ei_oran_uplane_unexpected_sequence_number_dl,
6372 | "Sequence number %u expected, but got %u",
6373 | result->expected_sequence_number, seq_id);
6374 | tap_info->missing_sns = (256 + seq_id - result->expected_sequence_number) % 256;
6375 | /* TODO: could add previous/next frame (in seqId tree?) ? */
6376 | }
6377 | }
6378 |
6379 | /* Checking UL timing within current slot. Disabled if limit set to 0. */
6380 | /* N.B., timing is relative to first seen frame,
6381 | not some notion of the beginning of the slot from sync, offset by some timing.. */
6382 | if (direction == DIR_UPLINK0 && us_allowed_for_ul_in_symbol > 0) {
6383 | uint32_t timing_key = get_timing_key(frameId, subframeId, slotId, symbolId);
6384 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
6385 | /* Set state on first pass */
6386 | ul_timing_for_slot* timing = (ul_timing_for_slot*)wmem_tree_lookup32(ul_symbol_timing, timing_key);
6387 | if (!timing) {
6388 | /* Allocate new state */
6389 | timing = wmem_new0(wmem_file_scope(), ul_timing_for_slot)((ul_timing_for_slot*)wmem_alloc0((wmem_file_scope()), sizeof (ul_timing_for_slot)));
6390 | timing->first_frame = pinfo->num;
6391 | timing->first_frame_time = pinfo->abs_ts;
6392 | timing->frames_seen_in_symbol = 1;
6393 | timing->last_frame_in_symbol = pinfo->num;
6394 | wmem_tree_insert32(ul_symbol_timing, timing_key, timing);
6395 | }
6396 | else {
6397 | /* Update existing state */
6398 | timing->frames_seen_in_symbol++;
6399 | timing->last_frame_in_symbol = pinfo->num;
6400 | }
6401 | }
6402 | else {
6403 | /* Subsequent passes - look up result */
6404 | ul_timing_for_slot* timing = (ul_timing_for_slot*)wmem_tree_lookup32(ul_symbol_timing, timing_key);
6405 | if (timing) { /* Really shouldn't fail! */
6406 | if (timing->frames_seen_in_symbol > 1) {
6407 | /* Work out gap between frames (in microseconds) back to frame carrying first seen symbol */
6408 | int seconds_between_packets = (int)
6409 | (pinfo->abs_ts.secs - timing->first_frame_time.secs);
6410 | int nseconds_between_packets =
6411 | pinfo->abs_ts.nsecs - timing->first_frame_time.nsecs;
6412 |
6413 |
6414 | /* Round to nearest microsecond. */
6415 | uint32_t total_gap = (seconds_between_packets*1000000) +
6416 | ((nseconds_between_packets+500) / 1000);
6417 |
6418 | /* Show how long it has been */
6419 | proto_item *ti = NULL((void*)0);
6420 | if (pinfo->num != timing->first_frame) {
6421 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_time, tvb, 0, 0, total_gap);
6422 | proto_item_set_generated(ti);
6423 | }
6424 |
6425 | if (total_gap > us_allowed_for_ul_in_symbol) {
6426 | expert_add_info_format(pinfo, ti, &ei_oran_ul_uplane_symbol_too_long,
6427 | "UL U-Plane Tx took longer (%u us) than limit set in preferences (%u us)",
6428 | total_gap, us_allowed_for_ul_in_symbol);
6429 | }
6430 |
6431 | /* Show how many frames were received */
6432 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_frames, tvb, 0, 0, timing->frames_seen_in_symbol);
6433 | proto_item_set_generated(ti);
6434 |
6435 | /* Link to first frame for this symbol */
6436 | if (pinfo->num != timing->first_frame) {
6437 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_first_frame, tvb, 0, 0, timing->first_frame);
6438 | proto_item_set_generated(ti);
6439 | }
6440 |
6441 | /* And also last frame */
6442 | if (pinfo->num != timing->last_frame_in_symbol) {
6443 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_last_frame, tvb, 0, 0, timing->last_frame_in_symbol);
6444 | proto_item_set_generated(ti);
6445 | }
6446 |
6447 | tap_info->ul_delay_in_us = total_gap;
6448 | }
6449 | }
6450 | }
6451 | }
6452 |
6453 |
6454 | /* Look up preferences for samples */
6455 | if (direction == DIR_UPLINK0) {
6456 | sample_bit_width = pref_sample_bit_width_uplink;
6457 | compression = pref_iqCompressionUplink;
6458 | includeUdCompHeader = pref_includeUdCompHeaderUplink;
6459 | } else {
6460 | sample_bit_width = pref_sample_bit_width_downlink;
6461 | compression = pref_iqCompressionDownlink;
6462 | includeUdCompHeader = pref_includeUdCompHeaderDownlink;
6463 | }
6464 |
6465 | /* If uplink, load any udCompHdr settings written by C-Plane */
6466 | bool_Bool ud_cmp_hdr_cplane = false0;
6467 | if (cplane_state && direction == 0) {
6468 | /* Initialise settings from udpCompHdr from C-Plane */
6469 | if (cplane_state->ul_ud_comp_hdr_set) {
6470 | sample_bit_width = cplane_state->ul_ud_comp_hdr_bit_width;
6471 | compression = cplane_state->ul_ud_comp_hdr_compression;
6472 | ud_cmp_hdr_cplane = true1;
6473 | }
6474 | }
6475 |
6476 | /* Need a valid value (e.g. 9, 14). 0 definitely won't work, as won't progress around loop! */
6477 | /* N.B. may yet be overwritten by udCompHdr settings in sections below! */
6478 | if (sample_bit_width == 0) {
6479 | expert_add_info_format(pinfo, protocol_item, &ei_oran_invalid_sample_bit_width,
6480 | "%cL Sample bit width from %s (%u) not valid, so can't decode sections",
6481 | (direction == DIR_UPLINK0) ? 'U' : 'D',
6482 | !ud_cmp_hdr_cplane ? "preference" : "C-Plane",
6483 | sample_bit_width);
6484 | return offset;
6485 | }
6486 |
6487 | unsigned bytesLeft;
6488 | unsigned number_of_sections = 0;
6489 | unsigned nBytesPerPrb =0;
6490 |
6491 | /* Add each section (not from count, just keep parsing until payload used) */
6492 | do {
6493 | /* Section subtree */
6494 | unsigned section_start_offset = offset;
6495 | proto_item *sectionHeading = proto_tree_add_string_format(oran_tree, hf_oran_u_section,
6496 | tvb, offset, 0, "", "Section");
6497 | proto_tree *section_tree = proto_item_add_subtree(sectionHeading, ett_oran_u_section);
6498 |
6499 | /* Section Header fields (darker green part) */
6500 |
6501 | /* sectionId */
6502 | uint32_t sectionId = 0;
6503 | proto_item *ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_section_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &sectionId);
6504 | if (sectionId == 4095) {
6505 | proto_item_append_text(ti, " (not default coupling C/U planes using sectionId)");
6506 | }
6507 | offset++;
6508 |
6509 | if (tap_info->num_section_ids < MAX_SECTION_IDs32) {
6510 | tap_info->section_ids[tap_info->num_section_ids++] = sectionId;
6511 | }
6512 |
6513 | /* rb */
6514 | uint32_t rb;
6515 | proto_tree_add_item_ret_uint(section_tree, hf_oran_rb, tvb, offset, 1, ENC_NA0x00000000, &rb);
6516 | /* symInc */
6517 | proto_tree_add_item(section_tree, hf_oran_symInc, tvb, offset, 1, ENC_NA0x00000000);
6518 | /* startPrbu */
6519 | uint32_t startPrbu = 0;
6520 | proto_tree_add_item_ret_uint(section_tree, hf_oran_startPrbu, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbu);
6521 | offset += 2;
6522 |
6523 | /* numPrbu */
6524 | uint32_t numPrbu = 0;
6525 | proto_tree_add_item_ret_uint(section_tree, hf_oran_numPrbu, tvb, offset, 1, ENC_NA0x00000000, &numPrbu);
6526 | offset += 1;
6527 |
6528 | proto_item *ud_comp_meth_item, *ud_comp_len_ti=NULL((void*)0);
6529 | uint32_t ud_comp_len;
6530 |
6531 | /* udCompHdr (if preferences indicate will be present) */
6532 | bool_Bool included = (includeUdCompHeader==1) || /* 1 means present.. */
6533 | (includeUdCompHeader==2 && udcomphdr_appears_present(state, direction, tvb, offset));
6534 | if (included) {
6535 | /* 7.5.2.10 */
6536 | /* Extract these values to inform how wide IQ samples in each PRB will be. */
6537 | offset = dissect_udcomphdr(tvb, pinfo, section_tree, offset, false0, &sample_bit_width,
6538 | &compression, &ud_comp_meth_item);
6539 |
6540 | /* Not part of udCompHdr */
6541 | proto_tree_add_item(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000);
6542 | offset += 1;
6543 | }
6544 | else {
6545 | /* No fields to dissect - just showing comp values from prefs */
6546 | /* iqWidth */
6547 | proto_item *iq_width_item = proto_tree_add_uint(section_tree, hf_oran_udCompHdrIqWidth_pref, tvb, 0, 0, sample_bit_width);
6548 | proto_item_append_text(iq_width_item, (ud_cmp_hdr_cplane) ? " (from c-plane)" : " (from preferences)");
6549 | proto_item_set_generated(iq_width_item);
6550 |
6551 | /* udCompMethod */
6552 | ud_comp_meth_item = proto_tree_add_uint(section_tree, hf_oran_udCompHdrMeth_pref, tvb, 0, 0, compression);
6553 | proto_item_append_text(ud_comp_meth_item, (ud_cmp_hdr_cplane) ? " (from c-plane)" : " (from preferences)");
6554 | proto_item_set_generated(ud_comp_meth_item);
6555 |
6556 | /* Point back to C-Plane, if used */
6557 | /* TODO: doesn't work with multiple port mappings using SE10.. */
6558 | if (ud_cmp_hdr_cplane) {
6559 | proto_item *cplane_ti = proto_tree_add_uint(section_tree, hf_oran_ul_cplane_ud_comp_hdr_frame, tvb, offset, 0, cplane_state->ul_ud_comp_hdr_frame);
6560 | proto_item_set_generated(cplane_ti);
6561 | }
6562 | }
6563 |
6564 | /* Not supported! TODO: other places where comp method is looked up (e.g., bfw?) */
6565 | switch (compression) {
6566 | case COMP_NONE0:
6567 | case COMP_BLOCK_FP1:
6568 | case BFP_AND_SELECTIVE_RE5:
6569 | break;
6570 | default:
6571 | expert_add_info_format(pinfo, ud_comp_meth_item, &ei_oran_unsupported_compression_method,
6572 | "Compression method %u (%s) not supported by dissector",
6573 | compression,
6574 | rval_to_str_const(compression, ud_comp_header_meth, "reserved"));
6575 | }
6576 |
6577 | /* udCompLen (when supported, methods 5,6,7,8) */
6578 | if (compression >= BFP_AND_SELECTIVE_RE5) {
6579 | bool_Bool supported = (pref_support_udcompLen==1) || /* supported */
6580 | (pref_support_udcompLen==2 && udcomplen_appears_present(includeUdCompHeader, tvb, offset));
6581 |
6582 | if (supported) {
6583 | ud_comp_len_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_udCompLen, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ud_comp_len);
6584 | if (ud_comp_len <= 1) {
6585 | proto_item_append_text(ud_comp_len_ti, " (reserved)");
6586 | }
6587 | /* TODO: report if less than a viable section in frame? */
6588 | /* Check that there is this much length left in the frame */
6589 | if ((int)ud_comp_len > tvb_reported_length_remaining(tvb, section_start_offset)) {
6590 | expert_add_info_format(pinfo, ud_comp_len_ti, &ei_oran_ud_comp_len_wrong_size,
6591 | "udCompLen indicates %u bytes in section, but only %u are left in frame",
6592 | ud_comp_len, tvb_reported_length_remaining(tvb, section_start_offset));
6593 | }
6594 | /* Actual length of section will be checked below, at the end of the section */
6595 | offset += 2;
6596 | }
6597 | }
6598 |
6599 | /* sReSMask1 + sReSMask2 (depends upon compression method) */
6600 | uint64_t sresmask1=0, sresmask2=0;
6601 | if (compression == BFP_AND_SELECTIVE_RE_WITH_MASKS7 ||
6602 | compression == MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8)
6603 | {
6604 | static int * const sres_mask1_2_flags[] = {
6605 | &hf_oran_sReSMask1_2_re12,
6606 | &hf_oran_sReSMask1_2_re11,
6607 | &hf_oran_sReSMask1_2_re10,
6608 | &hf_oran_sReSMask1_2_re9,
6609 | &hf_oran_sReSMask_re8,
6610 | &hf_oran_sReSMask_re7,
6611 | &hf_oran_sReSMask_re6,
6612 | &hf_oran_sReSMask_re5,
6613 | &hf_oran_sReSMask_re4,
6614 | &hf_oran_sReSMask_re3,
6615 | &hf_oran_sReSMask_re2,
6616 | &hf_oran_sReSMask_re1,
6617 | NULL((void*)0)
6618 | };
6619 |
6620 | /* reserved (4 bits) */
6621 | proto_tree_add_item(section_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
6622 | /* sReSMask1 (12 bits) */
6623 | proto_item *sresmask_ti;
6624 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(section_tree, tvb, offset,
6625 | hf_oran_sReSMask1,
6626 | ett_oran_sresmask,
6627 | sres_mask1_2_flags,
6628 | ENC_NA0x00000000,
6629 | &sresmask1);
6630 | offset += 2;
6631 | /* Count REs present */
6632 | unsigned res = 0;
6633 | for (unsigned n=0; n < 12; n++) {
6634 | if ((sresmask1 >> n) & 0x1) {
6635 | res++;
6636 | }
6637 | }
6638 | proto_item_append_text(sresmask_ti, " (%u REs)", res);
6639 |
6640 |
6641 | /* reserved (4 bits) */
6642 | proto_tree_add_item(section_tree, hf_oran_reserved_4bits, tvb, offset, 1, ENC_NA0x00000000);
6643 | /* sReSMask2 (12 bits) */
6644 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(section_tree, tvb, offset,
6645 | hf_oran_sReSMask2,
6646 | ett_oran_sresmask,
6647 | sres_mask1_2_flags,
6648 | ENC_NA0x00000000,
6649 | &sresmask2);
6650 | offset += 2;
6651 |
6652 | if (rb == 1) {
6653 | proto_item_append_text(sresmask_ti, " (ignored)");
6654 | if (sresmask2 != 0) {
6655 | expert_add_info(pinfo, ud_comp_len_ti, &ei_oran_sresmask2_not_zero_with_rb);
6656 | }
6657 | }
6658 | else {
6659 | /* Count REs present */
6660 | res = 0;
6661 | for (unsigned n=0; n < 12; n++) {
6662 | if ((sresmask2 >> n) & 0x1) {
6663 | res++;
6664 | }
6665 | }
6666 | proto_item_append_text(sresmask_ti, " (%u REs)", res);
6667 | }
6668 | }
6669 |
6670 | write_section_info(sectionHeading, pinfo, protocol_item, sectionId, startPrbu, numPrbu, rb);
6671 |
6672 | /* TODO: should this use the same pref as c-plane? */
6673 | if (numPrbu == 0) {
6674 | /* Special case for all PRBs (NR: the total number of PRBs may be > 255) */
6675 | numPrbu = pref_data_plane_section_total_rbs;
6676 | startPrbu = 0; /* may already be 0... */
6677 | }
6678 |
6679 | /* Add each PRB */
6680 | for (unsigned i = 0; i < numPrbu; i++) {
6681 | /* Create subtree */
6682 | proto_item *prbHeading = proto_tree_add_string_format(section_tree, hf_oran_samples_prb,
6683 | tvb, offset, 0,
6684 | "", "PRB");
6685 | proto_tree *rb_tree = proto_item_add_subtree(prbHeading, ett_oran_u_prb);
6686 | uint32_t exponent = 0;
6687 | uint16_t sresmask = 0;
6688 |
6689 | /* udCompParam (depends upon compression method) */
6690 | int before = offset;
6691 | offset = dissect_udcompparam(tvb, pinfo, rb_tree, offset, compression, &exponent, &sresmask, false0);
6692 | int udcompparam_len = offset-before;
6693 |
6694 | /* Show PRB number in root */
6695 | proto_item_append_text(prbHeading, " %3u", startPrbu + i*(1+rb));
6696 |
6697 | /* Work out how many REs / PRB */
6698 | unsigned res_per_prb = 12;
6699 | uint16_t sresmask_to_use = 0x0fff;
6700 |
6701 | if (compression >= BFP_AND_SELECTIVE_RE5) {
6702 | /* Work out which mask should be used */
6703 | if (compression==BFP_AND_SELECTIVE_RE5 || compression==MOD_COMPR_AND_SELECTIVE_RE6) {
6704 | /* Selective RE cases, use value from compModParam */
6705 | sresmask_to_use = (uint16_t)sresmask;
6706 | }
6707 | else {
6708 | /* With masks (in section). Choose between sresmask1 and sresmask2 */
6709 | if (rb==1 || (i%1)==0) {
6710 | /* Even values */
6711 | sresmask_to_use = (uint16_t)sresmask1;
6712 | }
6713 | else {
6714 | /* Odd values */
6715 | sresmask_to_use = (uint16_t)sresmask2;
6716 | }
6717 | }
6718 |
6719 | /* Count REs present using sresmask */
6720 | res_per_prb = 0;
6721 | /* Use sresmask to pick out which REs are present */
6722 | for (unsigned n=0; n<12; n++) {
6723 | if (sresmask_to_use & (1<<n)) {
6724 | res_per_prb++;
6725 | }
6726 | }
6727 | }
6728 |
6729 | /* N.B. bytes for samples need to be padded out to next byte
6730 | (certainly where there aren't 12 REs in PRB..) */
6731 | unsigned nBytesForSamples = (sample_bit_width * res_per_prb * 2 + 7) / 8;
6732 | nBytesPerPrb = nBytesForSamples + udcompparam_len;
6733 |
6734 | proto_tree_add_item(rb_tree, hf_oran_iq_user_data, tvb, offset, nBytesForSamples, ENC_NA0x00000000);
6735 |
6736 | tap_info->non_zero_re_in_current_prb = false0;
6737 |
6738 | /* Optionally trying to show I/Q RE values */
6739 | if (pref_showIQSampleValues) {
6740 | /* Individual values */
6741 | unsigned samples_offset = offset*8;
6742 | unsigned samples = 0;
6743 |
6744 | if (compression >= BFP_AND_SELECTIVE_RE5) {
6745 | /* Use sresmask to pick out which REs are present */
6746 | for (unsigned n=1; n<=12; n++) {
6747 | if (sresmask_to_use & (1<<(n-1))) {
6748 | samples_offset = dissect_oran_u_re(tvb, rb_tree,
6749 | n, samples_offset, tap_info, sample_bit_width, compression, exponent, &state->mod_comp_params, n);
6750 | samples++;
6751 | }
6752 | }
6753 | }
6754 | else {
6755 | /* All 12 REs are present */
6756 | for (unsigned n=1; n<=12; n++) {
6757 | samples_offset = dissect_oran_u_re(tvb, rb_tree,
6758 | n, samples_offset, tap_info, sample_bit_width, compression, exponent, &state->mod_comp_params, n);
6759 | samples++;
6760 | }
6761 | }
6762 | proto_item_append_text(prbHeading, " (%u REs)", samples);
6763 |
6764 | /* Was this PRB all zeros? */
6765 | if (!tap_info->non_zero_re_in_current_prb) {
6766 | tap_info->num_prbs_zero++;
6767 | /* Add a filter to make zero-valued PRBs more findable */
6768 | proto_tree_add_item(rb_tree, hf_oran_zero_prb, tvb,
6769 | samples_offset/8, nBytesForSamples, ENC_NA0x00000000);
6770 | proto_item_append_text(prbHeading, " (all zeros)");
6771 | }
6772 | }
6773 |
6774 | tap_info->num_prbs++;
6775 |
6776 |
6777 | /* Advance past samples */
6778 | offset += nBytesForSamples;
6779 |
6780 | /* Set end of prb subtree */
6781 | proto_item_set_end(prbHeading, tvb, offset);
6782 | }
6783 |
6784 | /* Set extent of section */
6785 | proto_item_set_len(sectionHeading, offset-section_start_offset);
6786 | if (ud_comp_len_ti != NULL((void*)0) && ((offset-section_start_offset != ud_comp_len))) {
6787 | expert_add_info_format(pinfo, ud_comp_len_ti, &ei_oran_ud_comp_len_wrong_size,
6788 | "udCompLen indicates %u bytes in section, but dissected %u instead",
6789 | ud_comp_len, offset-section_start_offset);
6790 | }
6791 |
6792 | bytesLeft = tvb_captured_length(tvb) - offset;
6793 | number_of_sections++;
6794 | } while (bytesLeft >= (4 + nBytesPerPrb)); /* FIXME: bad heuristic */
6795 |
6796 | /* Show number of sections found */
6797 | proto_item *ti = proto_tree_add_uint(oran_tree, hf_oran_numberOfSections, tvb, 0, 0, number_of_sections);
6798 | proto_item_set_generated(ti);
6799 |
6800 | /* Expert error if we are short of tvb by > 3 bytes */
6801 | if (tvb_reported_length_remaining(tvb, offset) > 3) {
6802 | expert_add_info_format(pinfo, protocol_item, &ei_oran_frame_length,
6803 | "%u bytes remain at end of frame - should be 0-3",
6804 | tvb_reported_length_remaining(tvb, offset));
6805 | }
6806 |
6807 | return tvb_captured_length(tvb);
6808 | }
6809 |
6810 |
6811 | /**********************************************************************/
6812 | /* Main dissection function. */
6813 | /* N.B. ecpri message type passed in as 'data' arg by eCPRI dissector */
6814 | static int
6815 | dissect_oran(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, void *data)
6816 | {
6817 | uint32_t ecpri_message_type = *(uint32_t *)data;
6818 | int offset = 0;
6819 |
6820 | /* Allocate and zero tap struct */
6821 | oran_tap_info *tap_info = wmem_new0(wmem_file_scope(), oran_tap_info)((oran_tap_info*)wmem_alloc0((wmem_file_scope()), sizeof(oran_tap_info )));
6822 | tap_info->pdu_size = pinfo->fd->pkt_len;
6823 |
6824 | switch (ecpri_message_type) {
6825 | case ECPRI_MT_IQ_DATA0:
6826 | offset = dissect_oran_u(tvb, pinfo, tree, tap_info, data);
6827 | break;
6828 | case ECPRI_MT_RT_CTRL_DATA2:
6829 | offset = dissect_oran_c(tvb, pinfo, tree, tap_info, data);
6830 | break;
6831 | default:
6832 | /* Not dissecting other types - assume these are handled by eCPRI dissector */
6833 | return 0;
6834 | }
6835 |
6836 | tap_queue_packet(oran_tap, pinfo, tap_info);
6837 |
6838 | return offset;
6839 | }
6840 |
6841 | static void oran_init_protocol(void)
6842 | {
6843 | udcomplen_heuristic_result_set = false0;
6844 | udcomplen_heuristic_result = false0;
6845 | }
6846 |
6847 |
6848 | /* Register the protocol with Wireshark. */
6849 | void
6850 | proto_register_oran(void)
6851 | {
6852 | static hf_register_info hf[] = {
6853 |
6854 | /* Section 5.1.3.2.7 */
6855 | { &hf_oran_du_port_id,
6856 | { "DU Port ID", "oran_fh_cus.du_port_id",
6857 | FT_UINT16, BASE_DEC,
6858 | NULL((void*)0), 0x0,
6859 | "Processing unit at O-RU - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6860 | },
6861 |
6862 | /* Section 5.1.3.2.7 */
6863 | { &hf_oran_bandsector_id,
6864 | { "BandSector ID", "oran_fh_cus.bandsector_id",
6865 | FT_UINT16, BASE_DEC,
6866 | NULL((void*)0), 0x0,
6867 | "Aggregated cell identified - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6868 | },
6869 |
6870 | /* Section 5.1.3.2.7 */
6871 | { &hf_oran_cc_id,
6872 | { "CC ID", "oran_fh_cus.cc_id",
6873 | FT_UINT16, BASE_DEC,
6874 | NULL((void*)0), 0x0,
6875 | "Component Carrier - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6876 | },
6877 |
6878 | /* Section 5.1.3.2.7 */
6879 | { &hf_oran_ru_port_id,
6880 | { "RU Port ID", "oran_fh_cus.ru_port_id",
6881 | FT_UINT16, BASE_DEC,
6882 | NULL((void*)0), 0x0,
6883 | "Logical flow - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6884 | },
6885 |
6886 | /* Section 5.1.3.2.8 */
6887 | { &hf_oran_sequence_id,
6888 | { "Sequence ID", "oran_fh_cus.sequence_id",
6889 | FT_UINT8, BASE_DEC,
6890 | NULL((void*)0), 0x0,
6891 | "The Sequence ID wraps around individually per eAxC", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6892 | },
6893 |
6894 | /* Section 5.1.3.2.8 */
6895 | { &hf_oran_e_bit,
6896 | { "E Bit", "oran_fh_cus.e_bit",
6897 | FT_UINT8, BASE_DEC,
6898 | VALS(e_bit)((0 ? (const struct _value_string*)0 : ((e_bit)))), 0x80,
6899 | "Indicate the last message of a subsequence (U-Plane only)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6900 | },
6901 |
6902 | /* Section 5.1.3.2.8 */
6903 | { &hf_oran_subsequence_id,
6904 | { "Subsequence ID", "oran_fh_cus.subsequence_id",
6905 | FT_UINT8, BASE_DEC,
6906 | NULL((void*)0), 0x7f,
6907 | "The subsequence ID (for eCPRI layer fragmentation)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6908 | },
6909 |
6910 | { &hf_oran_previous_frame,
6911 | { "Previous frame in stream", "oran_fh_cus.previous-frame",
6912 | FT_FRAMENUM, BASE_NONE,
6913 | FRAMENUM_TYPE(FT_FRAMENUM_NONE)((gpointer) (glong) (FT_FRAMENUM_NONE)), 0x0,
6914 | "Previous frame in sequence", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6915 | },
6916 |
6917 | /* Section 7.5.2.1 */
6918 | { &hf_oran_data_direction,
6919 | { "Data Direction", "oran_fh_cus.data_direction",
6920 | FT_UINT8, BASE_DEC,
6921 | VALS(data_direction_vals)((0 ? (const struct _value_string*)0 : ((data_direction_vals) ))), 0x80,
6922 | "gNB data direction", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
6923 | },
6924 |
6925 | /* Section 7.5.2.2 */
6926 | { &hf_oran_payload_version,
6927 | { "Payload Version", "oran_fh_cus.payloadVersion",
6928 | FT_UINT8, BASE_DEC,
6929 | NULL((void*)0), 0x70,
6930 | "Payload protocol version the following IEs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6931 | },
6932 |
6933 | /* Section 7.5.2.3 */
6934 | { &hf_oran_filter_index,
6935 | { "Filter Index", "oran_fh_cus.filterIndex",
6936 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
6937 | RVALS(filter_indices)((0 ? (const struct _range_string*)0 : ((filter_indices)))), 0x0f,
6938 | "used between IQ data and air interface, both in DL and UL", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6939 | },
6940 |
6941 | /* Section 7.5.2.4 */
6942 | { &hf_oran_frame_id,
6943 | { "Frame ID", "oran_fh_cus.frameId",
6944 | FT_UINT8, BASE_DEC,
6945 | NULL((void*)0), 0x0,
6946 | "A counter for 10 ms frames (wrapping period 2.56 seconds)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6947 | },
6948 |
6949 | /* Section 7.5.2.5 */
6950 | { &hf_oran_subframe_id,
6951 | { "Subframe ID", "oran_fh_cus.subframe_id",
6952 | FT_UINT8, BASE_DEC,
6953 | NULL((void*)0), 0xf0,
6954 | "A counter for 1 ms sub-frames within 10ms frame", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6955 | },
6956 |
6957 | /* Section 7.5.2.6 */
6958 | { &hf_oran_slot_id,
6959 | { "Slot ID", "oran_fh_cus.slotId",
6960 | FT_UINT16, BASE_DEC,
6961 | NULL((void*)0), 0x0fc0,
6962 | "Slot number within a 1ms sub-frame", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6963 | },
6964 |
6965 | /* Generated for convenience */
6966 | { &hf_oran_slot_within_frame,
6967 | { "Slot within frame", "oran_fh_cus.slot-within-frame",
6968 | FT_UINT16, BASE_DEC,
6969 | NULL((void*)0), 0x0,
6970 | "Slot within frame, to match DCT logs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6971 | },
6972 |
6973 | /* Section 7.5.2.7 */
6974 | { &hf_oran_start_symbol_id,
6975 | { "Start Symbol ID", "oran_fh_cus.startSymbolId",
6976 | FT_UINT8, BASE_DEC,
6977 | NULL((void*)0), 0x3f,
6978 | "The first symbol number within slot affected", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6979 | },
6980 |
6981 | /* Section 7.5.2.8 */
6982 | { &hf_oran_numberOfSections,
6983 | { "Number of Sections", "oran_fh_cus.numberOfSections",
6984 | FT_UINT8, BASE_DEC,
6985 | NULL((void*)0), 0x0,
6986 | "The number of section IDs included in this message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6987 | },
6988 |
6989 | /* Section 7.5.2.9 */
6990 | { &hf_oran_sectionType,
6991 | { "Section Type", "oran_fh_cus.sectionType",
6992 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
6993 | RVALS(section_types)((0 ? (const struct _range_string*)0 : ((section_types)))), 0x0,
6994 | "Determines the characteristics of U-plane data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
6995 | },
6996 |
6997 | /* Section 7.5.2.10 */
6998 | { &hf_oran_udCompHdr,
6999 | { "udCompHdr", "oran_fh_cus.udCompHdr",
7000 | FT_STRING, BASE_NONE,
7001 | NULL((void*)0), 0x0,
7002 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7003 | },
7004 |
7005 | /* Section 7.5.2.11 */
7006 | { &hf_oran_numberOfUEs,
7007 | { "Number Of UEs", "oran_fh_cus.numberOfUEs",
7008 | FT_UINT8, BASE_DEC,
7009 | NULL((void*)0), 0x0,
7010 | "Indicates number of UEs for which channel info is provided", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7011 | },
7012 |
7013 | /* Section 7.5.2.12 */
7014 | { &hf_oran_timeOffset,
7015 | { "Time Offset", "oran_fh_cus.timeOffset",
7016 | FT_UINT16, BASE_DEC,
7017 | NULL((void*)0), 0x0,
7018 | "from start of the slot to start of CP in samples", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7019 | },
7020 |
7021 | /* Section 7.5.2.13 */
7022 | { &hf_oran_frameStructure_fft,
7023 | { "FFT Size", "oran_fh_cus.frameStructure.fft",
7024 | FT_UINT8, BASE_HEX | BASE_RANGE_STRING0x00000100,
7025 | RVALS(frame_structure_fft)((0 ? (const struct _range_string*)0 : ((frame_structure_fft) ))), 0xf0,
7026 | "The FFT/iFFT size being used for all IQ data processing related to this message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7027 | },
7028 |
7029 | /* Section 7.5.2.13 */
7030 | { &hf_oran_frameStructure_subcarrier_spacing,
7031 | { "Subcarrier Spacing", "oran_fh_cus.frameStructure.spacing",
7032 | FT_UINT8, BASE_HEX | BASE_RANGE_STRING0x00000100,
7033 | RVALS(subcarrier_spacings)((0 ? (const struct _range_string*)0 : ((subcarrier_spacings) ))), 0x0f,
7034 | "The sub carrier spacing as well as the number of slots per 1ms sub-frame",
7035 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7036 | },
7037 |
7038 | /* Section 7.5.2.14 */
7039 | { &hf_oran_cpLength,
7040 | { "cpLength", "oran_fh_cus.cpLength",
7041 | FT_UINT16, BASE_DEC,
7042 | NULL((void*)0), 0x0,
7043 | "cyclic prefix length", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7044 | },
7045 |
7046 | { &hf_oran_timing_header,
7047 | { "Timing Header", "oran_fh_cus.timingHeader",
7048 | FT_STRING, BASE_NONE,
7049 | NULL((void*)0), 0x0,
7050 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7051 | },
7052 |
7053 | /* Section 7.5.3.1 */
7054 | { &hf_oran_section_id,
7055 | { "sectionId", "oran_fh_cus.sectionId",
7056 | FT_UINT16, BASE_DEC,
7057 | NULL((void*)0), 0xfff0,
7058 | "section identifier of data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7059 | },
7060 |
7061 | /* Section 7.5.3.2 */
7062 | { &hf_oran_rb,
7063 | { "rb", "oran_fh_cus.rb",
7064 | FT_UINT8, BASE_DEC,
7065 | VALS(rb_vals)((0 ? (const struct _value_string*)0 : ((rb_vals)))), 0x08,
7066 | "resource block indicator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7067 | },
7068 |
7069 | /* Section 7.5.5.3 */
7070 | { &hf_oran_symInc,
7071 | { "symInc", "oran_fh_cus.symInc",
7072 | FT_UINT8, BASE_DEC,
7073 | VALS(sym_inc_vals)((0 ? (const struct _value_string*)0 : ((sym_inc_vals)))), 0x04,
7074 | "Symbol Number Increment Command", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7075 | },
7076 |
7077 | /* Section 7.5.3.4 */
7078 | { &hf_oran_startPrbc,
7079 | { "startPrbc", "oran_fh_cus.startPrbc",
7080 | FT_UINT16, BASE_DEC,
7081 | NULL((void*)0), 0x03ff,
7082 | "Starting PRB of Control Plane Section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7083 | },
7084 |
7085 | /* Section 7.5.3.5 */
7086 | { &hf_oran_reMask_re1,
7087 | { "RE 1", "oran_fh_cus.reMask-RE1",
7088 | FT_BOOLEAN, 16,
7089 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x8000,
7090 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7091 | },
7092 | { &hf_oran_reMask_re2,
7093 | { "RE 2", "oran_fh_cus.reMask-RE2",
7094 | FT_BOOLEAN, 16,
7095 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x4000,
7096 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7097 | },
7098 | { &hf_oran_reMask_re3,
7099 | { "RE 3", "oran_fh_cus.reMask-RE3",
7100 | FT_BOOLEAN, 16,
7101 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x2000,
7102 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7103 | },
7104 | { &hf_oran_reMask_re4,
7105 | { "RE 4", "oran_fh_cus.reMask-RE4",
7106 | FT_BOOLEAN, 16,
7107 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x1000,
7108 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7109 | },
7110 | { &hf_oran_reMask_re5,
7111 | { "RE 5", "oran_fh_cus.reMask-RE5",
7112 | FT_BOOLEAN, 16,
7113 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0800,
7114 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7115 | },
7116 | { &hf_oran_reMask_re6,
7117 | { "RE 6", "oran_fh_cus.reMask-RE6",
7118 | FT_BOOLEAN, 16,
7119 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0400,
7120 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7121 | },
7122 | { &hf_oran_reMask_re7,
7123 | { "RE 7", "oran_fh_cus.reMask-RE7",
7124 | FT_BOOLEAN, 16,
7125 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0200,
7126 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7127 | },
7128 | { &hf_oran_reMask_re8,
7129 | { "RE 8", "oran_fh_cus.reMask-RE8",
7130 | FT_BOOLEAN, 16,
7131 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0100,
7132 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7133 | },
7134 | { &hf_oran_reMask_re9,
7135 | { "RE 9", "oran_fh_cus.reMask-RE9",
7136 | FT_BOOLEAN, 16,
7137 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0080,
7138 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7139 | },
7140 | { &hf_oran_reMask_re10,
7141 | { "RE 10", "oran_fh_cus.reMask-RE10",
7142 | FT_BOOLEAN, 16,
7143 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0040,
7144 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7145 | },
7146 | { &hf_oran_reMask_re11,
7147 | { "RE 11", "oran_fh_cus.reMask-RE11",
7148 | FT_BOOLEAN, 16,
7149 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0020,
7150 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7151 | },
7152 | { &hf_oran_reMask_re12,
7153 | { "RE 12", "oran_fh_cus.reMask-RE12",
7154 | FT_BOOLEAN, 16,
7155 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0010,
7156 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7157 | },
7158 | { &hf_oran_reMask,
7159 | { "RE Mask", "oran_fh_cus.reMask",
7160 | FT_UINT16, BASE_HEX,
7161 | NULL((void*)0), 0xfff0,
7162 | "The Resource Element (RE) mask within a PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7163 | },
7164 |
7165 | /* Section 7.5.3.6 */
7166 | { &hf_oran_numPrbc,
7167 | { "numPrbc", "oran_fh_cus.numPrbc",
7168 | FT_UINT8, BASE_DEC,
7169 | NULL((void*)0), 0x0,
7170 | "Number of contiguous PRBs per data section description", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7171 | },
7172 |
7173 | /* Section 7.5.3.7 */
7174 | { &hf_oran_numSymbol,
7175 | { "Number of Symbols", "oran_fh_cus.numSymbol",
7176 | FT_UINT8, BASE_DEC,
7177 | NULL((void*)0), 0x0f,
7178 | "Defines number of symbols to which the section control is applicable", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7179 | },
7180 |
7181 | /* Section 7.5.3.8 */
7182 | { &hf_oran_ef,
7183 | { "Extension Flag", "oran_fh_cus.ef",
7184 | FT_BOOLEAN, 8,
7185 | NULL((void*)0), 0x80,
7186 | "Indicates if more section extensions follow", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7187 | },
7188 |
7189 | /* Section 7.5.3.9 */
7190 | { &hf_oran_beamId,
7191 | { "Beam ID", "oran_fh_cus.beamId",
7192 | FT_UINT16, BASE_DEC,
7193 | NULL((void*)0), 0x7fff,
7194 | "Defines the beam pattern to be applied to the U-Plane data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7195 | },
7196 |
7197 | { &hf_oran_extension,
7198 | { "Extension", "oran_fh_cus.extension",
7199 | FT_STRING, BASE_NONE,
7200 | NULL((void*)0), 0x0,
7201 | "Section extension", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7202 | },
7203 |
7204 | /* Section 7.6.2.1 */
7205 | { &hf_oran_exttype,
7206 | { "extType", "oran_fh_cus.extType",
7207 | FT_UINT8, BASE_DEC,
7208 | VALS(exttype_vals)((0 ? (const struct _value_string*)0 : ((exttype_vals)))), 0x7f,
7209 | "The extension type, which provides additional parameters specific to subject data extension", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7210 | },
7211 |
7212 | /* Section 7.6.2.3 */
7213 | { &hf_oran_extlen,
7214 | { "extLen", "oran_fh_cus.extLen",
7215 | FT_UINT16, BASE_DEC,
7216 | NULL((void*)0), 0x0,
7217 | "Extension length in 32-bit words", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7218 | },
7219 |
7220 | /* Section 7.7.1 */
7221 | { &hf_oran_bfw,
7222 | { "bfw", "oran_fh_cus.bfw",
7223 | FT_STRING, BASE_NONE,
7224 | NULL((void*)0), 0x0,
7225 | "Set of weights for a particular antenna", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7226 | },
7227 | { &hf_oran_bfw_bundle,
7228 | { "Bundle", "oran_fh_cus.bfw.bundle",
7229 | FT_STRING, BASE_NONE,
7230 | NULL((void*)0), 0x0,
7231 | "Bundle of BFWs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7232 | },
7233 | { &hf_oran_bfw_bundle_id,
7234 | { "Bundle Id", "oran_fh_cus.bfw.bundleId",
7235 | FT_UINT32, BASE_DEC,
7236 | NULL((void*)0), 0x0,
7237 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7238 | },
7239 | /* Section 7.7.1.4 */
7240 | { &hf_oran_bfw_i,
7241 | { "bfwI", "oran_fh_cus.bfwI",
7242 | FT_FLOAT, BASE_NONE,
7243 | NULL((void*)0), 0x0,
7244 | "In-phase", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7245 | },
7246 | /* Section 7.7.1.5 */
7247 | { &hf_oran_bfw_q,
7248 | { "bfwQ", "oran_fh_cus.bfwQ",
7249 | FT_FLOAT, BASE_NONE,
7250 | NULL((void*)0), 0x0,
7251 | "Quadrature", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7252 | },
7253 |
7254 | /* Section 7.5.3.10 */
7255 | { &hf_oran_ueId,
7256 | { "UE ID", "oran_fh_cus.ueId",
7257 | FT_UINT16, BASE_DEC,
7258 | NULL((void*)0), 0x7fff,
7259 | "logical identifier for set of channel info", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7260 | },
7261 |
7262 | /* Section 7.5.3.11 */
7263 | { &hf_oran_freqOffset,
7264 | { "Frequency Offset", "oran_fh_cus.freqOffset",
7265 | FT_UINT24, BASE_DEC,
7266 | NULL((void*)0), 0x0,
7267 | "with respect to the carrier center frequency before additional filtering", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7268 | },
7269 |
7270 | /* Section 7.5.3.12 */
7271 | { &hf_oran_regularizationFactor,
7272 | { "Regularization Factor", "oran_fh_cus.regularizationFactor",
7273 | FT_INT16, BASE_DEC,
7274 | NULL((void*)0), 0x0,
7275 | "Signed value to support MMSE operation within O-RU", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7276 | },
7277 |
7278 | /* Section 7.5.3.14 */
7279 | { &hf_oran_laaMsgType,
7280 | { "LAA Message Type", "oran_fh_cus.laaMsgType",
7281 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7282 | RVALS(laaMsgTypes)((0 ? (const struct _range_string*)0 : ((laaMsgTypes)))), 0xf0,
7283 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7284 | },
7285 |
7286 | /* Section 7.5.3.15 */
7287 | { &hf_oran_laaMsgLen,
7288 | { "LAA Message Length", "oran_fh_cus.laaMsgLen",
7289 | FT_UINT8, BASE_DEC,
7290 | NULL((void*)0), 0x0f,
7291 | "number of 32-bit words in the LAA section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7292 | },
7293 |
7294 | /* Section 7.5.3.16 */
7295 | { &hf_oran_lbtHandle,
7296 | { "LBT Handle", "oran_fh_cus.lbtHandle",
7297 | FT_UINT16, BASE_HEX,
7298 | NULL((void*)0), 0x0,
7299 | "label to identify transaction", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7300 | },
7301 |
7302 | /* Section 7.5.3.17 */
7303 | { &hf_oran_lbtDeferFactor,
7304 | { "Defer Factor", "oran_fh_cus.lbtDeferFactor",
7305 | FT_UINT8, BASE_DEC,
7306 | NULL((void*)0), 0x07,
7307 | "Defer factor in sensing slots as described in 3GPP TS 36.213 Section 15.1.1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7308 | },
7309 |
7310 | /* Section 7.5.3.18 */
7311 | { &hf_oran_lbtBackoffCounter,
7312 | { "Backoff Counter", "oran_fh_cus.lbtBackoffCounter",
7313 | FT_UINT16, BASE_DEC,
7314 | NULL((void*)0), 0xffc0,
7315 | "LBT backoff counter in sensing slots as described in 3GPP TS 36.213 Section 15.1.1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7316 | },
7317 |
7318 | /* Section 7.5.3.19 */
7319 | { &hf_oran_lbtOffset,
7320 | { "LBT Offset", "oran_fh_cus.lbtOffset",
7321 | FT_UINT16, BASE_DEC,
7322 | NULL((void*)0), 0xffc0,
7323 | "LBT start time in microseconds from the beginning of the subframe scheduled by this message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7324 | },
7325 |
7326 | /* Section 7.5.3.20 */
7327 | { &hf_oran_MCOT,
7328 | { "Maximum Channel Occupancy Time", "oran_fh_cus.MCOT",
7329 | FT_UINT8, BASE_DEC,
7330 | NULL((void*)0), 0x3c,
7331 | "LTE TXOP duration in subframes as described in 3GPP TS 36.213 Section 15.1.1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7332 | },
7333 |
7334 | /* Section 7.5.3.21 */
7335 | { &hf_oran_lbtMode,
7336 | { "LBT Mode", "oran_fh_cus.lbtMode",
7337 | FT_UINT8, BASE_DEC,
7338 | VALS(lbtMode_vals)((0 ? (const struct _value_string*)0 : ((lbtMode_vals)))), 0x0,
7339 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7340 | },
7341 |
7342 | /* Section 7.5.3.22 */
7343 | { &hf_oran_lbtPdschRes,
7344 | { "lbtPdschRes", "oran_fh_cus.lbtPdschRes",
7345 | FT_UINT8, BASE_DEC,
7346 | VALS(lbtPdschRes_vals)((0 ? (const struct _value_string*)0 : ((lbtPdschRes_vals)))), 0xc0,
7347 | "LBT result of SFN/SF", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7348 | },
7349 |
7350 | /* Section 7.5.3.23 */
7351 | { &hf_oran_sfStatus,
7352 | { "sfStatus", "oran_fh_cus.sfStatus",
7353 | FT_BOOLEAN, 8,
7354 | TFS(&tfs_sfStatus)((0 ? (const struct true_false_string*)0 : ((&tfs_sfStatus )))), 0x10,
7355 | "Indicates whether the subframe was dropped or transmitted", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7356 | },
7357 |
7358 | /* Section 7.5.3.22 */
7359 | { &hf_oran_lbtDrsRes,
7360 | { "lbtDrsRes", "oran_fh_cus.lbtDrsRes",
7361 | FT_BOOLEAN, 8,
7362 | TFS(&tfs_fail_success)((0 ? (const struct true_false_string*)0 : ((&tfs_fail_success )))), 0x80,
7363 | "Indicates whether the subframe was dropped or transmitted", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7364 | },
7365 |
7366 | /* Section 7.5.3.25 */
7367 | { &hf_oran_initialPartialSF,
7368 | { "Initial partial SF", "oran_fh_cus.initialPartialSF",
7369 | FT_BOOLEAN, 8,
7370 | TFS(&tfs_partial_full_sf)((0 ? (const struct true_false_string*)0 : ((&tfs_partial_full_sf )))), 0x40,
7371 | "Indicates whether the initial SF in the LBT process is full or partial", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7372 | },
7373 |
7374 | /* Section 7.5.3.26. */
7375 | { &hf_oran_lbtBufErr,
7376 | { "lbtBufErr", "oran_fh_cus.lbtBufErr",
7377 | FT_BOOLEAN, 8,
7378 | TFS(&tfs_lbtBufErr)((0 ? (const struct true_false_string*)0 : ((&tfs_lbtBufErr )))), 0x80,
7379 | "LBT buffer error", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7380 | },
7381 |
7382 | /* Section 7.5.3.27 */
7383 | { &hf_oran_sfnSfEnd,
7384 | { "SFN/SF End", "oran_fh_cus.sfnSfEnd",
7385 | FT_UINT16, BASE_DEC,
7386 | NULL((void*)0), 0x0fff,
7387 | "SFN/SF by which the DRS window must end", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7388 | },
7389 |
7390 | /* Section 7.5.3.28 */
7391 | { &hf_oran_lbtCWConfig_H,
7392 | { "lbtCWConfig_H", "oran_fh_cus.lbtCWConfig_H",
7393 | FT_UINT8, BASE_DEC,
7394 | NULL((void*)0), 0x0,
7395 | "HARQ parameters for congestion window management", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7396 | },
7397 |
7398 | /* Section 7.5.3.29 */
7399 | { &hf_oran_lbtCWConfig_T,
7400 | { "lbtCWConfig_T", "oran_fh_cus.lbtCWConfig_T",
7401 | FT_UINT8, BASE_DEC,
7402 | NULL((void*)0), 0x0,
7403 | "TB parameters for congestion window management", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7404 | },
7405 |
7406 | /* Section 7.5.3.30 */
7407 | { &hf_oran_lbtTrafficClass,
7408 | { "lbtTrafficClass", "oran_fh_cus.lbtTrafficClass",
7409 | FT_UINT8, BASE_DEC,
7410 | VALS(lbtTrafficClass_vals)((0 ? (const struct _value_string*)0 : ((lbtTrafficClass_vals )))), 0x38,
7411 | "Traffic class priority for congestion window management", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7412 | },
7413 |
7414 | /* Section 7.5.3.31 */
7415 | { &hf_oran_lbtCWR_Rst,
7416 | { "lbtCWR_Rst", "oran_fh_cus.lbtCWR_Rst",
7417 | FT_BOOLEAN, 8,
7418 | TFS(&tfs_fail_success)((0 ? (const struct true_false_string*)0 : ((&tfs_fail_success )))), 0x80,
7419 | "notification about packet reception successful or not", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7420 | },
7421 |
7422 | /* Reserved fields */
7423 | { &hf_oran_reserved,
7424 | { "reserved", "oran_fh_cus.reserved",
7425 | FT_UINT64, BASE_HEX,
7426 | NULL((void*)0), 0x0,
7427 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7428 | },
7429 |
7430 | { &hf_oran_reserved_1bit,
7431 | { "reserved", "oran_fh_cus.reserved",
7432 | FT_UINT8, BASE_HEX,
7433 | NULL((void*)0), 0x80,
7434 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7435 | },
7436 | { &hf_oran_reserved_2bits,
7437 | { "reserved", "oran_fh_cus.reserved",
7438 | FT_UINT8, BASE_HEX,
7439 | NULL((void*)0), 0xc0,
7440 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7441 | },
7442 | { &hf_oran_reserved_3bits,
7443 | { "reserved", "oran_fh_cus.reserved",
7444 | FT_UINT8, BASE_HEX,
7445 | NULL((void*)0), 0xe0,
7446 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7447 | },
7448 | { &hf_oran_reserved_4bits,
7449 | { "reserved", "oran_fh_cus.reserved",
7450 | FT_UINT8, BASE_HEX,
7451 | NULL((void*)0), 0xf0,
7452 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7453 | },
7454 | { &hf_oran_reserved_last_4bits,
7455 | { "reserved", "oran_fh_cus.reserved",
7456 | FT_UINT8, BASE_HEX,
7457 | NULL((void*)0), 0x0f,
7458 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7459 | },
7460 | { &hf_oran_reserved_last_5bits,
7461 | { "reserved", "oran_fh_cus.reserved",
7462 | FT_UINT8, BASE_HEX,
7463 | NULL((void*)0), 0x1f,
7464 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7465 | },
7466 | { &hf_oran_reserved_6bits,
7467 | { "reserved", "oran_fh_cus.reserved",
7468 | FT_UINT8, BASE_HEX,
7469 | NULL((void*)0), 0xfc,
7470 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7471 | },
7472 | { &hf_oran_reserved_last_6bits,
7473 | { "reserved", "oran_fh_cus.reserved",
7474 | FT_UINT8, BASE_HEX,
7475 | NULL((void*)0), 0x3f,
7476 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7477 | },
7478 | { &hf_oran_reserved_7bits,
7479 | { "reserved", "oran_fh_cus.reserved",
7480 | FT_UINT8, BASE_HEX,
7481 | NULL((void*)0), 0xfe,
7482 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7483 | },
7484 | { &hf_oran_reserved_last_7bits,
7485 | { "reserved", "oran_fh_cus.reserved",
7486 | FT_UINT8, BASE_HEX,
7487 | NULL((void*)0), 0x7f,
7488 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7489 | },
7490 | { &hf_oran_reserved_8bits,
7491 | { "reserved", "oran_fh_cus.reserved",
7492 | FT_UINT8, BASE_HEX,
7493 | NULL((void*)0), 0x0,
7494 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7495 | },
7496 | { &hf_oran_reserved_16bits,
7497 | { "reserved", "oran_fh_cus.reserved",
7498 | FT_UINT16, BASE_HEX,
7499 | NULL((void*)0), 0x0,
7500 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7501 | },
7502 | { &hf_oran_reserved_15bits,
7503 | { "reserved", "oran_fh_cus.reserved",
7504 | FT_UINT16, BASE_HEX,
7505 | NULL((void*)0), 0x7fff,
7506 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7507 | },
7508 | { &hf_oran_reserved_bit1,
7509 | { "reserved", "oran_fh_cus.reserved",
7510 | FT_UINT8, BASE_HEX,
7511 | NULL((void*)0), 0x40,
7512 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7513 | },
7514 | { &hf_oran_reserved_bit2,
7515 | { "reserved", "oran_fh_cus.reserved",
7516 | FT_UINT8, BASE_HEX,
7517 | NULL((void*)0), 0x20,
7518 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7519 | },
7520 | { &hf_oran_reserved_bit4,
7521 | { "reserved", "oran_fh_cus.reserved",
7522 | FT_UINT8, BASE_HEX,
7523 | NULL((void*)0), 0x08,
7524 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7525 | },
7526 | { &hf_oran_reserved_bit5,
7527 | { "reserved", "oran_fh_cus.reserved",
7528 | FT_UINT8, BASE_HEX,
7529 | NULL((void*)0), 0x04,
7530 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7531 | },
7532 | { &hf_oran_reserved_bits123,
7533 | { "reserved", "oran_fh_cus.reserved",
7534 | FT_UINT8, BASE_HEX,
7535 | NULL((void*)0), 0x70,
7536 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7537 | },
7538 | { &hf_oran_reserved_bits456,
7539 | { "reserved", "oran_fh_cus.reserved",
7540 | FT_UINT8, BASE_HEX,
7541 | NULL((void*)0), 0x0e,
7542 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7543 | },
7544 |
7545 |
7546 | /* 7.7.11.10 */
7547 | { &hf_oran_bundle_offset,
7548 | { "BundleOffset", "oran_fh_cus.bundleOffset",
7549 | FT_UINT8, BASE_DEC,
7550 | NULL((void*)0), 0x3f,
7551 | "offset between start of first PRB bundle and startPrbc", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7552 | },
7553 | /* 7.7.11.9 */
7554 | { &hf_oran_cont_ind,
7555 | { "contInd", "oran_fh_cus.contInd",
7556 | FT_BOOLEAN, 8,
7557 | TFS(&continuity_indication_tfs)((0 ? (const struct true_false_string*)0 : ((&continuity_indication_tfs )))), 0x80,
7558 | "PRB region continuity flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7559 | },
7560 |
7561 | /* 7.7.1.2 bfwCompHdr (beamforming weight compression header) */
7562 | { &hf_oran_bfwCompHdr,
7563 | { "bfwCompHdr", "oran_fh_cus.bfwCompHdr",
7564 | FT_STRING, BASE_NONE,
7565 | NULL((void*)0), 0x0,
7566 | "Compression method and IQ bit width for beamforming weights", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7567 | },
7568 | { &hf_oran_bfwCompHdr_iqWidth,
7569 | { "IQ Bit Width", "oran_fh_cus.bfwCompHdr_iqWidth",
7570 | FT_UINT8, BASE_HEX,
7571 | VALS(bfw_comp_headers_iq_width)((0 ? (const struct _value_string*)0 : ((bfw_comp_headers_iq_width )))), 0xf0,
7572 | "IQ bit width for the beamforming weights", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7573 | },
7574 | { &hf_oran_bfwCompHdr_compMeth,
7575 | { "Compression Method", "oran_fh_cus.bfwCompHdr_compMeth",
7576 | FT_UINT8, BASE_HEX,
7577 | VALS(bfw_comp_headers_comp_meth)((0 ? (const struct _value_string*)0 : ((bfw_comp_headers_comp_meth )))), 0x0f,
7578 | "compression method for the beamforming weights", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7579 | },
7580 |
7581 | /* 7.5.3.32 */
7582 | { &hf_oran_ciCompParam,
7583 | { "ciCompParam", "oran_fh_cus.ciCompParam",
7584 | FT_STRING, BASE_NONE,
7585 | NULL((void*)0), 0x0,
7586 | "channel information compression parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7587 | },
7588 |
7589 | /* Table 7.5.3.32-1 */
7590 | { &hf_oran_blockScaler,
7591 | { "blockScaler", "oran_fh_cus.blockScaler",
7592 | FT_UINT8, BASE_HEX,
7593 | NULL((void*)0), 0x0,
7594 | "unsigned, 1 integer bit, 7 fractional bits", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7595 | },
7596 | { &hf_oran_compBitWidth,
7597 | { "compBitWidth", "oran_fh_cus.compBitWidth",
7598 | FT_UINT8, BASE_DEC,
7599 | NULL((void*)0), 0xf0,
7600 | "Length of I bits and length of Q bits after compression over entire PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7601 | },
7602 | { &hf_oran_compShift,
7603 | { "compShift", "oran_fh_cus.compShift",
7604 | FT_UINT8, BASE_DEC,
7605 | NULL((void*)0), 0x0f,
7606 | "The shift applied to the entire PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7607 | },
7608 |
7609 | { &hf_oran_active_beamspace_coefficient_n1,
7610 | { "N1", "oran_fh_cus.activeBeamspace_Coefficient_n1",
7611 | FT_BOOLEAN, 8,
7612 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x80,
7613 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7614 | },
7615 | { &hf_oran_active_beamspace_coefficient_n2,
7616 | { "N2", "oran_fh_cus.activeBeamspace_Coefficient_n2",
7617 | FT_BOOLEAN, 8,
7618 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x40,
7619 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7620 | },
7621 | { &hf_oran_active_beamspace_coefficient_n3,
7622 | { "N3", "oran_fh_cus.activeBeamspace_Coefficient_n3",
7623 | FT_BOOLEAN, 8,
7624 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x20,
7625 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7626 | },
7627 | { &hf_oran_active_beamspace_coefficient_n4,
7628 | { "N4", "oran_fh_cus.activeBeamspace_Coefficient_n4",
7629 | FT_BOOLEAN, 8,
7630 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x10,
7631 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7632 | },
7633 | { &hf_oran_active_beamspace_coefficient_n5,
7634 | { "N5", "oran_fh_cus.activeBeamspace_Coefficient_n5",
7635 | FT_BOOLEAN, 8,
7636 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x08,
7637 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7638 | },
7639 | { &hf_oran_active_beamspace_coefficient_n6,
7640 | { "N6", "oran_fh_cus.activeBeamspace_Coefficient_n6",
7641 | FT_BOOLEAN, 8,
7642 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x04,
7643 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7644 | },
7645 | { &hf_oran_active_beamspace_coefficient_n7,
7646 | { "N7", "oran_fh_cus.activeBeamspace_Coefficient_n7",
7647 | FT_BOOLEAN, 8,
7648 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x02,
7649 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7650 | },
7651 | { &hf_oran_active_beamspace_coefficient_n8,
7652 | { "N8", "oran_fh_cus.activeBeamspace_Coefficient_n8",
7653 | FT_BOOLEAN, 8,
7654 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x01,
7655 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7656 | },
7657 |
7658 | { &hf_oran_activeBeamspaceCoefficientMask,
7659 | { "activeBeamspaceCoefficientMask", "oran_fh_cus.activeBeamspaceCoefficientMask",
7660 | FT_UINT8, BASE_HEX,
7661 | NULL((void*)0), 0xff,
7662 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7663 | },
7664 | { &hf_oran_activeBeamspaceCoefficientMask_bits_set,
7665 | { "Array elements set", "oran_fh_cus.activeBeamspaceCoefficientMask.bits-set",
7666 | FT_UINT32, BASE_DEC,
7667 | NULL((void*)0), 0x0,
7668 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7669 | },
7670 |
7671 | /* Section 7.7.6.6 */
7672 | { &hf_oran_se6_repetition,
7673 | { "repetition", "oran_fh_cus.repetition",
7674 | FT_BOOLEAN, BASE_NONE,
7675 | TFS(&repetition_se6_tfs)((0 ? (const struct true_false_string*)0 : ((&repetition_se6_tfs )))), 0x0,
7676 | "Repetition of a highest priority data section for C-Plane", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7677 | },
7678 | /* 7.7.20.9 */
7679 | { &hf_oran_rbgSize,
7680 | { "rbgSize", "oran_fh_cus.rbgSize",
7681 | FT_UINT8, BASE_HEX,
7682 | VALS(rbg_size_vals)((0 ? (const struct _value_string*)0 : ((rbg_size_vals)))), 0x70,
7683 | "Number of PRBs of the resource block groups allocated by the bit mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7684 | },
7685 | /* 7.7.20.10 */
7686 | { &hf_oran_rbgMask,
7687 | { "rbgMask", "oran_fh_cus.rbgMask",
7688 | FT_UINT32, BASE_HEX,
7689 | NULL((void*)0), 0x0fffffff,
7690 | "Each bit indicates whether a corresponding resource block group is present", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7691 | },
7692 | /* 7.7.6.5. Also 7.7.12.3 and 7.7.19.5 */
7693 | { &hf_oran_noncontig_priority,
7694 | { "priority", "oran_fh_cus.priority",
7695 | FT_UINT8, BASE_HEX,
7696 | VALS(priority_vals)((0 ? (const struct _value_string*)0 : ((priority_vals)))), 0xc0,
7697 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7698 | },
7699 |
7700 | /* 7.7.6.4 */
7701 | { &hf_oran_symbol_mask,
7702 | { "symbolMask", "oran_fh_cus.symbolMask",
7703 | FT_UINT16, BASE_HEX,
7704 | NULL((void*)0), 0x3fff,
7705 | "Each bit indicates whether the rbgMask applies to a given symbol in the slot", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7706 | },
7707 | { &hf_oran_symbol_mask_s13,
7708 | { "symbol 13", "oran_fh_cus.symbolMask.symbol-13",
7709 | FT_BOOLEAN, 16,
7710 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x2000,
7711 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7712 | },
7713 | { &hf_oran_symbol_mask_s12,
7714 | { "symbol 12", "oran_fh_cus.symbolMask.symbol-12",
7715 | FT_BOOLEAN, 16,
7716 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x1000,
7717 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7718 | },
7719 | { &hf_oran_symbol_mask_s11,
7720 | { "symbol 11", "oran_fh_cus.symbolMask.symbol-11",
7721 | FT_BOOLEAN, 16,
7722 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0800,
7723 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7724 | },
7725 | { &hf_oran_symbol_mask_s10,
7726 | { "symbol 10", "oran_fh_cus.symbolMask.symbol-10",
7727 | FT_BOOLEAN, 16,
7728 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0400,
7729 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7730 | },
7731 | { &hf_oran_symbol_mask_s9,
7732 | { "symbol 9", "oran_fh_cus.symbolMask.symbol-9",
7733 | FT_BOOLEAN, 16,
7734 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0200,
7735 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7736 | },
7737 | { &hf_oran_symbol_mask_s8,
7738 | { "symbol 8", "oran_fh_cus.symbolMask.symbol-8",
7739 | FT_BOOLEAN, 16,
7740 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0100,
7741 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7742 | },
7743 | { &hf_oran_symbol_mask_s7,
7744 | { "symbol 7", "oran_fh_cus.symbolMask.symbol-7",
7745 | FT_BOOLEAN, 16,
7746 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0080,
7747 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7748 | },
7749 | { &hf_oran_symbol_mask_s6,
7750 | { "symbol 6", "oran_fh_cus.symbolMask.symbol-6",
7751 | FT_BOOLEAN, 16,
7752 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0040,
7753 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7754 | },
7755 | { &hf_oran_symbol_mask_s5,
7756 | { "symbol 5", "oran_fh_cus.symbolMask.symbol-5",
7757 | FT_BOOLEAN, 16,
7758 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0020,
7759 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7760 | },
7761 | { &hf_oran_symbol_mask_s4,
7762 | { "symbol 4", "oran_fh_cus.symbolMask.symbol-4",
7763 | FT_BOOLEAN, 16,
7764 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0010,
7765 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7766 | },
7767 | { &hf_oran_symbol_mask_s3,
7768 | { "symbol 3", "oran_fh_cus.symbolMask.symbol-3",
7769 | FT_BOOLEAN, 16,
7770 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0008,
7771 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7772 | },
7773 | { &hf_oran_symbol_mask_s2,
7774 | { "symbol 2", "oran_fh_cus.symbolMask.symbol-2",
7775 | FT_BOOLEAN, 16,
7776 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0004,
7777 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7778 | },
7779 | { &hf_oran_symbol_mask_s1,
7780 | { "symbol 1", "oran_fh_cus.symbolMask.symbol-1",
7781 | FT_BOOLEAN, 16,
7782 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0002,
7783 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7784 | },
7785 | { &hf_oran_symbol_mask_s0,
7786 | { "symbol 0", "oran_fh_cus.symbolMask.symbol-0",
7787 | FT_BOOLEAN, 16,
7788 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0001,
7789 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7790 | },
7791 |
7792 |
7793 | /* 7.7.22.2 */
7794 | { &hf_oran_ack_nack_req_id,
7795 | { "ackNackReqId", "oran_fh_cus.ackNackReqId",
7796 | FT_UINT16, BASE_HEX,
7797 | NULL((void*)0), 0x0,
7798 | "Indicates the ACK/NACK request ID of a section description", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7799 | },
7800 |
7801 | /* Subtree for next 2 items */
7802 | { &hf_oran_frequency_range,
7803 | { "Frequency Range", "oran_fh_cus.frequencyRange",
7804 | FT_STRING, BASE_NONE,
7805 | NULL((void*)0), 0x0,
7806 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7807 | },
7808 |
7809 | /* 7.7.12.4 */
7810 | { &hf_oran_off_start_prb,
7811 | { "offStartPrb", "oran_fh_cus.offStartPrb",
7812 | FT_UINT8, BASE_DEC,
7813 | NULL((void*)0), 0x0,
7814 | "Offset of PRB range start", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7815 | },
7816 | /* 7.7.12.5 */
7817 | { &hf_oran_num_prb,
7818 | { "numPrb", "oran_fh_cus.numPrb",
7819 | FT_UINT8, BASE_DEC,
7820 | NULL((void*)0), 0x0,
7821 | "Number of PRBs in PRB range", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7822 | },
7823 |
7824 | /* symbolId 8.3.3.7 */
7825 | { &hf_oran_symbolId,
7826 | { "Symbol Identifier", "oran_fh_cus.symbolId",
7827 | FT_UINT8, BASE_DEC,
7828 | NULL((void*)0), 0x3f,
7829 | "Identifies a symbol number within a slot", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7830 | },
7831 |
7832 | /* startPrbu 8.3.3.11 */
7833 | { &hf_oran_startPrbu,
7834 | { "startPrbu", "oran_fh_cus.startPrbu",
7835 | FT_UINT16, BASE_DEC,
7836 | NULL((void*)0), 0x03ff,
7837 | "starting PRB of user plane section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7838 | },
7839 |
7840 | /* numPrbu 8.3.3.12 */
7841 | { &hf_oran_numPrbu,
7842 | { "numPrbu", "oran_fh_cus.numPrbu",
7843 | FT_UINT8, BASE_DEC,
7844 | NULL((void*)0), 0x0,
7845 | "number of PRBs per user plane section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7846 | },
7847 |
7848 | /* 7.7.1.3 */
7849 | { &hf_oran_bfwCompParam,
7850 | { "bfwCompParam", "oran_fh_cus.bfwCompParam",
7851 | FT_STRING, BASE_NONE,
7852 | NULL((void*)0), 0x0,
7853 | "Beamforming weight compression parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7854 | },
7855 |
7856 | /* 6.3.3.13 */
7857 | { &hf_oran_udCompHdrMeth,
7858 | { "User Data Compression Method", "oran_fh_cus.udCompHdrMeth",
7859 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7860 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0f,
7861 | "Defines the compression method for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7862 | },
7863 | { &hf_oran_udCompHdrMeth_pref,
7864 | { "User Data Compression Method", "oran_fh_cus.udCompHdrMeth",
7865 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7866 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0,
7867 | "Defines the compression method for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7868 | },
7869 | /* 8.3.3.18 */
7870 | { &hf_oran_udCompLen,
7871 | { "udCompLen", "oran_fh_cus.udCompLen",
7872 | FT_UINT16, BASE_DEC,
7873 | NULL((void*)0), 0x0,
7874 | "PRB field length in octets", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7875 | },
7876 |
7877 | /* 6.3.3.13 */
7878 | { &hf_oran_udCompHdrIqWidth,
7879 | { "User Data IQ width", "oran_fh_cus.udCompHdrWidth",
7880 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7881 | RVALS(ud_comp_header_width)((0 ? (const struct _range_string*)0 : ((ud_comp_header_width )))), 0xf0,
7882 | "Defines the IQ bit width for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7883 | },
7884 | { &hf_oran_udCompHdrIqWidth_pref,
7885 | { "User Data IQ width", "oran_fh_cus.udCompHdrWidth",
7886 | FT_UINT8, BASE_DEC,
7887 | NULL((void*)0), 0x0,
7888 | "Defines the IQ bit width for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7889 | },
7890 |
7891 | { &hf_oran_sinrCompHdrIqWidth_pref,
7892 | { "SINR IQ width", "oran_fh_cus.sinrCompHdrWidth",
7893 | FT_UINT8, BASE_DEC,
7894 | NULL((void*)0), 0x0,
7895 | "Defines the IQ bit width for SINR data in section type 9", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7896 | },
7897 | { &hf_oran_sinrCompHdrMeth_pref,
7898 | { "SINR Compression Method", "oran_fh_cus.sinrCompHdrMeth",
7899 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
7900 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0,
7901 | "Defines the compression method for SINR data in section type 9", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7902 | },
7903 |
7904 | /* Section 8.3.3.15 (not always present - depends upon meth) */
7905 | { &hf_oran_udCompParam,
7906 | { "User Data Compression Parameter", "oran_fh_cus.udCompParam",
7907 | FT_STRING, BASE_NONE,
7908 | NULL((void*)0), 0x0,
7909 | "Applies to whatever compression method is specified by the associated sectionID's compMeth value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7910 | },
7911 | /* 8.3.3.18 */
7912 | { &hf_oran_sReSMask,
7913 | { "sReSMask", "oran_fh_cus.sReSMask",
7914 | FT_UINT16, BASE_HEX,
7915 | NULL((void*)0), 0xf0ff,
7916 | "selective RE sending mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7917 | },
7918 |
7919 | { &hf_oran_sReSMask_re12,
7920 | { "RE-12", "oran_fh_cus.sReSMask-re12",
7921 | FT_BOOLEAN, 16,
7922 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x8000,
7923 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7924 | },
7925 | { &hf_oran_sReSMask_re11,
7926 | { "RE-11", "oran_fh_cus.sReSMask-re11",
7927 | FT_BOOLEAN, 16,
7928 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x4000,
7929 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7930 | },
7931 | { &hf_oran_sReSMask_re10,
7932 | { "RE-10", "oran_fh_cus.sReSMask-re10",
7933 | FT_BOOLEAN, 16,
7934 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x2000,
7935 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7936 | },
7937 | { &hf_oran_sReSMask_re9,
7938 | { "RE-9", "oran_fh_cus.sReSMask-re9",
7939 | FT_BOOLEAN, 16,
7940 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x1000,
7941 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7942 | },
7943 | { &hf_oran_sReSMask_re8,
7944 | { "RE-8", "oran_fh_cus.sReSMask-re8",
7945 | FT_BOOLEAN, 16,
7946 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0080,
7947 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7948 | },
7949 | { &hf_oran_sReSMask_re7,
7950 | { "RE-7", "oran_fh_cus.sReSMask-re7",
7951 | FT_BOOLEAN, 16,
7952 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0040,
7953 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7954 | },
7955 | { &hf_oran_sReSMask_re6,
7956 | { "RE-6", "oran_fh_cus.sReSMask-re6",
7957 | FT_BOOLEAN, 16,
7958 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0020,
7959 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7960 | },
7961 | { &hf_oran_sReSMask_re5,
7962 | { "RE-5", "oran_fh_cus.sReSMask-re5",
7963 | FT_BOOLEAN, 16,
7964 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0010,
7965 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7966 | },
7967 | { &hf_oran_sReSMask_re4,
7968 | { "RE-4", "oran_fh_cus.sReSMask-re4",
7969 | FT_BOOLEAN, 16,
7970 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0008,
7971 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7972 | },
7973 | { &hf_oran_sReSMask_re3,
7974 | { "RE-3", "oran_fh_cus.sReSMask-re3",
7975 | FT_BOOLEAN, 16,
7976 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0004,
7977 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7978 | },
7979 | { &hf_oran_sReSMask_re2,
7980 | { "RE-2", "oran_fh_cus.sReSMask-re2",
7981 | FT_BOOLEAN, 16,
7982 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0002,
7983 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7984 | },
7985 | { &hf_oran_sReSMask_re1,
7986 | { "RE-1", "oran_fh_cus.sReSMask-re1",
7987 | FT_BOOLEAN, 16,
7988 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0001,
7989 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7990 | },
7991 |
7992 | /* 8.3.3.20 */
7993 | { &hf_oran_sReSMask1,
7994 | { "sReSMask1", "oran_fh_cus.sReSMask1",
7995 | FT_UINT16, BASE_HEX,
7996 | NULL((void*)0), 0x0fff,
7997 | "selective RE sending mask 1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
7998 | },
7999 | /* 8.3.3.21 */
8000 | { &hf_oran_sReSMask2,
8001 | { "sReSMask2", "oran_fh_cus.sReSMask2",
8002 | FT_UINT16, BASE_HEX,
8003 | NULL((void*)0), 0x0fff,
8004 | "selective RE sending mask 2", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8005 | },
8006 |
8007 | { &hf_oran_sReSMask1_2_re12,
8008 | { "RE-12", "oran_fh_cus.sReSMask-re12",
8009 | FT_BOOLEAN, 16,
8010 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0800,
8011 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8012 | },
8013 | { &hf_oran_sReSMask1_2_re11,
8014 | { "RE-11", "oran_fh_cus.sReSMask-re11",
8015 | FT_BOOLEAN, 16,
8016 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0400,
8017 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8018 | },
8019 | { &hf_oran_sReSMask1_2_re10,
8020 | { "RE-10", "oran_fh_cus.sReSMask-re10",
8021 | FT_BOOLEAN, 16,
8022 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0200,
8023 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8024 | },
8025 | { &hf_oran_sReSMask1_2_re9,
8026 | { "RE-9", "oran_fh_cus.sReSMask-re9",
8027 | FT_BOOLEAN, 16,
8028 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0100,
8029 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8030 | },
8031 |
8032 | /* Section 6.3.3.15 */
8033 | { &hf_oran_iSample,
8034 | { "iSample", "oran_fh_cus.iSample",
8035 | FT_FLOAT, BASE_NONE,
8036 | NULL((void*)0), 0x0,
8037 | "In-phase Sample value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8038 | },
8039 |
8040 | /* Section 6.3.3.16 */
8041 | { &hf_oran_qSample,
8042 | { "qSample", "oran_fh_cus.qSample",
8043 | FT_FLOAT, BASE_NONE,
8044 | NULL((void*)0), 0x0,
8045 | "Quadrature Sample value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8046 | },
8047 |
8048 | { &hf_oran_exponent,
8049 | { "Exponent", "oran_fh_cus.exponent",
8050 | FT_UINT8, BASE_DEC,
8051 | NULL((void*)0), 0x0f,
8052 | "Exponent applicable to the I & Q mantissas", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8053 | },
8054 |
8055 | { &hf_oran_iq_user_data,
8056 | { "IQ User Data", "oran_fh_cus.iq_user_data",
8057 | FT_BYTES, BASE_NONE,
8058 | NULL((void*)0), 0x0,
8059 | "Used for the In-phase and Quadrature sample mantissa", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8060 | },
8061 |
8062 |
8063 | { &hf_oran_u_section_ul_symbol_time,
8064 | { "Microseconds since first UL U-plane frame for this symbol", "oran_fh_cus.us-since-first-ul-frame",
8065 | FT_UINT32, BASE_DEC,
8066 | NULL((void*)0), 0x0,
8067 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8068 | },
8069 | { &hf_oran_u_section_ul_symbol_frames,
8070 | { "Number of UL frames sent for this symbol", "oran_fh_cus.number-ul-frames-in-symbol",
8071 | FT_UINT32, BASE_DEC,
8072 | NULL((void*)0), 0x0,
8073 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8074 | },
8075 | { &hf_oran_u_section_ul_symbol_first_frame,
8076 | { "First UL frame for this symbol", "oran_fh_cus.first-ul-frame-in-symbol",
8077 | FT_FRAMENUM, BASE_NONE,
8078 | FRAMENUM_TYPE(FT_FRAMENUM_NONE)((gpointer) (glong) (FT_FRAMENUM_NONE)), 0x0,
8079 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8080 | },
8081 | { &hf_oran_u_section_ul_symbol_last_frame,
8082 | { "Last UL frame for this symbol", "oran_fh_cus.last-ul-frame-in-symbol",
8083 | FT_FRAMENUM, BASE_NONE,
8084 | FRAMENUM_TYPE(FT_FRAMENUM_NONE)((gpointer) (glong) (FT_FRAMENUM_NONE)), 0x0,
8085 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8086 | },
8087 |
8088 | { &hf_oran_c_eAxC_ID,
8089 | { "c_eAxC_ID", "oran_fh_cus.c_eaxc_id",
8090 | FT_STRING, BASE_NONE,
8091 | NULL((void*)0), 0x0,
8092 | "This is a calculated field for the c_eAxC ID, which identifies the message stream", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8093 | },
8094 |
8095 | { &hf_oran_refa,
8096 | { "RefA", "oran_fh_cus.refa",
8097 | FT_STRING, BASE_NONE,
8098 | NULL((void*)0), 0x0,
8099 | "This is a calculated field for the RefA ID, which provides a reference in time", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8100 | },
8101 |
8102 |
8103 | /* Section 7.5.2.15 */
8104 | { &hf_oran_ciCompHdr,
8105 | { "ciCompHdr", "oran_fh_cus.ciCompHdr",
8106 | FT_STRING, BASE_NONE,
8107 | NULL((void*)0), 0x0,
8108 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8109 | },
8110 | { &hf_oran_ciCompHdrMeth,
8111 | { "User Data Compression Method", "oran_fh_cus.ciCompHdrMeth",
8112 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8113 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0e,
8114 | "Defines the compression method for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8115 | },
8116 | { &hf_oran_ciCompHdrIqWidth,
8117 | { "User Data IQ width", "oran_fh_cus.udCompHdrWidth",
8118 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8119 | RVALS(ud_comp_header_width)((0 ? (const struct _range_string*)0 : ((ud_comp_header_width )))), 0xf0,
8120 | "Defines the IQ bit width for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8121 | },
8122 | { &hf_oran_ciCompOpt,
8123 | { "ciCompOpt", "oran_fh_cus.ciCompOpt",
8124 | FT_UINT8, BASE_DEC,
8125 | VALS(ci_comp_opt_vals)((0 ? (const struct _value_string*)0 : ((ci_comp_opt_vals)))), 0x01,
8126 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8127 | },
8128 |
8129 | /* 7.7.11.7 */
8130 | { &hf_oran_disable_bfws,
8131 | { "disableBFWs", "oran_fh_cus.disableBFWs",
8132 | FT_BOOLEAN, 8,
8133 | NULL((void*)0), 0x80,
8134 | "Indicate if BFWs under section extension are disabled", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8135 | },
8136 | /* 7.7.11.8 */
8137 | { &hf_oran_rad,
8138 | { "RAD", "oran_fh_cus.rad",
8139 | FT_BOOLEAN, 8,
8140 | NULL((void*)0), 0x40,
8141 | "Reset After PRB Discontinuity", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8142 | },
8143 | /* 7.7.11.4 */
8144 | { &hf_oran_num_bund_prbs,
8145 | { "numBundPrb", "oran_fh_cus.numBundPrb",
8146 | FT_UINT8, BASE_DEC,
8147 | NULL((void*)0), 0x0,
8148 | "Number of bundled PRBs per BFWs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8149 | },
8150 | { &hf_oran_beam_id,
8151 | { "beamId", "oran_fh_cus.beamId",
8152 | FT_UINT16, BASE_DEC,
8153 | NULL((void*)0), 0x7fff,
8154 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8155 | },
8156 | { &hf_oran_num_weights_per_bundle,
8157 | { "Num weights per bundle", "oran_fh_cus.num_weights_per_bundle",
8158 | FT_UINT16, BASE_DEC,
8159 | NULL((void*)0), 0x0,
8160 | "From dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8161 | },
8162 |
8163 | { &hf_oran_samples_prb,
8164 | {"PRB", "oran_fh_cus.prb",
8165 | FT_STRING, BASE_NONE,
8166 | NULL((void*)0), 0x0,
8167 | "Grouping of samples for a particular Physical Resource Block", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8168 | },
8169 |
8170 | /* 7.5.3.13 */
8171 | { &hf_oran_ciSample,
8172 | { "ciSample", "oran_fh_cus.ciSample",
8173 | FT_STRING, BASE_NONE,
8174 | NULL((void*)0), 0x0,
8175 | "Sample (I and Q values)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8176 | },
8177 | { &hf_oran_ciIsample,
8178 | { "ciIsample", "oran_fh_cus.ciISample",
8179 | FT_FLOAT, BASE_NONE,
8180 | NULL((void*)0), 0x0,
8181 | "Channel information complex value - I part", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8182 | },
8183 | { &hf_oran_ciQsample,
8184 | { "ciQsample", "oran_fh_cus.ciQSample",
8185 | FT_FLOAT, BASE_NONE,
8186 | NULL((void*)0), 0x0,
8187 | "Channel information complex value - Q part", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8188 | },
8189 |
8190 | /* 7.7.10.2 */
8191 | { &hf_oran_beamGroupType,
8192 | { "beamGroupType", "oran_fh_cus.beamGroupType",
8193 | FT_UINT8, BASE_DEC,
8194 | VALS(beam_group_type_vals)((0 ? (const struct _value_string*)0 : ((beam_group_type_vals )))), 0xc0,
8195 | "The type of beam grouping", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8196 | },
8197 | /* 7.7.10.3 */
8198 | { &hf_oran_numPortc,
8199 | { "numPortc", "oran_fh_cus.numPortc",
8200 | FT_UINT8, BASE_DEC,
8201 | NULL((void*)0), 0x3f,
8202 | "The number of eAxC ports", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8203 | },
8204 |
8205 | /* 7.7.4.2 (1 bit) */
8206 | { &hf_oran_csf,
8207 | { "csf", "oran_fh_cus.csf",
8208 | FT_BOOLEAN, BASE_NONE,
8209 | NULL((void*)0), 0x0,
8210 | "constellation shift flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8211 | },
8212 | /* 7.7.4.3 */
8213 | { &hf_oran_modcompscaler,
8214 | { "modCompScaler", "oran_fh_cus.modcompscaler",
8215 | FT_UINT16, BASE_DEC,
8216 | NULL((void*)0), 0x7fff,
8217 | "modulation compression scaler value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8218 | },
8219 |
8220 | /* 7.7.5.1 */
8221 | { &hf_oran_modcomp_param_set,
8222 | { "Set", "oran_fh_cus.modcomp-param-set",
8223 | FT_STRING, BASE_NONE,
8224 | NULL((void*)0), 0x0,
8225 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8226 | },
8227 |
8228 |
8229 |
8230 | /* mcScaleReMask 7.7.5.2 (12 bits) */
8231 |
8232 | /* First entry (starts with msb within byte) */
8233 | { &hf_oran_mc_scale_re_mask_re1,
8234 | { "RE 1", "oran_fh_cus.mcscalermask-RE1",
8235 | FT_BOOLEAN, 16,
8236 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x8000,
8237 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8238 | },
8239 | { &hf_oran_mc_scale_re_mask_re2,
8240 | { "RE 2", "oran_fh_cus.mcscalermask-RE2",
8241 | FT_BOOLEAN, 16,
8242 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x4000,
8243 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8244 | },
8245 | { &hf_oran_mc_scale_re_mask_re3,
8246 | { "RE 3", "oran_fh_cus.mcscalermask-RE3",
8247 | FT_BOOLEAN, 16,
8248 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x2000,
8249 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8250 | },
8251 | { &hf_oran_mc_scale_re_mask_re4,
8252 | { "RE 4", "oran_fh_cus.mcscalermask-RE4",
8253 | FT_BOOLEAN, 16,
8254 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x1000,
8255 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8256 | },
8257 | { &hf_oran_mc_scale_re_mask_re5,
8258 | { "RE 5", "oran_fh_cus.mcscalermask-RE5",
8259 | FT_BOOLEAN, 16,
8260 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0800,
8261 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8262 | },
8263 | { &hf_oran_mc_scale_re_mask_re6,
8264 | { "RE 6", "oran_fh_cus.mcscalermask-RE6",
8265 | FT_BOOLEAN, 16,
8266 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0400,
8267 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8268 | },
8269 | { &hf_oran_mc_scale_re_mask_re7,
8270 | { "RE 7", "oran_fh_cus.mcscalermask-RE7",
8271 | FT_BOOLEAN, 16,
8272 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0200,
8273 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8274 | },
8275 | { &hf_oran_mc_scale_re_mask_re8,
8276 | { "RE 8", "oran_fh_cus.mcscalermask-RE8",
8277 | FT_BOOLEAN, 16,
8278 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0100,
8279 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8280 | },
8281 | { &hf_oran_mc_scale_re_mask_re9,
8282 | { "RE 9", "oran_fh_cus.mcscalermask-RE9",
8283 | FT_BOOLEAN, 16,
8284 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0080,
8285 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8286 | },
8287 | { &hf_oran_mc_scale_re_mask_re10,
8288 | { "RE 10", "oran_fh_cus.mcscalermask-RE10",
8289 | FT_BOOLEAN, 16,
8290 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0040,
8291 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8292 | },
8293 | { &hf_oran_mc_scale_re_mask_re11,
8294 | { "RE 11", "oran_fh_cus.mcscalermask-RE11",
8295 | FT_BOOLEAN, 16,
8296 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0020,
8297 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8298 | },
8299 | { &hf_oran_mc_scale_re_mask_re12,
8300 | { "RE 12", "oran_fh_cus.mcscalermask-RE12",
8301 | FT_BOOLEAN, 16,
8302 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0010,
8303 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8304 | },
8305 |
8306 | /* Even tries entry (starts with 5th bit within byte) */
8307 | { &hf_oran_mc_scale_re_mask_re1_even,
8308 | { "RE 1", "oran_fh_cus.mcscalermask-RE1",
8309 | FT_BOOLEAN, 16,
8310 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0800,
8311 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8312 | },
8313 | { &hf_oran_mc_scale_re_mask_re2_even,
8314 | { "RE 2", "oran_fh_cus.mcscalermask-RE2",
8315 | FT_BOOLEAN, 16,
8316 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0400,
8317 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8318 | },
8319 | { &hf_oran_mc_scale_re_mask_re3_even,
8320 | { "RE 3", "oran_fh_cus.mcscalermask-RE3",
8321 | FT_BOOLEAN, 16,
8322 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0200,
8323 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8324 | },
8325 | { &hf_oran_mc_scale_re_mask_re4_even,
8326 | { "RE 4", "oran_fh_cus.mcscalermask-RE4",
8327 | FT_BOOLEAN, 16,
8328 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0100,
8329 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8330 | },
8331 | { &hf_oran_mc_scale_re_mask_re5_even,
8332 | { "RE 5", "oran_fh_cus.mcscalermask-RE5",
8333 | FT_BOOLEAN, 16,
8334 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0080,
8335 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8336 | },
8337 | { &hf_oran_mc_scale_re_mask_re6_even,
8338 | { "RE 6", "oran_fh_cus.mcscalermask-RE6",
8339 | FT_BOOLEAN, 16,
8340 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0040,
8341 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8342 | },
8343 | { &hf_oran_mc_scale_re_mask_re7_even,
8344 | { "RE 7", "oran_fh_cus.mcscalermask-RE7",
8345 | FT_BOOLEAN, 16,
8346 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0020,
8347 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8348 | },
8349 | { &hf_oran_mc_scale_re_mask_re8_even,
8350 | { "RE 8", "oran_fh_cus.mcscalermask-RE8",
8351 | FT_BOOLEAN, 16,
8352 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0010,
8353 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8354 | },
8355 | { &hf_oran_mc_scale_re_mask_re9_even,
8356 | { "RE 9", "oran_fh_cus.mcscalermask-RE9",
8357 | FT_BOOLEAN, 16,
8358 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0008,
8359 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8360 | },
8361 | { &hf_oran_mc_scale_re_mask_re10_even,
8362 | { "RE 10", "oran_fh_cus.mcscalermask-RE10",
8363 | FT_BOOLEAN, 16,
8364 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0004,
8365 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8366 | },
8367 | { &hf_oran_mc_scale_re_mask_re11_even,
8368 | { "RE 11", "oran_fh_cus.mcscalermask-RE11",
8369 | FT_BOOLEAN, 16,
8370 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0002,
8371 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8372 | },
8373 | { &hf_oran_mc_scale_re_mask_re12_even,
8374 | { "RE 12", "oran_fh_cus.mcscalermask-RE12",
8375 | FT_BOOLEAN, 16,
8376 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0001,
8377 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8378 | },
8379 |
8380 | { &hf_oran_mc_scale_re_mask,
8381 | { "mcScaleReMask", "oran_fh_cus.mcscaleremask",
8382 | FT_UINT16, BASE_HEX,
8383 | NULL((void*)0), 0xfff0,
8384 | "modulation compression power scale RE mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8385 | },
8386 | { &hf_oran_mc_scale_re_mask_even,
8387 | { "mcScaleReMask", "oran_fh_cus.mcscaleremask",
8388 | FT_UINT16, BASE_HEX,
8389 | NULL((void*)0), 0x0fff,
8390 | "modulation compression power scale RE mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8391 | },
8392 |
8393 | /* mcScaleOffset 7.7.5.4 (15 bits) */
8394 | { &hf_oran_mc_scale_offset,
8395 | { "mcScaleOffset", "oran_fh_cus.mcscaleoffset",
8396 | FT_UINT24, BASE_DEC,
8397 | NULL((void*)0), 0x0,
8398 | "scaling value for modulation compression", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8399 | },
8400 | /* eAxCmask (7.7.7.2) */
8401 | { &hf_oran_eAxC_mask,
8402 | { "eAxC Mask", "oran_fh_cus.eaxcmask",
8403 | FT_UINT16, BASE_HEX,
8404 | NULL((void*)0), 0xffff,
8405 | "Which eAxC_ID values the C-Plane message applies to", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8406 | },
8407 | /* technology (interface name) 7.7.9.2 */
8408 | { &hf_oran_technology,
8409 | { "Technology", "oran_fh_cus.technology",
8410 | FT_UINT8, BASE_DEC,
8411 | VALS(interface_name_vals)((0 ? (const struct _value_string*)0 : ((interface_name_vals) ))), 0x0,
8412 | "Interface name (that C-PLane section applies to)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8413 | },
8414 | /* Exttype 14 (7.7.14.2) */
8415 | { &hf_oran_nullLayerInd,
8416 | { "nullLayerInd", "oran_fh_cus.nulllayerind",
8417 | FT_BOOLEAN, BASE_NONE,
8418 | NULL((void*)0), 0x0,
8419 | "Whether corresponding layer is nulling-layer or not", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8420 | },
8421 |
8422 | /* Exttype 19 */
8423 | /* 7.7.19.3 */
8424 | { &hf_oran_se19_repetition,
8425 | { "repetition", "oran_fh_cus.repetition",
8426 | FT_BOOLEAN, BASE_NONE,
8427 | TFS(&repetition_se19_tfs)((0 ? (const struct true_false_string*)0 : ((&repetition_se19_tfs )))), 0x0,
8428 | "repeat port info flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8429 | },
8430 | /* 7.7.19.8 */
8431 | /* TODO: break down into each RE as done for 7.5.3.5 ? */
8432 | { &hf_oran_portReMask,
8433 | { "portReMask", "oran_fh_cus.portReMask",
8434 | FT_BOOLEAN, 16,
8435 | TFS(&tfs_set_notset)((0 ? (const struct true_false_string*)0 : ((&tfs_set_notset )))), 0x0fff,
8436 | "RE bitmask per port", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8437 | },
8438 | /* 7.7.19.9 */
8439 | { &hf_oran_portSymbolMask,
8440 | { "portSymbolMask", "oran_fh_cus.portSymbolMask",
8441 | FT_BOOLEAN, 16,
8442 | TFS(&tfs_set_notset)((0 ? (const struct true_false_string*)0 : ((&tfs_set_notset )))), 0x3fff,
8443 | "Symbol bitmask port port", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8444 | },
8445 |
8446 | { &hf_oran_ext19_port,
8447 | {"Port", "oran_fh_cus.ext19.port",
8448 | FT_STRING, BASE_NONE,
8449 | NULL((void*)0), 0x0,
8450 | "Entry for a given port in ext19", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8451 | },
8452 |
8453 | /* Ext 13 */
8454 | { &hf_oran_prb_allocation,
8455 | {"PRB allocation", "oran_fh_cus.prb-allocation",
8456 | FT_STRING, BASE_NONE,
8457 | NULL((void*)0), 0x0,
8458 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8459 | },
8460 | /* 7.7.13.2 */
8461 | { &hf_oran_nextSymbolId,
8462 | { "nextSymbolId", "oran_fh_cus.nextSymbolId",
8463 | FT_UINT8, BASE_DEC,
8464 | NULL((void*)0), 0x3c,
8465 | "offset of PRB range start", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8466 | },
8467 | /* 7.7.13.3 */
8468 | { &hf_oran_nextStartPrbc,
8469 | { "nextStartPrbc", "oran_fh_cus.nextStartPrbc",
8470 | FT_UINT16, BASE_DEC,
8471 | NULL((void*)0), 0x03ff,
8472 | "number of PRBs in PRB range", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8473 | },
8474 |
8475 | /* Puncturing patters as appears in SE 20 */
8476 | { &hf_oran_puncPattern,
8477 | { "puncPattern", "oran_fh_cus.puncPattern",
8478 | FT_STRING, BASE_NONE,
8479 | NULL((void*)0), 0x0,
8480 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8481 | },
8482 |
8483 | /* 7.7.20.2 numPuncPatterns */
8484 | { &hf_oran_numPuncPatterns,
8485 | { "numPuncPatterns", "oran_fh_cus.numPuncPatterns",
8486 | FT_UINT8, BASE_DEC,
8487 | NULL((void*)0), 0x0,
8488 | "number of puncturing patterns", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8489 | },
8490 | /* 7.7.20.3 symbolMask */
8491 | { &hf_oran_symbolMask_ext20,
8492 | { "symbolMask", "oran_fh_cus.symbolMask",
8493 | FT_UINT16, BASE_HEX,
8494 | NULL((void*)0), 0xfffc,
8495 | "Bitmask where each bit indicates the symbols associated with the puncturing pattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8496 | },
8497 | /* 7.7.20.4 startPuncPrb */
8498 | { &hf_oran_startPuncPrb,
8499 | { "startPuncPrb", "oran_fh_cus.startPuncPrb",
8500 | FT_UINT16, BASE_DEC,
8501 | NULL((void*)0), 0x03ff,
8502 | "starting PRB to which one puncturing pattern applies", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8503 | },
8504 | /* 7.7.20.5 numPuncPrb */
8505 | { &hf_oran_numPuncPrb,
8506 | { "numPuncPrb", "oran_fh_cus.numPuncPrb",
8507 | FT_UINT8, BASE_DEC,
8508 | NULL((void*)0), 0x0,
8509 | "the number of PRBs of the puncturing pattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8510 | },
8511 | /* 7.7.20.6 puncReMask */
8512 | { &hf_oran_puncReMask,
8513 | { "puncReMask", "oran_fh_cus.puncReMask",
8514 | FT_UINT16, BASE_DEC,
8515 | NULL((void*)0), 0xffc0,
8516 | "puncturing pattern RE mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8517 | },
8518 | /* 7.7.20.12 multiSDScope */
8519 | { &hf_oran_multiSDScope,
8520 | { "multiSDScope", "oran_fh_cus.multiSDScope",
8521 | FT_BOOLEAN, 8,
8522 | TFS(&multi_sd_scope_tfs)((0 ? (const struct true_false_string*)0 : ((&multi_sd_scope_tfs )))), 0x02,
8523 | "multiple section description scope flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8524 | },
8525 | /* 7.7.20.4 rbgIncl */
8526 | { &hf_oran_RbgIncl,
8527 | { "rbgIncl", "oran_fh_cus.rbgIncl",
8528 | FT_BOOLEAN, 8,
8529 | NULL((void*)0), 0x01,
8530 | "rbg included flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8531 | },
8532 |
8533 | /* 7.7.21.2 ciPrbGroupSize */
8534 | { &hf_oran_ci_prb_group_size,
8535 | { "ciPrbGroupSize", "oran_fh_cus.ciPrbGroupSize",
8536 | FT_UINT8, BASE_DEC,
8537 | NULL((void*)0), 0x0,
8538 | "channel information PRB group size", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8539 | },
8540 | /* 7.21.3 */
8541 | { &hf_oran_prg_size_st5,
8542 | { "prgSize", "oran_fh_cus.prgSize",
8543 | FT_UINT8, BASE_DEC,
8544 | VALS(prg_size_st5_vals)((0 ? (const struct _value_string*)0 : ((prg_size_st5_vals))) ), 0x03,
8545 | "precoding resource block group size", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8546 | },
8547 | { &hf_oran_prg_size_st6,
8548 | { "prgSize", "oran_fh_cus.prgSize",
8549 | FT_UINT8, BASE_DEC,
8550 | VALS(prg_size_st6_vals)((0 ? (const struct _value_string*)0 : ((prg_size_st6_vals))) ), 0x03,
8551 | "precoding resource block group size", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8552 | },
8553 |
8554 | /* 7.7.17.2 numUeID */
8555 | { &hf_oran_num_ueid,
8556 | { "numUeID", "oran_fh_cus.numUeID",
8557 | FT_UINT8, BASE_DEC,
8558 | NULL((void*)0), 0x0,
8559 | "number of ueIDs per user", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8560 | },
8561 |
8562 | /* 7.7.16.2 antMask */
8563 | { &hf_oran_antMask,
8564 | { "antMask", "oran_fh_cus.antMask",
8565 | FT_UINT64, BASE_HEX,
8566 | NULL((void*)0), 0xffffffffffffffff,
8567 | "indices of antennas to be pre-combined per RX endpoint", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8568 | },
8569 |
8570 | /* 7.7.18.2 transmissionWindowOffset */
8571 | { &hf_oran_transmissionWindowOffset,
8572 | { "transmissionWindowOffset", "oran_fh_cus.transmissionWindowOffset",
8573 | FT_UINT16, BASE_DEC,
8574 | NULL((void*)0), 0x0,
8575 | "start of the transmission window as an offset to when the transmission window would have been without this parameter, i.e. (Ta3_max - Ta3_min)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8576 | },
8577 | /* 7.7.18.3 transmissionWindowSize */
8578 | { &hf_oran_transmissionWindowSize,
8579 | { "transmissionWindowSize", "oran_fh_cus.transmissionWindowSize",
8580 | FT_UINT16, BASE_DEC,
8581 | NULL((void*)0), 0x3fff,
8582 | "size of the transmission window in resolution µs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8583 | },
8584 | /* 7.7.18.4 toT */
8585 | { &hf_oran_toT,
8586 | { "toT", "oran_fh_cus.toT",
8587 | FT_UINT8, BASE_DEC,
8588 | VALS(type_of_transmission_vals)((0 ? (const struct _value_string*)0 : ((type_of_transmission_vals )))), 0x03,
8589 | "type of transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8590 | },
8591 |
8592 | /* 7.7.2.2 bfaCompHdr */
8593 | { &hf_oran_bfaCompHdr,
8594 | { "bfaCompHdr", "oran_fh_cus.bfaCompHdr",
8595 | FT_STRING, BASE_NONE,
8596 | NULL((void*)0), 0x0,
8597 | "beamforming attributes compression header", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8598 | },
8599 | /* 7.7.2.2-2: bfAzPtWidth */
8600 | { &hf_oran_bfAzPtWidth,
8601 | { "bfAzPtWidth", "oran_fh_cus.bfAzPtWidth",
8602 | FT_UINT8, BASE_DEC,
8603 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x38,
8604 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8605 | },
8606 | /* 7.7.2.2-3: bfZePtWidth */
8607 | { &hf_oran_bfZePtWidth,
8608 | { "bfZePtWidth", "oran_fh_cus.bfZePtWidth",
8609 | FT_UINT8, BASE_DEC,
8610 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x07,
8611 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8612 | },
8613 | /* 7.7.2.2-4: bfAz3ddWidth */
8614 | { &hf_oran_bfAz3ddWidth,
8615 | { "bfAz3ddWidth", "oran_fh_cus.bfAz3ddWidth",
8616 | FT_UINT8, BASE_DEC,
8617 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x38,
8618 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8619 | },
8620 | /* 7.7.2.2-5: bfZe3ddWidth */
8621 | { &hf_oran_bfZe3ddWidth,
8622 | { "bfZe3ddWidth", "oran_fh_cus.bfZe3ddWidth",
8623 | FT_UINT8, BASE_DEC,
8624 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x07,
8625 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8626 | },
8627 |
8628 | /* 7.7.2.3 bfAzPt */
8629 | { &hf_oran_bfAzPt,
8630 | { "bfAzPt", "oran_fh_cus.bfAzPt",
8631 | FT_UINT8, BASE_DEC,
8632 | NULL((void*)0), 0x0,
8633 | "beamforming azimuth pointing parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8634 | },
8635 | /* 7.7.2.4 bfZePt */
8636 | { &hf_oran_bfZePt,
8637 | { "bfZePt", "oran_fh_cus.bfZePt",
8638 | FT_UINT8, BASE_DEC,
8639 | NULL((void*)0), 0x0,
8640 | "beamforming zenith pointing parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8641 | },
8642 | /* 7.7.2.5 bfAz3dd */
8643 | { &hf_oran_bfAz3dd,
8644 | { "bfAz3dd", "oran_fh_cus.bfAz3dd",
8645 | FT_UINT8, BASE_DEC,
8646 | NULL((void*)0), 0x0,
8647 | "beamforming azimuth beamwidth parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8648 | },
8649 | /* 7.7.2.6 bfZe3dd */
8650 | { &hf_oran_bfZe3dd,
8651 | { "bfZe3dd", "oran_fh_cus.bfZe3dd",
8652 | FT_UINT8, BASE_DEC,
8653 | NULL((void*)0), 0x0,
8654 | "beamforming zenith beamwidth parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8655 | },
8656 |
8657 | /* 7.7.2.7 bfAzSl */
8658 | { &hf_oran_bfAzSl,
8659 | { "bfAzSl", "oran_fh_cus.bfAzSl",
8660 | FT_UINT8, BASE_DEC,
8661 | VALS(sidelobe_suppression_vals)((0 ? (const struct _value_string*)0 : ((sidelobe_suppression_vals )))), 0x38,
8662 | "beamforming azimuth sidelobe parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8663 | },
8664 | /* 7.7.2.8 bfZeSl */
8665 | { &hf_oran_bfZeSl,
8666 | { "bfZeSl", "oran_fh_cus.bfZeSl",
8667 | FT_UINT8, BASE_DEC,
8668 | VALS(sidelobe_suppression_vals)((0 ? (const struct _value_string*)0 : ((sidelobe_suppression_vals )))), 0x07,
8669 | "beamforming zenith sidelobe parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8670 | },
8671 |
8672 | /* 7.5.2.17 */
8673 | { &hf_oran_cmd_scope,
8674 | { "cmdScope", "oran_fh_cus.cmdScope",
8675 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8676 | RVALS(cmd_scope_vals)((0 ? (const struct _range_string*)0 : ((cmd_scope_vals)))), 0x0f,
8677 | "command scope", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8678 | },
8679 | /* 7.5.2.18 */
8680 | { &hf_oran_number_of_st4_cmds,
8681 | { "numberOfST4Cmds", "oran_fh_cus.numberOfST4Cmds",
8682 | FT_UINT8, BASE_DEC,
8683 | NULL((void*)0), 0x0,
8684 | "Number of Section Type 4 commands", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8685 | },
8686 |
8687 | { &hf_oran_st4_cmd_header,
8688 | { "Command common header", "oran_fh_cus.st4CmdCommonHeader",
8689 | FT_STRING, BASE_NONE,
8690 | NULL((void*)0), 0x0,
8691 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8692 | },
8693 |
8694 | /* 7.5.3.38 */
8695 | { &hf_oran_st4_cmd_type,
8696 | { "st4CmdType", "oran_fh_cus.st4CmdType",
8697 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8698 | RVALS(st4_cmd_type_vals)((0 ? (const struct _range_string*)0 : ((st4_cmd_type_vals))) ), 0x0,
8699 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8700 | },
8701 | /* 7.5.3.39 */
8702 | { &hf_oran_st4_cmd_len,
8703 | { "st4CmdLen", "oran_fh_cus.st4CmdLen",
8704 | FT_UINT16, BASE_DEC,
8705 | NULL((void*)0), 0x0,
8706 | "Length of command in 32-bit words", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8707 | },
8708 | /* 7.5.3.40 */
8709 | { &hf_oran_st4_cmd_num_slots,
8710 | { "numSlots", "oran_fh_cus.st4NumSlots",
8711 | FT_UINT8, BASE_DEC,
8712 | NULL((void*)0), 0x0,
8713 | "Contiguous slots for which command is applicable", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8714 | },
8715 | /* 7.5.3.41 */
8716 | { &hf_oran_st4_cmd_ack_nack_req_id,
8717 | { "ackNackReqId", "oran_fh_cus.ackNackReqId",
8718 | FT_UINT16, BASE_DEC,
8719 | NULL((void*)0), 0x0,
8720 | "ACK/NACK Request Id", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8721 | },
8722 |
8723 | { &hf_oran_st4_cmd,
8724 | { "Command", "oran_fh_cus.st4Cmd",
8725 | FT_STRING, BASE_NONE,
8726 | NULL((void*)0), 0x0,
8727 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8728 | },
8729 |
8730 | /* 7.5.3.52 */
8731 | { &hf_oran_sleepmode_trx,
8732 | { "sleepMode", "oran_fh_cus.sleepMode",
8733 | FT_UINT8, BASE_HEX,
8734 | VALS(sleep_mode_trx_vals)((0 ? (const struct _value_string*)0 : ((sleep_mode_trx_vals) ))), 0x03,
8735 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8736 | },
8737 | { &hf_oran_sleepmode_asm,
8738 | { "sleepMode", "oran_fh_cus.sleepMode",
8739 | FT_UINT8, BASE_HEX,
8740 | VALS(sleep_mode_asm_vals)((0 ? (const struct _value_string*)0 : ((sleep_mode_asm_vals) ))), 0x03,
8741 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8742 | },
8743 |
8744 | /* 7.5.3.51 */
8745 | { &hf_oran_log2maskbits,
8746 | { "log2MaskBits", "oran_fh_cus.log2MaskBits",
8747 | FT_UINT8, BASE_HEX,
8748 | VALS(log2maskbits_vals)((0 ? (const struct _value_string*)0 : ((log2maskbits_vals))) ), 0x3c,
8749 | "Number of bits to appear in antMask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8750 | },
8751 | /* 7.5.3.53 */
8752 | { &hf_oran_num_slots_ext,
8753 | { "numSlotsExt", "oran_fh_cus.numSlotsExt",
8754 | FT_UINT24, BASE_HEX,
8755 | NULL((void*)0), 0x0fffff,
8756 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8757 | },
8758 | /* 7.5.3.54 */
8759 | { &hf_oran_antMask_trx_control,
8760 | { "antMask", "oran_fh_cus.trxControl.antMask",
8761 | FT_BYTES, BASE_NONE,
8762 | NULL((void*)0), 0x0,
8763 | "which antennas should sleep or wake-up", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8764 | },
8765 | /* 7.5.3.55 */
8766 | { &hf_oran_ready,
8767 | { "ready", "oran_fh_cus.ready",
8768 | FT_BOOLEAN, 8,
8769 | TFS(&ready_tfs)((0 ? (const struct true_false_string*)0 : ((&ready_tfs)) )), 0x01,
8770 | "wake-up ready indicator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8771 | },
8772 | /* 7.5.3.34 */
8773 | { &hf_oran_number_of_acks,
8774 | { "numberOfAcks", "oran_fh_cus.numberOfAcks",
8775 | FT_UINT8, BASE_DEC,
8776 | NULL((void*)0), 0x0,
8777 | "number of ACKs for one eAxC_ID", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8778 | },
8779 | /* 7.5.3.35 */
8780 | { &hf_oran_number_of_nacks,
8781 | { "numberOfNacks", "oran_fh_cus.numberOfNacks",
8782 | FT_UINT8, BASE_DEC,
8783 | NULL((void*)0), 0x0,
8784 | "number of NACKs for one eAxC_ID", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8785 | },
8786 | /* 7.5.3.36 */
8787 | { &hf_oran_ackid,
8788 | { "ackId", "oran_fh_cus.ackId",
8789 | FT_UINT16, BASE_DEC,
8790 | NULL((void*)0), 0x0,
8791 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8792 | },
8793 | /* 7.5.3.37 */
8794 | { &hf_oran_nackid,
8795 | { "nackId", "oran_fh_cus.nackId",
8796 | FT_UINT16, BASE_DEC,
8797 | NULL((void*)0), 0x0,
8798 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8799 | },
8800 |
8801 | /* Links between acknack requests & responses */
8802 | { &hf_oran_acknack_request_frame,
8803 | { "Request Frame", "oran_fh_cus.ackNackId.request-frame",
8804 | FT_FRAMENUM, BASE_NONE,
8805 | FRAMENUM_TYPE(FT_FRAMENUM_REQUEST)((gpointer) (glong) (FT_FRAMENUM_REQUEST)), 0x0,
8806 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8807 | },
8808 | { &hf_oran_acknack_request_time,
8809 | { "Time since request in ms", "oran_fh_cus.ackNackId.time-since-request",
8810 | FT_UINT32, BASE_DEC,
8811 | NULL((void*)0), 0x0,
8812 | "Time between request and response", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8813 | },
8814 | { &hf_oran_acknack_request_type,
8815 | { "Request Type", "oran_fh_cus.ackNackId.request-type",
8816 | FT_UINT32, BASE_DEC,
8817 | VALS(acknack_type_vals)((0 ? (const struct _value_string*)0 : ((acknack_type_vals))) ), 0x0,
8818 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8819 | },
8820 | { &hf_oran_acknack_response_frame,
8821 | { "Response Frame", "oran_fh_cus.ackNackId.response-frame",
8822 | FT_FRAMENUM, BASE_NONE,
8823 | FRAMENUM_TYPE(FT_FRAMENUM_RESPONSE)((gpointer) (glong) (FT_FRAMENUM_RESPONSE)), 0x0,
8824 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8825 | },
8826 | { &hf_oran_acknack_response_time,
8827 | { "Time to response in ms", "oran_fh_cus.ackNackId.time-to-response",
8828 | FT_UINT32, BASE_DEC,
8829 | NULL((void*)0), 0x0,
8830 | "Time between request and response", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8831 | },
8832 |
8833 | /* 7.5.3.43 */
8834 | { &hf_oran_disable_tdbfns,
8835 | { "disableTDBFNs", "oran_fh_cus.disableTDBFNs",
8836 | FT_BOOLEAN, 8,
8837 | TFS(&disable_tdbfns_tfs)((0 ? (const struct true_false_string*)0 : ((&disable_tdbfns_tfs )))), 0x80,
8838 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8839 | },
8840 |
8841 | /* 7.5.3.44 */
8842 | { &hf_oran_td_beam_group,
8843 | { "tdBeamGrp", "oran_fh_cus.tdBeamGrp",
8844 | FT_UINT16, BASE_HEX,
8845 | NULL((void*)0), 0x7fff,
8846 | "Applies to symbolMask in command header", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8847 | },
8848 | /* 7.5.3.43 */
8849 | { &hf_oran_disable_tdbfws,
8850 | { "disableTDBFWs", "oran_fh_cus.disableTDBFWs",
8851 | FT_BOOLEAN, 8,
8852 | TFS(&beam_numbers_included_tfs)((0 ? (const struct true_false_string*)0 : ((&beam_numbers_included_tfs )))), 0x80,
8853 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8854 | },
8855 |
8856 | /* 7.5.3.56 */
8857 | { &hf_oran_td_beam_num,
8858 | { "tdBeamNum", "oran_fh_cus.tdBeamNum",
8859 | FT_UINT16, BASE_HEX,
8860 | NULL((void*)0), 0x7fff,
8861 | "time-domain beam number", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8862 | },
8863 |
8864 | /* 7.5.3.49 */
8865 | { &hf_oran_dir_pattern,
8866 | { "dirPattern", "oran_fh_cus.dirPattern",
8867 | FT_BOOLEAN, 16,
8868 | TFS(&symbol_direction_tfs)((0 ? (const struct true_false_string*)0 : ((&symbol_direction_tfs )))), 0x3fff,
8869 | "symbol data direction (gNB Tx/Rx) pattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8870 | },
8871 | /* 7.5.3.50 */
8872 | { &hf_oran_guard_pattern,
8873 | { "guardPattern", "oran_fh_cus.guardPattern",
8874 | FT_BOOLEAN, 16,
8875 | TFS(&symbol_guard_tfs)((0 ? (const struct true_false_string*)0 : ((&symbol_guard_tfs )))), 0x3fff,
8876 | "guard pattern bitmask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8877 | },
8878 |
8879 | /* For convenient filtering */
8880 | { &hf_oran_cplane,
8881 | { "C-Plane", "oran_fh_cus.c-plane",
8882 | FT_NONE, BASE_NONE,
8883 | NULL((void*)0), 0x0,
8884 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8885 | },
8886 | { &hf_oran_uplane,
8887 | { "U-Plane", "oran_fh_cus.u-plane",
8888 | FT_NONE, BASE_NONE,
8889 | NULL((void*)0), 0x0,
8890 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8891 | },
8892 | { &hf_oran_bf,
8893 | { "BeamForming", "oran_fh_cus.bf",
8894 | FT_NONE, BASE_NONE,
8895 | NULL((void*)0), 0x0,
8896 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8897 | },
8898 | { &hf_oran_zero_prb,
8899 | { "Zero PRB", "oran_fh_cus.zero-prb",
8900 | FT_NONE, BASE_NONE,
8901 | NULL((void*)0), 0x0,
8902 | "All of the REs in this PRB are zero", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8903 | },
8904 |
8905 | /* 5.1.3.2.7 */
8906 | { &hf_oran_ecpri_pcid,
8907 | { "ecpriPcid", "oran_fh_cus.ecpriPcid",
8908 | FT_NONE, BASE_NONE,
8909 | NULL((void*)0), 0x0,
8910 | "IQ data transfer message series identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8911 | },
8912 | { &hf_oran_ecpri_rtcid,
8913 | { "ecpriRtcid", "oran_fh_cus.ecpriRtcid",
8914 | FT_NONE, BASE_NONE,
8915 | NULL((void*)0), 0x0,
8916 | "Real time control data identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8917 | },
8918 | /* 5.1.3.2.8 */
8919 | { &hf_oran_ecpri_seqid,
8920 | { "ecpriSeqid", "oran_fh_cus.ecpriSeqid",
8921 | FT_NONE, BASE_NONE,
8922 | NULL((void*)0), 0x0,
8923 | "message identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8924 | },
8925 |
8926 | /* 7.7.23.2 */
8927 | { &hf_oran_num_sym_prb_pattern,
8928 | { "numSymPrbPattern", "oran_fh_cus.numSymPrbPattern",
8929 | FT_UINT8, BASE_DEC,
8930 | NULL((void*)0), 0xf0,
8931 | "number of symbol and resource block patterns", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8932 | },
8933 | /* 7.7.23.11 */
8934 | { &hf_oran_prb_mode,
8935 | { "prbMode", "oran_fh_cus.prbMode",
8936 | FT_BOOLEAN, 8,
8937 | TFS(&prb_mode_tfs)((0 ? (const struct true_false_string*)0 : ((&prb_mode_tfs )))), 0x01,
8938 | "PRB Mode", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8939 | },
8940 |
8941 | { &hf_oran_sym_prb_pattern,
8942 | { "symPrbPattern", "oran_fh_cus.symPrbPattern",
8943 | FT_STRING, BASE_NONE,
8944 | NULL((void*)0), 0x0,
8945 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8946 | },
8947 |
8948 | /* 7.7.23.3 */
8949 | { &hf_oran_sym_mask,
8950 | { "symMask", "oran_fh_cus.symMask",
8951 | FT_UINT16, BASE_HEX,
8952 | NULL((void*)0), 0x3fff,
8953 | "symbol mask part of symPrbPattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8954 | },
8955 | /* 7.7.23.5 */
8956 | {&hf_oran_num_mc_scale_offset,
8957 | {"numMcScaleOffset", "oran_fh_cus.numMcScaleOffset",
8958 | FT_UINT8, BASE_DEC,
8959 | NULL((void*)0), 0xf0,
8960 | "number of modulation compression scaling value per symPrbPattern",
8961 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8962 | },
8963 | /* 7.7.23.4 */
8964 | { &hf_oran_prb_pattern,
8965 | { "prbPattern", "oran_fh_cus.prbPattern",
8966 | FT_UINT8, BASE_DEC,
8967 | NULL((void*)0), 0x0f,
8968 | "resource block pattern part of symPrbPattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8969 | },
8970 |
8971 | /* 7.7.3.2 */
8972 | { &hf_oran_codebook_index,
8973 | { "codebookIndex", "oran_fh_cus.codebookIndex",
8974 | FT_UINT8, BASE_DEC,
8975 | NULL((void*)0), 0x0,
8976 | "precoder codebook used for transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8977 | },
8978 | /* 7.7.3.3 */
8979 | { &hf_oran_layerid,
8980 | { "layerID", "oran_fh_cus.layerID",
8981 | FT_UINT8, BASE_DEC,
8982 | NULL((void*)0), 0xf0,
8983 | "Layer ID for DL transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8984 | },
8985 | /* 7.7.3.5 */
8986 | { &hf_oran_numlayers,
8987 | { "numLayers", "oran_fh_cus.numLayers",
8988 | FT_UINT8, BASE_DEC,
8989 | NULL((void*)0), 0x0f,
8990 | "number of layers for DL transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8991 | },
8992 | /* 7.7.3.4 */
8993 | { &hf_oran_txscheme,
8994 | { "txScheme", "oran_fh_cus.txScheme",
8995 | FT_UINT8, BASE_DEC,
8996 | NULL((void*)0), 0xf0,
8997 | "transmission scheme", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8998 | },
8999 | /* 7.7.3.6 */
9000 | { &hf_oran_crs_remask,
9001 | { "crsReMask", "oran_fh_cus.crsReMask",
9002 | FT_UINT16, BASE_HEX,
9003 | NULL((void*)0), 0x0fff,
9004 | "CRS resource element mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9005 | },
9006 | /* 7.7.3.8 */
9007 | { &hf_oran_crs_shift,
9008 | { "crsShift", "oran_fh_cus.crsShift",
9009 | FT_UINT8, BASE_HEX,
9010 | NULL((void*)0), 0x80,
9011 | "CRS resource element mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9012 | },
9013 | /* 7.7.3.7 */
9014 | { &hf_oran_crs_symnum,
9015 | { "crsSymNum", "oran_fh_cus.crsSymNum",
9016 | FT_UINT8, BASE_DEC,
9017 | NULL((void*)0), 0x0f,
9018 | "CRS symbol number indication", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9019 | },
9020 | /* 7.7.3.9 */
9021 | { &hf_oran_beamid_ap1,
9022 | { "beamIdAP1", "oran_fh_cus.beamIdAP1",
9023 | FT_UINT16, BASE_DEC,
9024 | NULL((void*)0), 0x7f,
9025 | "beam id to be used for antenna port 1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9026 | },
9027 | /* 7.7.3.10 */
9028 | { &hf_oran_beamid_ap2,
9029 | { "beamIdAP2", "oran_fh_cus.beamIdAP2",
9030 | FT_UINT16, BASE_DEC,
9031 | NULL((void*)0), 0x7f,
9032 | "beam id to be used for antenna port 2", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9033 | },
9034 | /* 7.7.3.11 */
9035 | { &hf_oran_beamid_ap3,
9036 | { "beamIdAP3", "oran_fh_cus.beamIdAP3",
9037 | FT_UINT16, BASE_DEC,
9038 | NULL((void*)0), 0x7f,
9039 | "beam id to be used for antenna port 3", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9040 | },
9041 |
9042 | /* 7.7.10.3a */
9043 | { &hf_oran_port_list_index,
9044 | { "portListIndex", "oran_fh_cus.portListIndex",
9045 | FT_UINT8, BASE_DEC,
9046 | NULL((void*)0), 0x0,
9047 | "the index of an eAxC_ID in the port-list", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9048 | },
9049 |
9050 | { &hf_oran_alpn_per_sym,
9051 | { "alpnPerSym", "oran_fh_cus.alpnPerSym",
9052 | FT_UINT8, BASE_HEX,
9053 | VALS(alpn_per_sym_vals)((0 ? (const struct _value_string*)0 : ((alpn_per_sym_vals))) ), 0x80,
9054 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9055 | },
9056 | { &hf_oran_ant_dmrs_snr,
9057 | { "antDmrsSnr", "oran_fh_cus.antDmrsSnr",
9058 | FT_UINT8, BASE_HEX,
9059 | VALS(ant_dmrs_snr_vals)((0 ? (const struct _value_string*)0 : ((ant_dmrs_snr_vals))) ), 0x40,
9060 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9061 | },
9062 |
9063 | /* 7.7.24.6 */
9064 | { &hf_oran_user_group_size,
9065 | { "userGroupSize", "oran_fh_cus.userGroupSize",
9066 | FT_UINT8, BASE_DEC,
9067 | NULL((void*)0), 0x1f,
9068 | "number of UE data layers in the user group identified by userGroupId", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9069 | },
9070 | /* 7.7.24.7 */
9071 | { &hf_oran_user_group_id,
9072 | { "userGroupId", "oran_fh_cus.userGroupId",
9073 | FT_UINT8, BASE_DEC,
9074 | NULL((void*)0), 0x0,
9075 | "indicates user group described by the section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9076 | },
9077 | /* 7.7.24.8 */
9078 | { &hf_oran_entry_type,
9079 | { "entryType", "oran_fh_cus.entryType",
9080 | FT_UINT8, BASE_DEC,
9081 | VALS(entry_type_vals)((0 ? (const struct _value_string*)0 : ((entry_type_vals)))), 0xe0,
9082 | "indicates format of the entry", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9083 | },
9084 | /* 7.7.24.9 */
9085 | { &hf_oran_dmrs_port_number,
9086 | { "dmrsPortNumber", "oran_fh_cus.dmrsPortNumber",
9087 | FT_UINT8, BASE_DEC,
9088 | NULL((void*)0), 0x1f,
9089 | "DMRS antenna port number for the associated ueId", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9090 | },
9091 | /* 7.7.24.10 */
9092 | { &hf_oran_ueid_reset,
9093 | { "ueidReset", "oran_fh_cus.ueidReset",
9094 | FT_BOOLEAN, 8,
9095 | TFS(&tfs_ueid_reset)((0 ? (const struct true_false_string*)0 : ((&tfs_ueid_reset )))), 0x80,
9096 | "same UEID as the previous slot", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9097 | },
9098 | /* 7.7.24.11 */
9099 | { &hf_oran_dmrs_symbol_mask,
9100 | { "dmrsSymbolMask", "oran_fh_cus.dmrsSymbolMask",
9101 | FT_UINT16, BASE_HEX,
9102 | NULL((void*)0), 0x3fff,
9103 | "symbols within the slot containing DMRS", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9104 | },
9105 | { &hf_oran_dmrs_symbol_mask_s13,
9106 | { "symbol 13", "oran_fh_cus.dmrsSymbolMask.symbol-13",
9107 | FT_BOOLEAN, 16,
9108 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x2000,
9109 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9110 | },
9111 | { &hf_oran_dmrs_symbol_mask_s12,
9112 | { "symbol 12", "oran_fh_cus.dmrsSymbolMask.symbol-12",
9113 | FT_BOOLEAN, 16,
9114 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x1000,
9115 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9116 | },
9117 | { &hf_oran_dmrs_symbol_mask_s11,
9118 | { "symbol 11", "oran_fh_cus.dmrsSymbolMask.symbol-11",
9119 | FT_BOOLEAN, 16,
9120 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0800,
9121 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9122 | },
9123 | { &hf_oran_dmrs_symbol_mask_s10,
9124 | { "symbol 10", "oran_fh_cus.dmrsSymbolMask.symbol-10",
9125 | FT_BOOLEAN, 16,
9126 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0400,
9127 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9128 | },
9129 | { &hf_oran_dmrs_symbol_mask_s9,
9130 | { "symbol 9", "oran_fh_cus.dmrsSymbolMask.symbol-9",
9131 | FT_BOOLEAN, 16,
9132 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0200,
9133 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9134 | },
9135 | { &hf_oran_dmrs_symbol_mask_s8,
9136 | { "symbol 8", "oran_fh_cus.dmrsSymbolMask.symbol-8",
9137 | FT_BOOLEAN, 16,
9138 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0100,
9139 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9140 | },
9141 | { &hf_oran_dmrs_symbol_mask_s7,
9142 | { "symbol 7", "oran_fh_cus.dmrsSymbolMask.symbol-7",
9143 | FT_BOOLEAN, 16,
9144 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0080,
9145 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9146 | },
9147 | { &hf_oran_dmrs_symbol_mask_s6,
9148 | { "symbol 6", "oran_fh_cus.dmrsSymbolMask.symbol-6",
9149 | FT_BOOLEAN, 16,
9150 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0040,
9151 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9152 | },
9153 | { &hf_oran_dmrs_symbol_mask_s5,
9154 | { "symbol 5", "oran_fh_cus.dmrsSymbolMask.symbol-5",
9155 | FT_BOOLEAN, 16,
9156 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0020,
9157 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9158 | },
9159 | { &hf_oran_dmrs_symbol_mask_s4,
9160 | { "symbol 4", "oran_fh_cus.dmrsSymbolMask.symbol-4",
9161 | FT_BOOLEAN, 16,
9162 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0010,
9163 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9164 | },
9165 | { &hf_oran_dmrs_symbol_mask_s3,
9166 | { "symbol 3", "oran_fh_cus.dmrsSymbolMask.symbol-3",
9167 | FT_BOOLEAN, 16,
9168 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0008,
9169 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9170 | },
9171 | { &hf_oran_dmrs_symbol_mask_s2,
9172 | { "symbol 2", "oran_fh_cus.dmrsSymbolMask.symbol-2",
9173 | FT_BOOLEAN, 16,
9174 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0004,
9175 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9176 | },
9177 | { &hf_oran_dmrs_symbol_mask_s1,
9178 | { "symbol 1", "oran_fh_cus.dmrsSymbolMask.symbol-1",
9179 | FT_BOOLEAN, 16,
9180 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0002,
9181 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9182 | },
9183 | { &hf_oran_dmrs_symbol_mask_s0,
9184 | { "symbol 0", "oran_fh_cus.dmrsSymbolMask.symbol-0",
9185 | FT_BOOLEAN, 16,
9186 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0001,
9187 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9188 | },
9189 |
9190 | /* 7.7.24.12 */
9191 | { &hf_oran_scrambling,
9192 | { "scrambling", "oran_fh_cus.scrambling",
9193 | FT_UINT16, BASE_HEX,
9194 | NULL((void*)0), 0x0,
9195 | "used to calculate the seed value required to initialize pseudo-random generator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9196 | },
9197 | /* 7.7.24.13 */
9198 | { &hf_oran_nscid,
9199 | { "nscid", "oran_fh_cus.nscid",
9200 | FT_UINT8, BASE_HEX,
9201 | NULL((void*)0), 0x80,
9202 | "used to calculate the seed value for pseudo-random generator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9203 | },
9204 | /* 7.7.24.14 */
9205 | { &hf_oran_dtype,
9206 | { "dType", "oran_fh_cus.dType",
9207 | FT_UINT8, BASE_HEX,
9208 | VALS(dtype_vals)((0 ? (const struct _value_string*)0 : ((dtype_vals)))), 0x40,
9209 | "PUSCH DMRS configuration type", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9210 | },
9211 | /* 7.7.24.15 */
9212 | { &hf_oran_cmd_without_data,
9213 | { "cmdWithoutData", "oran_fh_cus.cmdWithoutData",
9214 | FT_UINT8, BASE_HEX,
9215 | NULL((void*)0), 0x30,
9216 | "number of DMRS CDM groups without data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9217 | },
9218 | /* 7.7.24.16 */
9219 | { &hf_oran_lambda,
9220 | { "lambda", "oran_fh_cus.lambda",
9221 | FT_UINT8, BASE_HEX,
9222 | NULL((void*)0), 0x0c,
9223 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9224 | },
9225 | /* 7.7.24.19 */
9226 | { &hf_oran_first_prb,
9227 | { "firstPrb", "oran_fh_cus.firstPrb",
9228 | FT_UINT16, BASE_DEC,
9229 | NULL((void*)0), 0x03fe,
9230 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9231 | },
9232 | /* 7.7.24.20 */
9233 | { &hf_oran_last_prb,
9234 | { "lastPrb", "oran_fh_cus.lastPrb",
9235 | FT_UINT16, BASE_DEC,
9236 | NULL((void*)0), 0x01ff,
9237 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9238 | },
9239 |
9240 | /* 7.7.24.17 */
9241 | /* TODO: add value_string */
9242 | { &hf_oran_low_papr_type,
9243 | { "lowPaprType", "oran_fh_cus.lowPaprType",
9244 | FT_UINT8, BASE_HEX,
9245 | VALS(papr_type_vals)((0 ? (const struct _value_string*)0 : ((papr_type_vals)))), 0x30,
9246 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9247 | },
9248 | /* 7.7.24.18 */
9249 | { &hf_oran_hopping_mode,
9250 | { "hoppingMode", "oran_fh_cus.hoppingMode",
9251 | FT_UINT8, BASE_HEX,
9252 | VALS(hopping_mode_vals)((0 ? (const struct _value_string*)0 : ((hopping_mode_vals))) ), 0x0c,
9253 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9254 | },
9255 |
9256 | { &hf_oran_tx_win_for_on_air_symbol_l,
9257 | { "txWinForOnAirSymbol", "oran_fh_cus.txWinForOnAirSymbol",
9258 | FT_UINT8, BASE_DEC,
9259 | NULL((void*)0), 0xf0,
9260 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9261 | },
9262 | { &hf_oran_tx_win_for_on_air_symbol_r,
9263 | { "txWinForOnAirSymbol", "oran_fh_cus.txWinForOnAirSymbol",
9264 | FT_UINT8, BASE_DEC,
9265 | NULL((void*)0), 0x0f,
9266 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9267 | },
9268 | /* 7.7.26.2 */
9269 | { &hf_oran_num_fo_fb,
9270 | { "numFoFb", "oran_fh_cus.numFoFb",
9271 | FT_UINT8, BASE_DEC,
9272 | NULL((void*)0), 0x7f,
9273 | "number of frequency offset feedback", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9274 | },
9275 | /* 7.7.26.3 */
9276 | { &hf_oran_freq_offset_fb,
9277 | { "freqOffsetFb", "oran_fh_cus.freqOffsetFb",
9278 | FT_UINT16, BASE_HEX_DEC | BASE_RANGE_STRING0x00000100,
9279 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
9280 | "UE frequency offset feedback", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9281 | },
9282 |
9283 | /* 7.7.28.2 */
9284 | { &hf_oran_num_ue_sinr_rpt,
9285 | { "numUeSinrRpt", "oran_fh_cus.numUeSinrRpt",
9286 | FT_UINT8, BASE_DEC,
9287 | NULL((void*)0), 0x1f,
9288 | "number of sinr reported UEs {1 - 12}", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9289 | },
9290 |
9291 | /* 7.5.2.19 */
9292 | { &hf_oran_num_sinr_per_prb,
9293 | { "numSinrPerPrb", "oran_fh_cus.numSinrPerPrb",
9294 | FT_UINT8, BASE_DEC,
9295 | VALS(num_sinr_per_prb_vals)((0 ? (const struct _value_string*)0 : ((num_sinr_per_prb_vals )))), 0x70,
9296 | "number of SINR values per PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9297 | },
9298 | { &hf_oran_num_sinr_per_prb_right,
9299 | { "numSinrPerPrb", "oran_fh_cus.numSinrPerPrb",
9300 | FT_UINT8, BASE_DEC,
9301 | VALS(num_sinr_per_prb_vals)((0 ? (const struct _value_string*)0 : ((num_sinr_per_prb_vals )))), 0x07,
9302 | "number of SINR values per PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9303 | },
9304 |
9305 | /* 7.5.3.68 */
9306 | { &hf_oran_sinr_value,
9307 | { "sinrValue", "oran_fh_cus.sinrValue",
9308 | FT_FLOAT, BASE_NONE,
9309 | NULL((void*)0), 0x0,
9310 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9311 | },
9312 |
9313 | { &hf_oran_measurement_report,
9314 | { "Measurement Report", "oran_fh_cus.measurement-report",
9315 | FT_STRING, BASE_NONE,
9316 | NULL((void*)0), 0x0,
9317 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9318 | },
9319 | /* 7.5.3.57 */
9320 | { &hf_oran_mf,
9321 | { "mf", "oran_fh_cus.mf",
9322 | FT_BOOLEAN, 8,
9323 | TFS(&measurement_flag_tfs)((0 ? (const struct true_false_string*)0 : ((&measurement_flag_tfs )))), 0x80,
9324 | "measurement flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9325 | },
9326 | /* 7.5.3.59 */
9327 | { &hf_oran_meas_data_size,
9328 | { "measDataSize", "oran_fh_cus.measDataSize",
9329 | FT_UINT16, BASE_DEC,
9330 | NULL((void*)0), 0x0,
9331 | "measurement data size (in words)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9332 | },
9333 |
9334 | /* 7.5.3.58 */
9335 | { &hf_oran_meas_type_id,
9336 | { "measTypeId", "oran_fh_cus.measTypeId",
9337 | FT_UINT8, BASE_DEC,
9338 | VALS(meas_type_id_vals)((0 ? (const struct _value_string*)0 : ((meas_type_id_vals))) ), 0x7F,
9339 | "measurement report type identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9340 | },
9341 | /* 7.5.3.66 */
9342 | { &hf_oran_num_elements,
9343 | { "numElements", "oran_fh_cus.numElements",
9344 | FT_UINT8, BASE_DEC,
9345 | NULL((void*)0), 0x0,
9346 | "measurement report type identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9347 | },
9348 | /* 7.5.3.60 */
9349 | { &hf_oran_ue_tae,
9350 | { "ueTae", "oran_fh_cus.ueTae",
9351 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
9352 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
9353 | "UE Timing Advance Error", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9354 | },
9355 | /* 7.5.3.61 */
9356 | { &hf_oran_ue_layer_power,
9357 | { "ueLayerPower", "oran_fh_cus.ueLayerPower",
9358 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
9359 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
9360 | "UE Layer Power", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9361 | },
9362 |
9363 | /* 7.5.3.62 */
9364 | { &hf_oran_ue_freq_offset,
9365 | { "ueFreqOffset", "oran_fh_cus.ueFreqOffset",
9366 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
9367 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
9368 | "UE frequency offset", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9369 | },
9370 | /* 7.5.3.63 */
9371 | { &hf_oran_ipn_power,
9372 | { "ipnPower", "oran_fh_cus.ipnPower",
9373 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
9374 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
9375 | "Interference plus Noise power", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9376 | },
9377 | /* 7.5.3.64 */
9378 | { &hf_oran_ant_dmrs_snr_val,
9379 | { "antDmrsSnrVal", "oran_fh_cus.antDmrsSnrVal",
9380 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
9381 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
9382 | "antenna DMRS-SNR", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9383 | },
9384 |
9385 | { &hf_oran_measurement_command,
9386 | { "Measurement Command", "oran_fh_cus.measurement-command",
9387 | FT_STRING, BASE_NONE,
9388 | NULL((void*)0), 0x0,
9389 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9390 | },
9391 |
9392 | /* 7.5.27.2 */
9393 | { &hf_oran_beam_type,
9394 | {"beamType", "oran_fh_cus.beamType",
9395 | FT_UINT16, BASE_DEC,
9396 | VALS(beam_type_vals)((0 ? (const struct _value_string*)0 : ((beam_type_vals)))), 0xc0,
9397 | NULL((void*)0),
9398 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9399 | },
9400 | /* 7.5.3.65 */
9401 | { &hf_oran_meas_cmd_size,
9402 | {"measCmdSize", "oran_fh_cus.measCmdSize",
9403 | FT_UINT16, BASE_DEC,
9404 | NULL((void*)0), 0x0,
9405 | "measurement command size in words",
9406 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9407 | },
9408 |
9409 | { &hf_oran_symbol_reordering_layer,
9410 | { "Layer", "oran_fh_cus.layer",
9411 | FT_STRING, BASE_NONE,
9412 | NULL((void*)0), 0x0,
9413 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9414 | },
9415 | { &hf_oran_dmrs_entry,
9416 | { "Entry", "oran_fh_cus.dmrs-entry",
9417 | FT_STRING, BASE_NONE,
9418 | NULL((void*)0), 0x0,
9419 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9420 | },
9421 |
9422 | { &hf_oran_c_section_common,
9423 | { "Common Section", "oran_fh_cus.c-plane.section.common",
9424 | FT_STRING, BASE_NONE,
9425 | NULL((void*)0), 0x0,
9426 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9427 | },
9428 | { &hf_oran_c_section,
9429 | { "Section", "oran_fh_cus.c-plane.section",
9430 | FT_STRING, BASE_NONE,
9431 | NULL((void*)0), 0x0,
9432 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9433 | },
9434 | { &hf_oran_u_section,
9435 | { "Section", "oran_fh_cus.u-plane.section",
9436 | FT_STRING, BASE_NONE,
9437 | NULL((void*)0), 0x0,
9438 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9439 | },
9440 |
9441 | /* Link back to UL C-plane where udCompHdr was recorded */
9442 | { &hf_oran_ul_cplane_ud_comp_hdr_frame,
9443 | { "C-Plane UL udCompHdr frame", "oran_fh_cus.ul-cplane.udCompHdr",
9444 | FT_FRAMENUM, BASE_NONE,
9445 | FRAMENUM_TYPE(FT_FRAMENUM_REQUEST)((gpointer) (glong) (FT_FRAMENUM_REQUEST)), 0x0,
9446 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9447 | },
9448 | };
9449 |
9450 | /* Setup protocol subtree array */
9451 | static int *ett[] = {
9452 | &ett_oran,
9453 | &ett_oran_ecpri_pcid,
9454 | &ett_oran_ecpri_rtcid,
9455 | &ett_oran_ecpri_seqid,
9456 | &ett_oran_section_type,
9457 | &ett_oran_u_timing,
9458 | &ett_oran_u_section,
9459 | &ett_oran_u_prb,
9460 | &ett_oran_section,
9461 | &ett_oran_iq,
9462 | &ett_oran_bfw_bundle,
9463 | &ett_oran_bfw,
9464 | &ett_oran_frequency_range,
9465 | &ett_oran_prb_cisamples,
9466 | &ett_oran_cisample,
9467 | &ett_oran_udcomphdr,
9468 | &ett_oran_udcompparam,
9469 | &ett_oran_cicomphdr,
9470 | &ett_oran_cicompparam,
9471 | &ett_oran_bfwcomphdr,
9472 | &ett_oran_bfwcompparam,
9473 | &ett_oran_ext19_port,
9474 | &ett_oran_prb_allocation,
9475 | &ett_oran_punc_pattern,
9476 | &ett_oran_bfacomphdr,
9477 | &ett_oran_modcomp_param_set,
9478 | &ett_oran_st4_cmd_header,
9479 | &ett_oran_st4_cmd,
9480 | &ett_oran_sym_prb_pattern,
9481 | &ett_oran_measurement_report,
9482 | &ett_oran_measurement_command,
9483 | &ett_oran_sresmask,
9484 | &ett_oran_c_section_common,
9485 | &ett_oran_c_section,
9486 | &ett_oran_remask,
9487 | &ett_oran_mc_scale_remask,
9488 | &ett_oran_symbol_reordering_layer,
9489 | &ett_oran_dmrs_entry,
9490 | &ett_oran_dmrs_symbol_mask,
9491 | &ett_oran_symbol_mask,
9492 | &ett_active_beamspace_coefficient_mask
9493 | };
9494 |
9495 | static int *ext_ett[HIGHEST_EXTTYPE28];
9496 | for (unsigned extno=0; extno<HIGHEST_EXTTYPE28; extno++) {
9497 | ext_ett[extno] = &ett_oran_c_section_extension[extno];
9498 | }
9499 |
9500 | expert_module_t* expert_oran;
9501 |
9502 | static ei_register_info ei[] = {
9503 | { &ei_oran_unsupported_bfw_compression_method, { "oran_fh_cus.unsupported_bfw_compression_method", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Unsupported BFW Compression Method", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9504 | { &ei_oran_invalid_sample_bit_width, { "oran_fh_cus.invalid_sample_bit_width", PI_UNDECODED0x05000000, PI_ERROR0x00800000, "Unsupported sample bit width", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9505 | { &ei_oran_reserved_numBundPrb, { "oran_fh_cus.reserved_numBundPrb", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "Reserved value of numBundPrb", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9506 | { &ei_oran_extlen_wrong, { "oran_fh_cus.extlen_wrong", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "extlen doesn't match number of dissected bytes", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9507 | { &ei_oran_invalid_eaxc_bit_width, { "oran_fh_cus.invalid_eaxc_bit_width", PI_UNDECODED0x05000000, PI_ERROR0x00800000, "Inconsistent eAxC bit width", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9508 | { &ei_oran_extlen_zero, { "oran_fh_cus.extlen_zero", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "extlen - zero is reserved value", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9509 | { &ei_oran_rbg_size_reserved, { "oran_fh_cus.rbg_size_reserved", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "rbgSize - zero is reserved value", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9510 | { &ei_oran_frame_length, { "oran_fh_cus.frame_length", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "there should be 0-3 bytes remaining after PDU in frame", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9511 | { &ei_oran_numprbc_ext21_zero, { "oran_fh_cus.numprbc_ext21_zero", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "numPrbc shall not be set to 0 when ciPrbGroupSize is configured", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9512 | { &ei_oran_ci_prb_group_size_reserved, { "oran_fh_cus.ci_prb_group_size_reserved", PI_MALFORMED0x07000000, PI_WARN0x00600000, "ciPrbGroupSize should be 2-254", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9513 | { &ei_oran_st8_nackid, { "oran_fh_cus.st8_nackid", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "operation for this ackId failed", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9514 | { &ei_oran_st4_no_cmds, { "oran_fh_cus.st4_nackid", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "Not valid to have no commands in ST4", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9515 | { &ei_oran_st4_zero_len_cmd, { "oran_fh_cus.st4_zero_len_cmd", PI_MALFORMED0x07000000, PI_WARN0x00600000, "ST4 cmd with length 0 is reserved", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9516 | { &ei_oran_st4_wrong_len_cmd, { "oran_fh_cus.st4_wrong_len_cmd", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "ST4 cmd with length not matching contents", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9517 | { &ei_oran_st4_unknown_cmd, { "oran_fh_cus.st4_unknown_cmd", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "ST4 cmd with unknown command code", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9518 | { &ei_oran_mcot_out_of_range, { "oran_fh_cus.mcot_out_of_range", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "MCOT should be 1-10", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9519 | { &ei_oran_se10_unknown_beamgrouptype, { "oran_fh_cus.se10_unknown_beamgrouptype", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE10 - unknown BeamGroupType value", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9520 | { &ei_oran_se10_not_allowed, { "oran_fh_cus.se10_not_allowed", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE10 - type not allowed for sectionType", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9521 | { &ei_oran_start_symbol_id_not_zero, { "oran_fh_cus.startsymbolid_shall_be_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "For ST4 commands 3&4, startSymbolId shall be 0", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9522 | { &ei_oran_trx_control_cmd_scope, { "oran_fh_cus.trx_command.bad_cmdscope", PI_MALFORMED0x07000000, PI_WARN0x00600000, "TRX command must have cmdScope of ARRAY-COMMAND", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9523 | { &ei_oran_unhandled_se, { "oran_fh_cus.se_not_handled", PI_UNDECODED0x05000000, PI_WARN0x00600000, "SE not recognised/handled by dissector", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9524 | { &ei_oran_bad_symbolmask, { "oran_fh_cus.bad_symbol_mask", PI_MALFORMED0x07000000, PI_WARN0x00600000, "For non-zero sleepMode, symbolMask must be 0x0 or 0x3ffff", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9525 | { &ei_oran_numslots_not_zero, { "oran_fh_cus.numslots_not_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "For ST4 TIME_DOMAIN_BEAM_WEIGHTS, numSlots should be 0", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9526 | { &ei_oran_version_unsupported, { "oran_fh_cus.version_unsupported", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Protocol version unsupported", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9527 | { &ei_oran_laa_msg_type_unsupported, { "oran_fh_cus.laa_msg_type_unsupported", PI_UNDECODED0x05000000, PI_WARN0x00600000, "laaMsgType unsupported", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9528 | { &ei_oran_se_on_unsupported_st, { "oran_fh_cus.se_on_unsupported_st", PI_MALFORMED0x07000000, PI_WARN0x00600000, "Section Extension should not appear on this Section Type", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9529 | { &ei_oran_cplane_unexpected_sequence_number_ul, { "oran_fh_cus.unexpected_seq_no_cplane.ul", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in C-Plane UL", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9530 | { &ei_oran_cplane_unexpected_sequence_number_dl, { "oran_fh_cus.unexpected_seq_no_cplane.dl", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in C-Plane DL", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9531 | { &ei_oran_uplane_unexpected_sequence_number_ul, { "oran_fh_cus.unexpected_seq_no_uplane.ul", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in U-Plane UL", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9532 | { &ei_oran_uplane_unexpected_sequence_number_dl, { "oran_fh_cus.unexpected_seq_no_uplane.dl", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in U-Plane DL", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9533 | { &ei_oran_acknack_no_request, { "oran_fh_cus.acknack_no_request", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Have ackNackId response, but no request", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9534 | { &ei_oran_udpcomphdr_should_be_zero, { "oran_fh_cus.udcomphdr_should_be_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "C-Plane udCompHdr in DL should be set to 0", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9535 | { &ei_oran_radio_fragmentation_c_plane, { "oran_fh_cus.radio_fragmentation_c_plane", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "Radio fragmentation not allowed in C-PLane", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9536 | { &ei_oran_radio_fragmentation_u_plane, { "oran_fh_cus.radio_fragmentation_u_plane", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Radio fragmentation in C-PLane not yet supported", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9537 | { &ei_oran_lastRbdid_out_of_range, { "oran_fh_cus.lastrbdid_out_of_range", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE 6 has bad rbgSize", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9538 | { &ei_oran_rbgMask_beyond_last_rbdid, { "oran_fh_cus.rbgmask_beyond_lastrbdid", PI_MALFORMED0x07000000, PI_WARN0x00600000, "rbgMask has bits set beyond lastRbgId", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9539 | { &ei_oran_unexpected_measTypeId, { "oran_fh_cus.unexpected_meastypeid", PI_MALFORMED0x07000000, PI_WARN0x00600000, "unexpected measTypeId", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9540 | { &ei_oran_unsupported_compression_method, { "oran_fh_cus.compression_type_unsupported", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Unsupported compression type", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9541 | { &ei_oran_ud_comp_len_wrong_size, { "oran_fh_cus.ud_comp_len_wrong_size", PI_MALFORMED0x07000000, PI_WARN0x00600000, "udCompLen does not match length of U-Plane section", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9542 | { &ei_oran_sresmask2_not_zero_with_rb, { "oran_fh_cus.sresmask2_not_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "sReSMask2 should be zero when rb set", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9543 | { &ei_oran_st6_rb_shall_be_0, { "oran_fh_cus.st6_rb_set", PI_MALFORMED0x07000000, PI_WARN0x00600000, "rb should not be set for Section Type 6", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9544 | { &ei_oran_st9_not_ul, { "oran_fh_cus.st9_not_ul", PI_MALFORMED0x07000000, PI_WARN0x00600000, "Section Type 9 should only be sent in uplink direction", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9545 | { &ei_oran_st10_numsymbol_not_14, { "oran_fh_cus.st10_numsymbol_not_14", PI_MALFORMED0x07000000, PI_WARN0x00600000, "numSymbol should be 14 for Section Type 10", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9546 | { &ei_oran_st10_startsymbolid_not_0, { "oran_fh_cus.st10_startsymbolid_not_0", PI_MALFORMED0x07000000, PI_WARN0x00600000, "startSymbolId should be 0 for Section Type 10", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9547 | { &ei_oran_st10_not_ul, { "oran_fh_cus.st10_not_ul", PI_MALFORMED0x07000000, PI_WARN0x00600000, "Section Type 10 should only be sent in uplink direction", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9548 | { &ei_oran_se24_nothing_to_inherit, { "oran_fh_cus.se24_nothing_to_inherit", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE10 doesn't have type 2 or 3 before trying to inherit", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9549 | { &ei_oran_num_sinr_per_prb_unknown, { "oran_fh_cus.unexpected_num_sinr_per_prb", PI_MALFORMED0x07000000, PI_WARN0x00600000, "invalid numSinrPerPrb value", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9550 | { &ei_oran_start_symbol_id_bits_ignored, { "oran_fh_cus.start_symbol_id_bits_ignored", PI_MALFORMED0x07000000, PI_WARN0x00600000, "some startSymbolId lower bits ignored", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9551 | { &ei_oran_user_group_id_reserved_value, { "oran_fh_cus.user_group_id.reserved_value", PI_MALFORMED0x07000000, PI_WARN0x00600000, "userGroupId value 255 is reserved", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9552 | { &ei_oran_port_list_index_zero, { "oran_fh_cus.port_list_index.zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "portListIndex should not be zero", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9553 | { &ei_oran_ul_uplane_symbol_too_long, { "oran_fh_cus.ul_uplane_symbol_tx_too_slow", PI_RECEIVE0x0f000000, PI_WARN0x00600000, "UL U-Plane Tx took too long for symbol (limit set in preference)", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
9554 | };
9555 |
9556 | /* Register the protocol name and description */
9557 | proto_oran = proto_register_protocol("O-RAN Fronthaul CUS", "O-RAN FH CUS", "oran_fh_cus");
9558 |
9559 | /* Allow dissector to find be found by name. */
9560 | register_dissector("oran_fh_cus", dissect_oran, proto_oran);
9561 |
9562 | /* Register the tap name. */
9563 | oran_tap = register_tap("oran-fh-cus");
9564 |
9565 | /* Required function calls to register the header fields and subtrees */
9566 | proto_register_field_array(proto_oran, hf, array_length(hf)(sizeof (hf) / sizeof (hf)[0]));
9567 | proto_register_subtree_array(ett, array_length(ett)(sizeof (ett) / sizeof (ett)[0]));
9568 | proto_register_subtree_array(ext_ett, array_length(ext_ett)(sizeof (ext_ett) / sizeof (ext_ett)[0]));
9569 |
9570 |
9571 | expert_oran = expert_register_protocol(proto_oran);
9572 | expert_register_field_array(expert_oran, ei, array_length(ei)(sizeof (ei) / sizeof (ei)[0]));
9573 |
9574 | module_t * oran_module = prefs_register_protocol(proto_oran, NULL((void*)0));
9575 |
9576 | /* prefs_register_static_text_preference(oran_module, "oran.stream", "", ""); */
9577 |
9578 | /* Register bit width/compression preferences separately by direction. */
9579 | prefs_register_uint_preference(oran_module, "oran.du_port_id_bits", "DU Port ID bits [a]",
9580 | "The bit width of DU Port ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_du_port_id_bits);
9581 | prefs_register_uint_preference(oran_module, "oran.bandsector_id_bits", "BandSector ID bits [b]",
9582 | "The bit width of BandSector ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_bandsector_id_bits);
9583 | prefs_register_uint_preference(oran_module, "oran.cc_id_bits", "CC ID bits [c]",
9584 | "The bit width of CC ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_cc_id_bits);
9585 | prefs_register_uint_preference(oran_module, "oran.ru_port_id_bits", "RU Port ID bits [d]",
9586 | "The bit width of RU Port ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_ru_port_id_bits);
9587 |
9588 | prefs_register_static_text_preference(oran_module, "oran.ul", "", "");
9589 |
9590 | /* Uplink userplane */
9591 | prefs_register_uint_preference(oran_module, "oran.iq_bitwidth_up", "IQ Bitwidth Uplink",
9592 | "The bit width of a sample in the Uplink (if no udcompHdr and no C-Plane)", 10, &pref_sample_bit_width_uplink);
9593 | prefs_register_enum_preference(oran_module, "oran.ud_comp_up", "Uplink User Data Compression",
9594 | "Uplink User Data Compression (if no udcompHdr and no C-Plane)", &pref_iqCompressionUplink, ul_compression_options, false0);
9595 | prefs_register_enum_preference(oran_module, "oran.ud_comp_hdr_up", "udCompHdr field is present for uplink",
9596 | "The udCompHdr field in U-Plane messages may or may not be present, depending on the "
9597 | "configuration of the O-RU. This preference instructs the dissector to expect "
9598 | "this field to be present in uplink messages",
9599 | &pref_includeUdCompHeaderUplink, udcomphdr_present_options, false0);
9600 | prefs_register_uint_preference(oran_module, "oran.ul_slot_us_limit", "Microseconds allowed for UL tx in symbol",
9601 | "Maximum number of microseconds allowed for UL slot transmission before expert warning (zero to disable). N.B. timing relative to first frame seen for same symbol",
9602 | 10, &us_allowed_for_ul_in_symbol);
9603 |
9604 |
9605 |
9606 | prefs_register_static_text_preference(oran_module, "oran.dl", "", "");
9607 |
9608 | /* Downlink userplane */
9609 | prefs_register_uint_preference(oran_module, "oran.iq_bitwidth_down", "IQ Bitwidth Downlink",
9610 | "The bit width of a sample in the Downlink (if no udcompHdr)", 10, &pref_sample_bit_width_downlink);
9611 | prefs_register_enum_preference(oran_module, "oran.ud_comp_down", "Downlink User Data Compression",
9612 | "Downlink User Data Compression", &pref_iqCompressionDownlink, dl_compression_options, false0);
9613 | prefs_register_enum_preference(oran_module, "oran.ud_comp_hdr_down", "udCompHdr field is present for downlink",
9614 | "The udCompHdr field in U-Plane messages may or may not be present, depending on the "
9615 | "configuration of the O-RU. This preference instructs the dissector to expect "
9616 | "this field to be present in downlink messages",
9617 | &pref_includeUdCompHeaderDownlink, udcomphdr_present_options, false0);
9618 |
9619 | prefs_register_static_text_preference(oran_module, "oran.sinr", "", "");
9620 |
9621 | /* SINR */
9622 | prefs_register_uint_preference(oran_module, "oran.iq_bitwidth_sinr", "IQ Bitwidth SINR",
9623 | "The bit width of a sample in SINR", 10, &pref_sample_bit_width_sinr);
9624 | prefs_register_enum_preference(oran_module, "oran.ud_comp_sinr", "SINR Compression",
9625 | "SINR Compression", &pref_iqCompressionSINR, ul_compression_options, false0);
9626 |
9627 |
9628 | /* BF-related */
9629 | prefs_register_static_text_preference(oran_module, "oran.bf", "", "");
9630 |
9631 | prefs_register_obsolete_preference(oran_module, "oran.num_weights_per_bundle");
9632 |
9633 | prefs_register_uint_preference(oran_module, "oran.num_bf_antennas", "Number of beam weights",
9634 | "Number of array elements that BF weights will be provided for", 10, &pref_num_bf_antennas);
9635 |
9636 | prefs_register_obsolete_preference(oran_module, "oran.num_bf_weights");
9637 |
9638 | prefs_register_bool_preference(oran_module, "oran.st6_4byte_alignment_required", "Use 4-byte alignment for ST6 sections",
9639 | "Default is 1-byte alignment", &st6_4byte_alignment);
9640 |
9641 |
9642 | /* Misc (and will seldom need to be accessed) */
9643 | prefs_register_static_text_preference(oran_module, "oran.misc", "", "");
9644 |
9645 | prefs_register_bool_preference(oran_module, "oran.show_iq_samples", "Show IQ Sample values",
9646 | "When enabled, for U-Plane frames show each I and Q value in PRB", &pref_showIQSampleValues);
9647 |
9648 | prefs_register_enum_preference(oran_module, "oran.support_udcomplen", "udCompLen supported",
9649 | "When enabled, U-Plane messages with relevant compression schemes will include udCompLen",
9650 | &pref_support_udcompLen, udcomplen_support_options, false0);
9651 |
9652 | prefs_register_uint_preference(oran_module, "oran.rbs_in_uplane_section", "Total RBs in User-Plane data section",
9653 | "This is used if numPrbu is signalled as 0", 10, &pref_data_plane_section_total_rbs);
9654 |
9655 | prefs_register_bool_preference(oran_module, "oran.unscaled_iq", "Show unscaled I/Q values",
9656 | "", &show_unscaled_values);
9657 |
9658 | prefs_register_obsolete_preference(oran_module, "oran.k_antenna_ports");
9659 |
9660 |
9661 | flow_states_table = wmem_tree_new_autoreset(wmem_epan_scope(), wmem_file_scope());
9662 | flow_results_table = wmem_tree_new_autoreset(wmem_epan_scope(), wmem_file_scope());
9663 | ul_symbol_timing = wmem_tree_new_autoreset(wmem_epan_scope(), wmem_file_scope());
9664 |
9665 | register_init_routine(&oran_init_protocol);
9666 | }
9667 |
9668 | /* Simpler form of proto_reg_handoff_oran which can be used if there are
9669 | * no prefs-dependent registration function calls. */
9670 | void
9671 | proto_reg_handoff_oran(void)
9672 | {
9673 | }
9674 |
9675 | /*
9676 | * Editor modelines - http://www.wireshark.org/tools/modelines.html
9677 | *
9678 | * Local Variables:
9679 | * c-basic-offset: 4
9680 | * tab-width: 8
9681 | * indent-tabs-mode: nil
9682 | * End:
9683 | *
9684 | * ex: set shiftwidth=4 tabstop=8 expandtab:
9685 | * :indentSize=4:tabSize=8:noTabs=true:
9686 | */