### Bug Summary

File: | builds/wireshark/wireshark/epan/dissectors/packet-oran.c
Warning: | line 7427, column 51 Access to field 'expected_sections' results in a dereference of a null pointer (loaded from variable 'result')

### Annotated Source Code

Press '?' to see keyboard shortcuts

Show analyzer invocation
clang -cc1 -cc1 -triple x86_64-pc-linux-gnu -analyze -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name packet-oran.c -analyzer-checker=core -analyzer-checker=apiModeling -analyzer-checker=unix -analyzer-checker=deadcode -analyzer-checker=security.insecureAPI.UncheckedReturn -analyzer-checker=security.insecureAPI.getpw -analyzer-checker=security.insecureAPI.gets -analyzer-checker=security.insecureAPI.mktemp -analyzer-checker=security.insecureAPI.mkstemp -analyzer-checker=security.insecureAPI.vfork -analyzer-checker=nullability.NullPassedToNonnull -analyzer-checker=nullability.NullReturnedFromNonnull -analyzer-output plist -w -setup-static-analyzer -mrelocation-model pic -pic-level 2 -fhalf-no-semantic-interposition -fno-delete-null-pointer-checks -mframe-pointer=all -relaxed-aliasing -fmath-errno -ffp-contract=on -fno-rounding-math -ffloat16-excess-precision=fast -fbfloat16-excess-precision=fast -mconstructor-aliases -funwind-tables=2 -target-cpu x86-64 -tune-cpu generic -debugger-tuning=gdb -fdebug-compilation-dir=/builds/wireshark/wireshark/build -fcoverage-compilation-dir=/builds/wireshark/wireshark/build -resource-dir /usr/lib/llvm-22/lib/clang/22 -isystem /usr/include/glib-2.0 -isystem /usr/lib/x86_64-linux-gnu/glib-2.0/include -isystem /builds/wireshark/wireshark/epan/dissectors -isystem /builds/wireshark/wireshark/build/epan/dissectors -isystem /usr/include/mit-krb5 -isystem /usr/include/libxml2 -isystem /builds/wireshark/wireshark/epan -D CARES_NO_DEPRECATED -D G_DISABLE_DEPRECATED -D G_DISABLE_SINGLE_INCLUDES -D WS_BUILD_DLL -D WS_DEBUG -D WS_DEBUG_UTF_8 -I /builds/wireshark/wireshark/build -I /builds/wireshark/wireshark -I /builds/wireshark/wireshark/include -D _GLIBCXX_ASSERTIONS -internal-isystem /usr/lib/llvm-22/lib/clang/22/include -internal-isystem /usr/local/include -internal-isystem /usr/lib/gcc/x86_64-linux-gnu/16/../../../../x86_64-linux-gnu/include -internal-externc-isystem /usr/include/x86_64-linux-gnu -internal-externc-isystem /include -internal-externc-isystem /usr/include -fmacro-prefix-map=/builds/wireshark/wireshark/= -fmacro-prefix-map=/builds/wireshark/wireshark/build/= -fmacro-prefix-map=../= -Wno-format-nonliteral -std=gnu17 -ferror-limit 19 -fvisibility=hidden -fwrapv -fwrapv-pointer -fstrict-flex-arrays=3 -stack-protector 2 -fstack-clash-protection -fcf-protection=full -fgnuc-version=4.2.1 -fskip-odr-check-in-gmf -fexceptions -fcolor-diagnostics -analyzer-output=html -faddrsig -fdwarf2-cfi-asm -o /builds/wireshark/wireshark/sbout/2026-07-20-100411-3661-1 -x c /builds/wireshark/wireshark/epan/dissectors/packet-oran.c

Keyboard shortcuts:

- Use 'j/k' keys for keyboard navigation
- Use 'Shift+S' to show/hide relevant lines
- Use '?' to toggle this window

Close
Show only relevant lines Show control flow arrows

1 | /* packet-oran.c
2 | * Routines for O-RAN fronthaul UC-plane dissection
3 | * Copyright 2020, Jan Schiefer, Keysight Technologies, Inc.
4 | * Copyright 2020- Martin Mathieson
5 | *
6 | * Wireshark - Network traffic analyzer
7 | * By Gerald Combs <gerald@wireshark.org>
8 | * Copyright 1998 Gerald Combs
9 | *
10 | * SPDX-License-Identifier: GPL-2.0-or-later
11 | */
12 |
13 | /*
14 | * Dissector for the O-RAN Fronthaul CUS protocol specification.
15 | * See https://specifications.o-ran.org/specifications, WG4, Fronthaul Interfaces Workgroup
16 | * The current implementation is based on the ORAN-WG4.CUS.0-v20.00 specification.
17 | * Note that other eCPRI message types are handled in packet-ecpri.c
18 | */
19 |
20 | #include <config.h>
21 |
22 | #include <math.h>
23 |
24 | #include <epan/packet.h>
25 | #include <epan/expert.h>
26 | #include <epan/prefs.h>
27 | #include <epan/tap.h>
28 | #include <epan/tfs.h>
29 | #include <epan/reassemble.h>
30 |
31 | #include <wsutil/ws_roundup.h>
32 | #include <wsutil/ws_padding_to.h>
33 |
34 | #include "epan/dissectors/packet-oran.h"
35 |
36 | /* N.B. dissector preferences are taking the place of (some) M-plane parameters,
37 | * so unfortunately it can be fiddly to get the preferences into a good state to
38 | * decode a given capture..
39 | * TODO:
40 | * - Detect/indicate signs of application layer fragmentation?
41 | * same eAxC in same symbol (same/different section ID?)
42 | * - Not handling M-plane setting for "little endian byte order" as applied to
43 | * IQ samples and beam weights does anyone use this?
44 | * - for section extensions, check more constraints (which other extension types
45 | * appear with them, order, repeated)
46 | * - re-order items (decl and hf definitions) to match spec order?
47 | * - track energy-saving status, and identify TRX or ASM commands as 'Sleep extension'
48 | * - when tracking between C-plane and U-plane, indicated in C-plane any missing sectionIds/PRBs/REs
49 | */
50 |
51 | /* Prototypes */
52 | void proto_register_oran(void);
53 |
54 | /* Initialize the protocol and registered fields */
55 | static int proto_oran;
56 |
57 | static int oran_tap = -1;
58 |
59 | static int hf_oran_du_port_id;
60 | static int hf_oran_bandsector_id;
61 | static int hf_oran_cc_id;
62 | static int hf_oran_ru_port_id;
63 | static int hf_oran_sequence_id;
64 | static int hf_oran_e_bit;
65 | static int hf_oran_subsequence_id;
66 | static int hf_oran_previous_frame;
67 |
68 | static int hf_oran_data_direction;
69 | static int hf_oran_payload_version;
70 | static int hf_oran_filter_index;
71 | static int hf_oran_frame_id;
72 | static int hf_oran_subframe_id;
73 | static int hf_oran_slot_id;
74 | static int hf_oran_slot_within_frame;
75 | static int hf_oran_start_symbol_id;
76 | static int hf_oran_numberOfSections;
77 | static int hf_oran_sectionType;
78 |
79 | static int hf_oran_udCompHdr;
80 | static int hf_oran_udCompHdrIqWidth;
81 | static int hf_oran_udCompHdrIqWidth_pref;
82 | static int hf_oran_udCompHdrMeth;
83 | static int hf_oran_udCompHdrMeth_pref;
84 | static int hf_oran_udCompLen;
85 | static int hf_oran_numberOfUEs;
86 | static int hf_oran_timeOffset;
87 | static int hf_oran_frameStructure_fft;
88 | static int hf_oran_frameStructure_subcarrier_spacing;
89 | static int hf_oran_cpLength;
90 | static int hf_oran_timing_header;
91 | static int hf_oran_section_id;
92 | static int hf_oran_rb;
93 | static int hf_oran_symInc;
94 | static int hf_oran_startPrbc;
95 | static int hf_oran_reMask_re1;
96 | static int hf_oran_reMask_re2;
97 | static int hf_oran_reMask_re3;
98 | static int hf_oran_reMask_re4;
99 | static int hf_oran_reMask_re5;
100 | static int hf_oran_reMask_re6;
101 | static int hf_oran_reMask_re7;
102 | static int hf_oran_reMask_re8;
103 | static int hf_oran_reMask_re9;
104 | static int hf_oran_reMask_re10;
105 | static int hf_oran_reMask_re11;
106 | static int hf_oran_reMask_re12;
107 | static int hf_oran_reMask;
108 | static int hf_oran_numPrbc;
109 | static int hf_oran_numSymbol;
110 | static int hf_oran_ef;
111 | static int hf_oran_beamId;
112 |
113 | static int hf_oran_sinrCompHdrIqWidth_pref;
114 | static int hf_oran_sinrCompHdrMeth_pref;
115 |
116 | static int hf_oran_ciCompHdr;
117 | static int hf_oran_ciCompHdrIqWidth;
118 | static int hf_oran_ciCompHdrMeth;
119 | static int hf_oran_ciCompOpt;
120 |
121 | static int hf_oran_extension;
122 | static int hf_oran_exttype;
123 | static int hf_oran_extlen;
124 |
125 | static int hf_oran_bfw_bundle;
126 | static int hf_oran_bfw_bundle_id;
127 | static int hf_oran_bfw;
128 | static int hf_oran_bfw_i;
129 | static int hf_oran_bfw_q;
130 |
131 | static int hf_oran_ueId;
132 | static int hf_oran_freqOffset;
133 | static int hf_oran_regularizationFactor;
134 | static int hf_oran_laaMsgType;
135 | static int hf_oran_laaMsgLen;
136 | static int hf_oran_lbtHandle;
137 | static int hf_oran_lbtDeferFactor;
138 | static int hf_oran_lbtBackoffCounter;
139 | static int hf_oran_lbtOffset;
140 | static int hf_oran_MCOT;
141 | static int hf_oran_lbtMode;
142 | static int hf_oran_sfnSfEnd;
143 | static int hf_oran_lbtPdschRes;
144 | static int hf_oran_sfStatus;
145 | static int hf_oran_initialPartialSF;
146 | static int hf_oran_lbtDrsRes;
147 | static int hf_oran_lbtBufErr;
148 | static int hf_oran_lbtTrafficClass;
149 | static int hf_oran_lbtCWConfig_H;
150 | static int hf_oran_lbtCWConfig_T;
151 | static int hf_oran_lbtCWR_Rst;
152 |
153 | static int hf_oran_reserved;
154 | static int hf_oran_reserved_1bit;
155 | static int hf_oran_reserved_2bits;
156 | static int hf_oran_reserved_3bits;
157 | static int hf_oran_reserved_4bits;
158 | static int hf_oran_reserved_last_4bits;
159 | static int hf_oran_reserved_last_5bits;
160 | static int hf_oran_reserved_6bits;
161 | static int hf_oran_reserved_last_6bits;
162 | static int hf_oran_reserved_7bits;
163 | static int hf_oran_reserved_last_7bits;
164 | static int hf_oran_reserved_8bits;
165 | static int hf_oran_reserved_16bits;
166 | static int hf_oran_reserved_15bits;
167 | static int hf_oran_reserved_bit1;
168 | static int hf_oran_reserved_bit2;
169 | static int hf_oran_reserved_bit4;
170 | static int hf_oran_reserved_bit5;
171 | static int hf_oran_reserved_bits123;
172 | static int hf_oran_reserved_bits456;
173 |
174 | static int hf_oran_bundle_offset;
175 | static int hf_oran_cont_ind;
176 |
177 | static int hf_oran_bfwCompHdr;
178 | static int hf_oran_bfwCompHdr_iqWidth;
179 | static int hf_oran_bfwCompHdr_compMeth;
180 | static int hf_oran_symbolId;
181 | static int hf_oran_startPrbu;
182 | static int hf_oran_numPrbu;
183 |
184 | static int hf_oran_udCompParam;
185 | static int hf_oran_sReSMask;
186 | static int hf_oran_sReSMask_re12;
187 | static int hf_oran_sReSMask_re11;
188 | static int hf_oran_sReSMask_re10;
189 | static int hf_oran_sReSMask_re9;
190 | static int hf_oran_sReSMask_re8;
191 | static int hf_oran_sReSMask_re7;
192 | static int hf_oran_sReSMask_re6;
193 | static int hf_oran_sReSMask_re5;
194 | static int hf_oran_sReSMask_re4;
195 | static int hf_oran_sReSMask_re3;
196 | static int hf_oran_sReSMask_re2;
197 | static int hf_oran_sReSMask_re1;
198 |
199 | static int hf_oran_sReSMask1;
200 | static int hf_oran_sReSMask2;
201 | static int hf_oran_sReSMask1_2_re12;
202 | static int hf_oran_sReSMask1_2_re11;
203 | static int hf_oran_sReSMask1_2_re10;
204 | static int hf_oran_sReSMask1_2_re9;
205 |
206 | static int hf_oran_bfwCompParam;
207 |
208 | static int hf_oran_iSample;
209 | static int hf_oran_qSample;
210 |
211 | static int hf_oran_ciCompParam;
212 |
213 | static int hf_oran_blockScaler;
214 | static int hf_oran_compBitWidth;
215 | static int hf_oran_compShift;
216 |
217 | static int hf_oran_active_beamspace_coefficient_n1;
218 | static int hf_oran_active_beamspace_coefficient_n2;
219 | static int hf_oran_active_beamspace_coefficient_n3;
220 | static int hf_oran_active_beamspace_coefficient_n4;
221 | static int hf_oran_active_beamspace_coefficient_n5;
222 | static int hf_oran_active_beamspace_coefficient_n6;
223 | static int hf_oran_active_beamspace_coefficient_n7;
224 | static int hf_oran_active_beamspace_coefficient_n8;
225 | static int hf_oran_activeBeamspaceCoefficientMask;
226 | static int hf_oran_activeBeamspaceCoefficientMask_bits_set;
227 |
228 | static int hf_oran_se6_repetition;
229 |
230 | static int hf_oran_rbgSize;
231 | static int hf_oran_rbgMask;
232 | static int hf_oran_noncontig_priority;
233 |
234 | static int hf_oran_symbol_mask;
235 | static int hf_oran_symbol_mask_s13;
236 | static int hf_oran_symbol_mask_s12;
237 | static int hf_oran_symbol_mask_s11;
238 | static int hf_oran_symbol_mask_s10;
239 | static int hf_oran_symbol_mask_s9;
240 | static int hf_oran_symbol_mask_s8;
241 | static int hf_oran_symbol_mask_s7;
242 | static int hf_oran_symbol_mask_s6;
243 | static int hf_oran_symbol_mask_s5;
244 | static int hf_oran_symbol_mask_s4;
245 | static int hf_oran_symbol_mask_s3;
246 | static int hf_oran_symbol_mask_s2;
247 | static int hf_oran_symbol_mask_s1;
248 | static int hf_oran_symbol_mask_s0;
249 |
250 | static int hf_oran_exponent;
251 | static int hf_oran_iq_user_data;
252 |
253 | static int hf_oran_disable_bfws;
254 | static int hf_oran_rad;
255 | static int hf_oran_num_bund_prbs;
256 | static int hf_oran_beam_id;
257 | static int hf_oran_num_weights_per_bundle;
258 |
259 | static int hf_oran_ack_nack_req_id;
260 |
261 | static int hf_oran_frequency_range;
262 | static int hf_oran_off_start_prb;
263 | static int hf_oran_num_prb;
264 |
265 | static int hf_oran_samples_prb;
266 | static int hf_oran_ciSample;
267 | static int hf_oran_ciIsample;
268 | static int hf_oran_ciQsample;
269 |
270 | static int hf_oran_beamGroupType;
271 | static int hf_oran_numPortc;
272 |
273 | static int hf_oran_csf;
274 | static int hf_oran_modcompscaler;
275 |
276 | static int hf_oran_modcomp_param_set;
277 | static int hf_oran_mc_scale_re_mask_re1;
278 | static int hf_oran_mc_scale_re_mask_re2;
279 | static int hf_oran_mc_scale_re_mask_re3;
280 | static int hf_oran_mc_scale_re_mask_re4;
281 | static int hf_oran_mc_scale_re_mask_re5;
282 | static int hf_oran_mc_scale_re_mask_re6;
283 | static int hf_oran_mc_scale_re_mask_re7;
284 | static int hf_oran_mc_scale_re_mask_re8;
285 | static int hf_oran_mc_scale_re_mask_re9;
286 | static int hf_oran_mc_scale_re_mask_re10;
287 | static int hf_oran_mc_scale_re_mask_re11;
288 | static int hf_oran_mc_scale_re_mask_re12;
289 | static int hf_oran_mc_scale_re_mask_re1_even;
290 | static int hf_oran_mc_scale_re_mask_re2_even;
291 | static int hf_oran_mc_scale_re_mask_re3_even;
292 | static int hf_oran_mc_scale_re_mask_re4_even;
293 | static int hf_oran_mc_scale_re_mask_re5_even;
294 | static int hf_oran_mc_scale_re_mask_re6_even;
295 | static int hf_oran_mc_scale_re_mask_re7_even;
296 | static int hf_oran_mc_scale_re_mask_re8_even;
297 | static int hf_oran_mc_scale_re_mask_re9_even;
298 | static int hf_oran_mc_scale_re_mask_re10_even;
299 | static int hf_oran_mc_scale_re_mask_re11_even;
300 | static int hf_oran_mc_scale_re_mask_re12_even;
301 |
302 | static int hf_oran_mc_scale_re_mask;
303 | static int hf_oran_mc_scale_re_mask_even;
304 |
305 | static int hf_oran_mc_scale_offset;
306 |
307 | static int hf_oran_eAxC_mask;
308 | static int hf_oran_technology;
309 | static int hf_oran_nullLayerInd;
310 |
311 | static int hf_oran_se19_repetition;
312 | static int hf_oran_portReMask;
313 | static int hf_oran_portSymbolMask;
314 |
315 | static int hf_oran_ext19_port;
316 |
317 | static int hf_oran_prb_allocation;
318 | static int hf_oran_nextSymbolId;
319 | static int hf_oran_nextStartPrbc;
320 |
321 | static int hf_oran_puncPattern;
322 | static int hf_oran_numPuncPatterns;
323 | static int hf_oran_symbolMask_ext20;
324 | static int hf_oran_startPuncPrb;
325 | static int hf_oran_numPuncPrb;
326 | static int hf_oran_puncReMask;
327 | static int hf_oran_multiSDScope;
328 | static int hf_oran_RbgIncl;
329 |
330 | static int hf_oran_ci_prb_group_size;
331 | static int hf_oran_prg_size_st5;
332 | static int hf_oran_prg_size_st6;
333 |
334 | static int hf_oran_num_ueid;
335 |
336 | static int hf_oran_antMask;
337 |
338 | static int hf_oran_transmissionWindowOffset;
339 | static int hf_oran_transmissionWindowSize;
340 | static int hf_oran_toT;
341 |
342 | static int hf_oran_bfaCompHdr;
343 | static int hf_oran_bfAzPtWidth;
344 | static int hf_oran_bfZePtWidth;
345 | static int hf_oran_bfAz3ddWidth;
346 | static int hf_oran_bfZe3ddWidth;
347 | static int hf_oran_bfAzPt;
348 | static int hf_oran_bfZePt;
349 | static int hf_oran_bfAz3dd;
350 | static int hf_oran_bfZe3dd;
351 | static int hf_oran_bfAzSl;
352 | static int hf_oran_bfZeSl;
353 |
354 | static int hf_oran_cmd_scope;
355 | static int hf_oran_number_of_st4_cmds;
356 |
357 | static int hf_oran_st4_cmd_header;
358 | static int hf_oran_st4_cmd_type;
359 | static int hf_oran_st4_cmd_len;
360 | static int hf_oran_st4_cmd_num_slots;
361 | static int hf_oran_st4_cmd_ack_nack_req_id;
362 |
363 | static int hf_oran_st4_cmd;
364 |
365 | static int hf_oran_sleepmode_trx;
366 | static int hf_oran_sleepmode_asm;
367 | static int hf_oran_log2maskbits;
368 | static int hf_oran_num_slots_ext;
369 | static int hf_oran_antMask_trx_control;
370 |
371 | static int hf_oran_ready;
372 | static int hf_oran_number_of_acks;
373 | static int hf_oran_number_of_nacks;
374 | static int hf_oran_ackid;
375 | static int hf_oran_nackid;
376 |
377 | static int hf_oran_acknack_request_frame;
378 | static int hf_oran_acknack_request_time;
379 | static int hf_oran_acknack_request_type;
380 | static int hf_oran_acknack_response_frame;
381 | static int hf_oran_acknack_response_time;
382 |
383 | static int hf_oran_disable_tdbfns;
384 | static int hf_oran_td_beam_group;
385 | static int hf_oran_disable_tdbfws;
386 | static int hf_oran_td_beam_num;
387 |
388 | static int hf_oran_dir_pattern;
389 | static int hf_oran_guard_pattern;
390 |
391 | static int hf_oran_ecpri_pcid;
392 | static int hf_oran_ecpri_rtcid;
393 | static int hf_oran_ecpri_seqid;
394 |
395 | static int hf_oran_num_sym_prb_pattern;
396 | static int hf_oran_prb_mode;
397 | static int hf_oran_sym_prb_pattern;
398 | static int hf_oran_sym_mask;
399 | static int hf_oran_num_mc_scale_offset;
400 | static int hf_oran_prb_pattern;
401 | static int hf_oran_prb_blk_offset;
402 | static int hf_oran_prb_blk_size;
403 |
404 | static int hf_oran_codebook_index;
405 | static int hf_oran_layerid;
406 | static int hf_oran_numlayers;
407 | static int hf_oran_txscheme;
408 | static int hf_oran_crs_remask;
409 | static int hf_oran_crs_shift;
410 | static int hf_oran_crs_symnum;
411 | static int hf_oran_beamid_ap1;
412 | static int hf_oran_beamid_ap2;
413 | static int hf_oran_beamid_ap3;
414 |
415 | static int hf_oran_port_list_index;
416 | static int hf_oran_alpn_per_sym;
417 | static int hf_oran_ant_dmrs_snr;
418 | static int hf_oran_user_group_size;
419 | static int hf_oran_user_group_id;
420 | static int hf_oran_entry_type;
421 | static int hf_oran_dmrs_port_number;
422 | static int hf_oran_ueid_reset;
423 |
424 | static int hf_oran_dmrs_symbol_mask;
425 | static int hf_oran_dmrs_symbol_mask_s13;
426 | static int hf_oran_dmrs_symbol_mask_s12;
427 | static int hf_oran_dmrs_symbol_mask_s11;
428 | static int hf_oran_dmrs_symbol_mask_s10;
429 | static int hf_oran_dmrs_symbol_mask_s9;
430 | static int hf_oran_dmrs_symbol_mask_s8;
431 | static int hf_oran_dmrs_symbol_mask_s7;
432 | static int hf_oran_dmrs_symbol_mask_s6;
433 | static int hf_oran_dmrs_symbol_mask_s5;
434 | static int hf_oran_dmrs_symbol_mask_s4;
435 | static int hf_oran_dmrs_symbol_mask_s3;
436 | static int hf_oran_dmrs_symbol_mask_s2;
437 | static int hf_oran_dmrs_symbol_mask_s1;
438 | static int hf_oran_dmrs_symbol_mask_s0;
439 |
440 | static int hf_oran_scrambling;
441 | static int hf_oran_nscid;
442 | static int hf_oran_dtype;
443 | static int hf_oran_cmd_without_data;
444 | static int hf_oran_lambda;
445 | static int hf_oran_first_prb;
446 | static int hf_oran_last_prb;
447 | static int hf_oran_low_papr_type;
448 | static int hf_oran_hopping_mode;
449 |
450 | static int hf_oran_tx_win_for_on_air_symbol_l;
451 | static int hf_oran_tx_win_for_on_air_symbol_r;
452 |
453 | static int hf_oran_num_fo_fb;
454 | static int hf_oran_freq_offset_fb;
455 |
456 | static int hf_oran_num_ue_sinr_rpt;
457 | static int hf_oran_num_sinr_per_prb;
458 | static int hf_oran_num_sinr_per_prb_right;
459 |
460 | static int hf_oran_sinr_value;
461 |
462 | static int hf_oran_measurement_report;
463 | static int hf_oran_mf;
464 | static int hf_oran_meas_data_size;
465 | static int hf_oran_meas_type_id;
466 | static int hf_oran_ipn_power;
467 | static int hf_oran_ue_tae;
468 | static int hf_oran_ue_layer_power;
469 | static int hf_oran_num_elements;
470 | static int hf_oran_ant_dmrs_snr_val;
471 | static int hf_oran_ue_freq_offset;
472 |
473 | static int hf_oran_measurement_command;
474 |
475 | static int hf_oran_beam_type;
476 | static int hf_oran_meas_cmd_size;
477 |
478 | static int hf_oran_symbol_reordering_layer;
479 | static int hf_oran_dmrs_entry;
480 |
481 | static int hf_oran_c_section_common;
482 | static int hf_oran_c_section;
483 | static int hf_oran_u_section;
484 |
485 | static int hf_oran_u_section_ul_symbol_time;
486 | static int hf_oran_u_section_ul_symbol_frames;
487 | static int hf_oran_u_section_ul_symbol_first_frame;
488 | static int hf_oran_u_section_ul_symbol_last_frame;
489 |
490 | static int hf_oran_cd_scg_size;
491 | static int hf_oran_cd_scg_phase_step;
492 |
493 | static int hf_oran_sinr_prb;
494 | static int hf_oran_oru_control_sinr_slot_mask_id;
495 | static int hf_oran_pos_meas;
496 |
497 | static int hf_oran_ue_radial_speed;
498 | static int hf_oran_ue_az_aoa;
499 | static int hf_oran_ue_ze_aoa;
500 | static int hf_oran_ue_pos_toa_offset;
501 |
502 | static int hf_oran_num_rep_ue;
503 | static int hf_oran_rep_ueid;
504 | static int hf_oran_is_last_rep;
505 | static int hf_oran_rep_index;
506 | static int hf_oran_num_reps;
507 |
508 | static int hf_oran_mcs_table;
509 | static int hf_oran_mcs_index;
510 |
511 | static int hf_oran_num_meas_req;
512 | static int hf_oran_num_of_ue_ant_ports;
513 | static int hf_oran_ue_rank;
514 | static int hf_oran_codebook_subset;
515 | static int hf_oran_full_pwr_mode;
516 | static int hf_oran_full_pwr_mode_2_tpmi_group;
517 |
518 | static int hf_oran_num_cand_ranks;
519 | static int hf_oran_ue_pref_rank;
520 | static int hf_oran_ue_tpmi_rank_y;
521 | static int hf_oran_ue_tpmi_rank_y_sinr_lx;
522 | static int hf_oran_ue_layer_pre_eq_sinr;
523 |
524 |
525 | /* Computed fields */
526 | static int hf_oran_c_eAxC_ID;
527 | static int hf_oran_refa;
528 |
529 | static int hf_oran_bfws_frame_defined;
530 | static int hf_oran_bfws_symbols_since_defined;
531 |
532 | static int hf_oran_corresponding_cplane_frame;
533 | static int hf_oran_corresponding_cplane_frame_time_delta;
534 | static int hf_oran_corresponding_uplane_frame;
535 | static int hf_oran_corresponding_uplane_frames_total;
536 |
537 |
538 | /* Convenient fields for filtering, mostly shown as hidden */
539 | static int hf_oran_cplane;
540 | static int hf_oran_uplane;
541 | static int hf_oran_bf; /* to match frames that configure beamforming in any way */
542 | static int hf_oran_zero_prb;
543 | static int hf_oran_nonzero_prb;
544 | static int hf_oran_bundle_weights_all_zero;
545 |
546 | static int hf_oran_ul_cplane_ud_comp_hdr_frame;
547 |
548 | /* For reassembly */
549 | static int hf_oran_fragments;
550 | static int hf_oran_fragment;
551 | static int hf_oran_fragment_overlap;
552 | static int hf_oran_fragment_overlap_conflict;
553 | static int hf_oran_fragment_multiple_tails;
554 | static int hf_oran_fragment_too_long_fragment;
555 | static int hf_oran_fragment_error;
556 | static int hf_oran_fragment_count;
557 | static int hf_oran_reassembled_in;
558 | static int hf_oran_reassembled_length;
559 | static int hf_oran_reassembled_data;
560 |
561 | static int hf_oran_payload;
562 |
563 |
564 | /* Subtrees */
565 | static int ett_oran;
566 | static int ett_oran_ecpri_rtcid;
567 | static int ett_oran_ecpri_pcid;
568 | static int ett_oran_ecpri_seqid;
569 | static int ett_oran_section;
570 | static int ett_oran_section_type;
571 | static int ett_oran_u_timing;
572 | static int ett_oran_u_section;
573 | static int ett_oran_u_prb;
574 | static int ett_oran_iq;
575 | static int ett_oran_bfw_bundle;
576 | static int ett_oran_bfw;
577 | static int ett_oran_frequency_range;
578 | static int ett_oran_prb_cisamples;
579 | static int ett_oran_cisample;
580 | static int ett_oran_udcomphdr;
581 | static int ett_oran_udcompparam;
582 | static int ett_oran_cicomphdr;
583 | static int ett_oran_cicompparam;
584 | static int ett_oran_bfwcomphdr;
585 | static int ett_oran_bfwcompparam;
586 | static int ett_oran_ext19_port;
587 | static int ett_oran_prb_allocation;
588 | static int ett_oran_punc_pattern;
589 | static int ett_oran_bfacomphdr;
590 | static int ett_oran_modcomp_param_set;
591 | static int ett_oran_st4_cmd_header;
592 | static int ett_oran_st4_cmd;
593 | static int ett_oran_sym_prb_pattern;
594 | static int ett_oran_measurement_report;
595 | static int ett_oran_measurement_command;
596 | static int ett_oran_sresmask;
597 | static int ett_oran_c_section_common;
598 | static int ett_oran_c_section;
599 | static int ett_oran_remask;
600 | static int ett_oran_mc_scale_remask;
601 | static int ett_oran_symbol_reordering_layer;
602 | static int ett_oran_dmrs_entry;
603 | static int ett_oran_dmrs_symbol_mask;
604 | static int ett_oran_symbol_mask;
605 | static int ett_oran_active_beamspace_coefficient_mask;
606 | static int ett_oran_sinr_prb;
607 |
608 | static int ett_oran_fragment;
609 | static int ett_oran_fragments;
610 |
611 | /* Reassembly table. */
612 | static reassembly_table oran_reassembly_table;
613 |
614 | static void *oran_key(const packet_info *pinfo _U___attribute__((unused)), const uint32_t id _U___attribute__((unused)), const void *data)
615 | {
616 | return (void *)data;
617 | }
618 |
619 | static void oran_free_key(void *ptr _U___attribute__((unused)))
620 | {
621 | }
622 |
623 | static reassembly_table_functions oran_reassembly_table_functions =
624 | {
625 | g_direct_hash,
626 | g_direct_equal,
627 | oran_key,
628 | oran_key,
629 | oran_free_key,
630 | oran_free_key
631 | };
632 |
633 | static const fragment_items oran_frag_items = {
634 | &ett_oran_fragment,
635 | &ett_oran_fragments,
636 | &hf_oran_fragments,
637 | &hf_oran_fragment,
638 | &hf_oran_fragment_overlap,
639 | &hf_oran_fragment_overlap_conflict,
640 | &hf_oran_fragment_multiple_tails,
641 | &hf_oran_fragment_too_long_fragment,
642 | &hf_oran_fragment_error,
643 | &hf_oran_fragment_count,
644 | &hf_oran_reassembled_in,
645 | &hf_oran_reassembled_length,
646 | &hf_oran_reassembled_data,
647 | "O-RAN FH CUS fragments"
648 | };
649 |
650 |
651 |
652 | /* Don't want all extensions to open and close together. Use [extType-1] entry */
653 | static int ett_oran_c_section_extension[HIGHEST_EXTTYPE32];
654 |
655 | /* Expert info */
656 | static expert_field ei_oran_unsupported_bfw_compression_method;
657 | static expert_field ei_oran_invalid_sample_bit_width;
658 | static expert_field ei_oran_reserved_numBundPrb;
659 | static expert_field ei_oran_extlen_wrong;
660 | static expert_field ei_oran_invalid_eaxc_bit_width;
661 | static expert_field ei_oran_extlen_zero;
662 | static expert_field ei_oran_rbg_size_reserved;
663 | static expert_field ei_oran_frame_length;
664 | static expert_field ei_oran_numprbc_ext21_zero;
665 | static expert_field ei_oran_ci_prb_group_size_reserved;
666 | static expert_field ei_oran_st8_nackid;
667 | static expert_field ei_oran_st4_no_cmds;
668 | static expert_field ei_oran_st4_zero_len_cmd;
669 | static expert_field ei_oran_st4_wrong_len_cmd;
670 | static expert_field ei_oran_st4_unknown_cmd;
671 | static expert_field ei_oran_mcot_out_of_range;
672 | static expert_field ei_oran_se10_unknown_beamgrouptype;
673 | static expert_field ei_oran_se10_not_allowed;
674 | static expert_field ei_oran_start_symbol_id_not_zero;
675 | static expert_field ei_oran_trx_control_cmd_scope;
676 | static expert_field ei_oran_unhandled_se;
677 | static expert_field ei_oran_bad_symbolmask;
678 | static expert_field ei_oran_numslots_not_zero;
679 | static expert_field ei_oran_version_unsupported;
680 | static expert_field ei_oran_laa_msg_type_unsupported;
681 | static expert_field ei_oran_se_on_unsupported_st;
682 | static expert_field ei_oran_cplane_unexpected_sequence_number_ul;
683 | static expert_field ei_oran_cplane_unexpected_sequence_number_dl;
684 | static expert_field ei_oran_uplane_unexpected_sequence_number_ul;
685 | static expert_field ei_oran_uplane_unexpected_sequence_number_dl;
686 | static expert_field ei_oran_acknack_no_request;
687 | static expert_field ei_oran_udpcomphdr_should_be_zero;
688 | static expert_field ei_oran_radio_fragmentation_c_plane;
689 | static expert_field ei_oran_lastRbdid_out_of_range;
690 | static expert_field ei_oran_rbgMask_beyond_last_rbdid;
691 | static expert_field ei_oran_unexpected_measTypeId;
692 | static expert_field ei_oran_unsupported_compression_method;
693 | static expert_field ei_oran_ud_comp_len_wrong_size;
694 | static expert_field ei_oran_sresmask2_not_zero_with_rb;
695 | static expert_field ei_oran_st6_rb_shall_be_0;
696 | static expert_field ei_oran_st9_not_ul;
697 | static expert_field ei_oran_st10_numsymbol_not_14;
698 | static expert_field ei_oran_st10_startsymbolid_not_0;
699 | static expert_field ei_oran_st10_not_ul;
700 | static expert_field ei_oran_se24_nothing_to_inherit;
701 | static expert_field ei_oran_num_sinr_per_prb_unknown;
702 | static expert_field ei_oran_start_symbol_id_bits_ignored;
703 | static expert_field ei_oran_user_group_id_reserved_value;
704 | static expert_field ei_oran_port_list_index_zero;
705 | static expert_field ei_oran_ul_uplane_symbol_too_long;
706 | static expert_field ei_oran_reserved_not_zero;
707 | static expert_field ei_oran_too_many_symbols;
708 | static expert_field ei_oran_se30_not_ul;
709 | static expert_field ei_oran_se30_unknown_ueid;
710 | static expert_field ei_oran_beamid_bfws_not_found;
711 | static expert_field ei_oran_syminc_set_for_uplane;
712 | static expert_field ei_oran_cplane_entry_not_found;
713 |
714 |
715 | /* These are the message types handled by this dissector. Others have handling in packet-ecpri.c */
716 | #define ECPRI_MT_IQ_DATA0 0
717 | #define ECPRI_MT_RT_CTRL_DATA2 2
718 |
719 |
720 | /* Preference settings - try to set reasonable defaults */
721 | static unsigned pref_du_port_id_bits = 4;
722 | static unsigned pref_bandsector_id_bits = 4;
723 | static unsigned pref_cc_id_bits = 4;
724 | static unsigned pref_ru_port_id_bits = 4;
725 |
726 | /* TODO: ideally should be per-flow */
727 | static unsigned pref_sample_bit_width_uplink = 14;
728 | static unsigned pref_sample_bit_width_downlink = 14;
729 | static unsigned pref_sample_bit_width_sinr = 14;
730 |
731 | /* TODO: these ideally should be per-flow too */
732 | static int pref_iqCompressionUplink = COMP_BLOCK_FP1;
733 | static int pref_iqCompressionDownlink = COMP_BLOCK_FP1;
734 |
735 | static int pref_iqCompressionSINR = COMP_BLOCK_FP1;
736 |
737 |
738 | /* Is udCompHeader present (both directions) */
739 | static int pref_includeUdCompHeaderUplink = 2; /* start using heuristic */
740 | static int pref_includeUdCompHeaderDownlink = 2; /* start using heuristic */
741 |
742 | /* Are we ignoring UL C-Plane udCompHdr? */
743 | static bool_Bool pref_override_ul_compression = false0;
744 |
745 | static unsigned pref_data_plane_section_total_rbs = 273;
746 | static unsigned pref_num_bf_antennas = 32;
747 | static bool_Bool pref_showIQSampleValues = true1;
748 |
749 | /* Based upon m-plane param, so will be system-wide */
750 | static int pref_support_udcompLen = 2; /* start heuristic, can force other settings if necessary */
751 | static bool_Bool udcomplen_heuristic_result_set = false0;
752 | static bool_Bool udcomplen_heuristic_result = false0;
753 |
754 | /* st6-4byte-alignment-required */
755 | static bool_Bool st6_4byte_alignment = false0;
756 |
757 | /* Requested, allows I/Q to be stored as integers.. */
758 | static bool_Bool show_unscaled_values = false0;
759 |
760 | /* Initialized off. Timing is in microseconds. */
761 | static unsigned us_allowed_for_ul_in_symbol = 0;
762 |
763 | /* Reassemble U-Plane (at Radio Transport layer) */
764 | static bool_Bool do_radio_transport_layer_reassembly = true1;
765 |
766 | /* Link U-plane back to C-plane using sectionIds */
767 | static bool_Bool link_planes_together = true1;
768 |
769 | static const enum_val_t dl_compression_options[] = {
770 | { "COMP_NONE", "No Compression", COMP_NONE0 },
771 | { "COMP_BLOCK_FP", "Block Floating Point Compression", COMP_BLOCK_FP1 },
772 | { "COMP_BLOCK_SCALE", "Block Scaling Compression", COMP_BLOCK_SCALE2 },
773 | { "COMP_U_LAW", "u-Law Compression", COMP_U_LAW3 },
774 | { "COMP_MODULATION", "Modulation Compression", COMP_MODULATION4 },
775 | { "BFP_AND_SELECTIVE_RE", "Block Floating Point + selective RE sending", BFP_AND_SELECTIVE_RE5 },
776 | { "MOD_COMPR_AND_SELECTIVE_RE", "Modulation Compression + selective RE sending", MOD_COMPR_AND_SELECTIVE_RE6 },
777 | { "BFP_AND_SELECTIVE_RE_WITH_MASKS", "Block Floating Point + selective RE sending with masks in section header", BFP_AND_SELECTIVE_RE_WITH_MASKS7 },
778 | { "MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS", "Modulation Compression + selective RE sending with masks in section header", MOD_COMPR_AND_SELECTIVE_RE6 },
779 | { NULL((void*)0), NULL((void*)0), 0 }
780 | };
781 |
782 | /* No Modulation compression in UL.. */
783 | static const enum_val_t ul_compression_options[] = {
784 | { "COMP_NONE", "No Compression", COMP_NONE0 },
785 | { "COMP_BLOCK_FP", "Block Floating Point Compression", COMP_BLOCK_FP1 },
786 | { "COMP_BLOCK_SCALE", "Block Scaling Compression", COMP_BLOCK_SCALE2 },
787 | { "COMP_U_LAW", "u-Law Compression", COMP_U_LAW3 },
788 | { "BFP_AND_SELECTIVE_RE", "Block Floating Point + selective RE sending", BFP_AND_SELECTIVE_RE5 },
789 | { "BFP_AND_SELECTIVE_RE_WITH_MASKS", "Block Floating Point + selective RE sending with masks in section header", BFP_AND_SELECTIVE_RE_WITH_MASKS7 },
790 | { NULL((void*)0), NULL((void*)0), 0 }
791 | };
792 |
793 | static const enum_val_t udcomplen_support_options[] = {
794 | { "NOT_SUPPORTED", "Not Supported", 0 },
795 | { "SUPPORTED", "Supported", 1 },
796 | { "HEURISTIC", "Attempt Heuristic", 2 },
797 | { NULL((void*)0), NULL((void*)0), 0 }
798 | };
799 |
800 | static const enum_val_t udcomphdr_present_options[] = {
801 | { "NOT_PRESENT", "Not Present", 0 },
802 | { "PRESENT", "Present", 1 },
803 | { "HEURISTIC", "Attempt Heuristic", 2 },
804 | { NULL((void*)0), NULL((void*)0), 0 }
805 | };
806 |
807 |
808 |
809 | static const value_string e_bit[] = {
810 | { 0, "More fragments follow" },
811 | { 1, "Last fragment" },
812 | { 0, NULL((void*)0)}
813 | };
814 |
815 | #define DIR_UPLINK0 0
816 | #define DIR_DOWNLINK1 1
817 |
818 |
819 | static const value_string data_direction_vals[] = {
820 | { DIR_UPLINK0, "Uplink" }, /* gNB Rx */
821 | { DIR_DOWNLINK1, "Downlink" }, /* gNB Tx */
822 | { 0, NULL((void*)0)}
823 | };
824 |
825 | static const value_string rb_vals[] = {
826 | { 0, "Every RB used" },
827 | { 1, "Every other RB used" },
828 | { 0, NULL((void*)0)}
829 | };
830 |
831 | static const value_string sym_inc_vals[] = {
832 | { 0, "Use the current symbol number" },
833 | { 1, "Increment the current symbol number" },
834 | { 0, NULL((void*)0)}
835 | };
836 |
837 | static const value_string lbtMode_vals[] = {
838 | { 0, "Full LBT (regular LBT, sending reservation signal until the beginning of the SF/slot)" },
839 | { 1, "Partial LBT (looking back 25 usec prior to transmission" },
840 | { 2, "Partial LBT (looking back 34 usec prior to transmission" },
841 | { 3, "Full LBT and stop (regular LBT, without sending reservation signal" },
842 | { 0, NULL((void*)0)}
843 | };
844 |
845 | static const value_string ue_rank_vals[] = {
846 | { 1, "1" },
847 | { 2, "2" },
848 | { 3, "3" },
849 | { 4, "4" },
850 | { 0, NULL((void*)0)}
851 | };
852 |
853 | static const value_string num_of_ue_ant_ports_vals[] = {
854 | { 2, "2" },
855 | { 4, "4" },
856 | { 0, NULL((void*)0)}
857 | };
858 |
859 | static const value_string codebook_subset_vals[] = {
860 | { 0, "nonCoherent" },
861 | { 1, "partialAndNonCoherent" },
862 | { 2, "fullyAndPartialAndNonCoherent" },
863 | { 3, "reserved" },
864 | { 0, NULL((void*)0)}
865 | };
866 |
867 |
868 | static const range_string filter_indices[] = {
869 | {0, 0, "standard channel filter"},
870 | {1, 1, "UL filter for PRACH preamble formats 0, 1, 2; min. passband 839 x 1.25kHz = 1048.75 kHz"},
871 | {2, 2, "UL filter for PRACH preamble format 3, min. passband 839 x 5 kHz = 4195 kHz"},
872 | {3, 3, "UL filter for PRACH preamble formats A1, A2, A3, B1, B2, B3, B4, C0, C2; min. passband 139 x \u0394fRA"},
873 | {4, 4, "UL filter for NPRACH 0, 1; min. passband 48 x 3.75KHz = 180 KHz"},
874 | {5, 5, "UL filter for PRACH preamble formats"},
875 | {8, 8, "UL filter NPUSCH"},
876 | {9, 9, "Mixed numerology and other channels except PRACH and NB-IoT"},
877 | {9, 15, "Reserved"},
878 | {0, 0, NULL((void*)0)}
879 | };
880 |
881 | /* 7.3.1-1 */
882 | static const range_string section_types[] = {
883 | { SEC_C_UNUSED_RB, SEC_C_UNUSED_RB, "Unused Resource Blocks or symbols in Downlink or Uplink" },
884 | { SEC_C_NORMAL, SEC_C_NORMAL, "Most DL/UL radio channels" },
885 | { SEC_C_RSVD2, SEC_C_RSVD2, "Reserved for future use" },
886 | { SEC_C_PRACH, SEC_C_PRACH, "PRACH and mixed-numerology channels" },
887 | { SEC_C_SLOT_CONTROL, SEC_C_SLOT_CONTROL, "Slot Configuration Control" },
888 | { SEC_C_UE_SCHED, SEC_C_UE_SCHED, "UE scheduling information (UE-ID assignment to section)" },
889 | { SEC_C_CH_INFO, SEC_C_CH_INFO, "Channel information" },
890 | { SEC_C_LAA, SEC_C_LAA, "LAA (License Assisted Access)" },
891 | { SEC_C_ACK_NACK_FEEDBACK, SEC_C_ACK_NACK_FEEDBACK, "ACK/NACK Feedback" },
892 | { SEC_C_SINR_REPORTING, SEC_C_SINR_REPORTING, "SINR Reporting" },
893 | { SEC_C_RRM_MEAS_REPORTS, SEC_C_RRM_MEAS_REPORTS, "RRM Measurement Reports" },
894 | { SEC_C_REQUEST_RRM_MEAS, SEC_C_REQUEST_RRM_MEAS, "Request RRM Measurements" },
895 | { 12, 255, "Reserved for future use" },
896 | { 0, 0, NULL((void*)0)} };
897 |
898 | static const range_string section_types_short[] = {
899 | { SEC_C_UNUSED_RB, SEC_C_UNUSED_RB, "(Unused RBs) " },
900 | { SEC_C_NORMAL, SEC_C_NORMAL, "(Most channels) " },
901 | { SEC_C_RSVD2, SEC_C_RSVD2, "(reserved) " },
902 | { SEC_C_PRACH, SEC_C_PRACH, "(PRACH/mixed-\u03bc)" },
903 | { SEC_C_SLOT_CONTROL, SEC_C_SLOT_CONTROL, "(Slot info) " },
904 | { SEC_C_UE_SCHED, SEC_C_UE_SCHED, "(UE scheduling info)" },
905 | { SEC_C_CH_INFO, SEC_C_CH_INFO, "(Channel info) " },
906 | { SEC_C_LAA, SEC_C_LAA, "(LAA) " },
907 | { SEC_C_ACK_NACK_FEEDBACK, SEC_C_ACK_NACK_FEEDBACK, "(ACK/NACK) " },
908 | { SEC_C_SINR_REPORTING, SEC_C_SINR_REPORTING, "(SINR Reporting) " },
909 | { SEC_C_RRM_MEAS_REPORTS, SEC_C_RRM_MEAS_REPORTS, "(RRM Meas Reports) " },
910 | { SEC_C_REQUEST_RRM_MEAS, SEC_C_REQUEST_RRM_MEAS, "(Req RRM Meas) " },
911 | { 12, 255, "Reserved for future use" },
912 | { 0, 0, NULL((void*)0) }
913 | };
914 |
915 | static const range_string ud_comp_header_width[] = {
916 | {0, 0, "I and Q are each 16 bits wide"},
917 | {1, 15, "Bit width of I and Q"},
918 | {0, 0, NULL((void*)0)} };
919 |
920 | /* Table 8.3.3.13-3 */
921 | static const range_string ud_comp_header_meth[] = {
922 | {COMP_NONE0, COMP_NONE0, "No compression" },
923 | {COMP_BLOCK_FP1, COMP_BLOCK_FP1, "Block floating point compression" },
924 | {COMP_BLOCK_SCALE2, COMP_BLOCK_SCALE2, "Block scaling" },
925 | {COMP_U_LAW3, COMP_U_LAW3, "Mu - law" },
926 | {COMP_MODULATION4, COMP_MODULATION4, "Modulation compression" },
927 | {BFP_AND_SELECTIVE_RE5, BFP_AND_SELECTIVE_RE5, "BFP + selective RE sending" },
928 | {MOD_COMPR_AND_SELECTIVE_RE6, MOD_COMPR_AND_SELECTIVE_RE6, "mod-compr + selective RE sending" },
929 | {BFP_AND_SELECTIVE_RE_WITH_MASKS7, BFP_AND_SELECTIVE_RE_WITH_MASKS7, "BFP + selective RE sending with masks in section header" },
930 | {MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8, MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8, "mod-compr + selective RE sending with masks in section header"},
931 | {9, 15, "Reserved"},
932 | {0, 0, NULL((void*)0)}
933 | };
934 |
935 | /* Table 7.5.2.13-2 */
936 | static const range_string frame_structure_fft[] = {
937 | {0, 0, "Reserved (no FFT/iFFT processing)"},
938 | {1, 3, "Reserved"},
939 | {4, 4, "FFT size 16"},
940 | {5, 5, "FFT size 32"},
941 | {6, 6, "FFT size 64"},
942 | {7, 7, "FFT size 128"},
943 | {8, 8, "FFT size 256"},
944 | {9, 9, "FFT size 512"},
945 | {10, 10, "FFT size 1024"},
946 | {11, 11, "FFT size 2048"},
947 | {12, 12, "FFT size 4096"},
948 | {13, 13, "FFT size 1536"},
949 | {14, 14, "FFT size 3072"},
950 | {15, 15, "Reserved"},
951 | {0, 0, NULL((void*)0)}
952 | };
953 |
954 | /* Table 7.5.2.13-3 */
955 | static const range_string subcarrier_spacings[] = {
956 | { 0, 0, "SCS 15 kHz, 1 slot/subframe, slot length 1 ms" },
957 | { 1, 1, "SCS 30 kHz, 2 slots/subframe, slot length 500 \u03bcs" },
958 | { 2, 2, "SCS 60 kHz, 4 slots/subframe, slot length 250 \u03bcs" },
959 | { 3, 3, "SCS 120 kHz, 8 slots/subframe, slot length 125 \u03bcs" },
960 | { 4, 4, "SCS 240 kHz, 16 slots/subframe, slot length 62.5 \u03bcs" },
961 | { 5, 11, "Reserved" }, /* N.B., 5 was 480kHz in early spec versions */
962 | { 12, 12, "SCS 1.25 kHz, 1 slot/subframe, slot length 1 ms" },
963 | { 13, 13, "SCS 3.75 kHz(LTE - specific), 1 slot/subframe, slot length 1 ms" },
964 | { 14, 14, "SCS 5 kHz, 1 slot/subframe, slot length 1 ms" },
965 | { 15, 15, "SCS 7.5 kHz(LTE - specific), 1 slot/subframe, slot length 1 ms" },
966 | { 0, 0, NULL((void*)0) }
967 | };
968 |
969 | /* Table 7.5.3.14-1 laaMsgType definition */
970 | static const range_string laaMsgTypes[] = {
971 | {0, 0, "LBT_PDSCH_REQ - lls - O-DU to O-RU request to obtain a PDSCH channel"},
972 | {1, 1, "LBT_DRS_REQ - lls - O-DU to O-RU request to obtain the channel and send DRS"},
973 | {2, 2, "LBT_PDSCH_RSP - O-RU to O-DU response, channel acq success or failure"},
974 | {3, 3, "LBT_DRS_RSP - O-RU to O-DU response, DRS sending success or failure"},
975 | {4, 4, "LBT_Buffer_Error - O-RU to O-DU response, reporting buffer overflow"},
976 | {5, 5, "LBT_CWCONFIG_REQ - O-DU to O-RU request, congestion window configuration"},
977 | {6, 6, "LBT_CWCONFIG_RST - O-RU to O-DU request, congestion window config, response"},
978 | {7, 15, "reserved for future methods"},
979 | {0, 0, NULL((void*)0)}
980 | };
981 |
982 | /* 7.7.26.3 */
983 | static const range_string freq_offset_fb_values[] = {
984 | {0, 0, "no frequency offset"},
985 | {8000, 8000, "value not provided"},
986 | {1, 30000, "positive frequency offset, (0, +0.5] subcarrier"},
987 | {0x8ad0, 0xffff, "negative frequency offset, [-0.5, 0) subcarrier"},
988 | {0x0, 0xffff, "reserved"},
989 | {0, 0, NULL((void*)0)}
990 | };
991 |
992 | /* 7.5.3.78 */
993 | static const range_string ue_tmpi_rank_sinr_vals[] = {
994 | {0, 0, "0 dB SINR"},
995 | {0x0001, 0x07ff, "positive SINR"},
996 | {0xf800, 0xffff, "-ve SINR"},
997 | {0x8000, 0x8000, "invalid measurement result"},
998 | {0x0, 0xffff, "reserved"},
999 | {0, 0, NULL((void*)0)}
1000 | };
1001 |
1002 |
1003 |
1004 | /* Table 7.5.2.19-1 */
1005 | static const value_string num_sinr_per_prb_vals[] = {
1006 | { 0, "1" },
1007 | { 1, "2" },
1008 | { 2, "3" },
1009 | { 3, "4" },
1010 | { 4, "6" },
1011 | { 5, "12" },
1012 | { 6, "1 SINR value per section for DFT-s-OFDM" },
1013 | { 7, "reserved" },
1014 | { 0, NULL((void*)0)}
1015 | };
1016 |
1017 | static const value_string meas_type_id_vals[] = {
1018 | { 1, "UE Timing Advance Error" },
1019 | { 2, "UE Layer power" },
1020 | { 3, "UE frequency offset" },
1021 | { 4, "Interference plus Noise for allocated PRBs" },
1022 | { 5, "Interference plus Noise for unallocated PRBs" },
1023 | { 6, "DMRS-SNR per antenna" },
1024 | { 7, "UE positioning measurement report" },
1025 | { 8, "UE radial speed measurement report" },
1026 | { 9, "UE post-equalization MU inteference measurement" },
1027 | { 10, "UE TPMI and rank recommendation measurement" },
1028 | { 11, "UE layer pre-equalization SINR report" },
1029 | { 0, NULL((void*)0)}
1030 | };
1031 |
1032 | static const value_string beam_type_vals[] = {
1033 | { 0, "List of beamId values" },
1034 | { 1, "Range of beamId values" },
1035 | { 0, NULL((void*)0)}
1036 | };
1037 |
1038 | /* 7.7.24.3 */
1039 | static const value_string entry_type_vals[] = {
1040 | { 0, "inherit config from preceding entry (2 or 3) ueIdReset=0" },
1041 | { 1, "inherit config from preceding entry (2 or 3) ueIdReset=1" },
1042 | { 2, "related parameters if have transform precoding disabled " },
1043 | { 3, "related parameters if have transform precoding enabled " },
1044 | { 0, NULL((void*)0)}
1045 | };
1046 |
1047 | /* Table 7.7.29.3-1 */
1048 | static const range_string cd_scg_size_vals[] = {
1049 | { 0, 0, "1 subcarrier" },
1050 | { 1, 1, "1 RB x N subcarriers" },
1051 | { 2, 2, "2 RB x N subcarriers" },
1052 | { 3, 3, "4 RB x N subcarriers" },
1053 | { 4, 4, "8 RB x N subcarriers" },
1054 | { 5, 5, "16 RB x N subcarriers" },
1055 | { 6, 6, "32 RB x N subcarriers" },
1056 | { 7, 15, "reserved"},
1057 | { 0, 0, NULL((void*)0)}
1058 | };
1059 |
1060 |
1061 | /* Table 7.6.1-1 */
1062 | static const value_string exttype_vals[] = {
1063 | {0, "Reserved"},
1064 | {1, "Beamforming weights"},
1065 | {2, "Beamforming attributes"},
1066 | {3, "DL Precoding configuration parameters and indications"},
1067 | {4, "Modulation compr. params"},
1068 | {5, "Modulation compression additional scaling parameters"},
1069 | {6, "Non-contiguous PRB allocation"},
1070 | {7, "Multiple-eAxC designation"},
1071 | {8, "Regularization factor"},
1072 | {9, "Dynamic Spectrum Sharing parameters"},
1073 | {10, "Multiple ports grouping"},
1074 | {11, "Flexible BF weights"},
1075 | {12, "Non-Contiguous PRB Allocation with Frequency Ranges"},
1076 | {13, "PRB Allocation with Frequency Hopping"},
1077 | {14, "Nulling-layer Info. for ueId-based beamforming"},
1078 | {15, "Mixed-numerology Info. for ueId-based beamforming"},
1079 | {16, "Section description for antenna mapping in UE channel information based UL beamforming"},
1080 | {17, "Section description for indication of user port group"},
1081 | {18, "Section description for Uplink Transmission Management"},
1082 | {19, "Compact beamforming information for multiple port"},
1083 | {20, "Puncturing extension"},
1084 | {21, "Variable PRB group size for channel information"},
1085 | {22, "ACK/NACK request"},
1086 | {23, "Multiple symbol modulation compression parameters"},
1087 | {24, "PUSCH DMRS configuration"},
1088 | {25, "Symbol reordering for DMRS-BF"},
1089 | {26, "Frequency offset feedback"},
1090 | {27, "O-DU controlled dimensionality reduction"},
1091 | {28, "O-DU controlled frequency resolution for SINR reporting"},
1092 | {29, "Cyclic delay adjustment"},
1093 | {30, "PUSCH repetition indication"},
1094 | {31, "MCS Information"},
1095 | {32, "Rank and TPMI measurement request"},
1096 | {0, NULL((void*)0)}
1097 | };
1098 | static value_string_ext exttype_vals_ext = VALUE_STRING_EXT_INIT(exttype_vals){ _try_val_to_str_ext_init, 0, (sizeof (exttype_vals) / sizeof ((exttype_vals)[0]))-1, exttype_vals, "exttype_vals", ((void *)0) };
1099 |
1100 |
1101 | /**************************************************************************************/
1102 | /* Keep track for each Section Extension, which section types are allowed to carry it */
1103 | typedef struct {
1104 | bool_Bool ST0;
1105 | bool_Bool ST1;
1106 | bool_Bool ST3;
1107 | bool_Bool ST5;
1108 | bool_Bool ST6;
1109 | bool_Bool ST10;
1110 | bool_Bool ST11;
1111 | } AllowedCTs_t;
1112 |
1113 |
1114 | static const AllowedCTs_t ext_cts[HIGHEST_EXTTYPE32] = {
1115 | /* ST0 ST1 ST3 ST5 ST6 ST10 ST11 */
1116 | { false0, true1, true1, false0, false0, false0, false0}, // SE 1 (1,3)
1117 | { false0, true1, true1, false0, false0, false0, false0}, // SE 2 (1,3)
1118 | { false0, true1, true1, false0, false0, false0, false0}, // SE 3 (1,3)
1119 | { false0, true1, true1, true1, false0, false0, false0}, // SE 4 (1,3,5)
1120 | { false0, true1, true1, true1, false0, false0, false0}, // SE 5 (1,3,5)
1121 | { false0, true1, true1, true1, false0, true1, true1 }, // SE 6 (1,3,5,10,11)
1122 | { true1, false0, false0, false0, false0, false0, false0}, // SE 7 (0)
1123 | { false0, false0, false0, true1, false0, false0, false0}, // SE 8 (5)
1124 | { true1, true1, true1, true1, true1, true1, true1 }, // SE 9 (all)
1125 | { false0, true1, true1, true1, false0, false0, false0}, // SE 10 (1,3,5)
1126 | { false0, true1, true1, false0, false0, false0, false0}, // SE 11 (1,3)
1127 | { false0, true1, true1, true1, false0, true1, true1 }, // SE 12 (1,3,5,10,11)
1128 | { false0, true1, true1, true1, false0, false0, false0}, // SE 13 (1,3,5)
1129 | { false0, false0, false0, true1, false0, false0, false0}, // SE 14 (5)
1130 | { false0, false0, false0, true1, true1, false0, false0}, // SE 15 (5,6)
1131 | { false0, false0, false0, true1, false0, false0, false0}, // SE 16 (5)
1132 | { false0, false0, false0, true1, false0, false0, false0}, // SE 17 (5)
1133 | { false0, true1, true1, true1, false0, false0, false0}, // SE 18 (1,3,5)
1134 | { false0, true1, true1, false0, false0, false0, false0}, // SE 19 (1,3)
1135 | { true1, true1, true1, true1, true1, true1, true1 }, // SE 20 (0,1,3,5,10,11)
1136 | { false0, false0, false0, true1, true1, false0, false0}, // SE 21 (5,6)
1137 | { true1, true1, true1, true1, true1, true1, true1 }, // SE 22 (all)
1138 | { false0, true1, true1, true1, false0, false0, false0}, // SE 23 (1,3,5)
1139 | { false0, false0, false0, true1, false0, false0, false0}, // SE 24 (5)
1140 | { false0, false0, false0, true1, false0, false0, false0}, // SE 25 (5)
1141 | { false0, false0, false0, true1, false0, false0, false0}, // SE 26 (5)
1142 | { false0, false0, false0, true1, false0, false0, false0}, // SE 27 (5)
1143 | { false0, false0, false0, true1, false0, false0, false0}, // SE 28 (5)
1144 | { false0, true1, true1, true1, false0, false0, false0}, // SE 29 (1,3,5)
1145 | { false0, false0, false0, true1, false0, false0, false0}, // SE 30 (5)
1146 | { false0, true1, true1, true1, false0, false0, false0}, // SE 31 (1,3,5)
1147 | { false0, false0, false0, true1, false0, false0, false0}, // SE 32 (5)
1148 | };
1149 |
1150 | static bool_Bool se_allowed_in_st(unsigned se, unsigned st)
1151 | {
1152 | if (se==0 || se>HIGHEST_EXTTYPE32) {
1153 | /* Don't know about new SE, so don't complain.. */
1154 | return true1;
1155 | }
1156 |
1157 | switch (st) {
1158 | case 0:
1159 | return ext_cts[se-1].ST0;
1160 | case 1:
1161 | return ext_cts[se-1].ST1;
1162 | case 3:
1163 | return ext_cts[se-1].ST3;
1164 | case 5:
1165 | return ext_cts[se-1].ST5;
1166 | case 6:
1167 | return ext_cts[se-1].ST6;
1168 | case 10:
1169 | return ext_cts[se-1].ST10;
1170 | case 11:
1171 | return ext_cts[se-1].ST11;
1172 | default:
1173 | /* New/unknown section type that includes 'ef'.. assume ok */
1174 | return true1;
1175 | }
1176 | }
1177 |
1178 | /************************************************************************************/
1179 |
1180 | /* Table 7.7.1.2-2 */
1181 | static const value_string bfw_comp_headers_iq_width[] = {
1182 | {0, "I and Q are 16 bits wide"},
1183 | {1, "I and Q are 1 bit wide"},
1184 | {2, "I and Q are 2 bits wide"},
1185 | {3, "I and Q are 3 bits wide"},
1186 | {4, "I and Q are 4 bits wide"},
1187 | {5, "I and Q are 5 bits wide"},
1188 | {6, "I and Q are 6 bits wide"},
1189 | {7, "I and Q are 7 bits wide"},
1190 | {8, "I and Q are 8 bits wide"},
1191 | {9, "I and Q are 9 bits wide"},
1192 | {10, "I and Q are 10 bits wide"},
1193 | {11, "I and Q are 11 bits wide"},
1194 | {12, "I and Q are 12 bits wide"},
1195 | {13, "I and Q are 13 bits wide"},
1196 | {14, "I and Q are 14 bits wide"},
1197 | {15, "I and Q are 15 bits wide"},
1198 | {0, NULL((void*)0)}
1199 | };
1200 |
1201 | /* Table 7.7.1.2-3 */
1202 | static const value_string bfw_comp_headers_comp_meth[] = {
1203 | {COMP_NONE0, "no compression"},
1204 | {COMP_BLOCK_FP1, "block floating point"},
1205 | {COMP_BLOCK_SCALE2, "block scaling"},
1206 | {COMP_U_LAW3, "u-law"},
1207 | {4, "beamspace compression type I"},
1208 | {5, "beamspace compression type II"},
1209 | {0, NULL((void*)0)}
1210 | };
1211 |
1212 | /* 7.7.6.2 rbgSize (resource block group size) */
1213 | static const value_string rbg_size_vals[] = {
1214 | {0, "reserved"},
1215 | {1, "1"},
1216 | {2, "2"},
1217 | {3, "3"},
1218 | {4, "4"},
1219 | {5, "6"},
1220 | {6, "8"},
1221 | {7, "16"},
1222 | {0, NULL((void*)0)}
1223 | };
1224 |
1225 | /* 7.7.6.5 */
1226 | static const value_string priority_vals[] = {
1227 | {0, "0"},
1228 | {1, "+1"},
1229 | {2, "-2 (reserved, should not be used)"},
1230 | {3, "-1"},
1231 | {0, NULL((void*)0)}
1232 | };
1233 |
1234 | /* 7.7.10.2 beamGroupType */
1235 | static const value_string beam_group_type_vals[] = {
1236 | {0x0, "common beam"},
1237 | {0x1, "beam matrix indication"},
1238 | {0x2, "beam vector listing"},
1239 | {0x3, "beamId/ueId listing with associated port-list index"},
1240 | {0, NULL((void*)0)}
1241 | };
1242 |
1243 | /* 7.7.9.2 technology (interface name) */
1244 | static const value_string interface_name_vals[] = {
1245 | {0x0, "LTE"},
1246 | {0x1, "NR"},
1247 | {0, NULL((void*)0)}
1248 | };
1249 |
1250 | /* 7.7.18.4 toT (type of transmission) */
1251 | static const value_string type_of_transmission_vals[] = {
1252 | {0x0, "normal transmission mode, data can be distributed in any way the O-RU is implemented to transmit data"},
1253 | {0x1, "uniformly distributed over the transmission window"},
1254 | {0x2, "Reserved"},
1255 | {0x3, "Reserved"},
1256 | {0, NULL((void*)0)}
1257 | };
1258 |
1259 | /* 7.7.2.2 (width of bfa parameters) */
1260 | static const value_string bfa_bw_vals[] = {
1261 | {0, "no bits, the field is not applicable (e.g., O-RU does not support it) or the default value shall be used"},
1262 | {1, "2-bit bitwidth"},
1263 | {2, "3-bit bitwidth"},
1264 | {3, "4-bit bitwidth"},
1265 | {4, "5-bit bitwidth"},
1266 | {5, "6-bit bitwidth"},
1267 | {6, "7-bit bitwidth"},
1268 | {7, "8-bit bitwidth"},
1269 | {0, NULL((void*)0)}
1270 | };
1271 |
1272 | /* 7.7.2.7 & 7.7.2.8 */
1273 | static const value_string sidelobe_suppression_vals[] = {
1274 | {0, "10 dB"},
1275 | {1, "15 dB"},
1276 | {2, "20 dB"},
1277 | {3, "25 dB"},
1278 | {4, "30 dB"},
1279 | {5, "35 dB"},
1280 | {6, "40 dB"},
1281 | {7, ">= 45 dB"},
1282 | {0, NULL((void*)0)}
1283 | };
1284 |
1285 | static const value_string lbtTrafficClass_vals[] = {
1286 | {1, "Priority 1"},
1287 | {2, "Priority 2"},
1288 | {3, "Priority 3"},
1289 | {4, "Priority 4"},
1290 | {0, NULL((void*)0)}
1291 | };
1292 |
1293 | /* 7.5.3.22 */
1294 | static const value_string lbtPdschRes_vals[] = {
1295 | {0, "not sensing – indicates that the O-RU is transmitting data"},
1296 | {1, "currently sensing – indicates the O-RU has not yet acquired the channel"},
1297 | {2, "success – indicates that the channel was successfully acquired"},
1298 | {3, "Failure – indicates expiration of the LBT timer. The LBT process should be reset"},
1299 | {0, NULL((void*)0)}
1300 | };
1301 |
1302 | /* Table 7.5.2.15-3 */
1303 | static const value_string ci_comp_opt_vals[] = {
1304 | {0, "compression per UE, one ciCompParam exists before the I/Q value of each UE"},
1305 | {1, "compression per PRB, one ciCompParam exists before the I/Q value of each PRB"},
1306 | {0, NULL((void*)0)}
1307 | };
1308 |
1309 | /* 7.5.2.17 */
1310 | static const range_string cmd_scope_vals[] = {
1311 | {0, 0, "ARRAY-COMMAND"},
1312 | {1, 1, "CARRIER-COMMAND"},
1313 | {2, 2, "O-RU-COMMAND"},
1314 | {3, 15, "reserved"},
1315 | {0, 0, NULL((void*)0)}
1316 | };
1317 |
1318 | /* N.B., table in 7.5.3.38 is truncated.. */
1319 | static const range_string st4_cmd_type_vals[] = {
1320 | {0, 0, "reserved for future command types"},
1321 | {1, 1, "TIME_DOMAIN_BEAM_CONFIG"},
1322 | {2, 2, "TDD_CONFIG_PATTERN"},
1323 | {3, 3, "TRX_CONTROL"},
1324 | {4, 4, "ASM"},
1325 | {5, 5, "TRX_CONTROL_BIDIR"},
1326 | {6, 255, "reserved for future command types"},
1327 | {0, 0, NULL((void*)0)}
1328 | };
1329 |
1330 | /* Table 7.5.3.51-1 */
1331 | static const value_string log2maskbits_vals[] = {
1332 | {0, "reserved"},
1333 | {1, "min antMask size is 16 bits.."},
1334 | {2, "min antMask size is 16 bits.."},
1335 | {3, "min antMask size is 16 bits.."},
1336 | {4, "16 bits"},
1337 | {5, "32 bits"},
1338 | {6, "64 bits"},
1339 | {7, "128 bits"},
1340 | {8, "256 bits"},
1341 | {9, "512 bits"},
1342 | {10, "1024 bits"},
1343 | {11, "2048 bits"},
1344 | {12, "4096 bits"},
1345 | {13, "8192 bits"},
1346 | {14, "16384 bits"},
1347 | {15, "reserved"},
1348 | {0, NULL((void*)0)}
1349 | };
1350 |
1351 | /* Table 16.1-1 Sleep modes */
1352 | static const value_string sleep_mode_trx_vals[] = {
1353 | { 0, "TRXC-mode0-wake-up-duration (symbol)"},
1354 | { 1, "TRXC-mode1-wake-up-duration (L)"},
1355 | { 2, "TRXC-mode2-wake-up-duration (M)"},
1356 | { 3, "TRXC-mode3-wake-up-duration (N)"},
1357 | { 0, NULL((void*)0)}
1358 | };
1359 |
1360 | static const value_string sleep_mode_asm_vals[] = {
1361 | { 0, "ASM-mode0-wake-up-duration (symbol)"},
1362 | { 1, "ASM-mode1-wake-up-duration (L)"},
1363 | { 2, "ASM-mode2-wake-up-duration (M)"},
1364 | { 3, "ASM-mode3-wake-up-duration (N)"},
1365 | { 0, NULL((void*)0)}
1366 | };
1367 |
1368 | /* 7.7.21.3.1 */
1369 | static const value_string prg_size_st5_vals[] = {
1370 | { 0, "reserved"},
1371 | { 1, "Precoding resource block group size as WIDEBAND"},
1372 | { 2, "Precoding resource block group size 2"},
1373 | { 3, "Precoding resource block group size 4"},
1374 | { 0, NULL((void*)0)}
1375 | };
1376 |
1377 | /* 7.7.21.3.2 */
1378 | static const value_string prg_size_st6_vals[] = {
1379 | { 0, "if ciPrbGroupSize is 2 or 4, then ciPrbGroupSize, else WIDEBAND"},
1380 | { 1, "Precoding resource block group size as WIDEBAND"},
1381 | { 2, "Precoding resource block group size 2"},
1382 | { 3, "Precoding resource block group size 4"},
1383 | { 0, NULL((void*)0)}
1384 | };
1385 |
1386 | /* 7.7.24.4 */
1387 | static const value_string alpn_per_sym_vals[] = {
1388 | { 0, "report one allocated IPN value per all allocated symbols with DMRS"},
1389 | { 1, "report one allocated IPN value per group of consecutive DMRS symbols"},
1390 | { 0, NULL((void*)0)}
1391 | };
1392 |
1393 | /* 7.7.24.5 */
1394 | static const value_string ant_dmrs_snr_vals[] = {
1395 | { 0, "O-RU shall not report the MEAS_ANT_DMRS_SNR"},
1396 | { 1, "O-RU shall report the MEAS_ANT_DMRS_SNR"},
1397 | { 0, NULL((void*)0)}
1398 | };
1399 |
1400 | /* 7.7.24.14 */
1401 | static const value_string dtype_vals[] = {
1402 | { 0, "assume DMRS configuration type 1"},
1403 | { 1, "assume DMRS configuration type 2"},
1404 | { 0, NULL((void*)0)}
1405 | };
1406 |
1407 | /* 7.7.24.17 */
1408 | static const value_string papr_type_vals[] = {
1409 | { 0, "sequence generator type 1 for short sequence lengths"},
1410 | { 1, "sequence generator type 1 for long sequence lengths"},
1411 | { 2, "sequence generator type 2 for short sequence lengths"},
1412 | { 3, "sequence generator type 2 for long sequence lengths"},
1413 | { 0, NULL((void*)0)}
1414 | };
1415 |
1416 | /* 7.7.24.18 */
1417 | static const value_string hopping_mode_vals[] = {
1418 | { 0, "neither group, nor sequence hopping is enabled"},
1419 | { 1, "group hopping is enabled and sequence hopping is disabled"},
1420 | { 2, "sequence hopping is enabled and group hopping is disabled"},
1421 | { 3, "reserved"},
1422 | { 0, NULL((void*)0)}
1423 | };
1424 |
1425 | /* Table 7.7.31.2-1 */
1426 | static const value_string mcs_table_vals[] = {
1427 | { 0, "MCS index table 1 for PDSCH and PUSCH without transform precoding" },
1428 | { 1, "MCS index table 2 for PDSCH and PUSCH without transform precoding" },
1429 | { 2, "MCS index table 3 for PDSCH and PUSCH without transform precoding" },
1430 | { 3, "MCS index table 4 for PDSCH" },
1431 | { 4, "MCS index table for PUSCH with transform precoding and 64QAM" },
1432 | { 5, "MCS index table 2 for PUSCH with transform precoding and 64QAM" },
1433 | { 0, NULL((void*)0)}
1434 | };
1435 |
1436 | /* 7.7.32.9 */
1437 | static const value_string full_pwr_mode_vals[] = {
1438 | { 0, "not configured"},
1439 | { 1, "full power mode 0"},
1440 | { 2, "full power mode 1"},
1441 | { 3, "full power mode 2"},
1442 | { 0, NULL((void*)0)}
1443 | };
1444 |
1445 |
1446 | static const true_false_string tfs_sfStatus =
1447 | {
1448 | "subframe was transmitted",
1449 | "subframe was dropped"
1450 | };
1451 |
1452 | static const true_false_string tfs_lbtBufErr =
1453 | {
1454 | "buffer overflow – data received at O-RU is larger than the available buffer size",
1455 | "reserved"
1456 | };
1457 |
1458 | static const true_false_string tfs_partial_full_sf = {
1459 | "partial SF",
1460 | "full SF"
1461 | };
1462 |
1463 | static const true_false_string disable_tdbfns_tfs = {
1464 | "beam numbers excluded",
1465 | "beam numbers included"
1466 | };
1467 |
1468 | static const true_false_string continuity_indication_tfs = {
1469 | "continuity between current and next bundle",
1470 | "discontinuity between current and next bundle"
1471 | };
1472 |
1473 | static const true_false_string prb_mode_tfs = {
1474 | "PRB-BLOCK mode",
1475 | "PRB-MASK mode"
1476 | };
1477 |
1478 | static const true_false_string symbol_direction_tfs = {
1479 | "DL symbol",
1480 | "UL symbol"
1481 | };
1482 |
1483 | static const true_false_string symbol_guard_tfs = {
1484 | "guard symbol",
1485 | "non-guard symbol"
1486 | };
1487 |
1488 | static const true_false_string beam_numbers_included_tfs = {
1489 | "time-domain beam numbers excluded in this command",
1490 | "time-domain beam numbers included in this command"
1491 | };
1492 |
1493 | static const true_false_string measurement_flag_tfs = {
1494 | "at least one additional measurement report or command after the current one",
1495 | "no additional measurement report or command"
1496 | };
1497 |
1498 | static const true_false_string repetition_se6_tfs = {
1499 | "repeated highest priority data section in the C-Plane message",
1500 | "no repetition"
1501 | };
1502 |
1503 | static const true_false_string repetition_se19_tfs = {
1504 | "per port information not present in the extension",
1505 | "per port info present in the extension"
1506 | };
1507 |
1508 | static const true_false_string tfs_report_no_report_pos_meas =
1509 | {
1510 | "Report MEAS_UE_POS for UE",
1511 | "Do not report UE_POS for UE"
1512 | };
1513 |
1514 |
1515 | /* Forward declaration */
1516 | static int dissect_udcompparam(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree, unsigned offset,
1517 | unsigned comp_meth,
1518 | uint32_t *exponent, uint16_t *sReSMask, bool_Bool for_sinr);
1519 |
1520 |
1521 | static const true_false_string ready_tfs = {
1522 | "message is a \"ready\" message",
1523 | "message is a ACK message"
1524 | };
1525 |
1526 | static const true_false_string multi_sd_scope_tfs = {
1527 | "Puncturing pattern applies to current and following sections",
1528 | "Puncturing pattern applies to current section"
1529 | };
1530 |
1531 | static const true_false_string tfs_ueid_reset = {
1532 | "cannot assume same UE as in preceding slot",
1533 | "can assume same UE as in preceding slot"
1534 | };
1535 |
1536 |
1537 | /* Config for (and later, worked-out allocations) bundles for ext11 (dynamic BFW) */
1538 | typedef struct {
1539 | /* Ext 6 config */
1540 | bool_Bool ext6_set;
1541 | uint8_t ext6_rbg_size; /* number of PRBs allocated by bitmask */
1542 |
1543 | uint8_t ext6_num_bits_set;
1544 | uint8_t ext6_bits_set[28]; /* Which bit position this entry has */
1545 | /* TODO: store an f value for each bit position? */
1546 |
1547 | /* Ext 12 config */
1548 | bool_Bool ext12_set;
1549 | unsigned ext12_num_pairs;
1550 | #define MAX_BFW_EXT12_PAIRS128 128
1551 | struct {
1552 | uint8_t off_start_prb;
1553 | uint8_t num_prb;
1554 | } ext12_pairs[MAX_BFW_EXT12_PAIRS128];
1555 |
1556 | /* Ext 13 config */
1557 | bool_Bool ext13_set;
1558 | unsigned ext13_num_start_prbs;
1559 | #define MAX_BFW_EXT13_ALLOCATIONS128 128
1560 | unsigned ext13_start_prbs[MAX_BFW_EXT13_ALLOCATIONS128];
1561 | /* TODO: store nextSymbolId here too? */
1562 |
1563 | /* Ext 21 config */
1564 | bool_Bool ext21_set;
1565 | uint8_t ext21_ci_prb_group_size;
1566 |
1567 | /* Results/settings (after calling ext11_work_out_bundles()) */
1568 | uint32_t num_bundles;
1569 | #define MAX_BFW_BUNDLES512 512
1570 | struct {
1571 | uint32_t start; /* first prb of bundle */
1572 | uint32_t end; /* last prb of bundle*/
1573 | bool_Bool is_orphan; /* true if not complete (i.e., end-start < numBundPrb) */
1574 | } bundles[MAX_BFW_BUNDLES512];
1575 | } ext11_settings_t;
1576 |
1577 |
1578 | /* Work out bundle allocation for ext 11. Take into account ext6/ext21, ext12 or ext13 in this section before ext 11. */
1579 | /* Won't be called with numBundPrb=0 */
1580 | static void ext11_work_out_bundles(unsigned startPrbc,
1581 | unsigned numPrbc,
1582 | unsigned numBundPrb, /* number of PRBs per (full) bundle */
1583 | ext11_settings_t *settings)
1584 | {
1585 | /* Allocation configured by ext 6 */
1586 | if (settings->ext6_set) {
1587 | unsigned bundles_per_entry = (settings->ext6_rbg_size / numBundPrb);
1588 |
1589 | /* Need to cope with these not dividing exactly, or even having more PRbs in a bundle that
1590 | rbg size. i.e. each bundle gets the correct number of PRBs until
1591 | all rbg entries are consumed... */
1592 |
1593 | /* TODO: need to check 7.9.4.2. Different cases depending upon value of RAD */
1594 |
1595 | if (bundles_per_entry == 0) {
1596 | bundles_per_entry = 1;
1597 | }
1598 |
1599 | /* Ext6 behaviour may also be affected by ext 21 */
1600 | if (settings->ext21_set) {
1601 | /* N.B., have already checked that numPrbc is not 0 */
1602 |
1603 | /* ciPrbGroupSize overrides number of contiguous PRBs in group */
1604 | bundles_per_entry = (settings->ext6_rbg_size / settings->ext21_ci_prb_group_size);
1605 |
1606 | /* numPrbc is the number of PRB groups per antenna - handled in call to dissect_bfw_bundle() */
1607 | }
1608 |
1609 | unsigned bundles_set = 0;
1610 | bool_Bool reached_orphan = false0;
1611 | /* For each bit set in ext6 rbg mask.. */
1612 | for (unsigned n=0;
1613 | !reached_orphan && n < (settings->ext6_num_bits_set * settings->ext6_rbg_size) / numBundPrb;
1614 | n++) {
1615 |
1616 | /* Watch out for array bound */
1617 | if (n >= 28) {
1618 | break;
1619 | }
1620 |
1621 | /* For each bundle... */
1622 |
1623 | /* TODO: Work out where first PRB is */
1624 | /* May not be the start of an rbg block... */
1625 | uint32_t prb_start = (settings->ext6_bits_set[n] * settings->ext6_rbg_size);
1626 |
1627 | /* For each bundle within identified rbgSize block */
1628 | for (unsigned m=0; !reached_orphan && m < bundles_per_entry; m++) {
1629 |
1630 | settings->bundles[bundles_set].start = startPrbc+prb_start+(m*numBundPrb);
1631 |
1632 | /* Start already beyond end, so doesn't count. */
1633 | if (settings->bundles[bundles_set].start > (startPrbc+numPrbc-1)) {
1634 | settings->num_bundles = bundles_set;
1635 | return;
1636 | }
1637 |
1638 | /* Bundle consists of numBundPrb bundles */
1639 | /* TODO: may involve PRBs from >1 rbg blocks.. */
1640 | settings->bundles[bundles_set].end = startPrbc+prb_start+((m+1)*numBundPrb)-1;
1641 | if (settings->bundles[bundles_set].end > (startPrbc+numPrbc-1)) {
1642 | /* Extends beyond end, so counts but is an orphan bundle */
1643 | settings->bundles[bundles_set].end = startPrbc+numPrbc-1;
1644 | settings->bundles[bundles_set].is_orphan = true1;
1645 | reached_orphan = true1;
1646 | }
1647 |
1648 | /* Get out if have reached array bound */
1649 | if (++bundles_set == MAX_BFW_BUNDLES512) {
1650 | return;
1651 | }
1652 | }
1653 | }
1654 | settings->num_bundles = bundles_set;
1655 | }
1656 |
1657 | /* Allocation configured by ext 12 */
1658 | else if (settings->ext12_set) {
1659 | /* First, allocate normally from startPrbc, numPrbc */
1660 | settings->num_bundles = (numPrbc+numBundPrb-1) / numBundPrb;
1661 |
1662 | /* Don't overflow settings->bundles[] ! */
1663 | settings->num_bundles = MIN(MAX_BFW_BUNDLES, settings->num_bundles)(((512) < (settings->num_bundles)) ? (512) : (settings-> num_bundles));
1664 |
1665 | for (uint32_t n=0; n < settings->num_bundles; n++) {
1666 | settings->bundles[n].start = startPrbc + n*numBundPrb;
1667 | settings->bundles[n].end = settings->bundles[n].start + numBundPrb-1;
1668 | /* Does it go beyond the end? */
1669 | if (settings->bundles[n].end > startPrbc+numPrbc) {
1670 | settings->bundles[n].end = startPrbc+numPrbc;
1671 | settings->bundles[n].is_orphan = true1;
1672 | }
1673 | }
1674 | if (settings->num_bundles == MAX_BFW_BUNDLES512) {
1675 | return;
1676 | }
1677 |
1678 | unsigned prb_offset = startPrbc + numPrbc;
1679 |
1680 | /* Loop over pairs, adding bundles for each */
1681 | for (unsigned p=0; p < settings->ext12_num_pairs; p++) {
1682 | prb_offset += settings->ext12_pairs[p].off_start_prb;
1683 | unsigned pair_bundles = (settings->ext12_pairs[p].num_prb+numBundPrb-1) / numBundPrb;
1684 |
1685 | for (uint32_t n=0; n < pair_bundles; n++) {
1686 | unsigned idx = settings->num_bundles;
1687 |
1688 | settings->bundles[idx].start = prb_offset + n*numBundPrb;
1689 | settings->bundles[idx].end = settings->bundles[idx].start + numBundPrb-1;
1690 | /* Does it go beyond the end? */
1691 | if (settings->bundles[idx].end > prb_offset + settings->ext12_pairs[p].num_prb) {
1692 | settings->bundles[idx].end = prb_offset + settings->ext12_pairs[p].num_prb;
1693 | settings->bundles[idx].is_orphan = true1;
1694 | }
1695 | /* Range check / return */
1696 | settings->num_bundles++;
1697 | if (settings->num_bundles == MAX_BFW_BUNDLES512) {
1698 | return;
1699 | }
1700 | }
1701 |
1702 | prb_offset += settings->ext12_pairs[p].num_prb;
1703 | }
1704 | }
1705 |
1706 | /* Allocation configured by ext 13 */
1707 | else if (settings->ext13_set) {
1708 | unsigned alloc_size = (numPrbc+numBundPrb-1) / numBundPrb;
1709 | settings->num_bundles = alloc_size * settings->ext13_num_start_prbs;
1710 |
1711 | /* Don't overflow settings->bundles[] ! */
1712 | settings->num_bundles = MIN(MAX_BFW_BUNDLES, settings->num_bundles)(((512) < (settings->num_bundles)) ? (512) : (settings-> num_bundles));
1713 |
1714 | for (unsigned alloc=0; alloc < settings->ext13_num_start_prbs; alloc++) {
1715 | unsigned alloc_start = alloc * alloc_size;
1716 | for (uint32_t n=0; n < alloc_size; n++) {
1717 | if ((alloc_start+n) >= MAX_BFW_BUNDLES512) {
1718 | /* ERROR */
1719 | return;
1720 | }
1721 | settings->bundles[alloc_start+n].start = settings->ext13_start_prbs[alloc] + startPrbc + n*numBundPrb;
1722 | settings->bundles[alloc_start+n].end = settings->bundles[alloc_start+n].start + numBundPrb-1;
1723 | if (settings->bundles[alloc_start+n].end > settings->ext13_start_prbs[alloc] + numPrbc) {
1724 | settings->bundles[alloc_start+n].end = settings->ext13_start_prbs[alloc] + numPrbc;
1725 | settings->bundles[alloc_start+n].is_orphan = true1;
1726 | }
1727 | }
1728 | }
1729 | }
1730 |
1731 | /* Case where bundles are not controlled by other extensions - just divide up range into bundles we have */
1732 | else {
1733 | settings->num_bundles = (numPrbc+numBundPrb-1) / numBundPrb; /* rounded up */
1734 |
1735 | /* Don't overflow settings->bundles[] */
1736 | settings->num_bundles = MIN(MAX_BFW_BUNDLES, settings->num_bundles)(((512) < (settings->num_bundles)) ? (512) : (settings-> num_bundles));
1737 |
1738 | /* For each bundle.. */
1739 | for (uint32_t n=0; n < settings->num_bundles; n++) {
1740 | /* Allocate start and end */
1741 | settings->bundles[n].start = startPrbc + n*numBundPrb;
1742 | settings->bundles[n].end = settings->bundles[n].start + numBundPrb - 1;
1743 | /* If would go beyond end of PRBs, limit and identify as orphan */
1744 | if (settings->bundles[n].end > startPrbc+numPrbc) {
1745 | settings->bundles[n].end = startPrbc+numPrbc;
1746 | settings->bundles[n].is_orphan = true1;
1747 | }
1748 | }
1749 | }
1750 | }
1751 |
1752 |
1753 | /* Modulation Compression configuration */
1754 | typedef struct {
1755 | /* Application of each entry is filtered by RE.
1756 | * TODO: should also be filtered by PRB + symbol... */
1757 | uint16_t mod_compr_re_mask;
1758 |
1759 | /* Settings to apply */
1760 | bool_Bool mod_compr_csf;
1761 | float mod_compr_scaler;
1762 | } mod_compr_config_t;
1763 |
1764 | /* Multiple configs with a section */
1765 | typedef struct {
1766 | uint16_t section_id;
1767 | uint32_t num_configs;
1768 |
1769 | #define MAX_MOD_COMPR_CONFIGS12 12
1770 | mod_compr_config_t configs[MAX_MOD_COMPR_CONFIGS12];
1771 | } section_mod_compr_config_t;
1772 |
1773 | /* Flow has separate configs for each section */
1774 | typedef struct {
1775 | uint16_t num_sections;
1776 |
1777 | /* Separate config for each section */
1778 | section_mod_compr_config_t sections[MAX_SECTION_IDs32];
1779 | } mod_compr_params_t;
1780 |
1781 |
1782 | typedef struct {
1783 | uint32_t frame_number;
1784 | nstime_t frame_time;
1785 |
1786 | /* Timing to match */
1787 | uint8_t frame;
1788 | uint8_t subframe;
1789 | uint8_t slot;
1790 | uint8_t startSymbol;
1791 |
1792 | bool_Bool in_use;
1793 | uint16_t startPrb;
1794 | uint16_t numPrb;
1795 | uint16_t numSymbols;
1796 | uint16_t beamIds[273];
1797 | } section_details_t;
1798 |
1799 | typedef struct {
1800 | uint16_t sectionId;
1801 | /* For the same sectionId, can have 2 currently active entries.. */
1802 | section_details_t details[2];
1803 | } expected_section_data_t;
1804 |
1805 |
1806 | /*******************************************************/
1807 | /* Overall state of a flow (eAxC/plane) */
1808 | typedef struct {
1809 | /* State for sequence analysis [each direction] */
1810 | bool_Bool last_frame_seen[2];
1811 | uint32_t last_frame[2];
1812 | uint8_t next_expected_sequence_number[2];
1813 |
1814 | /* expected frames. sectionId -> expected_section_data_t* */
1815 | wmem_tree_t *expected_sections[2]; /* [direction] */
1816 |
1817 | /* Table recording ackNack requests (ackNackId -> ack_nack_request_t*)
1818 | Note that this assumes that the same ackNackId will not be reused within a state,
1819 | which may well not be valid */
1820 | wmem_tree_t *ack_nack_requests;
1821 |
1822 | /* Store udCompHdr seen in C-Plane for UL - can be looked up and used by U-PLane.
1823 | Note that this appears in the common section header parts of ST1, ST3, ST5,
1824 | so can still be over-written per sectionId in the U-Plane */
1825 | unsigned ul_ud_comp_hdr_frame;
1826 | bool_Bool ul_ud_comp_hdr_set;
1827 | unsigned ul_ud_comp_hdr_bit_width;
1828 | int ul_ud_comp_hdr_compression;
1829 |
1830 | bool_Bool udcomphdrDownlink_heuristic_result_set;
1831 | bool_Bool udcomphdrDownlink_heuristic_result;
1832 | bool_Bool udcomphdrUplink_heuristic_result_set;
1833 | bool_Bool udcomphdrUplink_heuristic_result;
1834 |
1835 | /* Modulation compression params */
1836 | mod_compr_params_t mod_comp_params;
1837 | } flow_state_t;
1838 |
1839 | static section_mod_compr_config_t* get_mod_compr_section_to_write(flow_state_t *flow,
1840 | unsigned sectionId)
1841 | {
1842 | if (flow == NULL((void*)0)) {
1843 | return NULL((void*)0);
1844 | }
1845 |
1846 | /* Look for this section among existing entries */
1847 | for (unsigned s=0; s < flow->mod_comp_params.num_sections; s++) {
1848 | if (flow->mod_comp_params.sections[s].section_id == sectionId) {
1849 | return &flow->mod_comp_params.sections[s];
1850 | }
1851 | }
1852 |
1853 | /* Not found, so try to add a new one */
1854 | if (flow->mod_comp_params.num_sections >= MAX_SECTION_IDs32) {
1855 | /* Can't allocate one! */
1856 | return NULL((void*)0);
1857 | }
1858 | else {
1859 | flow->mod_comp_params.sections[flow->mod_comp_params.num_sections].section_id = sectionId;
1860 | return &flow->mod_comp_params.sections[flow->mod_comp_params.num_sections++];
1861 | }
1862 | }
1863 |
1864 | static section_mod_compr_config_t* get_mod_compr_section_to_read(flow_state_t *flow,
1865 | unsigned sectionId)
1866 | {
1867 | if (flow == NULL((void*)0)) {
1868 | return NULL((void*)0);
1869 | }
1870 |
1871 | /* Look for this section among existing entries */
1872 | for (unsigned s=0; s < flow->mod_comp_params.num_sections; s++) {
1873 | if (flow->mod_comp_params.sections[s].section_id == sectionId) {
1874 | return &flow->mod_comp_params.sections[s];
1875 | }
1876 | }
1877 |
1878 | /* Not found */
1879 | return NULL((void*)0);
1880 | }
1881 |
1882 |
1883 |
1884 | typedef struct {
1885 | uint32_t request_frame_number;
1886 | nstime_t request_frame_time;
1887 | enum {
1888 | SE22,
1889 | ST4Cmd1,
1890 | ST4Cmd2,
1891 | ST4Cmd3,
1892 | ST4Cmd4
1893 | } requestType;
1894 |
1895 | uint32_t response_frame_number;
1896 | nstime_t response_frame_time;
1897 | } ack_nack_request_t;
1898 |
1899 | static const value_string acknack_type_vals[] = {
1900 | { SE22, "SE 22" },
1901 | { ST4Cmd1, "ST4 (TIME_DOMAIN_BEAM_CONFIG)" },
1902 | { ST4Cmd2, "ST4 (TDD_CONFIG_PATTERN)" },
1903 | { ST4Cmd3, "ST4 (TRX_CONTROL)" },
1904 | { ST4Cmd4, "ST4 (ASM)" },
1905 | { 0, NULL((void*)0)}
1906 | };
1907 |
1908 | #define ORAN_C_PLANE0 0
1909 | #define ORAN_U_PLANE1 1
1910 |
1911 | /* Using parts of src/dst MAC address, so don't confuse UL messages with DL messages configuring UL.. */
1912 | static uint32_t make_flow_key(packet_info *pinfo, uint16_t eaxc_id, uint8_t plane, bool_Bool opposite_dir)
1913 | {
1914 | uint16_t eth_bits = 0;
1915 | if (pinfo->dl_src.len == 6 && pinfo->dl_dst.len == 6) {
1916 | /* Only using (most of) 2 bytes from addresses for now, but reluctant to make key longer.. */
1917 | const uint8_t *src_eth = (uint8_t*)pinfo->dl_src.data;
1918 | const uint8_t *dst_eth = (uint8_t*)pinfo->dl_dst.data;
1919 | if (!opposite_dir) {
1920 | eth_bits = (src_eth[0]<<8) | dst_eth[5];
1921 | }
1922 | else {
1923 | eth_bits = (dst_eth[0]<<8) | src_eth[5];
1924 | }
1925 | }
1926 | return eaxc_id | (plane << 16) | (eth_bits << 17);
1927 | }
1928 |
1929 |
1930 | /* Table maintained on first pass from flow_key(uint32_t) -> flow_state_t* */
1931 | static wmem_tree_t *flow_states_table;
1932 |
1933 | typedef struct {
1934 | uint32_t frame_number;
1935 | uint16_t sectionId;
1936 | uint32_t gap_in_usecs;
1937 | uint8_t symbol;
1938 | uint16_t startPrbu;
1939 | uint16_t numPrbu;
1940 | } corresponding_uplane_frame;
1941 |
1942 | /* Table consulted on subsequent passes: frame_num -> flow_result_t* */
1943 | static wmem_tree_t *flow_results_table;
1944 |
1945 | typedef struct {
1946 | /* Sequence analysis */
1947 | bool_Bool unexpected_seq_number;
1948 | uint8_t expected_sequence_number;
1949 | uint32_t previous_frame;
1950 |
1951 | /* sectionId -> expected_section_data_t* */
1952 | /* Frame only covers one direction */
1953 | wmem_tree_t *expected_sections;
1954 |
1955 | /* List of u-plane frames (corresponding_uplane_frame*) corresponding to a c-plane frame */
1956 | wmem_list_t *u_plane_frames;
1957 | } flow_result_t;
1958 |
1959 |
1960 | /* Uplink timing */
1961 | /* For a given symbol, track first to last UL frame to find out first-last time */
1962 | /* frameId (8) + subframeId (4) + slotId (6) + symbolId (6) = 24 bits */
1963 | /* N.B. if a capture lasts > 2.5s, may see same timing come around again... */
1964 | static uint32_t get_timing_key(uint8_t frameId, uint8_t subframeId, uint8_t slotId, uint8_t symbolId)
1965 | {
1966 | return symbolId + (slotId<<8) + (subframeId<<14) + (frameId<<18);
1967 | }
1968 |
1969 | typedef struct {
1970 | uint32_t first_frame;
1971 | nstime_t first_frame_time;
1972 | uint32_t frames_seen_in_symbol;
1973 | uint32_t last_frame_in_symbol;
1974 | } ul_timing_for_slot;
1975 |
1976 | /* Set during first pass. timing_key -> ul_timing_for_slot* */
1977 | static wmem_tree_t *ul_symbol_timing;
1978 |
1979 |
1980 | /* Tracking lifetimes of DL beamIds */
1981 | typedef struct {
1982 | uint32_t frame_defined;
1983 | uint32_t symbol_when_defined;
1984 | } bfw_definition;
1985 |
1986 | /* Maintained during first pass: beamId (from ext11) -> bfw_definition */
1987 | static wmem_tree_t *dl_beam_ids_defined;
1988 | /* Lookup where/when beamIds were defined (frameid:beamid) -> bfw_definition */
1989 | static wmem_tree_t *dl_beam_ids_results;
1990 |
1991 |
1992 | static void show_link_to_acknack_response(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo,
1993 | ack_nack_request_t *response);
1994 |
1995 |
1996 |
1997 |
1998 | static void write_pdu_label_and_info(proto_item *ti1, proto_item *ti2,
1999 | packet_info *pinfo, const char *format, ...) G_GNUC_PRINTF(4, 5)__attribute__((__format__ (__printf__, 4, 5)));
2000 |
2001 | /* Write the given formatted text to:
2002 | - the info column (if pinfo != NULL)
2003 | - 1 or 2 other labels (optional)
2004 | */
2005 | static void write_pdu_label_and_info(proto_item *ti1, proto_item *ti2,
2006 | packet_info *pinfo, const char *format, ...)
2007 | {
2008 | #define MAX_INFO_BUFFER256 256
2009 | char info_buffer[MAX_INFO_BUFFER256];
2010 | va_list ap;
2011 |
2012 | if ((ti1 == NULL((void*)0)) && (ti2 == NULL((void*)0)) && (pinfo == NULL((void*)0))) {
2013 | return;
2014 | }
2015 |
2016 | va_start(ap, format)__builtin_va_start(ap, format);
2017 | vsnprintf(info_buffer, MAX_INFO_BUFFER256, format, ap);
2018 | va_end(ap)__builtin_va_end(ap);
2019 |
2020 | /* Add to indicated places */
2021 | if (pinfo != NULL((void*)0)) {
2022 | col_append_str(pinfo->cinfo, COL_INFO, info_buffer);
2023 | }
2024 | if (ti1 != NULL((void*)0)) {
2025 | proto_item_append_text(ti1, "%s", info_buffer);
2026 | }
2027 | if (ti2 != NULL((void*)0)) {
2028 | proto_item_append_text(ti2, "%s", info_buffer);
2029 | }
2030 | }
2031 |
2032 | /* Add section labels (type + PRB range) for C-Plane, U-Plane */
2033 | static void
2034 | write_section_info(proto_item *section_heading, packet_info *pinfo, proto_item *protocol_item,
2035 | uint32_t section_id, uint32_t start_prbx, uint32_t num_prbx, uint32_t rb)
2036 | {
2037 | switch (num_prbx) {
2038 | case 0:
2039 | /* None -> all */
2040 | write_pdu_label_and_info(section_heading, protocol_item, pinfo, ", Id: %4d (all PRBs)", section_id);
2041 | break;
2042 | case 1:
2043 | /* Single PRB */
2044 | write_pdu_label_and_info(section_heading, protocol_item, pinfo, ", Id: %4d (PRB: %7u)", section_id, start_prbx);
2045 | break;
2046 | default:
2047 | /* Range */
2048 | write_pdu_label_and_info(section_heading, protocol_item, pinfo, ", Id: %4d (PRB: %3u-%3u%s)", section_id, start_prbx,
2049 | start_prbx + (num_prbx-1)*(1+rb), rb ? " (every-other)" : "");
2050 | }
2051 | }
2052 |
2053 | static void
2054 | write_channel_section_info(proto_item *section_heading, packet_info *pinfo,
2055 | uint32_t section_id, uint32_t ueId, uint32_t start_prbx, uint32_t num_prbx,
2056 | uint32_t num_trx)
2057 | {
2058 | switch (num_prbx) {
2059 | case 0:
2060 | /* TODO: ?? */
2061 | break;
2062 | case 1:
2063 | /* Single PRB */
2064 | write_pdu_label_and_info(section_heading, NULL((void*)0), pinfo,
2065 | ", Id: %4d (UEId=%5u PRB %7u, %2u antennas)",
2066 | section_id, ueId, start_prbx, num_trx);
2067 | break;
2068 | default:
2069 | /* Range */
2070 | write_pdu_label_and_info(section_heading, NULL((void*)0), pinfo,
2071 | ", Id: %4d (UEId=%5u PRBs %3u-%3u, %2u antennas)",
2072 | section_id, ueId, start_prbx, start_prbx+num_prbx-1, num_trx);
2073 | }
2074 | }
2075 |
2076 | /* Add a reserved field, and warn if value isn't 0 */
2077 | /* TODO: maybe add a pref not to output expert warning if becomes too annoying? */
2078 | static void add_reserved_field(proto_tree *tree, int hf, tvbuff_t *tvb, int offset, int len)
2079 | {
2080 | uint32_t reserved;
2081 | proto_item *res_ti = proto_tree_add_item_ret_uint(tree, hf, tvb, offset, len, ENC_NA0x00000000, &reserved);
2082 | if (reserved != 0) {
2083 | expert_add_info_format(NULL((void*)0), res_ti, &ei_oran_reserved_not_zero,
2084 | "reserved field saw value of 0x%x", reserved);
2085 | }
2086 | }
2087 |
2088 | /* 5.1.3.2.7 (real time control data / IQ data transfer message series identifier) */
2089 | static void
2090 | addPcOrRtcid(tvbuff_t *tvb, proto_tree *tree, unsigned *offset, int hf, uint16_t *eAxC, oran_tap_info *tap_info)
2091 | {
2092 | /* Subtree */
2093 | proto_item *oran_pcid_ti = proto_tree_add_item(tree, hf,
2094 | tvb, *offset, 2, ENC_NA0x00000000);
2095 | proto_tree *oran_pcid_tree = proto_item_add_subtree(oran_pcid_ti, ett_oran_ecpri_pcid);
2096 |
2097 | uint64_t duPortId, bandSectorId, ccId, ruPortId = 0;
2098 | int id_offset = *offset;
2099 |
2100 | /* All parts of eAxC should be above 0, and should total 16 bits (breakdown controlled by preferences) */
2101 | if (!((pref_du_port_id_bits > 0) && (pref_bandsector_id_bits > 0) && (pref_cc_id_bits > 0) && (pref_ru_port_id_bits > 0) &&
2102 | ((pref_du_port_id_bits + pref_bandsector_id_bits + pref_cc_id_bits + pref_ru_port_id_bits) == 16))) {
2103 | expert_add_info(NULL((void*)0), tree, &ei_oran_invalid_eaxc_bit_width);
2104 | *eAxC = 0;
2105 | *offset += 2;
2106 | return;
2107 | }
2108 |
2109 | unsigned bit_offset = *offset * 8;
2110 |
2111 | /* N.B. For sequence analysis / tapping, just interpret these 2 bytes as eAxC ID... */
2112 | *eAxC = tvb_get_uint16(tvb, *offset, ENC_BIG_ENDIAN0x00000000);
2113 |
2114 | /* DU Port ID */
2115 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_du_port_id, tvb, bit_offset, pref_du_port_id_bits, &duPortId, ENC_BIG_ENDIAN0x00000000);
2116 | bit_offset += pref_du_port_id_bits;
2117 | /* BandSector ID */
2118 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_bandsector_id, tvb, bit_offset, pref_bandsector_id_bits, &bandSectorId, ENC_BIG_ENDIAN0x00000000);
2119 | bit_offset += pref_bandsector_id_bits;
2120 | /* CC ID */
2121 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_cc_id, tvb, bit_offset, pref_cc_id_bits, &ccId, ENC_BIG_ENDIAN0x00000000);
2122 | bit_offset += pref_cc_id_bits;
2123 | /* RU Port ID */
2124 | proto_tree_add_bits_ret_val(oran_pcid_tree, hf_oran_ru_port_id, tvb, bit_offset, pref_ru_port_id_bits, &ruPortId, ENC_BIG_ENDIAN0x00000000);
2125 | *offset += 2;
2126 |
2127 | proto_item_append_text(oran_pcid_ti, " (DU_Port_ID: %d, BandSector_ID: %d, CC_ID: %d, RU_Port_ID: %d)",
2128 | (int)duPortId, (int)bandSectorId, (int)ccId, (int)ruPortId);
2129 | char id[16];
2130 | snprintf(id, 16, "%x:%x:%x:%x", (int)duPortId, (int)bandSectorId, (int)ccId, (int)ruPortId);
2131 | proto_item *pi = proto_tree_add_string(oran_pcid_tree, hf_oran_c_eAxC_ID, tvb, id_offset, 2, id);
2132 | proto_item_set_generated(pi);
2133 |
2134 | tap_info->eaxc = *eAxC;
2135 | tap_info->eaxc_du_port_id = (uint16_t)duPortId;
2136 | tap_info->eaxc_bandsector_id = (uint16_t)bandSectorId;
2137 | tap_info->eaxc_cc_id = (uint16_t)ccId;
2138 | tap_info->eaxc_ru_port_id = (uint16_t)ruPortId;
2139 | }
2140 |
2141 | /* Uniquely identify the U-plane stream that may need to be reassembled */
2142 | static uint32_t make_reassembly_id(uint32_t seqid, uint32_t direction, uint16_t eAxC,
2143 | uint8_t frameid, uint8_t subframeid,
2144 | uint8_t slotid, uint8_t symbolid)
2145 | {
2146 | /* N.B., no room in 32-bits for all of this info, so cut down some of the fields
2147 | and hope for no collisions */
2148 | return (seqid << 24) | (direction << 23) | (slotid << 22) | (subframeid << 18) |
2149 | (frameid << 9) | (symbolid << 6) | (eAxC & 0x3f);
2150 | }
2151 |
2152 | /* 5.1.3.2.8 ecpriSeqid (message identifier) */
2153 | /* Return out info that may be used for sequence number analysis and reassembly */
2154 | static int
2155 | addSeqid(tvbuff_t *tvb, proto_tree *oran_tree, int offset, int plane, uint32_t *seq_id, proto_item **seq_id_ti, packet_info *pinfo,
2156 | uint32_t *subseqid, uint32_t *e)
2157 | {
2158 | /* Subtree */
2159 | proto_item *seqIdItem = proto_tree_add_item(oran_tree, hf_oran_ecpri_seqid, tvb, offset, 2, ENC_NA0x00000000);
2160 | proto_tree *oran_seqid_tree = proto_item_add_subtree(seqIdItem, ett_oran_ecpri_seqid);
2161 |
2162 | /* Sequence ID (8 bits) */
2163 | *seq_id_ti = proto_tree_add_item_ret_uint(oran_seqid_tree, hf_oran_sequence_id, tvb, offset, 1, ENC_NA0x00000000, seq_id);
2164 | offset += 1;
2165 |
2166 | /* Show link back to previous sequence ID, if set */
2167 | flow_result_t *result = wmem_tree_lookup32(flow_results_table, pinfo->num);
2168 | if (result) {
2169 | proto_item *prev_ti = proto_tree_add_uint(oran_seqid_tree, hf_oran_previous_frame, tvb, 0, 0, result->previous_frame);
2170 | proto_item_set_generated(prev_ti);
2171 | }
2172 |
2173 | /* E bit */
2174 | proto_tree_add_item_ret_uint(oran_seqid_tree, hf_oran_e_bit, tvb, offset, 1, ENC_NA0x00000000, e);
2175 | /* Subsequence ID (7 bits) */
2176 | proto_tree_add_item_ret_uint(oran_seqid_tree, hf_oran_subsequence_id, tvb, offset, 1, ENC_NA0x00000000, subseqid);
2177 | offset += 1;
2178 |
2179 | /* radio-transport fragmentation not allowed for C-Plane messages */
2180 | if (plane == ORAN_C_PLANE0) {
2181 | if (*e !=1 || *subseqid != 0) {
2182 | expert_add_info(NULL((void*)0), seqIdItem, &ei_oran_radio_fragmentation_c_plane);
2183 | }
2184 | }
2185 |
2186 | /* Summary */
2187 | proto_item_append_text(seqIdItem, " (SeqId: %3d, E: %d, SubSeqId: %d)", *seq_id, *e, *subseqid);
2188 | return offset;
2189 | }
2190 |
2191 | static int dissect_symbolmask(tvbuff_t *tvb, proto_tree *tree, int offset, uint32_t *symbol_mask, proto_item **ti)
2192 | {
2193 | uint64_t temp_val;
2194 |
2195 | static int * const symbol_mask_flags[] = {
2196 | &hf_oran_symbol_mask_s13,
2197 | &hf_oran_symbol_mask_s12,
2198 | &hf_oran_symbol_mask_s11,
2199 | &hf_oran_symbol_mask_s10,
2200 | &hf_oran_symbol_mask_s9,
2201 | &hf_oran_symbol_mask_s8,
2202 | &hf_oran_symbol_mask_s7,
2203 | &hf_oran_symbol_mask_s6,
2204 | &hf_oran_symbol_mask_s5,
2205 | &hf_oran_symbol_mask_s4,
2206 | &hf_oran_symbol_mask_s3,
2207 | &hf_oran_symbol_mask_s2,
2208 | &hf_oran_symbol_mask_s1,
2209 | &hf_oran_symbol_mask_s0,
2210 | NULL((void*)0)
2211 | };
2212 |
2213 | proto_item *temp_ti = proto_tree_add_bitmask_ret_uint64(tree, tvb, offset,
2214 | hf_oran_symbol_mask,
2215 | ett_oran_symbol_mask, symbol_mask_flags,
2216 | ENC_BIG_ENDIAN0x00000000, &temp_val);
2217 | /* Set out parameters */
2218 | if (symbol_mask) {
2219 | *symbol_mask = (uint32_t)temp_val;
2220 | }
2221 | if (ti) {
2222 | *ti = temp_ti;
2223 | }
2224 | return offset+2;
2225 | }
2226 |
2227 | /* 7.7.1.2 bfwCompHdr (beamforming weight compression header) */
2228 | static int dissect_bfwCompHdr(tvbuff_t *tvb, proto_tree *tree, int offset,
2229 | uint32_t *iq_width, uint32_t *comp_meth, proto_item **comp_meth_ti)
2230 | {
2231 | /* Subtree */
2232 | proto_item *bfwcomphdr_ti = proto_tree_add_string_format(tree, hf_oran_bfwCompHdr,
2233 | tvb, offset, 1, "",
2234 | "bfwCompHdr");
2235 | proto_tree *bfwcomphdr_tree = proto_item_add_subtree(bfwcomphdr_ti, ett_oran_bfwcomphdr);
2236 |
2237 | /* Width and method */
2238 | proto_tree_add_item_ret_uint(bfwcomphdr_tree, hf_oran_bfwCompHdr_iqWidth,
2239 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, iq_width);
2240 | /* Special case: 0 -> 16 */
2241 | *iq_width = (*iq_width==0) ? 16 : *iq_width;
2242 | *comp_meth_ti = proto_tree_add_item_ret_uint(bfwcomphdr_tree, hf_oran_bfwCompHdr_compMeth,
2243 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, comp_meth);
2244 | offset++;
2245 |
2246 | /* Summary */
2247 | proto_item_append_text(bfwcomphdr_ti, " (IqWidth=%u, compMeth=%s)",
2248 | *iq_width,
2249 | val_to_str_const(*comp_meth, bfw_comp_headers_comp_meth, "reserved"));
2250 |
2251 | return offset;
2252 | }
2253 |
2254 | /* Return offset */
2255 | /* Returning number of entries set - would be good to also return an array of set TRX# so could show which array element
2256 | each BFW is actually for.. */
2257 | static int dissect_active_beamspace_coefficient_mask(tvbuff_t *tvb, proto_tree *tree, int offset, unsigned *num_trx_entries, uint16_t **trx_entries)
2258 | {
2259 | /* activeBeamspaceCoefficientMask - ceil(K/8) octets */
2260 | /* K is the number of elements in uncompressed beamforming weight vector.
2261 | * Calculated from parameters describing tx-array or tx-array */
2262 | unsigned k_octets = (pref_num_bf_antennas + 7) / 8;
2263 |
2264 | static uint16_t trx_enabled[1024];
2265 |
2266 | /* TODO: could use a bigger bitmask array, but for now just uses this bytes-worth for each byte */
2267 | static int * const mask_bits[] = {
2268 | &hf_oran_active_beamspace_coefficient_n1,
2269 | &hf_oran_active_beamspace_coefficient_n2,
2270 | &hf_oran_active_beamspace_coefficient_n3,
2271 | &hf_oran_active_beamspace_coefficient_n4,
2272 | &hf_oran_active_beamspace_coefficient_n5,
2273 | &hf_oran_active_beamspace_coefficient_n6,
2274 | &hf_oran_active_beamspace_coefficient_n7,
2275 | &hf_oran_active_beamspace_coefficient_n8,
2276 | NULL((void*)0)
2277 | };
2278 |
2279 | *num_trx_entries = 0;
2280 | uint64_t val;
2281 | for (unsigned n=0; n < k_octets; n++) {
2282 | proto_tree_add_bitmask_ret_uint64(tree, tvb, offset,
2283 | hf_oran_activeBeamspaceCoefficientMask,
2284 | ett_oran_active_beamspace_coefficient_mask, mask_bits,
2285 | ENC_BIG_ENDIAN0x00000000, &val);
2286 | offset++;
2287 | /* Add up the set bits for this byte (but be careful not to count beyond last real K bit..) */
2288 | for (unsigned b=0; b < 8; b++) {
2289 | if ((1 << b) & (unsigned)val) {
2290 | if (((n*8)+b) < pref_num_bf_antennas) {
2291 | if (*num_trx_entries < 1024-1) { /* Don't write beyond array (which should be plenty big) */
2292 | trx_enabled[(*num_trx_entries)++] = (n*8) + b + 1;
2293 | }
2294 | }
2295 | }
2296 | }
2297 | }
2298 | /* Set pointer to static array */
2299 | *trx_entries = trx_enabled;
2300 |
2301 | /* Show how many bits set */
2302 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_activeBeamspaceCoefficientMask_bits_set, tvb,
2303 | offset-k_octets, k_octets, *num_trx_entries);
2304 | proto_item_set_generated(ti);
2305 |
2306 | return offset;
2307 | }
2308 |
2309 | static void add_beam_id_to_tap(oran_tap_info *tap_info, uint16_t beam_id)
2310 | {
2311 | if (tap_info->num_beams < MAX_BEAMS_IN_FRAME32) {
2312 | tap_info->beams[tap_info->num_beams++] = beam_id;
2313 | }
2314 | }
2315 |
2316 |
2317 | /* 7.7.1.3 bfwCompParam (beamforming weight compression parameter).
2318 | * Depends upon passed-in bfwCompMeth (field may be empty) */
2319 | static int dissect_bfwCompParam(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo, int offset,
2320 | proto_item *meth_ti, uint32_t *bfw_comp_method,
2321 | uint32_t *exponent, bool_Bool *supported, unsigned *num_trx_entries, uint16_t **trx_entries)
2322 | {
2323 | if (*bfw_comp_method == COMP_NONE0) {
2324 | /* Absent! */
2325 | *num_trx_entries = 0;
2326 | *supported = true1;
2327 | return offset;
2328 | }
2329 |
2330 | /* Subtree */
2331 | proto_item *bfwcompparam_ti = proto_tree_add_string_format(tree, hf_oran_bfwCompParam,
2332 | tvb, offset, 1, "",
2333 | "bfwCompParam");
2334 | proto_tree *bfwcompparam_tree = proto_item_add_subtree(bfwcompparam_ti, ett_oran_bfwcompparam);
2335 |
2336 | proto_item_append_text(bfwcompparam_ti,
2337 | " (meth=%s)", val_to_str_const(*bfw_comp_method, bfw_comp_headers_comp_meth, "reserved"));
2338 |
2339 | *num_trx_entries = 0;
2340 | *supported = false0;
2341 | switch (*bfw_comp_method) {
2342 | case COMP_BLOCK_FP1: /* block floating point */
2343 | /* 4 reserved bits + exponent */
2344 | add_reserved_field(bfwcompparam_tree, hf_oran_reserved_4bits, tvb, offset, 1);
2345 | proto_tree_add_item_ret_uint(bfwcompparam_tree, hf_oran_exponent,
2346 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, exponent);
2347 | proto_item_append_text(bfwcompparam_ti, " exponent=%u", *exponent);
2348 | *supported = true1;
2349 | offset++;
2350 | break;
2351 | case COMP_BLOCK_SCALE2: /* block scaling */
2352 | /* Separate into integer and fractional bits? */
2353 | proto_tree_add_item(bfwcompparam_tree, hf_oran_blockScaler,
2354 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2355 | offset++;
2356 | break;
2357 | case COMP_U_LAW3: /* u-law */
2358 | /* compBitWidth, compShift */
2359 | proto_tree_add_item(bfwcompparam_tree, hf_oran_compBitWidth,
2360 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2361 | proto_tree_add_item(bfwcompparam_tree, hf_oran_compShift,
2362 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2363 | offset++;
2364 | break;
2365 | case 4: /* beamspace I (BLOCK SCALING) */
2366 | /* activeBeamspaceCoefficientMask */
2367 | offset = dissect_active_beamspace_coefficient_mask(tvb, bfwcompparam_tree, offset, num_trx_entries, trx_entries);
2368 | *bfw_comp_method = COMP_BLOCK_SCALE2;
2369 | *supported = false0; /* TODO: true once BLOCK SCALE is supported */
2370 | proto_tree_add_item(bfwcompparam_tree, hf_oran_blockScaler,
2371 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2372 | offset++;
2373 | break;
2374 | case 5: /* beamspace II (BLOCK FLOATING POINT) */
2375 | /* activeBeamspaceCoefficientMask */
2376 | offset = dissect_active_beamspace_coefficient_mask(tvb, bfwcompparam_tree, offset, num_trx_entries, trx_entries);
2377 | /* reserved (4 bits) + exponent (4 bits) */
2378 | add_reserved_field(bfwcompparam_tree, hf_oran_reserved_4bits, tvb, offset, 1);
2379 | proto_tree_add_item_ret_uint(bfwcompparam_tree, hf_oran_exponent, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, exponent);
2380 | offset += 1;
2381 | *bfw_comp_method = COMP_BLOCK_FP1;
2382 | *supported = true1;
2383 | break;
2384 |
2385 | default:
2386 | /* Not handled */
2387 | break;
2388 | }
2389 |
2390 | proto_item_set_end(bfwcompparam_ti, tvb, offset);
2391 |
2392 | /* Can't go on if compression scheme not supported */
2393 | if (!(*supported) && meth_ti) {
2394 | expert_add_info_format(pinfo, meth_ti, &ei_oran_unsupported_bfw_compression_method,
2395 | "BFW Compression method %u (%s) not decompressed by dissector",
2396 | *bfw_comp_method,
2397 | val_to_str_const(*bfw_comp_method, bfw_comp_headers_comp_meth, "reserved"));
2398 | }
2399 | return offset;
2400 | }
2401 |
2402 |
2403 | /* Special case for uncompressed/16-bit value */
2404 | static float uncompressed_to_float(uint32_t h)
2405 | {
2406 | int16_t i16 = h & 0x0000ffff;
2407 | if (show_unscaled_values) {
2408 | return (float)i16;
2409 | }
2410 | return ((float)i16) / 0x7fff;
2411 | }
2412 |
2413 | /* Decompress I/Q value, taking into account method, width, exponent, other input-specific methods */
2414 | static float decompress_value(uint32_t bits, uint32_t comp_method, uint8_t iq_width,
2415 | uint32_t exponent,
2416 | /* Modulation compression settings. N.B. should also pass in PRB + symbol? */
2417 | section_mod_compr_config_t *m_c_p, uint8_t re)
2418 | {
2419 | switch (comp_method) {
2420 | case COMP_NONE0: /* no compression */
2421 | return uncompressed_to_float(bits);
2422 |
2423 | case COMP_BLOCK_FP1: /* block floating point */
2424 | case BFP_AND_SELECTIVE_RE5:
2425 | {
2426 | /* A.1.3 Block Floating Point Decompression Algorithm */
2427 | int32_t cPRB = bits;
2428 | uint32_t scaler = 1 << exponent; /* i.e. 2^exponent */
2429 |
2430 | /* Check last bit, in case we need to flip to -ve */
2431 | if (cPRB >= (1<<(iq_width-1))) {
2432 | cPRB -= (1<<iq_width);
2433 | }
2434 |
2435 | /* Unscale (8.1.3.1) */
2436 | cPRB *= scaler;
2437 | if (show_unscaled_values) {
2438 | return (float)cPRB;
2439 | }
2440 |
2441 | uint32_t mantissa_scale_factor = 1 << (iq_width-1); /* 2^(mantissabits-1) */
2442 | uint32_t exp_scale_factor = 1 << 15; /* 2^(2^exponentbits - 1 ) The exponent bit width is fixed to 4, so the maximum exponent is 15 */
2443 |
2444 | float ret = cPRB / ((float)(mantissa_scale_factor*exp_scale_factor));
2445 | return ret;
2446 | }
2447 |
2448 | case COMP_BLOCK_SCALE2:
2449 | case COMP_U_LAW3:
2450 | /* Not supported! But will be reported as expert info outside of this function! */
2451 | return 0.0;
2452 |
2453 | case COMP_MODULATION4:
2454 | case MOD_COMPR_AND_SELECTIVE_RE6:
2455 | {
2456 | /* Described in A.5 (with pseudo code) */
2457 | /* N.B., Applies to downlink data only - is not used for BFW */
2458 |
2459 | /* Defaults if not overridden. TODO: what should these be? */
2460 | bool_Bool csf = false0;
2461 | float mcScaler = (float)(1 << 11);
2462 |
2463 | /* Find csf + mcScaler to use. Non-default configs gleaned from SE 4,5,23 */
2464 | /* TODO: should ideally be filtering by symbol and PRB too (as configured from SE23) */
2465 | if (re > 0 && m_c_p && m_c_p->num_configs > 0) {
2466 | for (unsigned c=0; c<m_c_p->num_configs; c++) {
2467 | if (m_c_p->configs[c].mod_compr_re_mask & (1 << (12-re))) {
2468 | /* Return first (should be only) found */
2469 | csf = m_c_p->configs[c].mod_compr_csf;
2470 | mcScaler = m_c_p->configs[c].mod_compr_scaler;
2471 | break;
2472 | }
2473 | }
2474 | }
2475 |
2476 | int32_t cPRB = bits;
2477 |
2478 | /* 2) Map iqSample to iqSampleFx */
2479 | /* Check last bit, in case we need to flip to -ve */
2480 | if (cPRB >= (1<<(iq_width-1))) {
2481 | cPRB -= (1<<iq_width);
2482 | }
2483 | float iqSampleFx = (float)cPRB / (1 << (iq_width-1));
2484 |
2485 |
2486 | /* 3) or 4) (b) - add unshifted value if csf set */
2487 | float csf_to_add = 0.0;
2488 | if (csf) {
2489 | /* Unshift the constellation point */
2490 | csf_to_add = (float)1.0 / (1 << (iq_width));
2491 | }
2492 | iqSampleFx += csf_to_add;
2493 |
2494 | /* 3) or 4) (c) - unscaling */
2495 | float iqSampleScaled = mcScaler * iqSampleFx * (float)sqrt(2);
2496 | return iqSampleScaled;
2497 | }
2498 |
2499 | default:
2500 | /* Not supported! But will be reported as expert info outside of this function! */
2501 | return 0.0;
2502 | }
2503 | }
2504 |
2505 | /* Out-of-range value used for special case */
2506 | #define ORPHAN_BUNDLE_NUMBER999 999
2507 |
2508 | /* Bundle of PRBs/TRX I/Q samples (ext 11) */
2509 | static uint32_t dissect_bfw_bundle(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo, unsigned offset,
2510 | proto_item *comp_meth_ti, uint32_t bfwcomphdr_comp_meth,
2511 | section_mod_compr_config_t *mod_compr_params,
2512 | uint32_t num_weights_per_bundle,
2513 | uint8_t iq_width,
2514 | unsigned bundle_number,
2515 | unsigned first_prb, unsigned last_prb, bool_Bool is_orphan,
2516 | uint32_t symbol_count,
2517 | section_details_t *section_details,
2518 | oran_tap_info *tap_info)
2519 | {
2520 | /* Set bundle name */
2521 | char bundle_name[32];
2522 | if (!is_orphan) {
2523 | snprintf(bundle_name, 32, "Bundle %3u", bundle_number);
2524 | }
2525 | else {
2526 | (void) g_strlcpy(bundle_name, "Orphaned ", 32);
2527 | }
2528 |
2529 | /* Create Bundle root */
2530 | proto_item *bundle_ti;
2531 | if (first_prb != last_prb) {
2532 | bundle_ti = proto_tree_add_string_format(tree, hf_oran_bfw_bundle,
2533 | tvb, offset, 0, "",
2534 | "%s: (PRBs %3u-%3u)",
2535 | bundle_name,
2536 | first_prb, last_prb);
2537 | }
2538 | else {
2539 | bundle_ti = proto_tree_add_string_format(tree, hf_oran_bfw_bundle,
2540 | tvb, offset, 0, "",
2541 | "%s: (PRB %3u)",
2542 | bundle_name,
2543 | first_prb);
2544 | }
2545 | proto_tree *bundle_tree = proto_item_add_subtree(bundle_ti, ett_oran_bfw_bundle);
2546 |
2547 | /* Generated bundle id */
2548 | proto_item *bundleid_ti = proto_tree_add_uint(bundle_tree, hf_oran_bfw_bundle_id, tvb, 0, 0,
2549 | bundle_number);
2550 | proto_item_set_generated(bundleid_ti);
2551 | proto_item_set_hidden(bundleid_ti);
2552 |
2553 | /* bfwCompParam */
2554 | bool_Bool compression_method_supported = false0;
2555 | unsigned exponent = 0;
2556 | unsigned num_trx_entries = 0;
2557 | uint16_t *trx_entries;
2558 | offset = dissect_bfwCompParam(tvb, bundle_tree, pinfo, offset, comp_meth_ti,
2559 | &bfwcomphdr_comp_meth, &exponent, &compression_method_supported,
2560 | &num_trx_entries, &trx_entries);
2561 |
2562 | /* Create Bundle subtree */
2563 | int bit_offset = offset*8;
2564 | int bfw_offset;
2565 |
2566 | /* contInd */
2567 | proto_tree_add_item(bundle_tree, hf_oran_cont_ind,
2568 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
2569 | /* beamId */
2570 | uint32_t beam_id;
2571 | proto_tree_add_item_ret_uint(bundle_tree, hf_oran_beam_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &beam_id);
2572 | proto_item_append_text(bundle_ti, " (beamId:%u) ", beam_id);
2573 | bit_offset += 16;
2574 | add_beam_id_to_tap(tap_info, beam_id);
2575 |
2576 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
2577 | if (section_details) {
2578 | for (unsigned prb = first_prb; prb <= last_prb; prb++) {
2579 | if (prb < 273) {
2580 | section_details->beamIds[prb] = beam_id;
2581 | }
2582 | }
2583 | }
2584 | }
2585 |
2586 | /* On first pass, record that beamId was defined here */
2587 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
2588 | bfw_definition *definition = wmem_new0(wmem_file_scope(), bfw_definition)((bfw_definition*)wmem_alloc0((wmem_file_scope()), sizeof(bfw_definition )));
2589 | definition->frame_defined = pinfo->num;
2590 | definition->symbol_when_defined = symbol_count;
2591 | wmem_tree_insert32(dl_beam_ids_defined, beam_id, definition);
2592 | }
2593 |
2594 |
2595 | /* Number of weights per bundle (from preference) */
2596 | proto_item *wpb_ti = proto_tree_add_uint(bundle_tree, hf_oran_num_weights_per_bundle, tvb, 0, 0,
2597 | num_weights_per_bundle);
2598 | proto_item_set_generated(wpb_ti);
2599 |
2600 | /* Add the weights for this bundle. Overwrite with what was seen in bfwCompParam if beamspace */
2601 | if (num_trx_entries != 0) {
2602 | num_weights_per_bundle = num_trx_entries;
2603 | }
2604 |
2605 | bool_Bool non_zero_weights_seen = false0;
2606 | int bit_offset_before_weights = bit_offset;
2607 | for (unsigned w=0; w < num_weights_per_bundle; w++) {
2608 |
2609 | uint16_t trx_index = (num_trx_entries) ? trx_entries[w] : w+1;
2610 |
2611 | /* Create subtree */
2612 | bfw_offset = bit_offset / 8;
2613 | uint8_t bfw_extent = ((bit_offset + (iq_width*2)) / 8) - bfw_offset;
2614 | proto_item *bfw_ti = proto_tree_add_string_format(bundle_tree, hf_oran_bfw,
2615 | tvb, bfw_offset, bfw_extent,
2616 | "", "TRX %3u: (", trx_index);
2617 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
2618 |
2619 | /* I */
2620 | /* Get bits, and convert to float. */
2621 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, iq_width, ENC_BIG_ENDIAN0x00000000);
2622 | if (bits) {
2623 | non_zero_weights_seen = true1;
2624 | }
2625 | float value = decompress_value(bits, bfwcomphdr_comp_meth, iq_width,
2626 | exponent, mod_compr_params, 0 /* RE */);
2627 | /* Add to tree. */
2628 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8, (iq_width+7)/8, value, "#%u=%f", w, value);
2629 | bit_offset += iq_width;
2630 | proto_item_append_text(bfw_ti, "I%u=%f ", w, value);
2631 |
2632 | /* Q */
2633 | /* Get bits, and convert to float. */
2634 | bits = tvb_get_bits32(tvb, bit_offset, iq_width, ENC_BIG_ENDIAN0x00000000);
2635 | if (bits) {
2636 | non_zero_weights_seen = true1;
2637 | }
2638 |
2639 | value = decompress_value(bits, bfwcomphdr_comp_meth, iq_width,
2640 | exponent, mod_compr_params, 0 /* RE */);
2641 | /* Add to tree. */
2642 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8, (iq_width+7)/8, value, "#%u=%f", w, value);
2643 | bit_offset += iq_width;
2644 | proto_item_append_text(bfw_ti, "Q%u=%f)", w, value);
2645 | }
2646 |
2647 | if (!non_zero_weights_seen) {
2648 | proto_tree_add_item(bundle_tree, hf_oran_bundle_weights_all_zero, tvb,
2649 | bit_offset_before_weights, (bit_offset+7)/8 - (bit_offset_before_weights/8), ENC_NA0x00000000);
2650 | }
2651 |
2652 | /* Set extent of bundle */
2653 | proto_item_set_end(bundle_ti, tvb, (bit_offset+7)/8);
2654 |
2655 | return (bit_offset+7)/8;
2656 | }
2657 |
2658 | /* Return new bit offset. in/out will always be byte-aligned.. */
2659 | static int dissect_ciCompParam(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo _U___attribute__((unused)), unsigned bit_offset,
2660 | unsigned comp_meth, uint8_t *exponent)
2661 | {
2662 | if (comp_meth == COMP_NONE0) {
2663 | /* Nothing in frame so don't even create subtree */
2664 | return bit_offset;
2665 | }
2666 |
2667 | /* Subtree */
2668 | proto_item *cicompparam_ti = proto_tree_add_string_format(tree, hf_oran_ciCompParam,
2669 | tvb, bit_offset/8, 1, "",
2670 | "ciCompParam");
2671 | proto_tree *cicompparam_tree = proto_item_add_subtree(cicompparam_ti, ett_oran_cicompparam);
2672 | uint32_t ci_exponent;
2673 |
2674 | /* Contents differ by compression method */
2675 | switch (comp_meth) {
2676 | case COMP_BLOCK_FP1:
2677 | add_reserved_field(cicompparam_tree, hf_oran_reserved_4bits, tvb, bit_offset/8, 1);
2678 | proto_tree_add_item_ret_uint(cicompparam_tree, hf_oran_exponent,
2679 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000, &ci_exponent);
2680 | *exponent = ci_exponent;
2681 | proto_item_append_text(cicompparam_ti, " (Exponent=%u)", ci_exponent);
2682 | bit_offset += 8; /* one byte */
2683 | break;
2684 | case COMP_BLOCK_SCALE2:
2685 | /* Separate into integer (1) and fractional (7) bits? */
2686 | proto_tree_add_item(cicompparam_tree, hf_oran_blockScaler,
2687 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000);
2688 | bit_offset += 8;
2689 | break;
2690 | case COMP_U_LAW3:
2691 | /* compBitWidth, compShift (4 bits each) */
2692 | proto_tree_add_item(cicompparam_tree, hf_oran_compBitWidth,
2693 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000);
2694 | proto_tree_add_item(cicompparam_tree, hf_oran_compShift,
2695 | tvb, bit_offset/8, 1, ENC_BIG_ENDIAN0x00000000);
2696 | bit_offset += 8;
2697 | break;
2698 |
2699 | default:
2700 | /* reserved, ? bytes of zeros.. */
2701 | break;
2702 | }
2703 |
2704 | return bit_offset;
2705 | }
2706 |
2707 | /* frameStructure (7.5.2.13) */
2708 | static unsigned dissect_frame_structure(proto_item *tree, tvbuff_t *tvb, unsigned offset,
2709 | uint32_t subframeId, uint32_t slotId)
2710 | {
2711 | uint32_t scs;
2712 | /* FFT Size (4 bits) */
2713 | proto_tree_add_item(tree, hf_oran_frameStructure_fft, tvb, offset, 1, ENC_NA0x00000000);
2714 | /* Subcarrier spacing (SCS) */
2715 | proto_tree_add_item_ret_uint(tree, hf_oran_frameStructure_subcarrier_spacing, tvb, offset, 1, ENC_NA0x00000000, &scs);
2716 |
2717 | /* Show slot within frame as a generated field. See table 7.5.13-3 */
2718 | uint32_t slots_per_subframe = 1;
2719 | if (scs <= 4) {
2720 | slots_per_subframe = 1 << scs;
2721 | }
2722 | if (scs <= 4 || scs >= 12) {
2723 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_slot_within_frame, tvb, 0, 0,
2724 | (slots_per_subframe*subframeId) + slotId);
2725 | proto_item_set_generated(ti);
2726 | }
2727 | return offset + 1;
2728 | }
2729 |
2730 | static unsigned dissect_csf(proto_item *tree, tvbuff_t *tvb, unsigned bit_offset,
2731 | unsigned iq_width, bool_Bool *p_csf)
2732 | {
2733 | proto_item *csf_ti;
2734 | uint64_t csf;
2735 | csf_ti = proto_tree_add_bits_ret_val(tree, hf_oran_csf, tvb, bit_offset, 1, &csf, ENC_BIG_ENDIAN0x00000000);
2736 | if (csf) {
2737 | /* Table 7.7.4.2-1 Constellation shift definition (index is udIqWidth) */
2738 | const char* shift_value[] = { "n/a", "1/2", "1/4", "1/8", "1/16", "1/32" };
2739 | if (iq_width >=1 && iq_width <= 5) {
2740 | proto_item_append_text(csf_ti, " (Shift Value is %s)", shift_value[iq_width]);
2741 | }
2742 | }
2743 |
2744 | /* Set out parameter */
2745 | if (p_csf != NULL((void*)0)) {
2746 | *p_csf = (csf!=0);
2747 | }
2748 | return bit_offset+1;
2749 | }
2750 |
2751 |
2752 | /* Section 7.
2753 | * N.B. these are the green parts of the tables showing Section Types, differing by section Type */
2754 | static int dissect_oran_c_section(tvbuff_t *tvb, proto_tree *tree, packet_info *pinfo,
2755 | flow_state_t* state,
2756 | uint32_t sectionType, oran_tap_info *tap_info, proto_item *protocol_item,
2757 | uint32_t subframeId, uint32_t frameId, uint32_t slotId, uint32_t startSymbolId,
2758 | uint8_t ci_iq_width, uint8_t ci_comp_meth, unsigned ci_comp_opt,
2759 | unsigned num_sinr_per_prb)
2760 | {
2761 | unsigned offset = 0;
2762 | proto_tree *c_section_tree = NULL((void*)0);
2763 | proto_item *sectionHeading = NULL((void*)0);
2764 |
2765 | /* Section subtree */
2766 | sectionHeading = proto_tree_add_string_format(tree, hf_oran_c_section,
2767 | tvb, offset, 0, "", "Section");
2768 | c_section_tree = proto_item_add_subtree(sectionHeading, ett_oran_c_section);
2769 |
2770 | uint32_t sectionId = 0;
2771 |
2772 | uint32_t startPrbc=0, startPrbu=0;
2773 | uint32_t numPrbc=0, numPrbu=0;
2774 | uint32_t ueId = 0;
2775 | proto_item *ueId_ti = NULL((void*)0);
2776 | uint32_t section_beamId = 0;
2777 | proto_item *section_beamId_ti = NULL((void*)0);
2778 | bool_Bool section_beamId_ignored = false0;
2779 |
2780 | proto_item *numsymbol_ti = NULL((void*)0);
2781 | bool_Bool numsymbol_ignored = false0;
2782 |
2783 | proto_item *numprbc_ti = NULL((void*)0);
2784 |
2785 | /* Config affecting ext11 bundles (initially unset) */
2786 | ext11_settings_t ext11_settings;
2787 | memset(&ext11_settings, 0, sizeof(ext11_settings));
2788 |
2789 | /* Section Type 10 needs to keep track of PRB range that should be reported
2790 | for msgTypeId=5 (Interference plus Noise for unallocated PRBs) */
2791 | /* All PRBs start as false */
2792 | #define MAX_PRBS273 273
2793 | bool_Bool prbs_for_st10_type5[MAX_PRBS273];
2794 | memset(&prbs_for_st10_type5, 0, sizeof(prbs_for_st10_type5));
2795 |
2796 | /* These UEIds are set by ST5, ST10 (single value), and extended by SE10 */
2797 | #define MAX_UEIDS16 16
2798 | uint32_t ueids[MAX_UEIDS16];
2799 | uint32_t number_of_ueids = 0;
2800 |
2801 |
2802 | bool_Bool extension_flag = false0;
2803 |
2804 | /* These sections (ST0, ST1, ST2, ST3, ST5, ST9, ST10, ST11) are similar, so handle as common with per-type differences */
2805 | if (((sectionType <= SEC_C_UE_SCHED) || (sectionType >= SEC_C_SINR_REPORTING)) &&
2806 | (sectionType != SEC_C_SLOT_CONTROL)) {
2807 |
2808 | /* sectionID */
2809 | proto_item *ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_section_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &sectionId);
2810 | if (sectionId == 4095) {
2811 | proto_item_append_text(ti, " (not default coupling C/U planes using sectionId)");
2812 | }
2813 | offset++;
2814 |
2815 | if (tap_info->num_section_ids < MAX_SECTION_IDs32) {
2816 | tap_info->section_ids[tap_info->num_section_ids++] = sectionId;
2817 | }
2818 |
2819 | /* rb */
2820 | uint32_t rb;
2821 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_rb, tvb, offset, 1, ENC_NA0x00000000, &rb);
2822 | /* symInc (1 bit) */
2823 | /* TODO: mark as ignored if SE6, SE12 or SE19 present */
2824 | if (sectionType != SEC_C_RRM_MEAS_REPORTS && /* Section Type 10 */
2825 | sectionType != SEC_C_REQUEST_RRM_MEAS) { /* Section Type 11 */
2826 | unsigned int sym_inc;
2827 | proto_item *sym_inc_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_symInc, tvb, offset, 1, ENC_NA0x00000000, &sym_inc);
2828 | if (sym_inc !=0 && (sectionType == SEC_C_SINR_REPORTING)) { /* Section Type 9 */
2829 | /* "0 shall be used" */
2830 | proto_item_append_text(sym_inc_ti, " (should be 0)");
2831 | }
2832 | }
2833 | else {
2834 | /* reserved (1 bit) */
2835 | add_reserved_field(c_section_tree, hf_oran_reserved_bit5, tvb, offset, 1);
2836 | }
2837 |
2838 | /* startPrbx and numPrbx */
2839 | if (sectionType == SEC_C_SINR_REPORTING) {
2840 | /* startPrbu (10 bits) */
2841 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_startPrbu, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbu);
2842 | offset += 2;
2843 |
2844 | /* numPrbu */
2845 | numprbc_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numPrbu, tvb, offset, 1, ENC_NA0x00000000, &numPrbu);
2846 | if (numPrbu == 0) {
2847 | proto_item_append_text(numprbc_ti, " (all PRBs - configured as %u)", pref_data_plane_section_total_rbs);
2848 | numPrbu = pref_data_plane_section_total_rbs;
2849 | }
2850 | offset += 1;
2851 | }
2852 | else {
2853 | /* startPrbc (10 bits) */
2854 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_startPrbc, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbc);
2855 | offset += 2;
2856 |
2857 | /* numPrbc */
2858 | numprbc_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numPrbc, tvb, offset, 1, ENC_NA0x00000000, &numPrbc);
2859 | if (numPrbc == 0) {
2860 | proto_item_append_text(numprbc_ti, " (all PRBs - configured as %u)", pref_data_plane_section_total_rbs);
2861 | /* TODO: should probably set to pref_data_plane_section_total_rbs, and define MAX_PRBS to > 273 ? */
2862 | numPrbc = MAX_PRBS273;
2863 | }
2864 | offset += 1;
2865 | }
2866 |
2867 | /* Start with range from section. May get changed by SE6, SE12, SE20 */
2868 | for (unsigned n=startPrbc; n < startPrbc+numPrbc; n++) {
2869 | if (n < MAX_PRBS273) {
2870 | prbs_for_st10_type5[n] = true1;
2871 | }
2872 | }
2873 |
2874 | if (sectionType != SEC_C_SINR_REPORTING) { /* *NOT* Section Type 9 */
2875 | static int * const remask_flags[] = {
2876 | &hf_oran_reMask_re1,
2877 | &hf_oran_reMask_re2,
2878 | &hf_oran_reMask_re3,
2879 | &hf_oran_reMask_re4,
2880 | &hf_oran_reMask_re5,
2881 | &hf_oran_reMask_re6,
2882 | &hf_oran_reMask_re7,
2883 | &hf_oran_reMask_re8,
2884 | &hf_oran_reMask_re9,
2885 | &hf_oran_reMask_re10,
2886 | &hf_oran_reMask_re11,
2887 | &hf_oran_reMask_re12,
2888 | NULL((void*)0)
2889 | };
2890 |
2891 | /* reMask */
2892 | uint64_t remask;
2893 | proto_tree_add_bitmask_ret_uint64(c_section_tree, tvb, offset,
2894 | hf_oran_reMask, ett_oran_remask, remask_flags, ENC_BIG_ENDIAN0x00000000, &remask);
2895 | offset++;
2896 | /* numSymbol */
2897 | uint32_t numSymbol;
2898 | numsymbol_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numSymbol, tvb, offset, 1, ENC_NA0x00000000, &numSymbol);
2899 | if ((sectionType == SEC_C_RRM_MEAS_REPORTS) && (numSymbol != 14)) { /* Section type 10 must have 14 symbols */
2900 | proto_item_append_text(numsymbol_ti, " (for ST10, should be 14!)");
2901 | expert_add_info_format(pinfo, numsymbol_ti, &ei_oran_st10_numsymbol_not_14,
2902 | "numSymbol should be 14 for ST10 - found %u", numSymbol);
2903 | }
2904 | if ((startSymbolId + numSymbol) > 14) {
2905 | /* Warn if startSymbol + numSymbol would be > 14 */
2906 | expert_add_info_format(pinfo, numsymbol_ti, &ei_oran_too_many_symbols,
2907 | "startSymbolId (%u) + numSymbol (%u) exceeds max of 14",
2908 | startSymbolId, numSymbol);
2909 | }
2910 | offset++;
2911 |
2912 | /* [ef] (extension flag) */
2913 | switch (sectionType) {
2914 | case SEC_C_UNUSED_RB: /* Section Type 0 */
2915 | case SEC_C_NORMAL: /* Section Type 1 */
2916 | case SEC_C_PRACH: /* Section Type 3 */
2917 | case SEC_C_UE_SCHED: /* Section Type 5 */
2918 | case SEC_C_RRM_MEAS_REPORTS: /* Section Type 10 */
2919 | case SEC_C_REQUEST_RRM_MEAS: /* Section Type 11 */
2920 | proto_tree_add_item_ret_boolean(c_section_tree, hf_oran_ef, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &extension_flag);
2921 | break;
2922 | default:
2923 | /* Other section types don't support extensions */
2924 | break;
2925 | }
2926 |
2927 | write_section_info(sectionHeading, pinfo, protocol_item, sectionId, startPrbc, numPrbc, rb);
2928 | proto_item_append_text(sectionHeading, ", Symbols: %2u", numSymbol);
2929 |
2930 | if (numPrbc == 0) {
2931 | /* Special case for all PRBs */
2932 | numPrbc = pref_data_plane_section_total_rbs;
2933 | startPrbc = 0; /* may already be 0... */
2934 | }
2935 | }
2936 | else {
2937 | /* Section Type 9 */
2938 | write_section_info(sectionHeading, pinfo, protocol_item, sectionId, startPrbu, numPrbu, rb);
2939 | proto_item_append_text(sectionHeading, ", numSinrPerPrb: %2u", num_sinr_per_prb);
2940 | }
2941 |
2942 | /* Section type specific fields (after 'numSymbol') */
2943 | switch (sectionType) {
2944 | case SEC_C_UNUSED_RB: /* Section Type 0 - Table 7.4.2-1 */
2945 | /* reserved (15 bits) */
2946 | add_reserved_field(c_section_tree, hf_oran_reserved_15bits, tvb, offset, 2);
2947 | offset += 2;
2948 | break;
2949 |
2950 | case SEC_C_NORMAL: /* Section Type 1 - Table 7.4.3-1 */
2951 | /* beamId */
2952 | section_beamId_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &section_beamId);
2953 | offset += 2;
2954 |
2955 | /* beamId might get invalidated by e.g., ext-6, ext-11, so unused value will still be shown here.. */
2956 | proto_item_append_text(sectionHeading, ", BeamId: %d", section_beamId);
2957 | break;
2958 |
2959 | case SEC_C_PRACH: /* Section Type 3 - Table 7.4.5-1 */
2960 | {
2961 | /* beamId */
2962 | section_beamId_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &section_beamId);
2963 | offset += 2;
2964 |
2965 | /* freqOffset */
2966 | int32_t freqOffset; /* Yes, this is signed, so the cast is intentional. */
2967 | proto_item *freq_offset_item = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_freqOffset, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000, (uint32_t*)&freqOffset);
2968 | freqOffset |= 0xff000000; /* Must sign-extend */
2969 | proto_item_set_text(freq_offset_item, "Frequency offset: %d \u0394f", freqOffset);
2970 | offset += 3;
2971 |
2972 | /* reserved (8 bits) */
2973 | add_reserved_field(c_section_tree, hf_oran_reserved_8bits, tvb, offset, 1);
2974 | offset += 1;
2975 |
2976 | /* beamId might get invalidated by e.g., ext-6, ext-11, so unused value will still be shown here.. */
2977 | proto_item_append_text(sectionHeading, ", BeamId: %d, FreqOffset: %d \u0394f", section_beamId, freqOffset);
2978 | break;
2979 | }
2980 |
2981 | case SEC_C_UE_SCHED: /* Section Type 5 - Table 7.4.7-1 */
2982 | case SEC_C_RRM_MEAS_REPORTS: /* Section Type 10 - Table 7.4.12-1 */
2983 | /* ueId */
2984 | ueId_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_ueId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ueId);
2985 | offset += 2;
2986 | if (ueId == 0x7fff) {
2987 | proto_item_append_text(ueId_ti, " (PRBs not scheduled for eAxC ID in transport header)");
2988 | }
2989 | else {
2990 | ueids[number_of_ueids++] = ueId;
2991 | }
2992 |
2993 | proto_item_append_text(sectionHeading, ", UEId: %d", ueId);
2994 | break;
2995 |
2996 | case SEC_C_SINR_REPORTING: /* Section Type 9 - SINR Reporting */
2997 | {
2998 | /* Hidden filter for bf (DMFS-BF) */
2999 | proto_item *bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
3000 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
3001 |
3002 | unsigned bit_offset = offset*8;
3003 |
3004 | /* sinr iqWidth */
3005 | proto_item *iq_width_item = proto_tree_add_uint(c_section_tree, hf_oran_sinrCompHdrIqWidth_pref, tvb, 0, 0, pref_sample_bit_width_sinr);
3006 | proto_item_append_text(iq_width_item, " (from preferences)");
3007 | proto_item_set_generated(iq_width_item);
3008 |
3009 | /* sinr compMethod */
3010 | proto_item *sinr_comp_meth_item = proto_tree_add_uint(c_section_tree, hf_oran_sinrCompHdrMeth_pref, tvb, 0, 0, pref_iqCompressionSINR);
3011 | proto_item_append_text(sinr_comp_meth_item, " (from preferences)");
3012 | proto_item_set_generated(sinr_comp_meth_item);
3013 |
3014 | /* Add SINR entries for each PRB */
3015 | for (unsigned prb=startPrbu; prb < startPrbu+numPrbu; prb++) {
3016 | /* Create a subtree for each PRB */
3017 | proto_item *prb_ti = proto_tree_add_string_format(c_section_tree, hf_oran_sinr_prb,
3018 | tvb, offset, 0, "", "PRB %3u (", prb);
3019 | proto_tree *prb_tree = proto_item_add_subtree(prb_ti, ett_oran_sinr_prb);
3020 |
3021 | /* Each prb starts byte-aligned */
3022 | bit_offset = ((bit_offset+7)/8) * 8;
3023 |
3024 | /* N.B., using width/method from UL U-plane preferences, not certain that this is correct.. */
3025 |
3026 | /* sinrCompParam (udCompParam format, may be empty) */
3027 | uint32_t exponent = 0; /* N.B. init to silence warnings, but will always be set if read in COMP_BLOCK_FP case */
3028 | uint16_t sReSMask;
3029 | bit_offset = dissect_udcompparam(tvb, pinfo, prb_tree, bit_offset/8,
3030 | pref_iqCompressionSINR, &exponent, &sReSMask,
3031 | true1) * 8; /* last param is for_sinr */
3032 |
3033 | /* sinrValues for this PRB. */
3034 | /* TODO: not sure how numSinrPerPrb interacts with rb==1... */
3035 | for (unsigned n=0; n < num_sinr_per_prb; n++) {
3036 | unsigned sinr_bits = tvb_get_bits32(tvb, bit_offset, pref_sample_bit_width_sinr, ENC_BIG_ENDIAN0x00000000);
3037 |
3038 | /* Using SINR compression settings from preferences */
3039 | float value = decompress_value(sinr_bits,
3040 | pref_iqCompressionSINR, pref_sample_bit_width_sinr,
3041 | exponent,
3042 | NULL((void*)0) /* no ModCompr for SINR */, 0 /* RE */);
3043 | unsigned sample_len_in_bytes = ((bit_offset%8)+pref_sample_bit_width_sinr+7)/8;
3044 | proto_item *val_ti = proto_tree_add_float(prb_tree, hf_oran_sinr_value, tvb,
3045 | bit_offset/8, sample_len_in_bytes, value);
3046 | proto_item_append_text(prb_ti, " %8f", value);
3047 |
3048 | /* Show here which subcarriers share which values (they all divide 12..) */
3049 | if (num_sinr_per_prb == 12) {
3050 | proto_item_append_text(val_ti, " (PRB=%u, subcarrier %u)",
3051 | startPrbu+((prb-startPrbu)*(rb+1)), n*(12/num_sinr_per_prb));
3052 | }
3053 | else {
3054 | proto_item_append_text(val_ti, " (PRB=%u, subcarriers %u-%u)",
3055 | startPrbu+((prb-startPrbu)*(rb+1)),
3056 | n*(12/num_sinr_per_prb), (n+1)*(12/num_sinr_per_prb)-1);
3057 | }
3058 | bit_offset += pref_sample_bit_width_sinr;
3059 | }
3060 |
3061 | /* 1-byte alignment per PRB (7.2.11) */
3062 | offset = (bit_offset+7)/8;
3063 | bit_offset = offset*8;
3064 |
3065 | proto_item_append_text(prb_ti, ")");
3066 | proto_item_set_end(prb_ti, tvb, offset);
3067 | }
3068 | break;
3069 | }
3070 | case SEC_C_REQUEST_RRM_MEAS: /* Section Type 11 - Request RRM Measurements */
3071 | /* Reserved (15 bits) */
3072 | add_reserved_field(c_section_tree, hf_oran_reserved_15bits, tvb, offset, 2);
3073 | offset += 2;
3074 | break;
3075 |
3076 | default:
3077 | break;
3078 | }
3079 | }
3080 | else if (sectionType == SEC_C_CH_INFO) { /* Section Type 6 */
3081 | /* ef */
3082 | proto_tree_add_item_ret_boolean(c_section_tree, hf_oran_ef, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &extension_flag);
3083 | /* ueId */
3084 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_ueId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ueId);
3085 | offset += 2;
3086 | /* regularizationFactor */
3087 | proto_tree_add_item(c_section_tree, hf_oran_regularizationFactor, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3088 | offset += 2;
3089 | /* reserved (4 bits) */
3090 | add_reserved_field(c_section_tree, hf_oran_reserved_4bits, tvb, offset, 1);
3091 | /* rb ("Value=0 shall be set") */
3092 | uint32_t rb;
3093 | proto_item *rb_ti = proto_tree_add_item_ret_uint(c_section_tree, hf_oran_rb, tvb, offset, 1, ENC_NA0x00000000, &rb);
3094 | if (rb != 0) {
3095 | proto_item_append_text(rb_ti, " (should be set to 0)");
3096 | expert_add_info(pinfo, rb_ti, &ei_oran_st6_rb_shall_be_0);
3097 | }
3098 | /* symInc */
3099 | proto_tree_add_item(c_section_tree, hf_oran_symInc, tvb, offset, 1, ENC_NA0x00000000);
3100 | /* startPrbc */
3101 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_startPrbc, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbc);
3102 | offset += 2;
3103 | /* numPrbc */
3104 | proto_tree_add_item_ret_uint(c_section_tree, hf_oran_numPrbc, tvb, offset, 1, ENC_NA0x00000000, &numPrbc);
3105 | offset += 1;
3106 |
3107 | /* Hidden filter for bf */
3108 | proto_item *bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
3109 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
3110 |
3111 | /* ciIsample,ciQsample pairs */
3112 | unsigned m;
3113 | unsigned prb;
3114 | uint32_t bit_offset = offset*8;
3115 |
3116 | /* Antenna count from preference */
3117 | unsigned num_trx = pref_num_bf_antennas;
3118 |
3119 | write_channel_section_info(sectionHeading, pinfo,
3120 | sectionId, ueId, startPrbc, numPrbc, num_trx);
3121 |
3122 | bool_Bool first_prb = true1;
3123 | uint8_t exponent = 0;
3124 | for (prb=startPrbc; prb < startPrbc+numPrbc; prb++) {
3125 |
3126 | /* PRB subtree */
3127 | unsigned prb_start_offset = bit_offset;
3128 | proto_item *prb_ti = proto_tree_add_string_format(c_section_tree, hf_oran_samples_prb,
3129 | tvb, bit_offset/8, 0,
3130 | "", "PRB=%u", prb);
3131 | proto_tree *prb_tree = proto_item_add_subtree(prb_ti, ett_oran_prb_cisamples);
3132 |
3133 | /* There may be a ciCompParam here.. */
3134 | if (first_prb || ci_comp_opt==1) {
3135 | bit_offset = dissect_ciCompParam(tvb, prb_tree, pinfo, bit_offset, ci_comp_meth, &exponent);
3136 | }
3137 | first_prb = false0;
3138 |
3139 | /* Antennas */
3140 | for (m=0; m < num_trx; m++) {
3141 |
3142 | unsigned sample_offset = bit_offset / 8;
3143 | uint8_t sample_extent = ((bit_offset + (ci_iq_width*2)) / 8) - sample_offset;
3144 |
3145 | /* Create subtree for antenna */
3146 | proto_item *sample_ti = proto_tree_add_string_format(prb_tree, hf_oran_ciSample,
3147 | tvb, sample_offset, sample_extent,
3148 | "", "TRX=%2u: ", m);
3149 | proto_tree *sample_tree = proto_item_add_subtree(sample_ti, ett_oran_cisample);
3150 |
3151 | /* I */
3152 | /* Get bits, and convert to float. */
3153 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, ci_iq_width, ENC_BIG_ENDIAN0x00000000);
3154 | float value = decompress_value(bits, ci_comp_meth, ci_iq_width, exponent, NULL((void*)0) /* no ModCompr for ST6 */, 0 /* RE */);
3155 |
3156 | /* Add to tree. */
3157 | proto_tree_add_float_format_value(sample_tree, hf_oran_ciIsample, tvb, bit_offset/8, (ci_iq_width+7)/8, value, "#%u=%f", m, value);
3158 | bit_offset += ci_iq_width;
3159 | proto_item_append_text(sample_ti, "I%u=%f ", m, value);
3160 |
3161 | /* Q */
3162 | /* Get bits, and convert to float. */
3163 | bits = tvb_get_bits32(tvb, bit_offset, ci_iq_width, ENC_BIG_ENDIAN0x00000000);
3164 | value = decompress_value(bits, ci_comp_meth, ci_iq_width, exponent, NULL((void*)0) /* no ModCompr for ST6 */, 0 /* RE */);
3165 |
3166 | /* Add to tree. */
3167 | proto_tree_add_float_format_value(sample_tree, hf_oran_ciQsample, tvb, bit_offset/8, (ci_iq_width+7)/8, value, "#%u=%f", m, value);
3168 | bit_offset += ci_iq_width;
3169 | proto_item_append_text(sample_ti, "Q%u=%f ", m, value);
3170 | }
3171 | proto_item_set_len(prb_ti, (bit_offset-prb_start_offset+7)/8);
3172 | }
3173 |
3174 | /* Pad out by 1 or 4 bytes, according to preference */
3175 | if (!st6_4byte_alignment) {
3176 | offset = (bit_offset + 7) / 8;
3177 | }
3178 | else {
3179 | int mode = bit_offset % 32;
3180 | if (mode != 0) {
3181 | offset = (bit_offset + (32-mode))/8;
3182 | }
3183 | else {
3184 | offset = bit_offset/8;
3185 | }
3186 | }
3187 | proto_item_set_end(c_section_tree, tvb, offset);
3188 | }
3189 |
3190 |
3191 | expected_section_data_t *data_section = NULL((void*)0);
3192 | unsigned index_to_use = 0;
3193 |
3194 | /* On first pass, allocate a section entry to use */
3195 | if (link_planes_together && !PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
3196 |
3197 | /* Look for existing entry for sectionId to overwrite first. */
3198 | uint8_t direction = !tap_info->uplink;
3199 | data_section = wmem_tree_lookup32(state->expected_sections[direction],
3200 | sectionId);
3201 | if (data_section == NULL((void*)0)) {
3202 | /* None, so create */
3203 | data_section = wmem_new0(wmem_file_scope(), expected_section_data_t)((expected_section_data_t*)wmem_alloc0((wmem_file_scope()), sizeof (expected_section_data_t)));
3204 | wmem_tree_insert32(state->expected_sections[direction],
3205 | sectionId,
3206 | data_section);
3207 | }
3208 |
3209 | /* If 2nd entry not in use, use that one */
3210 | if (!data_section->details[1].in_use) {
3211 | index_to_use = 1;
3212 | }
3213 | else {
3214 | /* Both in use, so replace the older of the 2 entries */
3215 | if (data_section->details[1].frame_number < data_section->details[0].frame_number) {
3216 | index_to_use = 1;
3217 | }
3218 | }
3219 |
3220 | if (data_section) {
3221 | section_details_t *details = &data_section->details[index_to_use];
3222 |
3223 | details->in_use = true1;
3224 | details->frame = frameId;
3225 | details->subframe = subframeId;
3226 | details->slot = slotId;
3227 | details->startSymbol = startSymbolId;
3228 |
3229 | details->frame_number = pinfo->num;
3230 | details->frame_time = pinfo->abs_ts;
3231 | data_section->sectionId = sectionId;
3232 | details->startPrb = startPrbc;
3233 | details->numPrb = numPrbc;
3234 | for (unsigned prb = startPrbc; prb <= startPrbc+numPrbc; prb++) {
3235 | if (prb < 273) {
3236 | details->beamIds[prb] = section_beamId;
3237 | }
3238 | }
3239 | }
3240 | }
3241 |
3242 | bool_Bool seen_se10 = false0;
3243 | uint32_t numPortc = 0;
3244 | proto_item *bf_ti = NULL((void*)0);
3245 |
3246 | /* Section extension commands */
3247 | while (extension_flag) {
3248 | int extension_start_offset = offset;
3249 |
3250 | /* Prefetch extType so can use specific extension type ett */
3251 | uint32_t exttype = tvb_get_uint8(tvb, offset) & 0x7f;
3252 | uint32_t exttype_ett_index = exttype;
3253 | if (exttype == 0 || exttype > HIGHEST_EXTTYPE32) {
3254 | /* Just use first one if out of range */
3255 | exttype_ett_index = 1;
3256 | }
3257 |
3258 | /* Create subtree for each extension (with summary) */
3259 | proto_item *extension_ti = proto_tree_add_string_format(c_section_tree, hf_oran_extension,
3260 | tvb, offset, 0, "", "Extension");
3261 | proto_tree *extension_tree = proto_item_add_subtree(extension_ti, ett_oran_c_section_extension[exttype_ett_index-1]);
3262 |
3263 | /* ef (i.e. another extension after this one?) */
3264 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_ef, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &extension_flag);
3265 |
3266 | /* extType */
3267 | proto_item *exttype_ti;
3268 | exttype_ti = proto_tree_add_item(extension_tree, hf_oran_exttype, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3269 | offset++;
3270 | proto_item_append_text(sectionHeading, " (ext-%u)", exttype);
3271 |
3272 | proto_item_append_text(extension_ti, " (ext-%u: %s)", exttype, val_to_str_ext_const(exttype, &exttype_vals_ext, "Reserved"));
3273 |
3274 | /* Don't tap if out of range. */
3275 | if (exttype > 0 && exttype <= HIGHEST_EXTTYPE32) {
3276 | tap_info->extensions[exttype] = true1;
3277 | }
3278 |
3279 | /* Is this SE allowed for this section type? */
3280 | if (!se_allowed_in_st(exttype, sectionType)) {
3281 | expert_add_info_format(pinfo, extension_tree, &ei_oran_se_on_unsupported_st,
3282 | "SE %u (%s) should not appear in ST %u (%s)!",
3283 | exttype, val_to_str_ext_const(exttype, &exttype_vals_ext, "Reserved"),
3284 | sectionType, rval_to_str_const(sectionType, section_types, "Unknown"));
3285 | }
3286 |
3287 |
3288 | /* extLen (number of 32-bit words) */
3289 | uint32_t extlen_len = ((exttype==11)||(exttype==19)||(exttype==20)) ? 2 : 1; /* Extensions 11/19/20 are special */
3290 | uint32_t extlen;
3291 | proto_item *extlen_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_extlen, tvb,
3292 | offset, extlen_len, ENC_BIG_ENDIAN0x00000000, &extlen);
3293 | proto_item_append_text(extlen_ti, " (%u bytes)", extlen*4);
3294 | offset += extlen_len;
3295 | if (extlen == 0) {
3296 | expert_add_info(pinfo, extlen_ti, &ei_oran_extlen_zero);
3297 | /* Break out to avoid infinitely looping! */
3298 | break;
3299 | }
3300 |
3301 | bool_Bool ext_unhandled = false0;
3302 |
3303 | switch (exttype) {
3304 |
3305 | case 1: /* SE 1: Beamforming Weights */
3306 | {
3307 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
3308 | proto_item *comp_meth_ti = NULL((void*)0);
3309 |
3310 | /* Hidden filter for bf */
3311 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
3312 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
3313 |
3314 | /* bfwCompHdr (2 subheaders - bfwIqWidth and bfwCompMeth)*/
3315 | offset = dissect_bfwCompHdr(tvb, extension_tree, offset,
3316 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
3317 |
3318 | /* bfwCompParam */
3319 | uint32_t exponent = 0;
3320 | bool_Bool compression_method_supported = false0;
3321 | unsigned num_trx = 0;
3322 | uint16_t *trx; /* ptr to array */
3323 | offset = dissect_bfwCompParam(tvb, extension_tree, pinfo, offset, comp_meth_ti,
3324 | &bfwcomphdr_comp_meth, &exponent, &compression_method_supported,
3325 | &num_trx, &trx);
3326 |
3327 | /* Can't show details of unsupported compression method */
3328 | if (!compression_method_supported) {
3329 | break;
3330 | }
3331 |
3332 | /* We know:
3333 | - iq_width (above)
3334 | - numBfWeights (taken from preference)
3335 | - remaining bytes in extension
3336 | We can therefore derive TRX (number of antennas).
3337 | */
3338 |
3339 | bool_Bool using_array = false0;
3340 |
3341 | /* I & Q samples
3342 | May know how many entries from activeBeamspaceCoefficientMask. */
3343 | if (num_trx == 0) {
3344 | /* Don't know how many there will be, so just fill available bytes... */
3345 | unsigned weights_bytes = (extlen*4)-3;
3346 | unsigned num_weights_pairs = (weights_bytes*8) / (bfwcomphdr_iq_width*2);
3347 | num_trx = num_weights_pairs;
3348 | }
3349 | else {
3350 | using_array = true1;
3351 | num_trx = pref_num_bf_antennas;
3352 | }
3353 |
3354 | int bit_offset = offset*8;
3355 |
3356 | for (unsigned n=0; n < num_trx; n++) {
3357 | /* Create antenna subtree */
3358 | int bfw_offset = bit_offset / 8;
3359 |
3360 | uint16_t trx_index = (using_array) ? trx[n] : n+1;
3361 |
3362 | proto_item *bfw_ti = proto_tree_add_string_format(extension_tree, hf_oran_bfw,
3363 | tvb, bfw_offset, 0, "", "TRX %3u: (", trx_index);
3364 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
3365 |
3366 | /* I value */
3367 | /* Get bits, and convert to float. */
3368 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
3369 | float value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent,
3370 | NULL((void*)0) /* no ModCompr */, 0 /* RE */);
3371 | /* Add to tree. */
3372 | proto_tree_add_float(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8,
3373 | (bfwcomphdr_iq_width+7)/8, value);
3374 | bit_offset += bfwcomphdr_iq_width;
3375 | proto_item_append_text(bfw_ti, "I=%f ", value);
3376 |
3377 | /* Leave a gap between I and Q values */
3378 | proto_item_append_text(bfw_ti, " ");
3379 |
3380 | /* Q value */
3381 | /* Get bits, and convert to float. */
3382 | bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
3383 | value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent,
3384 | NULL((void*)0) /* no ModCompr */, 0 /* RE */);
3385 | /* Add to tree. */
3386 | proto_tree_add_float(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8,
3387 | (bfwcomphdr_iq_width+7)/8, value);
3388 | bit_offset += bfwcomphdr_iq_width;
3389 | proto_item_append_text(bfw_ti, "Q=%f", value);
3390 |
3391 | proto_item_append_text(bfw_ti, ")");
3392 | proto_item_set_len(bfw_ti, (bit_offset+7)/8 - bfw_offset);
3393 | }
3394 | /* Need to round to next byte */
3395 | offset = (bit_offset+7)/8;
3396 |
3397 | break;
3398 | }
3399 |
3400 | case 2: /* SE 2: Beamforming attributes */
3401 | {
3402 | /* Hidden filter for bf */
3403 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
3404 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
3405 |
3406 | /* bfaCompHdr (get widths of fields to follow) */
3407 | uint32_t bfAzPtWidth, bfZePtWidth, bfAz3ddWidth, bfZe3ddWidth;
3408 | /* subtree */
3409 | proto_item *bfa_ti = proto_tree_add_string_format(extension_tree, hf_oran_bfaCompHdr,
3410 | tvb, offset, 2, "", "bfaCompHdr");
3411 | proto_tree *bfa_tree = proto_item_add_subtree(bfa_ti, ett_oran_bfacomphdr);
3412 |
3413 | /* reserved (2 bits) */
3414 | add_reserved_field(bfa_tree, hf_oran_reserved_2bits, tvb, offset, 1);
3415 | /* bfAzPtWidth (3 bits) */
3416 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfAzPtWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfAzPtWidth);
3417 | /* bfZePtWidth (3 bits) */
3418 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfZePtWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfZePtWidth);
3419 | offset += 1;
3420 |
3421 | /* reserved (2 bits) */
3422 | add_reserved_field(bfa_tree, hf_oran_reserved_2bits, tvb, offset, 1);
3423 | /* bfAz3ddWidth (3 bits) */
3424 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfAz3ddWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfAz3ddWidth);
3425 | /* bfZe3ddWidth (3 bits) */
3426 | proto_tree_add_item_ret_uint(bfa_tree, hf_oran_bfZe3ddWidth, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &bfZe3ddWidth);
3427 | offset += 1;
3428 |
3429 | unsigned bit_offset = offset*8;
3430 |
3431 | /* bfAzPt */
3432 | if (bfAzPtWidth > 0) {
3433 | proto_tree_add_bits_item(extension_tree, hf_oran_bfAzPt, tvb, bit_offset, bfAzPtWidth+1, ENC_BIG_ENDIAN0x00000000);
3434 | bit_offset += (bfAzPtWidth+1);
3435 | }
3436 | /* bfZePt */
3437 | if (bfZePtWidth > 0) {
3438 | proto_tree_add_bits_item(extension_tree, hf_oran_bfZePt, tvb, bit_offset, bfZePtWidth+1, ENC_BIG_ENDIAN0x00000000);
3439 | bit_offset += (bfZePtWidth+1);
3440 | }
3441 | /* bfAz3dd */
3442 | if (bfAz3ddWidth > 0) {
3443 | proto_tree_add_bits_item(extension_tree, hf_oran_bfAz3dd, tvb, bit_offset, bfAz3ddWidth+1, ENC_BIG_ENDIAN0x00000000);
3444 | bit_offset += (bfAz3ddWidth+1);
3445 | }
3446 | /* bfZe3dd */
3447 | if (bfZe3ddWidth > 0) {
3448 | proto_tree_add_bits_item(extension_tree, hf_oran_bfZe3dd, tvb, bit_offset, bfZe3ddWidth+1, ENC_BIG_ENDIAN0x00000000);
3449 | bit_offset += (bfZe3ddWidth+1);
3450 | }
3451 |
3452 | /* Pad to next byte (unless last 2 fields already fit in this one) */
3453 | if ((bit_offset % 8) > 2) {
3454 | offset = (bit_offset+7) / 8;
3455 | }
3456 | else {
3457 | offset = bit_offset / 8;
3458 | }
3459 |
3460 | /* bfAzSl (3 bits) */
3461 | proto_tree_add_item(extension_tree, hf_oran_bfAzSl, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3462 | /* bfZeSl (3 bits) */
3463 | proto_tree_add_item(extension_tree, hf_oran_bfZeSl, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3464 | offset += 1;
3465 | break;
3466 | }
3467 |
3468 | case 3: /* SE 3: DL precoding parameters */
3469 | {
3470 | /* codebookindex (8 bits) */
3471 | /* "This parameter is not used and shall be set to zero." */
3472 | proto_tree_add_item(extension_tree, hf_oran_codebook_index, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3473 | offset += 1;
3474 | /* layerid */
3475 | uint32_t layerid;
3476 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_layerid, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &layerid);
3477 | /* numLayers */
3478 | proto_tree_add_item(extension_tree, hf_oran_numlayers, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3479 | offset += 1;
3480 |
3481 | /* Stop here for non-first data layer */
3482 | if (layerid != 0 && layerid != 0xf) {
3483 | break;
3484 | }
3485 |
3486 | /* First data layer case */
3487 | /* txScheme */
3488 | proto_tree_add_item(extension_tree, hf_oran_txscheme, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3489 | /* crsReMask */
3490 | proto_tree_add_item(extension_tree, hf_oran_crs_remask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3491 | offset += 2;
3492 |
3493 | /* crsShift (1 bit) */
3494 | proto_tree_add_item(extension_tree, hf_oran_crs_shift, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3495 | /* reserved (3 bits) */
3496 | add_reserved_field(extension_tree, hf_oran_reserved_bits123, tvb, offset, 1);
3497 | /* crsSymNum (4 bits) */
3498 | proto_tree_add_item(extension_tree, hf_oran_crs_symnum, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3499 | offset += 1;
3500 | /* reserved (8 bits) */
3501 | add_reserved_field(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1);
3502 | offset += 1;
3503 |
3504 | /* reserved (1 bit) */
3505 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
3506 | /* beamIdAP1 (15 bits) */
3507 | proto_tree_add_item(extension_tree, hf_oran_beamid_ap1, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3508 | offset += 2;
3509 | /* reserved (1 bit) */
3510 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
3511 | /* beamIdAP2 (15 bits) */
3512 | proto_tree_add_item(extension_tree, hf_oran_beamid_ap2, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3513 | offset += 2;
3514 | /* reserved (1 bit) */
3515 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
3516 | /* beamIdAP3 (15 bits) */
3517 | proto_tree_add_item(extension_tree, hf_oran_beamid_ap3, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3518 | offset += 2;
3519 | break;
3520 | }
3521 |
3522 | case 4: /* SE 4: Modulation compression params (5.4.7.4) (single sets) */
3523 | {
3524 | /* csf */
3525 | bool_Bool csf;
3526 | dissect_csf(extension_tree, tvb, offset*8, ci_iq_width, &csf);
3527 |
3528 | /* modCompScaler */
3529 | uint32_t modCompScaler;
3530 | proto_item *ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_modcompscaler,
3531 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &modCompScaler);
3532 | offset += 2;
3533 |
3534 | /* Work out and show floating point value too. exponent and mantissa are both unsigned */
3535 | uint16_t exponent = (modCompScaler >> 11) & 0x000f; /* m.s. 4 bits */
3536 | uint16_t mantissa = modCompScaler & 0x07ff; /* l.s. 11 bits */
3537 | float value = ((float)mantissa/(1<<11)) * ((float)1.0 / (1 << exponent));
3538 | proto_item_append_text(ti, " (%f)", value);
3539 |
3540 | section_mod_compr_config_t* sect_config = get_mod_compr_section_to_write(state, sectionId);
3541 |
3542 | /* Store these params in this flow's state */
3543 | if (sect_config && sect_config->num_configs < MAX_MOD_COMPR_CONFIGS12) {
3544 | unsigned i = sect_config->num_configs;
3545 | sect_config->configs[i].mod_compr_re_mask = 0xfff; /* Covers all REs */
3546 | sect_config->configs[i].mod_compr_csf = csf;
3547 | sect_config->configs[i].mod_compr_scaler = value;
3548 | sect_config->num_configs++;
3549 | }
3550 | break;
3551 | }
3552 |
3553 | case 5: /* SE 5: Modulation Compression Additional Parameters (7.7.5) (multiple sets) */
3554 | {
3555 | /* Applies only to section types 1,3 and 5 */
3556 | /* N.B. there may be multiple instances of this SE in the same frame */
3557 |
3558 | /* There may be one or 2 entries, depending upon extlen */
3559 | int sets = 1, reserved_bits = 0;
3560 | switch (extlen) {
3561 | case 2:
3562 | sets = 1;
3563 | reserved_bits = 20;
3564 | break;
3565 | case 3:
3566 | sets = 2;
3567 | reserved_bits = 24;
3568 | break;
3569 | case 4:
3570 | /* sets can be 3 or 4, depending upon whether last 28 bits are 0.. */
3571 | if ((tvb_get_ntohl(tvb, offset+10) & 0x0fffffff) == 0) {
3572 | sets = 3;
3573 | reserved_bits = 28;
3574 | }
3575 | else {
3576 | sets = 4;
3577 | reserved_bits = 0;
3578 | }
3579 | break;
3580 |
3581 | default:
3582 | /* Malformed error!!! */
3583 | expert_add_info_format(pinfo, extlen_ti, &ei_oran_extlen_wrong,
3584 | "For section 5, extlen must be 2, 3 or 4, but %u was dissected",
3585 | extlen);
3586 | break;
3587 | }
3588 |
3589 | unsigned bit_offset = offset*8;
3590 | /* Dissect each set */
3591 | for (int n=0; n < sets; n++) {
3592 | /* Subtree for each set */
3593 | unsigned set_start_offset = bit_offset/8;
3594 | proto_item *set_ti = proto_tree_add_string(extension_tree, hf_oran_modcomp_param_set,
3595 | tvb, set_start_offset, 0, "");
3596 | proto_tree *set_tree = proto_item_add_subtree(set_ti, ett_oran_modcomp_param_set);
3597 |
3598 | uint64_t mcScaleReMask, mcScaleOffset;
3599 | bool_Bool csf;
3600 |
3601 | /* mcScaleReMask (12 bits). Defines which REs the following csf and mcScaleOffset apply to */
3602 | static int * const remask_flags[] = {
3603 | &hf_oran_mc_scale_re_mask_re1,
3604 | &hf_oran_mc_scale_re_mask_re2,
3605 | &hf_oran_mc_scale_re_mask_re3,
3606 | &hf_oran_mc_scale_re_mask_re4,
3607 | &hf_oran_mc_scale_re_mask_re5,
3608 | &hf_oran_mc_scale_re_mask_re6,
3609 | &hf_oran_mc_scale_re_mask_re7,
3610 | &hf_oran_mc_scale_re_mask_re8,
3611 | &hf_oran_mc_scale_re_mask_re9,
3612 | &hf_oran_mc_scale_re_mask_re10,
3613 | &hf_oran_mc_scale_re_mask_re11,
3614 | &hf_oran_mc_scale_re_mask_re12,
3615 | NULL((void*)0)
3616 | };
3617 | /* Same as above, but offset by 4 bits */
3618 | static int * const remask_flags_even[] = {
3619 | &hf_oran_mc_scale_re_mask_re1_even,
3620 | &hf_oran_mc_scale_re_mask_re2_even,
3621 | &hf_oran_mc_scale_re_mask_re3_even,
3622 | &hf_oran_mc_scale_re_mask_re4_even,
3623 | &hf_oran_mc_scale_re_mask_re5_even,
3624 | &hf_oran_mc_scale_re_mask_re6_even,
3625 | &hf_oran_mc_scale_re_mask_re7_even,
3626 | &hf_oran_mc_scale_re_mask_re8_even,
3627 | &hf_oran_mc_scale_re_mask_re9_even,
3628 | &hf_oran_mc_scale_re_mask_re10_even,
3629 | &hf_oran_mc_scale_re_mask_re11_even,
3630 | &hf_oran_mc_scale_re_mask_re12_even,
3631 | NULL((void*)0)
3632 | };
3633 |
3634 | /* RE Mask (12 bits) */
3635 | proto_tree_add_bitmask_ret_uint64(set_tree, tvb, bit_offset / 8,
3636 | (n % 2) ? hf_oran_mc_scale_re_mask_even : hf_oran_mc_scale_re_mask,
3637 | ett_oran_mc_scale_remask,
3638 | (n % 2) ? remask_flags_even : remask_flags, ENC_BIG_ENDIAN0x00000000, &mcScaleReMask);
3639 | bit_offset += 12;
3640 |
3641 | /* csf (1 bit) */
3642 | bit_offset = dissect_csf(set_tree, tvb, bit_offset, ci_iq_width, &csf);
3643 | /* mcScaleOffset (15 bits) */
3644 | proto_item *ti = proto_tree_add_bits_ret_val(set_tree, hf_oran_mc_scale_offset, tvb, bit_offset, 15, &mcScaleOffset, ENC_BIG_ENDIAN0x00000000);
3645 | uint16_t exponent = (mcScaleOffset >> 11) & 0x000f; /* m.s. 4 bits */
3646 | uint16_t mantissa = mcScaleOffset & 0x07ff; /* l.s. 11 bits */
3647 | float mcScaleOffset_value = ((float)mantissa/(1<<11)) * ((float)1.0 / (1 << exponent));
3648 | proto_item_append_text(ti, " (%f)", mcScaleOffset_value);
3649 | bit_offset += 15;
3650 |
3651 | section_mod_compr_config_t* sect_config = get_mod_compr_section_to_write(state, sectionId);
3652 |
3653 | /* Record this config */
3654 | if (sect_config && sect_config->num_configs < MAX_MOD_COMPR_CONFIGS12) {
3655 | unsigned i = sect_config->num_configs;
3656 | sect_config->configs[i].mod_compr_re_mask = (uint16_t)mcScaleReMask;
3657 | sect_config->configs[i].mod_compr_csf = csf;
3658 | sect_config->configs[i].mod_compr_scaler = mcScaleOffset_value;
3659 | sect_config->num_configs++;
3660 | }
3661 |
3662 | /* Summary */
3663 | proto_item_set_len(set_ti, (bit_offset+7)/8 - set_start_offset);
3664 | proto_item_append_text(set_ti, " (mcScaleReMask=0x%03x csf=%5s mcScaleOffset=%f)",
3665 | (unsigned)mcScaleReMask, tfs_get_true_false(csf)tfs_get_string(csf, ((void*)0)), mcScaleOffset_value);
3666 | }
3667 |
3668 | proto_item_append_text(extension_ti, " (%u sets)", sets);
3669 |
3670 | /* Reserved (variable-length) */
3671 | if (reserved_bits) {
3672 | proto_tree_add_bits_item(extension_tree, hf_oran_reserved, tvb, bit_offset, reserved_bits, ENC_BIG_ENDIAN0x00000000);
3673 | bit_offset += reserved_bits;
3674 | }
3675 |
3676 | offset = bit_offset/8;
3677 | break;
3678 | }
3679 |
3680 | case 6: /* SE 6: Non-contiguous PRB allocation in time and frequency domain */
3681 | {
3682 | /* numSymbol not used in this case */
3683 | if (numsymbol_ti && !numsymbol_ignored) {
3684 | proto_item_append_text(numsymbol_ti, " (ignored)");
3685 | numsymbol_ignored = true1;
3686 | }
3687 |
3688 | /* Will update ext6 recorded info */
3689 | ext11_settings.ext6_set = true1;
3690 |
3691 | /* repetition */
3692 | proto_tree_add_bits_item(extension_tree, hf_oran_se6_repetition, tvb, offset*8, 1, ENC_BIG_ENDIAN0x00000000);
3693 | /* rbgSize (PRBs per bit set in rbgMask) */
3694 | uint32_t rbgSize;
3695 | proto_item *rbg_size_ti;
3696 | rbg_size_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_rbgSize, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &rbgSize);
3697 | if (rbgSize == 0) {
3698 | /* N.B. this is only true if "se6-rb-bit-supported" is set... */
3699 | expert_add_info(pinfo, rbg_size_ti, &ei_oran_rbg_size_reserved);
3700 | }
3701 | /* rbgMask (28 bits) */
3702 | uint32_t rbgMask;
3703 | proto_item *rbgmask_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_rbgMask, tvb, offset, 4, ENC_BIG_ENDIAN0x00000000, &rbgMask);
3704 | if (rbgSize == 0) {
3705 | proto_item_append_text(rbgmask_ti, " (value ignored since rbgSize is 0)");
3706 | }
3707 |
3708 | /* TODO: if receiver detects non-zero bits outside the valid range, those shall be ignored. */
3709 | offset += 4;
3710 | /* priority */
3711 | proto_tree_add_item(extension_tree, hf_oran_noncontig_priority, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3712 | /* symbolMask */
3713 | offset = dissect_symbolmask(tvb, extension_tree, offset, NULL((void*)0), NULL((void*)0));
3714 |
3715 | /* Look up rbg_size enum -> value */
3716 | switch (rbgSize) {
3717 | case 0:
3718 | /* N.B. reserved, but covered above with expert info (would remain 0) */
3719 | break;
3720 | case 1:
3721 | ext11_settings.ext6_rbg_size = 1; break;
3722 | case 2:
3723 | ext11_settings.ext6_rbg_size = 2; break;
3724 | case 3:
3725 | ext11_settings.ext6_rbg_size = 3; break;
3726 | case 4:
3727 | ext11_settings.ext6_rbg_size = 4; break;
3728 | case 5:
3729 | ext11_settings.ext6_rbg_size = 6; break;
3730 | case 6:
3731 | ext11_settings.ext6_rbg_size = 8; break;
3732 | case 7:
3733 | ext11_settings.ext6_rbg_size = 16; break;
3734 | /* N.B., encoded in 3 bits, so no other values are possible */
3735 | }
3736 |
3737 | /* Set to looked-up value */
3738 | rbgSize = ext11_settings.ext6_rbg_size;
3739 |
3740 | uint32_t lastRbgid = 0;
3741 | if (rbgSize != 0) {
3742 | /* The O-DU shall not use combinations of startPrbc, numPrbc and rbgSize leading to a value of lastRbgid larger than 27 */
3743 | /* i.e., leftmost bit used should not need to go off left end of rbgMask! */
3744 | lastRbgid = (uint32_t)ceil((numPrbc + (startPrbc % rbgSize)) / (float)rbgSize) - 1;
3745 | if (lastRbgid > 27) {
3746 | expert_add_info_format(pinfo, rbg_size_ti, &ei_oran_lastRbdid_out_of_range,
3747 | "SE6: rbgSize (%u) not compatible with startPrbc(%u) and numPrbc(%u)",
3748 | rbgSize, startPrbc, numPrbc);
3749 | break;
3750 | }
3751 | }
3752 |
3753 | /* Record (and count) which bits are set in rbgMask */
3754 | bool_Bool first_seen = false0;
3755 | unsigned first_seen_pos=0, last_seen_pos=0;
3756 | for (unsigned n=0; n < 28 && ext11_settings.ext6_num_bits_set < 28; n++) {
3757 | if ((rbgMask >> n) & 0x01) {
3758 | ext11_settings.ext6_bits_set[ext11_settings.ext6_num_bits_set++] = n;
3759 | if (!first_seen) {
3760 | first_seen = true1;
3761 | first_seen_pos = n;
3762 | }
3763 | last_seen_pos = n;
3764 | }
3765 | }
3766 |
3767 | /* Show how many bits were set in rbgMask */
3768 | proto_item_append_text(rbgmask_ti, " (%u bits set)", ext11_settings.ext6_num_bits_set);
3769 | /* Also, that is the range of bits */
3770 | if (first_seen) {
3771 | proto_item_append_text(rbgmask_ti, " (%u bits spread)", last_seen_pos-first_seen_pos+1);
3772 |
3773 | /* Complain if last set bit is beyond lastRbgid */
3774 | if (last_seen_pos > lastRbgid) {
3775 | expert_add_info_format(pinfo, rbgmask_ti, &ei_oran_rbgMask_beyond_last_rbdid,
3776 | "SE6: rbgMask (0x%07x) has bit %u set, but lastRbgId is %u",
3777 | rbgMask, last_seen_pos, lastRbgid);
3778 | }
3779 | }
3780 |
3781 | /* Also update prbs_for_st10_type5[] */
3782 | if (sectionType == 10 && rbgSize != 0) {
3783 | /* Unset all entries */
3784 | memset(&prbs_for_st10_type5, 0, sizeof(prbs_for_st10_type5));
3785 |
3786 | /* Work out which PRB first bit corresponds to */
3787 | unsigned firstPrbStart = (startPrbc/rbgSize) * rbgSize;
3788 |
3789 | /* Add PRBs corresponding to each bit set */
3790 | for (unsigned n=0; n < 28 ; n++) {
3791 | if ((rbgMask >> n) & 0x01) {
3792 | /* Lazy way to clip any values that lie outside of range for section */
3793 | for (unsigned p=0; p < rbgSize; p++) {
3794 | unsigned start = firstPrbStart + (n*rbgSize);
3795 | if ((start+p < MAX_PRBS273) && (start+p >= startPrbc) && (start+p <= startPrbc+numPrbc-1)) {
3796 | prbs_for_st10_type5[start+p] = true1;
3797 | }
3798 | }
3799 | }
3800 | }
3801 | }
3802 |
3803 | break;
3804 | }
3805 |
3806 | case 7: /* SE 7: eAxC mask */
3807 | /* Allow ST0 to address multiple eAxC_ID values for transmission blanking */
3808 | proto_tree_add_item(extension_tree, hf_oran_eAxC_mask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3809 | offset += 2;
3810 | break;
3811 |
3812 | case 8: /* SE 8: Regularization factor */
3813 | proto_tree_add_item(extension_tree, hf_oran_regularizationFactor, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
3814 | offset += 2;
3815 | break;
3816 |
3817 | case 9: /* SE 9: Dynamic Spectrum Sharing parameters */
3818 | proto_tree_add_item(extension_tree, hf_oran_technology, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
3819 | offset += 1;
3820 | add_reserved_field(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1);
3821 | offset += 1;
3822 | break;
3823 |
3824 | case 10: /* SE 10: Group configuration of multiple ports */
3825 | {
3826 | seen_se10 = true1;
3827 |
3828 | /* beamGroupType */
3829 | uint32_t beam_group_type = 0;
3830 | proto_item *bgt_ti;
3831 | bgt_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_beamGroupType,
3832 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &beam_group_type);
3833 | proto_item_append_text(extension_ti, " (%s)", val_to_str_const(beam_group_type, beam_group_type_vals, "Unknown"));
3834 |
3835 | /* numPortc */
3836 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_numPortc,
3837 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPortc);
3838 | offset++;
3839 |
3840 | /* Will append all beamId values to extension_ti, regardless of beamGroupType */
3841 | unsigned n;
3842 |
3843 | switch (beam_group_type) {
3844 | case 0x0: /* common beam */
3845 | case 0x1: /* beam matrix indication */
3846 | /* Reserved byte */
3847 | add_reserved_field(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1);
3848 | offset++;
3849 |
3850 | /* Explain how entries are allocated */
3851 | if (beam_group_type == 0x0) {
3852 | proto_item_append_text(extension_ti, " (all %u ueid/Beam entries are %u)", numPortc, ueId);
3853 | }
3854 | else {
3855 | /* 'numPortc' consecutive BeamIds from section header */
3856 | proto_item_append_text(extension_ti, " (ueId/beam entries are %u -> %u)", ueId, ueId+numPortc);
3857 | }
3858 |
3859 | if (sectionType == 5) {
3860 | /* These types are not allowed */
3861 | expert_add_info_format(pinfo, bgt_ti, &ei_oran_se10_not_allowed,
3862 | "SE10: beamGroupType %u is not allowed for section type 5", beam_group_type);
3863 | }
3864 | break;
3865 |
3866 | case 0x2: /* beam vector listing */
3867 | {
3868 | proto_item_append_text(extension_ti, " [ ");
3869 |
3870 | /* Beam listing vector case */
3871 | /* Work out how many port beam entries there is room for */
3872 | /* Using numPortC as visible in issue 18116 */
3873 | for (n=0; n < numPortc; n++) {
3874 | /* 1 reserved bit */
3875 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
3876 |
3877 | /* port beam ID (or UEID) (15 bits) */
3878 | uint32_t id;
3879 | proto_item *beamid_or_ueid_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_beamId,
3880 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &id);
3881 | proto_item_append_text(beamid_or_ueid_ti, " port #%u beam ID (or UEId) %u", n, id);
3882 | offset += 2;
3883 |
3884 | if (id != 0x7fff) {
3885 | if (number_of_ueids < MAX_UEIDS16) {
3886 | ueids[number_of_ueids++] = id;
3887 | }
3888 | }
3889 |
3890 | proto_item_append_text(extension_ti, "%u ", id);
3891 | }
3892 |
3893 | proto_item_append_text(extension_ti, "]");
3894 | break;
3895 | }
3896 | case 0x3: /* beamId/ueId listing with associated port-list index */
3897 | {
3898 | proto_item_append_text(extension_ti, " [ ");
3899 |
3900 | if (numPortc > 0) {
3901 | /* first portListIndex is outside loop */
3902 | uint32_t port_list_index;
3903 | proto_item *pli_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_port_list_index, tvb,
3904 | offset, 1, ENC_BIG_ENDIAN0x00000000, &port_list_index);
3905 | if (port_list_index == 0) {
3906 | /* Value 0 is reserved */
3907 | expert_add_info(pinfo, pli_ti, &ei_oran_port_list_index_zero);
3908 | }
3909 | offset += 1;
3910 |
3911 | for (n=0; n < numPortc-1; n++) {
3912 | /* 1 reserved bit */
3913 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
3914 |
3915 | /* port beam ID (or UEID) */
3916 | uint32_t id;
3917 | proto_item *beamid_or_ueid_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_beamId,
3918 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &id);
3919 | proto_item_append_text(beamid_or_ueid_ti, " port #%u beam ID (or UEId) %u", n, id);
3920 | offset += 2;
3921 |
3922 | if (id != 0x7fff) {
3923 | if (number_of_ueids < MAX_UEIDS16) {
3924 | ueids[number_of_ueids++] = id;
3925 | }
3926 | }
3927 |
3928 | /* subsequent portListIndex */
3929 | pli_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_port_list_index, tvb,
3930 | offset, 1, ENC_BIG_ENDIAN0x00000000, &port_list_index);
3931 | if (port_list_index == 0) {
3932 | /* Value 0 is reserved */
3933 | expert_add_info(pinfo, pli_ti, &ei_oran_port_list_index_zero);
3934 | }
3935 | offset += 1;
3936 |
3937 | proto_item_append_text(extension_ti, "%u:%u ", port_list_index, id);
3938 | }
3939 | }
3940 |
3941 | proto_item_append_text(extension_ti, "]");
3942 | break;
3943 | }
3944 |
3945 |
3946 | default:
3947 | /* Warning for unsupported/reserved value */
3948 | expert_add_info(NULL((void*)0), bgt_ti, &ei_oran_se10_unknown_beamgrouptype);
3949 | break;
3950 | }
3951 | break;
3952 | }
3953 |
3954 | case 11: /* SE 11: Flexible Weights Extension Type */
3955 | {
3956 | /* Hidden filter for bf */
3957 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
3958 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
3959 |
3960 | /* beamId in section header should be ignored. Guard against appending multiple times.. */
3961 | if (section_beamId_ti && !section_beamId_ignored) {
3962 | proto_item_append_text(section_beamId_ti, " (ignored)");
3963 | section_beamId_ignored = true1;
3964 | }
3965 |
3966 | bool_Bool disableBFWs;
3967 | uint32_t numBundPrb;
3968 | bool_Bool rad;
3969 |
3970 | /* disableBFWs */
3971 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_disable_bfws,
3972 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disableBFWs);
3973 | if (disableBFWs) {
3974 | proto_item_append_text(extension_ti, " (disableBFWs)");
3975 | }
3976 |
3977 | /* RAD */
3978 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_rad,
3979 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &rad);
3980 | /* bundleOffset (6 bits) */
3981 | proto_tree_add_item(extension_tree, hf_oran_bundle_offset, tvb,
3982 | offset, 1, ENC_BIG_ENDIAN0x00000000);
3983 | offset++;
3984 |
3985 | /* numBundPrb (number of prbs in each bundle) */
3986 | proto_item *num_bund_prb_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_bund_prbs,
3987 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numBundPrb);
3988 | offset++;
3989 | /* value zero is reserved.. */
3990 | if (numBundPrb == 0) {
3991 | expert_add_info(pinfo, num_bund_prb_ti, &ei_oran_reserved_numBundPrb);
3992 | }
3993 |
3994 | uint32_t num_bundles;
3995 | bool_Bool orphaned_prbs = false0;
3996 |
3997 | /* N.B. glibly assuming that Mu=1 */
3998 | uint32_t symbol_count = (frameId*20 + slotId) * 14 + startSymbolId;
3999 |
4000 | if (!disableBFWs) {
4001 | /********************************************/
4002 | /* Table 7.7.1.1-1 */
4003 | /********************************************/
4004 |
4005 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
4006 | proto_item *comp_meth_ti = NULL((void*)0);
4007 |
4008 | /* bfwCompHdr (2 subheaders - bfwIqWidth and bfwCompMeth)*/
4009 | offset = dissect_bfwCompHdr(tvb, extension_tree, offset,
4010 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
4011 |
4012 | /* Work out number of bundles, but take care not to divide by zero. */
4013 | if (numBundPrb == 0) {
4014 | break;
4015 | }
4016 |
4017 | /* Work out bundles! */
4018 | ext11_work_out_bundles(startPrbc, numPrbc, numBundPrb, &ext11_settings);
4019 | num_bundles = ext11_settings.num_bundles;
4020 |
4021 | /* Add (complete) bundles */
4022 | for (unsigned b=0; b < num_bundles; b++) {
4023 | offset = dissect_bfw_bundle(tvb, extension_tree, pinfo, offset,
4024 | comp_meth_ti, bfwcomphdr_comp_meth,
4025 | NULL((void*)0) /* no ModCompr */,
4026 | (ext11_settings.ext21_set) ?
4027 | numPrbc :
4028 | pref_num_bf_antennas,
4029 | bfwcomphdr_iq_width,
4030 | b, /* bundle number */
4031 | ext11_settings.bundles[b].start,
4032 | ext11_settings.bundles[b].end,
4033 | ext11_settings.bundles[b].is_orphan,
4034 | symbol_count,
4035 | (link_planes_together && data_section) ? &data_section->details[index_to_use] : NULL((void*)0),
4036 | tap_info);
4037 | if (!offset) {
4038 | break;
4039 | }
4040 | }
4041 | if (num_bundles > 0) {
4042 | /* Set flag from last bundle entry */
4043 | orphaned_prbs = ext11_settings.bundles[num_bundles-1].is_orphan;
4044 | }
4045 | }
4046 | else {
4047 | /********************************************/
4048 | /* Table 7.7.1.1-2 */
4049 | /* No weights in this case */
4050 | /********************************************/
4051 |
4052 | /* Work out number of bundles, but take care not to divide by zero. */
4053 | if (numBundPrb == 0) {
4054 | break;
4055 | }
4056 |
4057 | ext11_work_out_bundles(startPrbc, numPrbc, numBundPrb, &ext11_settings);
4058 | num_bundles = ext11_settings.num_bundles;
4059 |
4060 | for (unsigned n=0; n < num_bundles; n++) {
4061 | /* contInd */
4062 | proto_tree_add_item(extension_tree, hf_oran_cont_ind,
4063 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4064 | /* beamId */
4065 | /* N.B., only added to tap_info if not 0 or ignored (after SEs seen) */
4066 | uint32_t beam_id;
4067 | proto_item *beamid_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_beam_id,
4068 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &beam_id);
4069 | if (!ext11_settings.bundles[n].is_orphan) {
4070 | proto_item_append_text(beamid_ti, " (PRBs %3u-%3u) (Bundle %2u)",
4071 | ext11_settings.bundles[n].start,
4072 | ext11_settings.bundles[n].end,
4073 | n);
4074 | }
4075 | else {
4076 | orphaned_prbs = true1;
4077 | proto_item_append_text(beamid_ti, " (PRBs %3u-%3u) (Orphaned PRBs)",
4078 | ext11_settings.bundles[n].start,
4079 | ext11_settings.bundles[n].end);
4080 | }
4081 | offset += 2;
4082 |
4083 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
4084 | if (data_section) {
4085 | /* Set beamId only for range of PRBs */
4086 | for (unsigned prb = ext11_settings.bundles[n].start; prb <= ext11_settings.bundles[n].end; prb++) {
4087 | if (prb < 273) {
4088 | data_section->details[index_to_use].beamIds[prb] = beam_id;
4089 | }
4090 | }
4091 | }
4092 | }
4093 |
4094 | /* Look for where BFWs were sent for this beamId */
4095 | bfw_definition *definition;
4096 |
4097 | wmem_tree_key_t key[3];
4098 | key[0].length = 1;
4099 | key[0].key = &pinfo->num;
4100 | key[1].length = 1;
4101 | key[1].key = &beam_id;
4102 | key[2].length = 0;
4103 | key[2].key = NULL((void*)0);
4104 |
4105 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
4106 | /* Look up current result */
4107 | definition = wmem_tree_lookup32(dl_beam_ids_defined, beam_id);
4108 | if (definition != NULL((void*)0)) {
4109 | /* Add to results table for this frame */
4110 | wmem_tree_insert32_array(dl_beam_ids_results, key, definition);
4111 | }
4112 | }
4113 | else {
4114 | /* Look up from result table */
4115 | definition = wmem_tree_lookup32_array(dl_beam_ids_results, key);
4116 | }
4117 |
4118 | /* Show link back to frame where/when beamId was defined */
4119 | if (definition && definition->frame_defined != 0 && definition->frame_defined != pinfo->num) {
4120 | proto_item *defined_ti = proto_tree_add_uint(extension_tree, hf_oran_bfws_frame_defined, tvb, offset, 0, definition->frame_defined);
4121 | proto_item_set_generated(defined_ti);
4122 | proto_item *since_ti = proto_tree_add_uint(extension_tree, hf_oran_bfws_symbols_since_defined, tvb, offset, 0,
4123 | symbol_count - definition->symbol_when_defined);
4124 | proto_item_set_generated(since_ti);
4125 | }
4126 | else {
4127 | expert_add_info_format(NULL((void*)0), beamid_ti, &ei_oran_beamid_bfws_not_found,
4128 | "ext11 for beamId %u and disableBFWs set, but can't find definition", beam_id);
4129 | }
4130 | }
4131 |
4132 | }
4133 |
4134 | /* Add summary to extension root */
4135 | if (orphaned_prbs) {
4136 | proto_item_append_text(extension_ti, " (%u full bundles + orphaned)", num_bundles-1);
4137 | }
4138 | else {
4139 | proto_item_append_text(extension_ti, " (%u bundles)", num_bundles);
4140 | }
4141 | }
4142 |
4143 | break;
4144 |
4145 | case 12: /* SE 12: Non-Contiguous PRB Allocation with Frequency Ranges */
4146 | {
4147 | /* numSymbol not used in this case */
4148 | if (numsymbol_ti && !numsymbol_ignored) {
4149 | proto_item_append_text(numsymbol_ti, " (ignored)");
4150 | numsymbol_ignored = true1;
4151 | }
4152 |
4153 | ext11_settings.ext12_set = true1;
4154 |
4155 | /* priority */
4156 | proto_tree_add_item(extension_tree, hf_oran_noncontig_priority, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4157 |
4158 | /* symbolMask */
4159 | offset = dissect_symbolmask(tvb, extension_tree, offset, NULL((void*)0), NULL((void*)0));
4160 |
4161 | /* There are now 'R' pairs of (offStartPrb, numPrb) values. Fill extlen bytes with values. If last one is not set,
4162 | should be populated with 0s. */
4163 | uint32_t extlen_remaining_bytes = (extlen*4) - 4;
4164 | uint8_t prb_index;
4165 |
4166 | /* This is for ST10/ST11. First pair starts after frames signalled there */
4167 | uint16_t st10_st11_offset = startPrbc + numPrbc;
4168 |
4169 | for (prb_index = 1; extlen_remaining_bytes > 0; prb_index++)
4170 | {
4171 | /* Create a subtree for each pair */
4172 | proto_item *pair_ti = proto_tree_add_string(extension_tree, hf_oran_frequency_range,
4173 | tvb, offset, 2, "");
4174 | proto_tree *pair_tree = proto_item_add_subtree(pair_ti, ett_oran_frequency_range);
4175 |
4176 | /* offStartPrb */
4177 | uint32_t off_start_prb;
4178 | proto_tree_add_item_ret_uint(pair_tree, hf_oran_off_start_prb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &off_start_prb);
4179 | offset++;
4180 |
4181 | /* numPrb */
4182 | uint32_t num_prb;
4183 | proto_tree_add_item_ret_uint(pair_tree, hf_oran_num_prb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_prb);
4184 | offset++;
4185 |
4186 | extlen_remaining_bytes -= 2;
4187 |
4188 | /* Last pair may be 0,0 if not used. Check for this */
4189 | if ((extlen_remaining_bytes == 0) && (off_start_prb == 0) && (num_prb == 0)) {
4190 | proto_item_append_text(pair_ti, " (not used)");
4191 | }
4192 | /* Add summary to pair root item, and configure details in ext11_settings */
4193 | else {
4194 | proto_item_append_text(pair_ti, "(%u) [%u : %u]",
4195 | prb_index, off_start_prb, num_prb);
4196 | proto_item_append_text(extension_ti, "[%u : %u]",
4197 | off_start_prb, num_prb);
4198 | if (ext11_settings.ext12_num_pairs < MAX_BFW_EXT12_PAIRS128) {
4199 | ext11_settings.ext12_pairs[ext11_settings.ext12_num_pairs].off_start_prb = off_start_prb;
4200 | ext11_settings.ext12_pairs[ext11_settings.ext12_num_pairs++].num_prb = num_prb;
4201 | }
4202 |
4203 | /* Also update PRBs to be covered for ST10 type 5 */
4204 | /* Original range from section is added to.. */
4205 | /* TODO: I don't think this is quite right.. */
4206 | for (unsigned prb=st10_st11_offset+off_start_prb; prb < st10_st11_offset+off_start_prb+num_prb; prb++) {
4207 | if (prb < MAX_PRBS273) {
4208 | prbs_for_st10_type5[prb] = true1;
4209 | }
4210 | }
4211 |
4212 | /* Any next pair will begin after this one */
4213 | st10_st11_offset += (off_start_prb + num_prb);
4214 | }
4215 | }
4216 | break;
4217 | }
4218 |
4219 | case 13: /* SE 13: PRB Allocation with Frequency Hopping */
4220 | {
4221 | /* Will update settings for ext11 */
4222 | ext11_settings.ext13_set = true1;
4223 |
4224 | uint32_t extlen_remaining_bytes = (extlen*4) - 2;
4225 | uint8_t allocation_index;
4226 |
4227 | unsigned prev_next_symbol_id = 0, prev_next_start_prbc = 0;
4228 |
4229 | for (allocation_index = 1; extlen_remaining_bytes > 0; allocation_index++)
4230 | {
4231 | /* Subtree for allocation */
4232 | proto_item *allocation_ti = proto_tree_add_string(extension_tree, hf_oran_prb_allocation,
4233 | tvb, offset, 2, "");
4234 | proto_tree *allocation_tree = proto_item_add_subtree(allocation_ti, ett_oran_prb_allocation);
4235 |
4236 | /* Reserved (2 bits) */
4237 | add_reserved_field(allocation_tree, hf_oran_reserved_2bits, tvb, offset, 1);
4238 |
4239 | /* nextSymbolId (4 bits) */
4240 | uint32_t next_symbol_id;
4241 | proto_tree_add_item_ret_uint(allocation_tree, hf_oran_nextSymbolId, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &next_symbol_id);
4242 |
4243 | /* nextStartPrbc (10 bits) */
4244 | uint32_t next_start_prbc;
4245 | proto_tree_add_item_ret_uint(allocation_tree, hf_oran_nextStartPrbc, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &next_start_prbc);
4246 | offset += 2;
4247 |
4248 | /* Add summary to allocation root item */
4249 | proto_item_append_text(allocation_ti, "(%u) nextSymbolId=%3u, nextStartPrbc=%u",
4250 | allocation_index, next_symbol_id, next_start_prbc);
4251 |
4252 | /* Checking for duplicates (expected if e.g. had only 2 entries but extlen bytes still to fill */
4253 | if ((allocation_index > 1) && (next_symbol_id == prev_next_symbol_id) && (next_start_prbc == prev_next_start_prbc)) {
4254 | proto_item_append_text(allocation_ti, " (repeated - to fill up extlen)");
4255 | }
4256 | else {
4257 | /* Add entry for configuring ext11. don't store out of range */
4258 | if (ext11_settings.ext13_num_start_prbs < MAX_BFW_EXT13_ALLOCATIONS128) {
4259 | ext11_settings.ext13_start_prbs[ext11_settings.ext13_num_start_prbs++] = next_start_prbc;
4260 | }
4261 | }
4262 | prev_next_symbol_id = next_symbol_id;
4263 | prev_next_start_prbc = next_start_prbc;
4264 |
4265 | extlen_remaining_bytes -= 2;
4266 | }
4267 | break;
4268 | }
4269 |
4270 | case 14: /* SE 14: Nulling-layer Info. for ueId-based beamforming */
4271 | /* Hidden filter for bf (DMRS BF) */
4272 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
4273 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
4274 |
4275 | if (!seen_se10) {
4276 | proto_tree_add_item(extension_tree, hf_oran_nullLayerInd, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4277 | offset += 1;
4278 | add_reserved_field(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1);
4279 | offset += 1;
4280 | }
4281 | else {
4282 | /* Loop over numPortc++1 (from SE 10) nullLayerInd fields */
4283 | for (unsigned port=0; port < numPortc+1; port++) {
4284 | proto_tree_add_item(extension_tree, hf_oran_nullLayerInd, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4285 | offset += 1;
4286 | }
4287 | }
4288 | break;
4289 |
4290 | case 15: /* SE 15: Mixed-numerology Info. for ueId-based beamforming */
4291 | {
4292 | /* frameStructure */
4293 | offset = dissect_frame_structure(extension_tree, tvb, offset,
4294 | subframeId, slotId);
4295 | /* freqOffset */
4296 | proto_tree_add_item(extension_tree, hf_oran_freqOffset, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
4297 | offset += 3;
4298 | /* cpLength */
4299 | proto_item *cplength_ti = proto_tree_add_item(extension_tree, hf_oran_cpLength, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4300 | if (sectionType != 0 && sectionType != 3) {
4301 | proto_item_append_text(cplength_ti, " (ignored - used only with ST0 and ST3)");
4302 | }
4303 | offset += 2;
4304 | break;
4305 | }
4306 |
4307 | case 16: /* SE 16: Antenna mapping in UE channel information based UL beamforming */
4308 | {
4309 | /* Just filling available bytes with antMask entries.
4310 | N.B., if SE 10 also used, could associate each antMask with (beamId or UEId) RX eAxC */
4311 | uint32_t extlen_remaining_bytes = (extlen*4) - 2;
4312 | unsigned num_ant_masks = extlen_remaining_bytes / 8;
4313 | for (unsigned n=0; n < num_ant_masks; n++) {
4314 | proto_item *ti = proto_tree_add_item(extension_tree, hf_oran_antMask, tvb, offset, 8, ENC_BIG_ENDIAN0x00000000);
4315 | proto_item_append_text(ti, " (RX eAxC #%u)", n+1);
4316 | offset += 8;
4317 | }
4318 | break;
4319 | }
4320 |
4321 | case 17: /* SE 17: Indication of user port group. Applies to ST5 + SE10 with group type 1 (beam matrix indication) */
4322 | {
4323 | uint32_t extlen_remaining_bytes = (extlen*4) - 2;
4324 | uint32_t end_bit = (offset+extlen_remaining_bytes) * 8;
4325 | uint32_t ueid_index = 1;
4326 |
4327 | /* "the preceding Section Type and extension messages implicitly provide the number of scheduled users" */
4328 | for (uint32_t bit_offset=offset*8; (bit_offset < end_bit) && (ueid_index <= number_of_ueids); bit_offset+=4, ueid_index++) {
4329 | /* numUeId (Number of UE Ids per user) */
4330 | proto_item *ti = proto_tree_add_bits_item(extension_tree, hf_oran_num_ueid, tvb, bit_offset, 4, ENC_BIG_ENDIAN0x00000000);
4331 | /* TODO: show ueids[ueid_index] here too? */
4332 | proto_item_append_text(ti, " (user #%u)", ueid_index);
4333 | }
4334 | break;
4335 | }
4336 |
4337 | case 18: /* SE 18: Uplink transmission management */
4338 | /* transmissionWindowOffset */
4339 | proto_tree_add_item(extension_tree, hf_oran_transmissionWindowOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4340 | offset += 2;
4341 | /* reserved (2 bits) */
4342 | add_reserved_field(extension_tree, hf_oran_reserved_2bits, tvb, offset, 1);
4343 | /* transmissionWindowSize (14 bits) */
4344 | proto_tree_add_item(extension_tree, hf_oran_transmissionWindowSize, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4345 | offset += 2;
4346 |
4347 | /* reserved (6 bits) */
4348 | add_reserved_field(extension_tree, hf_oran_reserved_6bits, tvb, offset, 1);
4349 | /* toT (2 bits) */
4350 | proto_tree_add_item(extension_tree, hf_oran_toT, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4351 | offset += 1;
4352 | break;
4353 |
4354 | case 19: /* SE 19: Compact beamforming information for multiple port */
4355 | {
4356 | /* beamId in section header should be ignored. Guard against appending multiple times.. */
4357 | if (section_beamId_ti && !section_beamId_ignored) {
4358 | proto_item_append_text(section_beamId_ti, " (ignored)");
4359 | section_beamId_ignored = true1;
4360 | }
4361 |
4362 | /* numSymbol not used in this case */
4363 | if (numsymbol_ti && !numsymbol_ignored) {
4364 | proto_item_append_text(numsymbol_ti, " (ignored)");
4365 | numsymbol_ignored = true1;
4366 | }
4367 |
4368 | /* disableBFWs */
4369 | bool_Bool disableBFWs;
4370 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_disable_bfws,
4371 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disableBFWs);
4372 | if (disableBFWs) {
4373 | proto_item_append_text(extension_ti, " (disableBFWs)");
4374 | }
4375 | /* repetition (1 bit) */
4376 | uint64_t repetition;
4377 | proto_tree_add_bits_ret_val(extension_tree, hf_oran_se19_repetition, tvb, (offset*8)+1, 1, &repetition, ENC_BIG_ENDIAN0x00000000);
4378 | /* numPortc (6 bits) */
4379 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_numPortc,
4380 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPortc);
4381 | offset++;
4382 |
4383 | /* priority (2 bits) */
4384 | proto_tree_add_item(extension_tree, hf_oran_noncontig_priority, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4385 | /* symbolMask (14 bits) */
4386 | offset = dissect_symbolmask(tvb, extension_tree, offset, NULL((void*)0), NULL((void*)0));
4387 |
4388 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
4389 | proto_item *comp_meth_ti = NULL((void*)0);
4390 |
4391 | if (!repetition) {
4392 |
4393 | if (!disableBFWs) {
4394 | /* bfwCompHdr */
4395 | offset = dissect_bfwCompHdr(tvb, extension_tree, offset,
4396 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
4397 | }
4398 |
4399 | /* Add entries for each port */
4400 | for (unsigned port=0; port < numPortc; port++) {
4401 |
4402 | /* Create subtree for port entry*/
4403 | int port_start_offset = offset;
4404 | proto_item *port_ti = proto_tree_add_string_format(extension_tree, hf_oran_ext19_port,
4405 | tvb, offset, 0,
4406 | "", "Port %u: ", port);
4407 | proto_tree *port_tree = proto_item_add_subtree(port_ti, ett_oran_ext19_port);
4408 |
4409 | /* Reserved (4 bits) */
4410 | add_reserved_field(port_tree, hf_oran_reserved_4bits, tvb, offset, 1);
4411 | /* portReMask (12 bits) */
4412 | proto_tree_add_item(port_tree, hf_oran_portReMask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4413 | offset += 2;
4414 |
4415 | /* Reserved (2 bits) */
4416 | add_reserved_field(port_tree, hf_oran_reserved_2bits, tvb, offset, 1);
4417 | /* portSymbolMask (14 bits) */
4418 | proto_tree_add_item(port_tree, hf_oran_portSymbolMask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4419 | offset += 2;
4420 |
4421 | /* Reserved (1 bit) */
4422 | add_reserved_field(port_tree, hf_oran_reserved_1bit, tvb, offset, 1);
4423 | /* beamID (15 bits) */
4424 | uint16_t beamId;
4425 | proto_tree_add_item_ret_uint16(port_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &beamId);
4426 | proto_item_append_text(port_ti, " (beamId=%u)", beamId);
4427 | offset += 2;
4428 |
4429 | /* No weights present */
4430 | if (!disableBFWs) {
4431 | /*******************************************************************/
4432 | /* Table 7.7.19.1-1 (there is no part -2 for disableBFWs case...), */
4433 | /* but for SE 11, bfwCompParam was only present for !disableBFWs */
4434 | /*******************************************************************/
4435 |
4436 | /* bfwCompParam */
4437 | bool_Bool compression_method_supported = false0;
4438 | uint32_t exponent = 0;
4439 | unsigned num_trx_entries = 0;
4440 | uint16_t *trx;
4441 | offset = dissect_bfwCompParam(tvb, port_tree, pinfo, offset, comp_meth_ti,
4442 | &bfwcomphdr_comp_meth, &exponent, &compression_method_supported,
4443 | &num_trx_entries, &trx);
4444 |
4445 | int bit_offset = offset*8;
4446 | int bfw_offset;
4447 |
4448 | /* Add weights for each TRX */
4449 | unsigned trx_to_add = (num_trx_entries==0) ? pref_num_bf_antennas : num_trx_entries;
4450 | for (unsigned b=0; b < trx_to_add; b++) {
4451 |
4452 | uint16_t trx_index = (num_trx_entries) ? trx[b] : b+1;
4453 |
4454 | /* Create BFW subtree */
4455 | bfw_offset = bit_offset / 8;
4456 | uint8_t bfw_extent = ((bit_offset + (bfwcomphdr_iq_width*2)) / 8) - bfw_offset;
4457 | proto_item *bfw_ti = proto_tree_add_string_format(port_tree, hf_oran_bfw,
4458 | tvb, bfw_offset, bfw_extent,
4459 | "", "TRX %u: (", trx_index);
4460 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
4461 |
4462 | /* I */
4463 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
4464 | float value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent, NULL((void*)0) /* no ModCompr */, 0 /* RE */);
4465 | /* Add to tree. */
4466 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8,
4467 | (bfwcomphdr_iq_width+7)/8, value, "#%u=%f", b, value);
4468 | bit_offset += bfwcomphdr_iq_width;
4469 | proto_item_append_text(bfw_ti, "I%u=%f ", b, value);
4470 |
4471 | /* Q */
4472 | bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
4473 | value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent, NULL((void*)0) /* no ModCompr */, 0 /* RE */);
4474 | /* Add to tree. */
4475 | proto_tree_add_float_format_value(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8,
4476 | (bfwcomphdr_iq_width+7)/8, value, "#%u=%f", b, value);
4477 | bit_offset += bfwcomphdr_iq_width;
4478 | proto_item_append_text(bfw_ti, "Q%u=%f)", b, value);
4479 | }
4480 |
4481 | offset = (bit_offset+7)/8;
4482 | }
4483 | else {
4484 | /* No weights... */
4485 | }
4486 |
4487 | /* Set length of this port entry */
4488 | proto_item_set_len(port_ti, offset-port_start_offset);
4489 | }
4490 | }
4491 | break;
4492 | }
4493 |
4494 | case 20: /* SE 20: Puncturing extension */
4495 | {
4496 | /* numPuncPatterns */
4497 | uint32_t numPuncPatterns;
4498 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_numPuncPatterns, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPuncPatterns);
4499 | offset += 1;
4500 |
4501 | /* Add each puncturing pattern */
4502 | for (uint32_t n=0; n < numPuncPatterns; n++) {
4503 | unsigned pattern_start_offset = offset;
4504 |
4505 | /* Subtree for this puncturing pattern */
4506 | proto_item *pattern_ti = proto_tree_add_string_format(extension_tree, hf_oran_puncPattern,
4507 | tvb, offset, 0,
4508 | "", "Puncturing Pattern: %u/%u", n+1, numPuncPatterns);
4509 | proto_tree *pattern_tree = proto_item_add_subtree(pattern_ti, ett_oran_punc_pattern);
4510 |
4511 | /* SymbolMask (14 bits) */
4512 | proto_tree_add_item(pattern_tree, hf_oran_symbolMask_ext20, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4513 | offset += 1;
4514 |
4515 | uint32_t startPuncPrb, numPuncPrb;
4516 |
4517 | /* startPuncPrb (10 bits) */
4518 | proto_tree_add_item_ret_uint(pattern_tree, hf_oran_startPuncPrb, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPuncPrb);
4519 | offset += 2;
4520 | /* numPuncPrb (8 bits) */
4521 | proto_tree_add_item_ret_uint(pattern_tree, hf_oran_numPuncPrb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numPuncPrb);
4522 | offset += 1;
4523 |
4524 | proto_item_append_text(pattern_ti, " [%u->%u]", startPuncPrb, startPuncPrb+numPuncPrb-1);
4525 |
4526 | /* Make a hole in range of PRBs to report */
4527 | for (unsigned p=startPuncPrb; p < startPuncPrb+numPuncPrb; p++) {
4528 | if (p < MAX_PRBS273) {
4529 | prbs_for_st10_type5[p] = false0;
4530 | }
4531 | }
4532 |
4533 | /* puncReMask (12 bits) */
4534 | proto_tree_add_item(pattern_tree, hf_oran_puncReMask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4535 | offset += 1;
4536 | /* rb (1 bit) */
4537 | proto_item *rb_ti = proto_tree_add_item(pattern_tree, hf_oran_rb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4538 | /* reserved (1 bit) */
4539 | add_reserved_field(pattern_tree, hf_oran_reserved_bit5, tvb, offset, 1);
4540 | /* multiSDScope (1 bit) */
4541 | proto_tree_add_item(pattern_tree, hf_oran_multiSDScope, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4542 | /* rbgIncl (1 bit) */
4543 | bool_Bool rbgIncl;
4544 | proto_tree_add_item_ret_boolean(pattern_tree, hf_oran_RbgIncl, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &rbgIncl);
4545 | offset += 1;
4546 |
4547 | if (rbgIncl) {
4548 | /* reserved (1 bit) */
4549 | add_reserved_field(pattern_tree, hf_oran_reserved_1bit, tvb, offset, 1);
4550 | /* rbgSize(3 bits) */
4551 | proto_tree_add_item(pattern_tree, hf_oran_rbgSize, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4552 | /* rbgMask (28 bits) */
4553 | proto_tree_add_item(pattern_tree, hf_oran_rbgMask, tvb, offset, 4, ENC_BIG_ENDIAN0x00000000);
4554 | offset += 4;
4555 |
4556 | proto_item_append_text(rb_ti, " (ignored)");
4557 | }
4558 |
4559 | proto_item_set_len(pattern_ti, offset-pattern_start_offset);
4560 | }
4561 |
4562 | break;
4563 | }
4564 | case 21: /* SE 21: Variable PRB group size for channel information */
4565 | {
4566 | /* ciPrbGroupSize */
4567 | uint32_t ci_prb_group_size;
4568 | proto_item *prb_group_size_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_ci_prb_group_size, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &ci_prb_group_size);
4569 | offset += 1;
4570 |
4571 | switch (ci_prb_group_size) {
4572 | case 0:
4573 | case 1:
4574 | case 255:
4575 | /* Reserved value */
4576 | expert_add_info_format(pinfo, prb_group_size_ti, &ei_oran_ci_prb_group_size_reserved,
4577 | "SE 11 ciPrbGroupSize is reserved value %u - must be 2-254",
4578 | ci_prb_group_size);
4579 | break;
4580 | default:
4581 | /* This value affects how SE 11 is interpreted */
4582 | ext11_settings.ext21_set = true1;
4583 | ext11_settings.ext21_ci_prb_group_size = ci_prb_group_size;
4584 |
4585 | if (numPrbc == 0) {
4586 | expert_add_info(pinfo, numprbc_ti, &ei_oran_numprbc_ext21_zero);
4587 | }
4588 | break;
4589 | }
4590 |
4591 | /* reserved (6 bits) */
4592 | add_reserved_field(extension_tree, hf_oran_reserved_6bits, tvb, offset, 1);
4593 |
4594 | /* prgSize (2 bits). Interpretation depends upon section type (5 or 6), but also mplane parameters? */
4595 | if (sectionType == SEC_C_UE_SCHED) { /* Section Type 5 */
4596 | proto_tree_add_item(extension_tree, hf_oran_prg_size_st5, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4597 | }
4598 | else if (sectionType == SEC_C_CH_INFO) { /* Section Type 6 */
4599 | proto_tree_add_item(extension_tree, hf_oran_prg_size_st6, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4600 | }
4601 | offset += 1;
4602 | break;
4603 | }
4604 |
4605 | case 22: /* SE 22: ACK/NACK request */
4606 | {
4607 | uint32_t ack_nack_req_id;
4608 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_ack_nack_req_id, tvb, offset, 2,
4609 | ENC_BIG_ENDIAN0x00000000, &ack_nack_req_id);
4610 | offset += 2;
4611 |
4612 | if (state) {
4613 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
4614 | /* Add this request into conversation state on first pass */
4615 | ack_nack_request_t *request_details = wmem_new0(wmem_file_scope(), ack_nack_request_t)((ack_nack_request_t*)wmem_alloc0((wmem_file_scope()), sizeof (ack_nack_request_t)));
4616 | request_details->request_frame_number = pinfo->num;
4617 | request_details->request_frame_time = pinfo->abs_ts;
4618 | request_details->requestType = SE22;
4619 | /* Insert into flow's tree */
4620 | wmem_tree_insert32(state->ack_nack_requests, ack_nack_req_id, request_details);
4621 | }
4622 | else {
4623 | /* Try to link forward to ST8 response */
4624 | ack_nack_request_t *response = wmem_tree_lookup32(state->ack_nack_requests,
4625 | ack_nack_req_id);
4626 | if (response) {
4627 | show_link_to_acknack_response(extension_tree, tvb, pinfo, response);
4628 | }
4629 | }
4630 | }
4631 | break;
4632 | }
4633 |
4634 | case 23: /* SE 23: Arbitrary symbol pattern modulation compression parameters */
4635 | {
4636 | /* Green common header */
4637 |
4638 | /* numSymPrbPattern (4 bits) */
4639 | uint32_t num_sym_prb_pattern;
4640 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_sym_prb_pattern, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_sym_prb_pattern);
4641 | /* reserved (3 bits) */
4642 | add_reserved_field(extension_tree, hf_oran_reserved_bits456, tvb, offset, 1);
4643 | /* prbMode (1 bit) */
4644 | bool_Bool prb_mode;
4645 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_prb_mode, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &prb_mode);
4646 | offset += 1;
4647 |
4648 | /* reserved (8 bits) */
4649 | add_reserved_field(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1);
4650 | offset += 1;
4651 |
4652 | /* Dissect each SymPrbPattern */
4653 | for (uint32_t n=0; n < num_sym_prb_pattern; n++) {
4654 |
4655 | /* Subtree */
4656 | proto_item *pattern_ti = proto_tree_add_string_format(extension_tree, hf_oran_sym_prb_pattern,
4657 | tvb, offset, 1, "",
4658 | prb_mode ? "PRB-BLOCK" : "PRB-MASK");
4659 | proto_tree *pattern_tree = proto_item_add_subtree(pattern_ti, ett_oran_sym_prb_pattern);
4660 |
4661 |
4662 | /* Orange part */
4663 |
4664 | /* Reserved (2 bits) */
4665 | add_reserved_field(pattern_tree, hf_oran_reserved_2bits, tvb, offset, 1);
4666 | /* symMask (14 bits) */
4667 | proto_tree_add_item(pattern_tree, hf_oran_sym_mask, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4668 | offset += 2;
4669 | /* numMcScaleOffset (4 bits) */
4670 | uint32_t numMcScaleOffset;
4671 | proto_tree_add_item_ret_uint(pattern_tree, hf_oran_num_mc_scale_offset, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &numMcScaleOffset);
4672 |
4673 | if (!prb_mode) { /* PRB-MASK */
4674 | /* prbPattern (4 bits) */
4675 | proto_tree_add_item(pattern_tree, hf_oran_prb_pattern, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4676 | offset += 1;
4677 | /* reserved (8 bits) */
4678 | add_reserved_field(pattern_tree, hf_oran_reserved_8bits, tvb, offset, 1);
4679 | offset += 1;
4680 | /* reserved (4 bits) */
4681 | add_reserved_field(pattern_tree, hf_oran_reserved_4bits, tvb, offset, 1);
4682 | }
4683 | else { /* PRB-BLOCK */
4684 | /* prbBlkOffset (8 bits) */
4685 | proto_tree_add_item(pattern_tree, hf_oran_prb_blk_offset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4686 | offset += 1;
4687 | /* prbBlkSize (8 bits) */
4688 | proto_tree_add_item(pattern_tree, hf_oran_prb_blk_size, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4689 | offset += 1;
4690 | }
4691 |
4692 | for (unsigned c=0; c < numMcScaleOffset; c++) {
4693 | if (c > 0) {
4694 | /* reserved (4 bits) */
4695 | add_reserved_field(pattern_tree, hf_oran_reserved_4bits, tvb, offset, 1);
4696 | }
4697 |
4698 | static int * const remask_flags_even[] = {
4699 | &hf_oran_mc_scale_re_mask_re1_even,
4700 | &hf_oran_mc_scale_re_mask_re2_even,
4701 | &hf_oran_mc_scale_re_mask_re3_even,
4702 | &hf_oran_mc_scale_re_mask_re4_even,
4703 | &hf_oran_mc_scale_re_mask_re5_even,
4704 | &hf_oran_mc_scale_re_mask_re6_even,
4705 | &hf_oran_mc_scale_re_mask_re7_even,
4706 | &hf_oran_mc_scale_re_mask_re8_even,
4707 | &hf_oran_mc_scale_re_mask_re9_even,
4708 | &hf_oran_mc_scale_re_mask_re10_even,
4709 | &hf_oran_mc_scale_re_mask_re11_even,
4710 | &hf_oran_mc_scale_re_mask_re12_even,
4711 | NULL((void*)0)
4712 | };
4713 |
4714 | /* mcScaleReMask (12 bits). Defines which REs the following csf and mcScaleOffset apply to */
4715 | uint64_t mcScaleReMask, mcScaleOffset;
4716 | proto_tree_add_bitmask_ret_uint64(pattern_tree, tvb, offset,
4717 | hf_oran_mc_scale_re_mask_even,
4718 | ett_oran_mc_scale_remask,
4719 | remask_flags_even, ENC_BIG_ENDIAN0x00000000, &mcScaleReMask);
4720 | offset += 2;
4721 |
4722 | /* csf (1 bit) */
4723 | bool_Bool csf;
4724 | dissect_csf(pattern_tree, tvb, offset*8, ci_iq_width, &csf);
4725 | /* mcScaleOffset (15 bits) */
4726 | proto_item *ti = proto_tree_add_bits_ret_val(pattern_tree, hf_oran_mc_scale_offset, tvb, offset*8 + 1, 15, &mcScaleOffset, ENC_BIG_ENDIAN0x00000000);
4727 | uint16_t exponent = (mcScaleOffset >> 11) & 0x000f; /* m.s. 4 bits */
4728 | uint16_t mantissa = mcScaleOffset & 0x07ff; /* l.s. 11 bits */
4729 | float mcScaleOffset_value = ((float)mantissa/(1<<11)) * ((float)1.0 / (1 << exponent));
4730 | proto_item_append_text(ti, " (%f)", mcScaleOffset_value);
4731 |
4732 | offset += 2;
4733 |
4734 | /* Record this config. */
4735 | /* TODO: at some point, will also want to store/use PRB + symbol filters */
4736 | section_mod_compr_config_t* sect_config = get_mod_compr_section_to_write(state, sectionId);
4737 |
4738 | if (sect_config && sect_config->num_configs < MAX_MOD_COMPR_CONFIGS12) {
4739 | unsigned i = sect_config->num_configs;
4740 | sect_config->configs[i].mod_compr_re_mask = (uint16_t)mcScaleReMask;
4741 | sect_config->configs[i].mod_compr_csf = csf;
4742 | sect_config->configs[i].mod_compr_scaler = mcScaleOffset_value;
4743 | sect_config->num_configs++;
4744 | }
4745 | }
4746 |
4747 | proto_item_set_end(pattern_ti, tvb, offset);
4748 | }
4749 | break;
4750 | }
4751 |
4752 | case 24: /* SE 24: PUSCH DMRS configuration */
4753 | {
4754 | /* Hidden filter for bf (DMRS BF) */
4755 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
4756 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
4757 |
4758 | /* alpnPerSym (1 bit) */
4759 | proto_tree_add_item(extension_tree, hf_oran_alpn_per_sym, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4760 | /* antDmrsSnr (1 bit) */
4761 | proto_tree_add_item(extension_tree, hf_oran_ant_dmrs_snr, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4762 | /* reserved (1 bit) */
4763 | add_reserved_field(extension_tree, hf_oran_reserved_bit2, tvb, offset, 1);
4764 | /* userGroupSize (5 bits) */
4765 | uint32_t user_group_size;
4766 | proto_item *ugs_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_user_group_size, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &user_group_size);
4767 | if (user_group_size == 0) {
4768 | proto_item_append_text(ugs_ti, " (not used)");
4769 | }
4770 | else if (user_group_size > 12) {
4771 | proto_item_append_text(ugs_ti, " (reserved)");
4772 | }
4773 | offset += 1;
4774 | /* userGroupId (8 bits)*/
4775 | uint32_t user_group_id;
4776 | proto_item *ugi_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_user_group_id, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &user_group_id);
4777 | if (user_group_id == 0) {
4778 | /* TODO: Value 0 can happen in several cases, described in 7.7.24.7.. */
4779 | }
4780 | if (user_group_id == 255) {
4781 | /* Value 255 is reserved */
4782 | expert_add_info(pinfo, ugi_ti, &ei_oran_user_group_id_reserved_value);
4783 | }
4784 | offset += 1;
4785 |
4786 | bool_Bool seen_value_to_inherit = false0;
4787 | bool_Bool inherited_config_has_transform_precoding = false0;
4788 | int dmrs_configs_seen = 0;
4789 |
4790 | /* Dissect each entry until reach number of configured ueIds (or run out of extlen bytes..) */
4791 | uint32_t ueid_index = 0;
4792 | while ((offset < (extension_start_offset + extlen*4)) && (ueid_index < number_of_ueids)) {
4793 | dmrs_configs_seen++;
4794 |
4795 | /* Subtree */
4796 | proto_item *entry_ti = proto_tree_add_string_format(extension_tree, hf_oran_dmrs_entry,
4797 | tvb, offset, 0, "",
4798 | "Entry");
4799 | proto_tree *entry_tree = proto_item_add_subtree(entry_ti, ett_oran_dmrs_entry);
4800 |
4801 | /* entryType (3 bits) */
4802 | uint32_t entry_type;
4803 | proto_item *entry_type_ti;
4804 | entry_type_ti = proto_tree_add_item_ret_uint(entry_tree, hf_oran_entry_type, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &entry_type);
4805 | if (entry_type > 3) {
4806 | proto_item_append_text(entry_type_ti, " (reserved)");
4807 | }
4808 |
4809 | /* dmrsPortNumber (5 bits). Values 0-11 allowed */
4810 | unsigned int dmrs_port_number;
4811 | proto_item *dpn_ti = proto_tree_add_item_ret_uint(entry_tree, hf_oran_dmrs_port_number, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &dmrs_port_number);
4812 | if (dmrs_port_number > 11) {
4813 | proto_item_append_text(dpn_ti, " (12-31 are reserved)");
4814 | }
4815 | offset += 1;
4816 |
4817 | /* What follows depends upon entryType */
4818 | switch (entry_type) {
4819 | case 0: /* dmrsPortNumber config same as previous, ueId ueIdReset=0 */
4820 | case 1: /* dmrsPortNumber config same as previous, ueId ueIdReset=1 */
4821 | /* No further fields for these */
4822 | /* Error here if no previous values to inherit!! */
4823 | if (!seen_value_to_inherit) {
4824 | expert_add_info_format(pinfo, entry_type_ti, &ei_oran_se24_nothing_to_inherit,
4825 | "SE24: have seen entry type %u, but no previous config (type 2 or 3) to inherit config from", entry_type);
4826 |
4827 | }
4828 | /* TODO: would be useful to repeat whole inherited config here? */
4829 | break;
4830 |
4831 | case 2: /* transform precoding disabled */
4832 | case 3: /* transform precoding enabled */
4833 | {
4834 | /* Type 2/3 are very similar.. */
4835 |
4836 | /* ueIdReset (1 bit) */
4837 | proto_tree_add_item(entry_tree, hf_oran_ueid_reset, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4838 | /* posMeas (1 bit) */
4839 | proto_tree_add_item(entry_tree, hf_oran_pos_meas, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4840 |
4841 | /* dmrsSymbolMask (14 bits) */
4842 | static int * const dmrs_symbol_mask_flags[] = {
4843 | &hf_oran_dmrs_symbol_mask_s13,
4844 | &hf_oran_dmrs_symbol_mask_s12,
4845 | &hf_oran_dmrs_symbol_mask_s11,
4846 | &hf_oran_dmrs_symbol_mask_s10,
4847 | &hf_oran_dmrs_symbol_mask_s9,
4848 | &hf_oran_dmrs_symbol_mask_s8,
4849 | &hf_oran_dmrs_symbol_mask_s7,
4850 | &hf_oran_dmrs_symbol_mask_s6,
4851 | &hf_oran_dmrs_symbol_mask_s5,
4852 | &hf_oran_dmrs_symbol_mask_s4,
4853 | &hf_oran_dmrs_symbol_mask_s3,
4854 | &hf_oran_dmrs_symbol_mask_s2,
4855 | &hf_oran_dmrs_symbol_mask_s1,
4856 | &hf_oran_dmrs_symbol_mask_s0,
4857 | NULL((void*)0)
4858 | };
4859 | proto_tree_add_bitmask(entry_tree, tvb, offset,
4860 | hf_oran_dmrs_symbol_mask, ett_oran_dmrs_symbol_mask, dmrs_symbol_mask_flags, ENC_BIG_ENDIAN0x00000000);
4861 | offset += 2;
4862 |
4863 | /* scrambling */
4864 | proto_tree_add_item(entry_tree, hf_oran_scrambling, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4865 | offset += 2;
4866 |
4867 | /* nscid (1 bit) */
4868 | proto_tree_add_item(entry_tree, hf_oran_nscid, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4869 |
4870 | /* These 5 bits differ depending upon entry type */
4871 | if (entry_type == 2) { /* type 2 */
4872 | /* dType (1 bit) */
4873 | proto_tree_add_item(entry_tree, hf_oran_dtype, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4874 | /* cdmWithoutData (2 bits) */
4875 | proto_tree_add_item(entry_tree, hf_oran_cmd_without_data, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4876 | /* lambda (2 bits) */
4877 | proto_tree_add_item(entry_tree, hf_oran_lambda, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4878 | }
4879 | else { /* type 3 */
4880 | /* reserved (1 bit) */
4881 | add_reserved_field(entry_tree, hf_oran_reserved_bit1, tvb, offset, 1);
4882 | /* lowPaprType (2 bits) */
4883 | proto_tree_add_item(entry_tree, hf_oran_low_papr_type, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4884 | /* hoppingMode (2 bits) */
4885 | proto_tree_add_item(entry_tree, hf_oran_hopping_mode, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
4886 | }
4887 |
4888 | /* firstPrb (9 bits) */
4889 | proto_tree_add_item(entry_tree, hf_oran_first_prb, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4890 | offset += 1;
4891 | /* lastPrb (9 bits) */
4892 | proto_tree_add_item(entry_tree, hf_oran_last_prb, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
4893 | offset += 2;
4894 | /* Reserved (16 bits) */
4895 | add_reserved_field(entry_tree, hf_oran_reserved_16bits, tvb, offset, 2);
4896 | offset += 2;
4897 |
4898 | /* Could now see entry types 0 or 1 - they have these values to inherit */
4899 | seen_value_to_inherit = true1;
4900 | inherited_config_has_transform_precoding = (entry_type == 3);
4901 | break;
4902 | }
4903 |
4904 | default:
4905 | /* reserved - expert info */
4906 | break;
4907 | }
4908 |
4909 | proto_item_append_text(entry_ti, " [UEId=%u] (dmrsPortNumber=%2u) (type %u - %s) ",
4910 | ueids[ueid_index++], dmrs_port_number, entry_type, val_to_str_const(entry_type, entry_type_vals, "Unknown"));
4911 | proto_item_set_end(entry_ti, tvb, offset);
4912 |
4913 | if (entry_type <= 1) {
4914 | proto_item_append_text(entry_ti, " [transform-precoding %s]",
4915 | inherited_config_has_transform_precoding ? "enabled" : "disabled");
4916 | }
4917 | }
4918 |
4919 | proto_item_append_text(extension_ti, " (%d DMRS configs seen)", dmrs_configs_seen);
4920 | break;
4921 | }
4922 |
4923 | case 25: /* SE 25: Symbol reordering for DMRS-BF */
4924 | /* Just dissect each available block of 7 bytes as the 14 symbols for a layer,
4925 | where each layer could be one or apply to all layers. */
4926 | {
4927 | /* TODO: should only appear in one section of a message - check? */
4928 | unsigned layer = 0;
4929 | proto_item *layer_ti;
4930 | while (offset+7 <= (extension_start_offset + extlen*4)) {
4931 | /* Layer subtree */
4932 | layer_ti = proto_tree_add_string_format(extension_tree, hf_oran_symbol_reordering_layer,
4933 | tvb, offset, 7, "",
4934 | "Layer");
4935 | proto_tree *layer_tree = proto_item_add_subtree(layer_ti, ett_oran_symbol_reordering_layer);
4936 |
4937 | /* All 14 symbols for a layer (or all layers) */
4938 | for (unsigned s=0; s < 14; s++) {
4939 | proto_item *sym_ti;
4940 | /* txWinForOnAirSymbol */
4941 | unsigned int tx_win_for_on_air_symbol;
4942 | sym_ti = proto_tree_add_item_ret_uint(layer_tree,
4943 | (s % 2) ? hf_oran_tx_win_for_on_air_symbol_r : hf_oran_tx_win_for_on_air_symbol_l,
4944 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &tx_win_for_on_air_symbol);
4945 | if (tx_win_for_on_air_symbol == 0x0F) {
4946 | /* Ordering not affected */
4947 | proto_item_append_text(sym_ti, " (sym %u - no info)", s);
4948 | }
4949 | else {
4950 | proto_item_append_text(sym_ti, " (sym %u)", s);
4951 | }
4952 | if (s % 2) {
4953 | offset += 1;
4954 | }
4955 | }
4956 |
4957 | proto_item_append_text(layer_ti, " (layer %u)", ++layer);
4958 | proto_item_append_text(extension_ti, " (layer %u)", layer);
4959 | }
4960 | /* Set layer subtree label */
4961 | if (layer == 1) {
4962 | proto_item_append_text(layer_ti, " (all)");
4963 | proto_item_append_text(extension_ti, " (all)");
4964 | }
4965 | if (layer == 0) {
4966 | /* TODO: are no layers valid? What does it mean? */
4967 | proto_item_append_text(extension_ti, " (none)");
4968 | }
4969 | break;
4970 | }
4971 |
4972 | case 26: /* SE 26: Frequency offset feedback */
4973 | /* Reserved (8 bits) */
4974 | add_reserved_field(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1);
4975 | offset += 1;
4976 | /* Reserved (1 bit) */
4977 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
4978 | /* numFoFb (7 bits) */
4979 | unsigned num_fo_fb;
4980 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_fo_fb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_fo_fb);
4981 | offset += 1;
4982 |
4983 | /* Add each freqOffsetFb value */
4984 | for (unsigned n=0; n < num_fo_fb; n++) {
4985 | unsigned freq_offset_fb;
4986 | /* freqOffsetFb (16 bits) */
4987 | proto_item *offset_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_freq_offset_fb,
4988 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &freq_offset_fb);
4989 | /* Show if maps onto a -ve number */
4990 | if ((freq_offset_fb >= 0x8ad0) && (freq_offset_fb <= 0xffff)) {
4991 | proto_item_append_text(offset_ti, "(value %d)", -1 - (0xffff-freq_offset_fb));
4992 | }
4993 | proto_item_append_text(offset_ti, " [#%u]", n+1);
4994 | offset += 2;
4995 | }
4996 | break;
4997 |
4998 | case 27: /* SE 27: O-DU controlled dimensionality reduction */
4999 | {
5000 | /* Hidden filter for bf (DMRS BF) */
5001 | bf_ti = proto_tree_add_item(tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
5002 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
5003 |
5004 | /* beamType (2 bits) */
5005 | unsigned beam_type;
5006 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_beam_type, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &beam_type);
5007 | /* reserved (6 bits) */
5008 | add_reserved_field(extension_tree, hf_oran_reserved_last_6bits, tvb, offset, 1);
5009 | offset += 1;
5010 |
5011 | /* numElements */
5012 | unsigned num_elements;
5013 | proto_item *num_elements_ti = proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_elements, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_elements);
5014 | if (num_elements == 0) {
5015 | num_elements = 256;
5016 | proto_item_append_text(num_elements_ti, " (256");
5017 | }
5018 |
5019 | offset += 1;
5020 |
5021 | /* beamId value(s) */
5022 | switch (beam_type) {
5023 | case 0:
5024 | for (unsigned n=0; n < num_elements; n++) {
5025 | /* reserved (1 bit) + beamId */
5026 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
5027 | proto_tree_add_item(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5028 | offset += 2;
5029 | }
5030 | break;
5031 | case 1:
5032 | /* reserved (1 bit) + beamId */
5033 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
5034 | proto_tree_add_item(c_section_tree, hf_oran_beamId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5035 | offset += 2;
5036 | break;
5037 | default:
5038 | /* Unknown type... */
5039 | break;
5040 | }
5041 | break;
5042 | }
5043 |
5044 | case 28: /* SE 28: O-DU controlled frequency resolution for SINR reporting */
5045 | {
5046 | /* reserved (3 bits) */
5047 | add_reserved_field(extension_tree, hf_oran_reserved_3bits, tvb, offset, 1);
5048 | /* numUeSinrRpt (5 bits) */
5049 | uint32_t num_ue_sinr_rpt;
5050 | proto_tree_add_item_ret_uint(extension_tree, hf_oran_num_ue_sinr_rpt, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_ue_sinr_rpt);
5051 | offset += 1;
5052 |
5053 | for (uint32_t n=0; n < num_ue_sinr_rpt; n++) {
5054 | /* reserved (1 bit) */
5055 | add_reserved_field(extension_tree, (n % 2) ? hf_oran_reserved_bit4 : hf_oran_reserved_1bit,
5056 | tvb, offset, 1);
5057 |
5058 | /* numSinrPerPrb (3 bits). Taken from alternate nibbles within byte. */
5059 | proto_tree_add_item(extension_tree, (n % 2) ? hf_oran_num_sinr_per_prb_right : hf_oran_num_sinr_per_prb,
5060 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5061 | if (n % 2) {
5062 | offset += 1;
5063 | }
5064 | }
5065 |
5066 | /* May need to skip beyond half-used byte */
5067 | if (num_ue_sinr_rpt % 2) {
5068 | offset += 1;
5069 | }
5070 | break;
5071 | }
5072 |
5073 | case 29: /* SE 29: Cyclic delay adjustment */
5074 | /* reserved (4 bits) */
5075 | add_reserved_field(extension_tree, hf_oran_reserved_4bits, tvb, offset, 1);
5076 | /* cdScgSize (4 bits) */
5077 | proto_tree_add_item(extension_tree, hf_oran_cd_scg_size, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5078 | offset += 1;
5079 |
5080 | /* cdScgPhaseStep */
5081 | proto_tree_add_item(extension_tree, hf_oran_cd_scg_phase_step, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5082 | offset += 1;
5083 | break;
5084 |
5085 | case 30: /* SE 30: PUSCH repetition indication */
5086 | {
5087 | /* Only valid for UL */
5088 | if (!tap_info->uplink) {
5089 | expert_add_info(pinfo, extension_ti, &ei_oran_se30_not_ul);
5090 | }
5091 |
5092 | /* ueids[], number_of_ueids may have been rewritten by SE10 */
5093 |
5094 | /* reserved (4 bits) */
5095 | add_reserved_field(extension_tree, hf_oran_reserved_4bits, tvb, offset, 1);
5096 | /* numRepUe (4 bits) */
5097 | uint8_t num_rep_ue;
5098 | proto_tree_add_item_ret_uint8(extension_tree, hf_oran_num_rep_ue, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_rep_ue);
5099 | offset ++;
5100 | /* reserved (8 bits) */
5101 | add_reserved_field(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1);
5102 | offset += 1;
5103 |
5104 | if (num_rep_ue == 1) {
5105 | /* SE10 *not* present. N.B. this should tally with number_of_ueids being set to only 1? */
5106 | /* reserved (1 bit) */
5107 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
5108 | /* isLastRep (1 bit). Value meaningless here? */
5109 | proto_tree_add_item(extension_tree, hf_oran_is_last_rep, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5110 | /* repIndex (6 bits) */
5111 | proto_tree_add_item(extension_tree, hf_oran_rep_index, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5112 | offset += 1;
5113 |
5114 | /* reserved (2 bits) */
5115 | add_reserved_field(extension_tree, hf_oran_reserved_2bits, tvb, offset, 1);
5116 | /* numReps (6 bits) */
5117 | uint8_t num_reps;
5118 | proto_tree_add_item_ret_uint8(extension_tree, hf_oran_num_reps, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_reps);
5119 | /* TODO: should numReps be 0 here? */
5120 | offset += 1;
5121 |
5122 | /* reserved (2 bits) */
5123 | add_reserved_field(extension_tree, hf_oran_reserved_16bits, tvb, offset, 2);
5124 | offset += 2;
5125 |
5126 | }
5127 | else {
5128 | /* SE10 present */
5129 | bool_Bool is_last_rep = false0;
5130 | /* TODO: should is_last_rep (also) cause loop exit? */
5131 | for (uint8_t ue_idx=0; (ue_idx < num_rep_ue) && !is_last_rep; ue_idx++) {
5132 | /* reserved (1 bit) */
5133 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
5134 | /* isLastRep (1 bit) */
5135 | proto_tree_add_item_ret_boolean(extension_tree, hf_oran_is_last_rep, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &is_last_rep);
5136 | /* repIndex (6 bits) */
5137 | proto_tree_add_item(extension_tree, hf_oran_rep_index, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5138 | offset += 1;
5139 |
5140 | /* reserved (2 bits) */
5141 | add_reserved_field(extension_tree, hf_oran_reserved_2bits, tvb, offset, 1);
5142 | /* numReps (6 bits) */
5143 | uint8_t num_reps;
5144 | proto_item *num_reps_ti = proto_tree_add_item_ret_uint8(extension_tree, hf_oran_num_reps, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_reps);
5145 | /* TODO: values 33-63 are reserved */
5146 | if (num_reps > 32) {
5147 | proto_item_append_text(num_reps_ti, " (reserved)");
5148 | }
5149 | offset += 1;
5150 |
5151 | for (uint8_t rep=0; rep < num_reps; rep++) {
5152 | /* reserved (1 bit) */
5153 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
5154 | /* repUeId (15 bits) */
5155 | /* TODO: should be fetching and comparing with ueids[] from SE10? */
5156 | uint16_t ueid;
5157 | proto_item *ueid_ti = proto_tree_add_item_ret_uint16(extension_tree, hf_oran_rep_ueid, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ueid);
5158 |
5159 | /* Check that this ueid is recognised (among ueids[], number_of_ueids) */
5160 | bool_Bool matched = false0;
5161 | for (unsigned u=0; u < number_of_ueids; u++) {
5162 | if (ueid == ueids[u])
5163 | matched = true1;
5164 | }
5165 | if (!matched) {
5166 | expert_add_info_format(pinfo, ueid_ti, &ei_oran_se30_unknown_ueid,
5167 | "SE 30 mentions UEId %u - not seen in SE10", ueid);
5168 | }
5169 | offset += 2;
5170 | }
5171 | }
5172 | }
5173 | break;
5174 | }
5175 | case 31: /* SE 31: MCS Information */
5176 | {
5177 | /* TODO: show ueid (from ST5 or SE10) as generated field? Maybe add a subtree for each entry? */
5178 | for (uint32_t u=0; u < number_of_ueids; u++) {
5179 | /* reserved (4 bits) */
5180 | add_reserved_field(extension_tree, hf_oran_reserved_4bits, tvb, offset, 1);
5181 | /* mcsTable (4 bits) */
5182 | proto_tree_add_item(extension_tree, hf_oran_mcs_table, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5183 | offset += 1;
5184 |
5185 | /* reserved (2 bits) */
5186 | add_reserved_field(extension_tree, hf_oran_reserved_4bits, tvb, offset, 1);
5187 | /* mcsIndex (6 bits) */
5188 | proto_tree_add_item(extension_tree, hf_oran_mcs_index, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5189 | }
5190 | break;
5191 | }
5192 |
5193 | case 32: /* SE 32: Rank and TPMI measurement request */
5194 | {
5195 | /* reserved (3 bits) */
5196 | add_reserved_field(extension_tree, hf_oran_reserved_3bits, tvb, offset, 1);
5197 | /* numMeasReq (5 bits) */
5198 | uint8_t num_meas_req;
5199 | proto_tree_add_item_ret_uint8(extension_tree, hf_oran_num_meas_req, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_meas_req);
5200 | offset += 1;
5201 |
5202 | /* reserved (8 bits) */
5203 | add_reserved_field(extension_tree, hf_oran_reserved_8bits, tvb, offset, 1);
5204 | offset += 1;
5205 |
5206 | /* Show each measurement request */
5207 | for (unsigned r=0; r < num_meas_req; r++) {
5208 | /* Reserved (1 bit) */
5209 | add_reserved_field(extension_tree, hf_oran_reserved_1bit, tvb, offset, 1);
5210 | /* ueId (14 bits) */
5211 | proto_tree_add_item(extension_tree, hf_oran_ueId, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5212 | offset += 2;
5213 |
5214 | /* numOfUeAntPorts (4 bits) */
5215 | proto_tree_add_item(extension_tree, hf_oran_num_of_ue_ant_ports, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5216 | /* ueRank (4 bits) */
5217 | proto_tree_add_item(extension_tree, hf_oran_ue_rank, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5218 | offset += 1;
5219 |
5220 | /* codebookSubset (2 bits) */
5221 | proto_tree_add_item(extension_tree, hf_oran_codebook_subset, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5222 | /* TODO: tpmiIndex (6 bits) */
5223 | offset += 1;
5224 |
5225 | /* fullPwrMode (2 bits) */
5226 | proto_tree_add_item(extension_tree, hf_oran_full_pwr_mode, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5227 | /* fullPwrMode2TmpiGroup (14 bits) */
5228 | /* TODO: add as a bitset */
5229 | proto_tree_add_item(extension_tree, hf_oran_full_pwr_mode_2_tpmi_group, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5230 | offset += 2;
5231 |
5232 | /* reserved (2 bytes) */
5233 | add_reserved_field(extension_tree, hf_oran_reserved_16bits, tvb, offset, 2);
5234 | offset += 2;
5235 | }
5236 | break;
5237 | }
5238 |
5239 | default:
5240 | /* Other/unexpected extension types */
5241 | expert_add_info_format(pinfo, exttype_ti, &ei_oran_unhandled_se,
5242 | "SE %u (%s) not supported by dissector",
5243 | exttype, val_to_str_ext_const(exttype, &exttype_vals_ext, "Reserved"));
5244 | ext_unhandled = true1;
5245 | break;
5246 | }
5247 |
5248 | /* Check offset compared with extlen. There should be 0-3 bytes of padding */
5249 | int num_padding_bytes = (extension_start_offset + (extlen*4) - offset);
5250 | if (!ext_unhandled && ((num_padding_bytes<0) || (num_padding_bytes>3))) {
5251 | expert_add_info_format(pinfo, extlen_ti, &ei_oran_extlen_wrong,
5252 | "extlen signalled %u bytes (+ 0-3 bytes padding), but %u were dissected",
5253 | extlen*4, offset-extension_start_offset);
5254 | }
5255 |
5256 | /* Move offset to beyond signalled length of extension */
5257 | offset = extension_start_offset + (extlen*4);
5258 |
5259 | /* Set length of extension header. */
5260 | proto_item_set_len(extension_ti, extlen*4);
5261 | }
5262 | /* End of section extension handling */
5263 |
5264 | /* Tap section beamId if not overwritten by SEs */
5265 | if (!section_beamId_ignored && section_beamId != 0) {
5266 | add_beam_id_to_tap(tap_info, section_beamId);
5267 | }
5268 |
5269 |
5270 | /* RRM measurement reports have measurement reports *after* extensions */
5271 | if (sectionType == SEC_C_RRM_MEAS_REPORTS) /* Section Type 10 */
5272 | {
5273 | /* Hidden filter for bf (DMFS-BF). No BF weights though.. */
5274 | bf_ti = proto_tree_add_item(c_section_tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
5275 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
5276 |
5277 | bool_Bool mf;
5278 | do {
5279 | /* Measurement report subtree */
5280 | proto_item *mr_ti = proto_tree_add_string_format(c_section_tree, hf_oran_measurement_report,
5281 | tvb, offset, 1, "", "Measurement Report");
5282 | proto_tree *mr_tree = proto_item_add_subtree(mr_ti, ett_oran_measurement_report);
5283 | unsigned report_start_offset = offset;
5284 |
5285 | /* measurement flag (i.e., more reports after this one) (1 bit) */
5286 | proto_tree_add_item_ret_boolean(mr_tree, hf_oran_mf, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &mf);
5287 |
5288 | /* measTypeId (7 bits) */
5289 | uint32_t meas_type_id;
5290 | proto_item *meas_type_id_ti;
5291 | meas_type_id_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_meas_type_id, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &meas_type_id);
5292 | offset += 1;
5293 |
5294 | /* Common to all measurement types */
5295 | unsigned num_elements = 0;
5296 | if (meas_type_id == 6) {
5297 | /* numElements */
5298 | proto_tree_add_item_ret_uint(mr_tree, hf_oran_num_elements, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_elements);
5299 | }
5300 | else {
5301 | /* All other meas ids have a reserved byte */
5302 | add_reserved_field(mr_tree, hf_oran_reserved_8bits, tvb, offset, 1);
5303 | }
5304 | offset += 1;
5305 |
5306 | /* measDataSize (16 bits). N.B. begins at mf field, i.e. 2 bytes before this one */
5307 | unsigned meas_data_size;
5308 | proto_item *meas_data_size_ti;
5309 | meas_data_size_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_meas_data_size, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &meas_data_size);
5310 | meas_data_size *= 4;
5311 | proto_item_append_text(meas_data_size_ti, " (%u bytes)", meas_data_size);
5312 | offset += 2;
5313 |
5314 | /* Summary for measurement report root */
5315 | proto_item_append_text(mr_ti, " (measTypeId=%u - %s)",
5316 | meas_type_id, val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
5317 | /* And section header */
5318 | proto_item_append_text(tree, " (%s)", val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
5319 | /* And Info column */
5320 | col_append_fstr(pinfo->cinfo, COL_INFO, " (%s)", val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
5321 |
5322 | /* Handle specific message type fields */
5323 | switch (meas_type_id) {
5324 | case 1:
5325 | {
5326 | /* ueTae */
5327 | unsigned ue_tae;
5328 | proto_item *ue_tae_ti;
5329 | ue_tae_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_tae, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_tae);
5330 | /* Show if maps onto a -ve number */
5331 | if ((ue_tae >= 0x8ad0) && (ue_tae <= 0xffff)) {
5332 | proto_item_append_text(ue_tae_ti, "(value %d)", -1 - (0xffff-ue_tae));
5333 | }
5334 | offset += 2;
5335 |
5336 | /* Reserved (16 bits) */
5337 | add_reserved_field(mr_tree, hf_oran_reserved_16bits, tvb, offset, 2);
5338 | offset += 2;
5339 | break;
5340 | }
5341 | case 2:
5342 | /* ueLayerPower entries (how many? for now just use up meas_data_size..) */
5343 | /* TODO: add number of distinct dmrsPortNumber entries seen in SE24 and save in state? */
5344 | /* Or would it make sense to use the preference 'pref_num_bf_antennas' ? */
5345 | for (unsigned n=0; n < (meas_data_size-4)/2; n++) {
5346 | unsigned ue_layer_power;
5347 | proto_item *ue_layer_power_ti;
5348 | ue_layer_power_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_layer_power, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_layer_power);
5349 | /* Show if maps onto a -ve number */
5350 | if ((ue_layer_power >= 0x8ad0) && (ue_layer_power <= 0xffff)) {
5351 | proto_item_append_text(ue_layer_power_ti, "(value %d)", -1 - (0xffff-ue_layer_power));
5352 | }
5353 | offset += 2;
5354 | }
5355 | /* padding out to 4 bytes */
5356 | break;
5357 | case 3:
5358 | {
5359 | /* ueFreqOffset */
5360 | unsigned ue_freq_offset;
5361 | proto_item *ue_freq_offset_ti;
5362 | ue_freq_offset_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_freq_offset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_freq_offset);
5363 | /* Show if maps onto a -ve number */
5364 | if ((ue_freq_offset >= 0x8ad0) && (ue_freq_offset <= 0xffff)) {
5365 | proto_item_append_text(ue_freq_offset_ti, "(value %d)", -1 - (0xffff-ue_freq_offset));
5366 | }
5367 | offset += 2;
5368 |
5369 | /* Reserved (16 bits) */
5370 | add_reserved_field(mr_tree, hf_oran_reserved_16bits, tvb, offset, 2);
5371 | offset += 2;
5372 | break;
5373 | }
5374 | case 4:
5375 | case 5:
5376 | /* reserved (2 bits) */
5377 | add_reserved_field(mr_tree, hf_oran_reserved_2bits, tvb, offset, 1);
5378 | /* symbolMask (14 bits) */
5379 | offset = dissect_symbolmask(tvb, mr_tree, offset, NULL((void*)0), NULL((void*)0));
5380 |
5381 | /* 2 bytes for each PRB ipnPower */
5382 | for (unsigned prb=0; prb<MAX_PRBS273; prb++) {
5383 | /* Skip if should not be reported */
5384 | if (!prbs_for_st10_type5[prb]) {
5385 | continue;
5386 | }
5387 | unsigned ipn_power;
5388 | proto_item *ipn_power_ti;
5389 | /* ipnPower (2 bytes) */
5390 | ipn_power_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ipn_power, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ipn_power);
5391 | proto_item_append_text(ipn_power_ti, " (PRB %3d)", prb);
5392 | /* Show if maps onto a -ve number */
5393 | if ((ipn_power >= 0x8ad0) && (ipn_power <= 0xffff)) {
5394 | proto_item_append_text(ipn_power_ti, " (value %d)", -1 - (0xffff-ipn_power));
5395 | }
5396 | offset += 2;
5397 | }
5398 | /* padding out to 4 bytes */
5399 | break;
5400 | case 6:
5401 | /* antDmrsSnrVal entries */
5402 | for (unsigned n=0; n < num_elements; n++) {
5403 | unsigned snr_value;
5404 | proto_item *snr_value_ti;
5405 | /* antDmrsSnrVal (2 bytes) */
5406 | snr_value_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ant_dmrs_snr_val, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &snr_value);
5407 | proto_item_append_text(snr_value_ti, " (elem %2u)", n+1);
5408 | /* Show if maps onto a -ve number */
5409 | if ((snr_value >= 0x8ad0) && (snr_value <= 0xffff)) {
5410 | proto_item_append_text(snr_value_ti, " (value %d)", -1 - (0xffff-snr_value));
5411 | }
5412 | offset += 2;
5413 | }
5414 | break;
5415 | case 7:
5416 | {
5417 | /* UE positioning measurement report */
5418 | float start_value;
5419 |
5420 | /* ueAzAoa (16 bits) */
5421 | uint32_t ue_az_aoa;
5422 | proto_item *ue_az_aoa_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_az_aoa, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_az_aoa);
5423 | if (ue_az_aoa <= 0xE0F) {
5424 | if (ue_az_aoa >= 0x0708) {
5425 | start_value = (ue_az_aoa-0x0708) * (float)0.1;
5426 | proto_item_append_text(ue_az_aoa_ti, " (%.1f <= val < %.1f degrees)", start_value, start_value + (float)0.1);
5427 | }
5428 | else {
5429 | start_value = 180 + (ue_az_aoa * (float)0.1);
5430 | proto_item_append_text(ue_az_aoa_ti, " (%.1f <= val < %.1f degrees)", start_value, start_value + (float)0.1);
5431 | }
5432 | }
5433 | else if (ue_az_aoa == 0xffff) {
5434 | proto_item_append_text(ue_az_aoa_ti, " (invalid measurement result)");
5435 | }
5436 | else {
5437 | proto_item_append_text(ue_az_aoa_ti, " (reserved)");
5438 | }
5439 | offset += 2;
5440 |
5441 | /* Reserved (16 bits) */
5442 | add_reserved_field(mr_tree, hf_oran_reserved_16bits, tvb, offset, 2);
5443 | offset += 2;
5444 |
5445 | /* ueZeAoa (16 bits) */
5446 | uint32_t ue_ze_aoa;
5447 | proto_item *ue_ze_aoa_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_ze_aoa, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_ze_aoa);
5448 | if (ue_ze_aoa <= 0x707) {
5449 | start_value = ue_ze_aoa * (float)0.1;
5450 | proto_item_append_text(ue_ze_aoa_ti, " (%.1f <= val < %.1f degrees)", start_value, start_value + (float)0.1);
5451 | }
5452 | else if (ue_az_aoa == 0xffff) {
5453 | proto_item_append_text(ue_ze_aoa_ti, " (invalid measurement result)");
5454 | }
5455 | else {
5456 | proto_item_append_text(ue_ze_aoa_ti, " (reserved)");
5457 | }
5458 | offset += 2;
5459 |
5460 | /* Reserved (16 bits) */
5461 | add_reserved_field(mr_tree, hf_oran_reserved_16bits, tvb, offset, 2);
5462 | offset += 2;
5463 |
5464 | /* uePosToaOffset (16 bits) */
5465 | uint32_t ue_pos_toa_offset;
5466 | proto_item *ue_pos_toa_offset_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_pos_toa_offset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ue_pos_toa_offset);
5467 | if (ue_pos_toa_offset == 0) {
5468 | proto_item_append_text(ue_pos_toa_offset_ti, " (no UE ToA offset, 0 symbols)");
5469 | }
5470 | else if (ue_pos_toa_offset <= 0x7fff) {
5471 | proto_item_append_text(ue_pos_toa_offset_ti, " (+ve UE ToA offset)");
5472 | }
5473 | else if (ue_pos_toa_offset == 0x8000) {
5474 | proto_item_append_text(ue_pos_toa_offset_ti, " (invalid measurement result)");
5475 | }
5476 | else {
5477 | proto_item_append_text(ue_pos_toa_offset_ti, " (-ve UE ToA offset)");
5478 | }
5479 | offset += 2;
5480 |
5481 | /* Reserved (16 bits) */
5482 | add_reserved_field(mr_tree, hf_oran_reserved_16bits, tvb, offset, 2);
5483 | offset += 2;
5484 | break;
5485 | }
5486 | case 8:
5487 | {
5488 | /* UE radial speed measurement report */
5489 |
5490 | /* ueRadialSpeed (16 bits) */
5491 | uint32_t radial_speed;
5492 | proto_item *radial_speed_ti = proto_tree_add_item_ret_uint(mr_tree, hf_oran_ue_radial_speed, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &radial_speed);
5493 | if (radial_speed <= 10000) {
5494 | proto_item_append_text(radial_speed_ti, " (%.1f km/h)", radial_speed * (float)0.1);
5495 | }
5496 | else if (radial_speed == 0x8000) {
5497 | proto_item_append_text(radial_speed_ti, " (invalid measurement result)");
5498 | }
5499 | else {
5500 | proto_item_append_text(radial_speed_ti, " (reserved value)");
5501 | }
5502 | offset += 2;
5503 |
5504 | /* Reserved (16 bits) */
5505 | add_reserved_field(mr_tree, hf_oran_reserved_16bits, tvb, offset, 2);
5506 | offset += 2;
5507 | break;
5508 | }
5509 | case 9:
5510 | {
5511 | /* TODO: UE post-equalization MU interference measurement */
5512 |
5513 | /* reserved (16 bits) */
5514 | add_reserved_field(mr_tree, hf_oran_reserved_16bits, tvb, offset, 2);
5515 | offset += 2;
5516 |
5517 | /* TODO: muInterferenceLevel (all layers * all PRB blocks) */
5518 | break;
5519 | }
5520 | case 10:
5521 | {
5522 | /* UE TPMI and rank recommendation measurement */
5523 |
5524 | /* numCandRanks (4 bits - only 1-4 valid) */
5525 | uint8_t num_cand_ranks;
5526 | proto_tree_add_item_ret_uint8(mr_tree, hf_oran_num_cand_ranks, tvb, offset, 1, ENC_NA0x00000000, &num_cand_ranks);
5527 | if (num_cand_ranks > 4) {
5528 | num_cand_ranks = 4;
5529 | }
5530 | if (num_cand_ranks < 1) {
5531 | num_cand_ranks = 1;
5532 | }
5533 |
5534 | /* uePrefRank (4 bits) */
5535 | add_reserved_field(mr_tree, hf_oran_ue_pref_rank, tvb, offset, 1);
5536 | offset += 1;
5537 |
5538 | for (uint8_t cand_rank=1; cand_rank <= num_cand_ranks; cand_rank++) {
5539 | /* ueTpmiRankY (1 byte) */
5540 | proto_item *rank_y_ti = proto_tree_add_item(mr_tree, hf_oran_ue_tpmi_rank_y,
5541 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5542 | proto_item_append_text(rank_y_ti, " (rank %u)", cand_rank);
5543 |
5544 | offset += 1;
5545 |
5546 | for (uint8_t sinr = 1; sinr <= cand_rank; sinr++) {
5547 | /* ueTpmiRankYSinrLX (2 bytes) */
5548 | proto_item *rank_y_sinr_x_ti = proto_tree_add_item(mr_tree, hf_oran_ue_tpmi_rank_y_sinr_lx,
5549 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5550 | proto_item_append_text(rank_y_sinr_x_ti, " (rank %u, sinr %u)", cand_rank, sinr);
5551 | offset += 2;
5552 | }
5553 | }
5554 | break;
5555 | }
5556 | case 11:
5557 | {
5558 | /* UE layer pre-equalization SINR report */
5559 | /* TODO: how to know how many layers? Just fill up available data? */
5560 | unsigned num_layers = (meas_data_size-1) * 4;
5561 | for (unsigned layer=0; layer < num_layers; layer++) {
5562 | /* ueLayerPreEqSinr (2 bytes each) */
5563 | proto_item *pre_eq_sinr_ti = proto_tree_add_item(mr_tree, hf_oran_ue_layer_pre_eq_sinr,
5564 | tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
5565 | proto_item_append_text(pre_eq_sinr_ti, " (layer %u)", layer);
5566 | offset += 2;
5567 | }
5568 | break;
5569 | }
5570 |
5571 | default:
5572 | /* Anything else is not expected */
5573 | expert_add_info_format(pinfo, meas_type_id_ti, &ei_oran_unexpected_measTypeId,
5574 | "measTypeId %u (%s) not supported - only 1-6 are expected",
5575 | meas_type_id,
5576 | val_to_str_const(meas_type_id, meas_type_id_vals, "reserved"));
5577 | break;
5578 |
5579 | }
5580 |
5581 | /* Pad out to next 4 bytes */
5582 | offset += WS_PADDING_TO_4(offset-report_start_offset)((4U - ((offset-report_start_offset) % 4U)) % 4U);
5583 |
5584 | /* TODO: verify dissected size of report vs meas_data_size? */
5585 |
5586 | /* End of measurement report tree */
5587 | proto_item_set_end(mr_ti, tvb, offset);
5588 | } while (mf);
5589 | }
5590 |
5591 | /* Request for RRM Measurements has measurement commands after extensions */
5592 | else if (sectionType == SEC_C_REQUEST_RRM_MEAS) /* Section Type 11 */
5593 | {
5594 | bool_Bool mf = true1;
5595 | do {
5596 | /* Measurement command subtree */
5597 | proto_item *mc_ti = proto_tree_add_string_format(c_section_tree, hf_oran_measurement_command,
5598 | tvb, offset, 8, "", "Measurement Command");
5599 | proto_tree *mc_tree = proto_item_add_subtree(mc_ti, ett_oran_measurement_command);
5600 |
5601 | /* mf (1 bit). 1st measurement command is always preset */
5602 | proto_tree_add_item_ret_boolean(mc_tree, hf_oran_mf, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &mf);
5603 |
5604 | /* measTypeId (7 bits) */
5605 | uint32_t meas_type_id;
5606 | proto_item *meas_type_id_ti;
5607 | meas_type_id_ti = proto_tree_add_item_ret_uint(mc_tree, hf_oran_meas_type_id, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &meas_type_id);
5608 | offset += 1;
5609 |
5610 | proto_item *meas_command_ti;
5611 | uint32_t meas_command_size;
5612 |
5613 | switch (meas_type_id) {
5614 | case 5: /* command for IpN for unallocated PRBs */
5615 | /* reserved (1 byte) */
5616 | add_reserved_field(mc_tree, hf_oran_reserved_8bits, tvb, offset, 1);
5617 | offset += 1;
5618 | /* measCmdSize. Presumably number of words so in future could skip unrecognised command types.. */
5619 | meas_command_ti = proto_tree_add_item_ret_uint(mc_tree, hf_oran_meas_cmd_size, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &meas_command_size);
5620 | proto_item_append_text(meas_command_ti, " (%u bytes)", meas_command_size*4);
5621 | offset += 2;
5622 | /* reserved (2 bits) */
5623 | add_reserved_field(mc_tree, hf_oran_reserved_2bits, tvb, offset, 1);
5624 | /* symbolMask (14 bits) */
5625 | offset = dissect_symbolmask(tvb, mc_tree, offset, NULL((void*)0), NULL((void*)0));
5626 | /* reserved (16 bits) */
5627 | add_reserved_field(mc_tree, hf_oran_reserved_16bits, tvb, offset, 2);
5628 | offset += 2;
5629 | break;
5630 |
5631 | default:
5632 | /* Anything else is not expected */
5633 | expert_add_info_format(pinfo, meas_type_id_ti, &ei_oran_unexpected_measTypeId,
5634 | "measTypeId %u (%s) not supported - only 5 is expected",
5635 | meas_type_id,
5636 | val_to_str_const(meas_type_id, meas_type_id_vals, "reserved"));
5637 | break;
5638 | }
5639 | proto_item_append_text(mc_ti, " (%s)", val_to_str_const(meas_type_id, meas_type_id_vals, "unknown"));
5640 |
5641 | } while (mf);
5642 | }
5643 |
5644 | /* Set extent of overall section */
5645 | proto_item_set_len(sectionHeading, offset);
5646 |
5647 | return offset;
5648 | }
5649 |
5650 | /* Dissect udCompHdr (user data compression header, 7.5.2.10) */
5651 | /* bit_width and comp_meth are out params */
5652 | static int dissect_udcomphdr(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, unsigned offset,
5653 | bool_Bool cplane, bool_Bool ignore,
5654 | unsigned *bit_width, unsigned *comp_meth, proto_item **comp_meth_ti,
5655 | oran_tap_info *tap_info)
5656 | {
5657 | /* Subtree */
5658 | proto_item *udcomphdr_ti = proto_tree_add_string_format(tree, hf_oran_udCompHdr,
5659 | tvb, offset, 1, "",
5660 | "udCompHdr");
5661 | proto_tree *udcomphdr_tree = proto_item_add_subtree(udcomphdr_ti, ett_oran_udcomphdr);
5662 |
5663 | /* udIqWidth */
5664 | uint32_t hdr_iq_width;
5665 | proto_item *iq_width_item = proto_tree_add_item_ret_uint(udcomphdr_tree, hf_oran_udCompHdrIqWidth , tvb, offset, 1, ENC_NA0x00000000, &hdr_iq_width);
5666 | *bit_width = (hdr_iq_width) ? hdr_iq_width : 16;
5667 | proto_item_append_text(iq_width_item, " (%u bits)", *bit_width);
5668 |
5669 | /* udCompMeth */
5670 | uint32_t ud_comp_meth;
5671 | *comp_meth_ti = proto_tree_add_item_ret_uint(udcomphdr_tree, hf_oran_udCompHdrMeth, tvb, offset, 1, ENC_NA0x00000000, &ud_comp_meth);
5672 | if (comp_meth) {
5673 | *comp_meth = ud_comp_meth;
5674 | }
5675 |
5676 | /* Populate tap header with compression settings */
5677 | if (!ignore) {
5678 | tap_info->compression_methods |= (1 << ud_comp_meth);
5679 | tap_info->compression_width = MAX(tap_info->compression_width, hdr_iq_width)(((tap_info->compression_width) > (hdr_iq_width)) ? (tap_info ->compression_width) : (hdr_iq_width));
5680 | /* Summary */
5681 | proto_item_append_text(udcomphdr_ti, " (IqWidth=%u, udCompMeth=%s)",
5682 | *bit_width, rval_to_str_const(ud_comp_meth, ud_comp_header_meth, "Unknown"));
5683 | }
5684 | else {
5685 | proto_item_append_text(udcomphdr_ti, " (ignored)");
5686 | if (hdr_iq_width || ud_comp_meth) {
5687 | if (cplane) {
5688 | /* Only ignore DL for cplane */
5689 | expert_add_info_format(pinfo, udcomphdr_ti, &ei_oran_udpcomphdr_should_be_zero,
5690 | "udCompHdr in C-Plane for DL should be 0 - found 0x%02x",
5691 | tvb_get_uint8(tvb, offset));
5692 | }
5693 | else {
5694 | /* TODO: Ignore UL if using m-plane/preference setting rather than c-plane, but wrong to be set? */
5695 | /* expert_add_info_format(pinfo, udcomphdr_ti, &ei_oran_udpcomphdr_should_be_zero,
5696 | "udCompHdr in C-Plane for UL should be 0 - found 0x%02x",
5697 | tvb_get_uint8(tvb, offset));
5698 | */
5699 | }
5700 |
5701 | }
5702 | }
5703 | return offset+1;
5704 | }
5705 |
5706 | /* Dissect udCompParam (user data compression parameter, 8.3.3.15) */
5707 | /* bit_width and comp_meth are out params */
5708 | static int dissect_udcompparam(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree, unsigned offset,
5709 | unsigned comp_meth,
5710 | uint32_t *exponent, uint16_t *sReSMask,
5711 | bool_Bool for_sinr)
5712 | {
5713 | if (for_sinr && (comp_meth != COMP_BLOCK_FP1)) {
5714 | /* sinrCompParam only present when bfp is used */
5715 | return offset;
5716 | }
5717 |
5718 | if (comp_meth == COMP_NONE0 ||
5719 | comp_meth == COMP_MODULATION4 ||
5720 | comp_meth == MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8) {
5721 |
5722 | /* Not even creating a subtree for udCompMeth 0, 4, 8 */
5723 | return offset;
5724 | }
5725 |
5726 | /* Subtree */
5727 | unsigned start_offset = offset;
5728 | proto_item *udcompparam_ti = proto_tree_add_string_format(tree, hf_oran_udCompParam,
5729 | tvb, offset, 1, "",
5730 | (for_sinr) ? "sinrCompParam" : "udCompParam");
5731 | proto_tree *udcompparam_tree = proto_item_add_subtree(udcompparam_ti, ett_oran_udcompparam);
5732 |
5733 | /* Show comp_meth as a generated field */
5734 | proto_item *meth_ti = proto_tree_add_uint(udcompparam_tree, hf_oran_udCompHdrMeth_pref, tvb, 0, 0, comp_meth);
5735 | proto_item_set_generated(meth_ti);
5736 |
5737 | uint32_t param_exponent;
5738 | uint64_t param_sresmask;
5739 |
5740 | static int * const sres_mask_flags[] = {
5741 | &hf_oran_sReSMask_re12,
5742 | &hf_oran_sReSMask_re11,
5743 | &hf_oran_sReSMask_re10,
5744 | &hf_oran_sReSMask_re9,
5745 | &hf_oran_sReSMask_re8,
5746 | &hf_oran_sReSMask_re7,
5747 | &hf_oran_sReSMask_re6,
5748 | &hf_oran_sReSMask_re5,
5749 | &hf_oran_sReSMask_re4,
5750 | &hf_oran_sReSMask_re3,
5751 | &hf_oran_sReSMask_re2,
5752 | &hf_oran_sReSMask_re1,
5753 | NULL((void*)0)
5754 | };
5755 |
5756 | switch (comp_meth) {
5757 | case COMP_BLOCK_FP1: /* 1 */
5758 | case BFP_AND_SELECTIVE_RE_WITH_MASKS7: /* 7 */
5759 | /* reserved (4 bits) */
5760 | add_reserved_field(udcompparam_tree, hf_oran_reserved_4bits, tvb, offset, 1);
5761 | /* exponent (4 bits) */
5762 | proto_tree_add_item_ret_uint(udcompparam_tree, hf_oran_exponent,
5763 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &param_exponent);
5764 | *exponent = param_exponent;
5765 | proto_item_append_text(udcompparam_ti, " (Exponent=%u)", param_exponent);
5766 | offset += 1;
5767 | break;
5768 |
5769 | case COMP_BLOCK_SCALE2: /* 2 */
5770 | /* Separate into integer and fractional bits? */
5771 | proto_tree_add_item(udcompparam_tree, hf_oran_blockScaler,
5772 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5773 | offset++;
5774 | break;
5775 |
5776 | case COMP_U_LAW3: /* 3 */
5777 | /* compBitWidth, compShift */
5778 | proto_tree_add_item(udcompparam_tree, hf_oran_compBitWidth,
5779 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5780 | proto_tree_add_item(udcompparam_tree, hf_oran_compShift,
5781 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
5782 | offset += 1;
5783 | break;
5784 |
5785 | case BFP_AND_SELECTIVE_RE5: /* 5 */
5786 | {
5787 | /* sReSMask (exponent in middle!) */
5788 | proto_item *sresmask_ti;
5789 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(udcompparam_tree, tvb, offset,
5790 | hf_oran_sReSMask,
5791 | ett_oran_sresmask,
5792 | sres_mask_flags,
5793 | ENC_NA0x00000000,
5794 | &param_sresmask);
5795 |
5796 | /* Get rid of exponent-shaped gap */
5797 | param_sresmask = ((param_sresmask >> 4) & 0x0f00) | (param_sresmask & 0xff);
5798 | unsigned res = 0;
5799 | for (unsigned n=0; n < 12; n++) {
5800 | if ((param_sresmask >> n) & 0x1) {
5801 | res++;
5802 | }
5803 | }
5804 | proto_item_append_text(sresmask_ti, " (%2u REs)", res);
5805 |
5806 | /* exponent */
5807 | proto_tree_add_item_ret_uint(udcompparam_tree, hf_oran_exponent,
5808 | tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &param_exponent);
5809 | *sReSMask = (uint16_t)param_sresmask;
5810 | *exponent = param_exponent;
5811 |
5812 | proto_item_append_text(udcompparam_ti, " (exponent=%u, %u REs)", *exponent, res);
5813 | offset += 2;
5814 | break;
5815 | }
5816 |
5817 | case MOD_COMPR_AND_SELECTIVE_RE6: /* 6 */
5818 | {
5819 | /* sReSMask (exponent in middle!) */
5820 | proto_item *sresmask_ti;
5821 |
5822 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(udcompparam_tree, tvb, offset,
5823 | hf_oran_sReSMask,
5824 | ett_oran_sresmask,
5825 | sres_mask_flags,
5826 | ENC_NA0x00000000,
5827 | &param_sresmask);
5828 |
5829 | /* Get rid of reserved-shaped gap */
5830 | param_sresmask = ((param_sresmask >> 4) & 0x0f00) | (param_sresmask & 0xff);
5831 | unsigned res = 0;
5832 | for (unsigned n=0; n < 12; n++) {
5833 | if ((param_sresmask >> n) & 0x1) {
5834 | res++;
5835 | }
5836 | }
5837 | proto_item_append_text(sresmask_ti, " (%u REs)", res);
5838 |
5839 | /* reserved (4 bits) */
5840 | add_reserved_field(udcompparam_tree, hf_oran_reserved_last_4bits, tvb, offset, 1);
5841 | *sReSMask = (uint16_t)param_sresmask;
5842 |
5843 | proto_item_append_text(udcompparam_ti, " (%u REs)", res);
5844 | offset += 2;
5845 | break;
5846 | }
5847 |
5848 | default:
5849 | /* reserved (set to all zeros), but how many bytes?? */
5850 | break;
5851 | }
5852 |
5853 | proto_item_set_len(udcompparam_ti, offset-start_offset);
5854 | return offset;
5855 | }
5856 |
5857 |
5858 | /* Dissect ciCompHdr (channel information compression header, 7.5.2.15) */
5859 | /* bit_width and comp_meth are out params */
5860 | static int dissect_cicomphdr(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree, unsigned offset,
5861 | unsigned *bit_width, unsigned *comp_meth, uint8_t *comp_opt)
5862 | {
5863 | /* Subtree */
5864 | proto_item *cicomphdr_ti = proto_tree_add_string_format(tree, hf_oran_ciCompHdr,
5865 | tvb, offset, 1, "",
5866 | "ciCompHdr");
5867 | proto_tree *cicomphdr_tree = proto_item_add_subtree(cicomphdr_ti, ett_oran_cicomphdr);
5868 |
5869 | /* ciIqWidth */
5870 | uint32_t hdr_iq_width;
5871 | proto_item *iq_width_item = proto_tree_add_item_ret_uint(cicomphdr_tree, hf_oran_ciCompHdrIqWidth , tvb, offset, 1, ENC_NA0x00000000, &hdr_iq_width);
5872 | hdr_iq_width = (hdr_iq_width) ? hdr_iq_width : 16;
5873 | if (bit_width) {
5874 | *bit_width = hdr_iq_width;
5875 | }
5876 | proto_item_append_text(iq_width_item, " (%u bits)", hdr_iq_width);
5877 |
5878 | /* ciCompMeth */
5879 | uint32_t ci_comp_meth;
5880 | proto_tree_add_item_ret_uint(cicomphdr_tree, hf_oran_ciCompHdrMeth, tvb, offset, 1, ENC_NA0x00000000, &ci_comp_meth);
5881 | if (comp_meth) {
5882 | *comp_meth = ci_comp_meth;
5883 | }
5884 |
5885 | /* ciCompOpt */
5886 | uint32_t opt;
5887 | proto_tree_add_item_ret_uint(cicomphdr_tree, hf_oran_ciCompOpt, tvb, offset, 1, ENC_NA0x00000000, &opt);
5888 | *comp_opt = opt;
5889 | offset += 1;
5890 |
5891 | /* Summary */
5892 | proto_item_append_text(cicomphdr_ti, " (IqWidth=%u, ciCompMeth=%s, ciCompOpt=%s)",
5893 | hdr_iq_width,
5894 | rval_to_str_const(ci_comp_meth, ud_comp_header_meth, "Unknown"),
5895 | (*comp_opt) ? "compression per PRB" : "compression per UE");
5896 | return offset;
5897 | }
5898 |
5899 | static void dissect_payload_version(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo, unsigned offset)
5900 | {
5901 | unsigned version;
5902 | proto_item *ti = proto_tree_add_item_ret_uint(tree, hf_oran_payload_version, tvb, offset, 1, ENC_NA0x00000000, &version);
5903 | if (version != 1) {
5904 | expert_add_info_format(pinfo, ti, &ei_oran_version_unsupported,
5905 | "PayloadVersion %u not supported by dissector (only 1 is known)",
5906 | version);
5907 | /* TODO: should throw an exception? */
5908 | }
5909 | }
5910 |
5911 | static void show_link_to_acknack_request(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo,
5912 | ack_nack_request_t *request)
5913 | {
5914 | /* Request frame */
5915 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_acknack_request_frame,
5916 | tvb, 0, 0, request->request_frame_number);
5917 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
5918 |
5919 | /* Work out gap between frames (in ms) */
5920 | int seconds_between_packets = (int)
5921 | (pinfo->abs_ts.secs - request->request_frame_time.secs);
5922 | int nseconds_between_packets =
5923 | pinfo->abs_ts.nsecs - request->request_frame_time.nsecs;
5924 |
5925 | int total_gap = (seconds_between_packets*1000) +
5926 | ((nseconds_between_packets+500000) / 1000000);
5927 |
5928 | ti = proto_tree_add_uint(tree, hf_oran_acknack_request_time,
5929 | tvb, 0, 0, total_gap);
5930 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
5931 |
5932 | /* Type of request */
5933 | ti = proto_tree_add_uint(tree, hf_oran_acknack_request_type,
5934 | tvb, 0, 0, request->requestType);
5935 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
5936 | }
5937 |
5938 | static void show_link_to_acknack_response(proto_tree *tree, tvbuff_t *tvb, packet_info *pinfo,
5939 | ack_nack_request_t *response)
5940 | {
5941 | if (response->response_frame_number == 0) {
5942 | /* Requests may not get a response, and can't always tell when to expect one */
5943 | return;
5944 | }
5945 |
5946 | /* Response frame */
5947 | proto_item *ti = proto_tree_add_uint(tree, hf_oran_acknack_response_frame,
5948 | tvb, 0, 0, response->response_frame_number);
5949 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
5950 |
5951 | /* Work out gap between frames (in ms) */
5952 | int seconds_between_packets = (int)
5953 | (response->response_frame_time.secs - pinfo->abs_ts.secs);
5954 | int nseconds_between_packets =
5955 | response->response_frame_time.nsecs - pinfo->abs_ts.nsecs;
5956 |
5957 | int total_gap = (seconds_between_packets*1000) +
5958 | ((nseconds_between_packets+500000) / 1000000);
5959 |
5960 | ti = proto_tree_add_uint(tree, hf_oran_acknack_response_time,
5961 | tvb, 0, 0, total_gap);
5962 | PROTO_ITEM_SET_GENERATED(ti)proto_item_set_generated((ti));
5963 | }
5964 |
5965 |
5966 |
5967 | /* Control plane dissector (section 7). */
5968 | static int dissect_oran_c(tvbuff_t *tvb, packet_info *pinfo,
5969 | proto_tree *tree, oran_tap_info *tap_info, void *data _U___attribute__((unused)))
5970 | {
5971 | /* Hidden filter for plane */
5972 | proto_item *plane_ti = proto_tree_add_item(tree, hf_oran_cplane, tvb, 0, 0, ENC_NA0x00000000);
5973 | PROTO_ITEM_SET_HIDDEN(plane_ti)proto_item_set_hidden((plane_ti));
5974 |
5975 | /* Set up structures needed to add the protocol subtree and manage it */
5976 | unsigned offset = 0;
5977 |
5978 | col_set_str(pinfo->cinfo, COL_PROTOCOL, "O-RAN-FH-C");
5979 | col_set_str(pinfo->cinfo, COL_INFO, "C-Plane");
5980 |
5981 | tap_info->userplane = false0;
5982 |
5983 | /* Create display subtree for the protocol */
5984 | proto_item *protocol_item = proto_tree_add_item(tree, proto_oran, tvb, 0, -1, ENC_NA0x00000000);
5985 | proto_item_append_text(protocol_item, "-C");
5986 | proto_tree *oran_tree = proto_item_add_subtree(protocol_item, ett_oran);
5987 |
5988 | /* ecpriRtcid (eAxC ID) */
5989 | uint16_t eAxC;
5990 | addPcOrRtcid(tvb, oran_tree, &offset, hf_oran_ecpri_rtcid, &eAxC, tap_info);
5991 | tap_info->eaxc = eAxC;
5992 |
5993 | /* Look up any existing conversation state for eAxC+plane */
5994 | uint32_t key = make_flow_key(pinfo, eAxC, ORAN_C_PLANE0, false0);
5995 | flow_state_t* state = (flow_state_t*)wmem_tree_lookup32(flow_states_table, key);
5996 |
5997 | /* Message identifier */
5998 | uint32_t seq_id, sub_seq_id, e;
5999 | proto_item *seq_id_ti;
6000 | offset = addSeqid(tvb, oran_tree, offset, ORAN_C_PLANE0, &seq_id, &seq_id_ti, pinfo, &sub_seq_id, &e);
6001 |
6002 | /* Section common subtree */
6003 | int section_tree_offset = offset;
6004 | proto_item *sectionHeading = proto_tree_add_string_format(oran_tree, hf_oran_c_section_common,
6005 | tvb, offset, 0, "", "C-Plane Section Type ");
6006 | proto_tree *section_tree = proto_item_add_subtree(sectionHeading, ett_oran_c_section_common);
6007 |
6008 | /* Peek ahead at the section type */
6009 | uint32_t sectionType = 0;
6010 | sectionType = tvb_get_uint8(tvb, offset+5);
6011 |
6012 | uint32_t scs = 0;
6013 | proto_item *scs_ti = NULL((void*)0);
6014 |
6015 | /* dataDirection */
6016 | uint32_t direction = 0;
6017 | proto_item *datadir_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_data_direction, tvb, offset, 1, ENC_NA0x00000000, &direction);
6018 | tap_info->uplink = (direction==0);
6019 |
6020 | /* Update/report status of conversation */
6021 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
6022 |
6023 | if (state == NULL((void*)0)) {
6024 | /* Allocate new state */
6025 | state = wmem_new0(wmem_file_scope(), flow_state_t)((flow_state_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_state_t )));
6026 | state->ack_nack_requests = wmem_tree_new(wmem_file_scope());
6027 | wmem_tree_insert32(flow_states_table, key, state);
6028 | /* Tables for each direction */
6029 | state->expected_sections[0] = wmem_tree_new(wmem_file_scope());
6030 | state->expected_sections[1] = wmem_tree_new(wmem_file_scope());
6031 | }
6032 |
6033 | /* Check sequence analysis status */
6034 | if (state->last_frame_seen[direction] && (seq_id != state->next_expected_sequence_number[direction])) {
6035 | /* Store this result */
6036 | flow_result_t *result = wmem_new0(wmem_file_scope(), flow_result_t)((flow_result_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_result_t )));
6037 | result->unexpected_seq_number = true1;
6038 | result->expected_sequence_number = state->next_expected_sequence_number[direction];
6039 | result->previous_frame = state->last_frame[direction];
6040 | result->u_plane_frames = wmem_list_new(wmem_file_scope());
6041 | wmem_tree_insert32(flow_results_table, pinfo->num, result);
6042 | }
6043 | /* Update conversation info */
6044 | state->last_frame[direction] = pinfo->num;
6045 | state->last_frame_seen[direction] = true1;
6046 | state->next_expected_sequence_number[direction] = (seq_id+1) % 256;
6047 | }
6048 |
6049 | /* Show any issues associated with this frame number */
6050 | flow_result_t *result = wmem_tree_lookup32(flow_results_table, pinfo->num);
6051 | if (result!=NULL((void*)0) && result->unexpected_seq_number) {
6052 | expert_add_info_format(pinfo, seq_id_ti,
6053 | (direction == DIR_UPLINK0) ?
6054 | &ei_oran_cplane_unexpected_sequence_number_ul :
6055 | &ei_oran_cplane_unexpected_sequence_number_dl,
6056 | "Sequence number %u expected, but got %u",
6057 | result->expected_sequence_number, seq_id);
6058 |
6059 | /* Update tap info */
6060 | uint32_t missing_sns = (256 + seq_id - result->expected_sequence_number) % 256;
6061 | /* Don't get confused by being slightly out of order.. */
6062 | if (missing_sns < 128) {
6063 | tap_info->missing_sns = missing_sns;
6064 | }
6065 | else {
6066 | tap_info->missing_sns = 0;
6067 | }
6068 |
6069 | /* TODO: could add previous/next frames (in seqId tree?) ? */
6070 | }
6071 |
6072 | /* payloadVersion */
6073 | dissect_payload_version(section_tree, tvb, pinfo, offset);
6074 |
6075 | /* filterIndex */
6076 | if (sectionType == SEC_C_SLOT_CONTROL || sectionType == SEC_C_ACK_NACK_FEEDBACK) {
6077 | /* scs (for ST4 and ST8) */
6078 | scs_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_frameStructure_subcarrier_spacing, tvb, offset, 1, ENC_NA0x00000000, &scs);
6079 | }
6080 | else if (sectionType == SEC_C_RRM_MEAS_REPORTS || sectionType == SEC_C_REQUEST_RRM_MEAS) {
6081 | /* reserved (4 bits) */
6082 | add_reserved_field(section_tree, hf_oran_reserved_last_4bits, tvb, offset, 1);
6083 | }
6084 | else if (sectionType != SEC_C_LAA) {
6085 | /* filterIndex (most common case) */
6086 | proto_tree_add_item(section_tree, hf_oran_filter_index, tvb, offset, 1, ENC_NA0x00000000);
6087 | }
6088 | offset += 1;
6089 |
6090 | unsigned ref_a_offset = offset;
6091 | /* frameId */
6092 | uint32_t frameId = 0;
6093 | proto_tree_add_item_ret_uint(section_tree, hf_oran_frame_id, tvb, offset, 1, ENC_NA0x00000000, &frameId);
6094 | tap_info->frame = frameId;
6095 | offset += 1;
6096 |
6097 | /* subframeId */
6098 | uint32_t subframeId = 0;
6099 | proto_tree_add_item_ret_uint(section_tree, hf_oran_subframe_id, tvb, offset, 1, ENC_NA0x00000000, &subframeId);
6100 | /* slotId */
6101 | uint32_t slotId = 0;
6102 | proto_tree_add_item_ret_uint(section_tree, hf_oran_slot_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &slotId);
6103 | tap_info->slot = slotId;
6104 | offset++;
6105 |
6106 | /* startSymbolId */
6107 | uint32_t startSymbolId = 0;
6108 | proto_item *ssid_ti = NULL((void*)0);
6109 | if ((sectionType == SEC_C_ACK_NACK_FEEDBACK) || /* Section Type 8 */
6110 | (sectionType == SEC_C_SINR_REPORTING)) { /* Section Type 9 */
6111 | /* symbolId */
6112 | proto_tree_add_item_ret_uint(section_tree, hf_oran_symbolId, tvb, offset, 1, ENC_NA0x00000000, &startSymbolId);
6113 | }
6114 | else if (sectionType != SEC_C_LAA) {
6115 | /* startSymbolId is in most section types */
6116 | ssid_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_start_symbol_id, tvb, offset, 1, ENC_NA0x00000000, &startSymbolId);
6117 | if (startSymbolId && (sectionType == SEC_C_RRM_MEAS_REPORTS)) { /* Section Type 10 */
6118 | proto_item_append_text(ssid_ti, " (should be 0 for ST10!)");
6119 | expert_add_info_format(pinfo, ssid_ti, &ei_oran_st10_startsymbolid_not_0,
6120 | "startSymbolId should be 0 for ST10 - found %u", startSymbolId);
6121 | }
6122 | }
6123 | else {
6124 | /* reserved (6 bits) */
6125 | add_reserved_field(section_tree, hf_oran_reserved_last_6bits, tvb, offset, 1);
6126 | }
6127 | offset++;
6128 |
6129 |
6130 | char id[16];
6131 | snprintf(id, 16, "%u-%u-%u-%u", frameId, subframeId, slotId, startSymbolId);
6132 | proto_item *pi = proto_tree_add_string(section_tree, hf_oran_refa, tvb, ref_a_offset, 3, id);
6133 | proto_item_set_generated(pi);
6134 |
6135 | uint32_t cmd_scope = 0;
6136 | bool_Bool st8_ready = false0;
6137 |
6138 | /* numberOfSections (or whatever section has instead) */
6139 | uint32_t nSections = 0;
6140 | if (sectionType == SEC_C_SLOT_CONTROL) { /* Section Type 4 */
6141 | /* Slot Control has these fields instead */
6142 | /* reserved (4 bits) */
6143 | add_reserved_field(section_tree, hf_oran_reserved_4bits, tvb, offset, 1);
6144 | /* cmdScope (4 bits) */
6145 | proto_tree_add_item_ret_uint(section_tree, hf_oran_cmd_scope, tvb, offset, 1, ENC_NA0x00000000, &cmd_scope);
6146 | }
6147 | else if (sectionType == SEC_C_ACK_NACK_FEEDBACK) { /* Section Type 8 */
6148 | /* reserved (7 bits) */
6149 | add_reserved_field(section_tree, hf_oran_reserved_7bits, tvb, offset, 1);
6150 | /* ready (1 bit) */
6151 | /* TODO: when set, ready in slotId+1.. */
6152 | proto_tree_add_item_ret_boolean(section_tree, hf_oran_ready, tvb, offset, 1, ENC_NA0x00000000, &st8_ready);
6153 | if (!st8_ready) {
6154 | /* SCS value is ignored, and may be set to any value by O-RU */
6155 | proto_item_append_text(scs_ti, " (ignored)");
6156 | }
6157 | }
6158 | else if (sectionType != SEC_C_LAA) {
6159 | /* numberOfSections */
6160 | proto_tree_add_item_ret_uint(section_tree, hf_oran_numberOfSections, tvb, offset, 1, ENC_NA0x00000000, &nSections);
6161 | }
6162 | else {
6163 | add_reserved_field(section_tree, hf_oran_reserved_8bits, tvb, offset, 1);
6164 | }
6165 | offset++;
6166 |
6167 | /* sectionType */
6168 | proto_tree_add_item_ret_uint(section_tree, hf_oran_sectionType, tvb, offset, 1, ENC_NA0x00000000, &sectionType);
6169 | offset += 1;
6170 |
6171 | /* Check that dataDirection is consistent with section type */
6172 | if (sectionType == SEC_C_SINR_REPORTING && direction != 0) { /* Section Type 9 */
6173 | expert_add_info(pinfo, datadir_ti, &ei_oran_st9_not_ul);
6174 | }
6175 | if (sectionType == SEC_C_RRM_MEAS_REPORTS && direction != 0) { /* Section Type 10 */
6176 | expert_add_info(pinfo, datadir_ti, &ei_oran_st10_not_ul);
6177 | }
6178 |
6179 | /* Note this section type in stats */
6180 | if (sectionType < SEC_C_MAX_INDEX) {
6181 | tap_info->section_types[sectionType] = true1;
6182 | }
6183 |
6184 | /* Section-type-specific fields following common header (white entries in Section Type diagrams) */
6185 | unsigned bit_width = 0;
6186 | unsigned comp_meth = 0;
6187 | proto_item *comp_meth_ti;
6188 | unsigned ci_comp_method = 0;
6189 | uint8_t ci_comp_opt = 0;
6190 |
6191 | uint32_t num_ues = 0;
6192 | uint32_t number_of_acks = 0, number_of_nacks = 0;
6193 |
6194 | uint32_t num_sinr_per_prb = 0;
6195 |
6196 | switch (sectionType) {
6197 | case SEC_C_UNUSED_RB: /* Section Type 0 */
6198 | /* timeOffset */
6199 | proto_tree_add_item(section_tree, hf_oran_timeOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6200 | offset += 2;
6201 | /* frameStructure */
6202 | offset = dissect_frame_structure(section_tree, tvb, offset,
6203 | subframeId, slotId);
6204 |
6205 | /* cpLength */
6206 | proto_tree_add_item(section_tree, hf_oran_cpLength, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6207 | offset += 2;
6208 | /* reserved (8 bits) */
6209 | add_reserved_field(section_tree, hf_oran_reserved_8bits, tvb, offset, 1);
6210 | offset += 1;
6211 | break;
6212 |
6213 | case SEC_C_NORMAL: /* Section Type 1 */
6214 | case SEC_C_UE_SCHED: /* Section Type 5 */
6215 | /* udCompHdr */
6216 | offset = dissect_udcomphdr(tvb, pinfo, section_tree, offset,
6217 | true1, direction==0 && pref_override_ul_compression, /* ignore for DL or if using mplane for UL settings */
6218 | &bit_width, &comp_meth, &comp_meth_ti, tap_info);
6219 | /* reserved (8 bits) */
6220 | add_reserved_field(section_tree, hf_oran_reserved_8bits, tvb, offset, 1);
6221 | offset += 1;
6222 | break;
6223 |
6224 | case SEC_C_SLOT_CONTROL: /* Section Type 4 */
6225 | break;
6226 |
6227 | case SEC_C_PRACH: /* Section Type 3 */
6228 | /* timeOffset */
6229 | proto_tree_add_item(section_tree, hf_oran_timeOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6230 | offset += 2;
6231 | /* frameStructure */
6232 | offset = dissect_frame_structure(section_tree, tvb, offset,
6233 | subframeId, slotId);
6234 | /* cpLength */
6235 | proto_tree_add_item(section_tree, hf_oran_cpLength, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6236 | offset += 2;
6237 | /* udCompHdr */
6238 | offset = dissect_udcomphdr(tvb, pinfo, section_tree, offset,
6239 | true1, direction==0 && pref_override_ul_compression, /* ignore for DL or if using mplane for UL settings */
6240 | &bit_width, &comp_meth, &comp_meth_ti, tap_info);
6241 | break;
6242 |
6243 | case SEC_C_CH_INFO: /* Section Type 6 */
6244 | /* numberOfUEs */
6245 | proto_tree_add_item_ret_uint(section_tree, hf_oran_numberOfUEs, tvb, offset, 1, ENC_NA0x00000000, &num_ues);
6246 | offset += 1;
6247 | /* ciCompHdr (was reserved) */
6248 | offset = dissect_cicomphdr(tvb, pinfo, section_tree, offset, &bit_width, &ci_comp_method, &ci_comp_opt);
6249 |
6250 | /* Number of sections may not be filled in (at all, or correctly), so set to the number of UEs.
6251 | The data entries are per-UE... they don't have a sectionID, but they could have section extensions... */
6252 | if (nSections == 0 || num_ues > nSections) {
6253 | nSections = num_ues;
6254 | }
6255 | break;
6256 |
6257 | case SEC_C_RSVD2:
6258 | break;
6259 |
6260 | case SEC_C_LAA: /* Section Type 7 */
6261 | add_reserved_field(section_tree, hf_oran_reserved_16bits, tvb, offset, 2);
6262 | offset += 2;
6263 | break;
6264 |
6265 | case SEC_C_ACK_NACK_FEEDBACK: /* Section Type 8 */
6266 | /* numberOfAcks (1 byte) */
6267 | proto_tree_add_item_ret_uint(section_tree, hf_oran_number_of_acks, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &number_of_acks);
6268 | offset += 1;
6269 | /* numberOfNacks (1 byte) */
6270 | proto_tree_add_item_ret_uint(section_tree, hf_oran_number_of_nacks, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &number_of_nacks);
6271 | offset += 1;
6272 |
6273 | /* Show ACKs and NACKs. For both, try to link back to request. */
6274 | for (unsigned int n=1; n <= number_of_acks; n++) {
6275 | uint32_t ackid;
6276 | proto_item *ack_ti;
6277 | ack_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_ackid, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ackid);
6278 | offset += 2;
6279 |
6280 | /* Look up request table in state (which really should be set by now, but test anyway). */
6281 | if (state && state->ack_nack_requests) {
6282 | ack_nack_request_t *request = wmem_tree_lookup32(state->ack_nack_requests, ackid);
6283 | if (request != NULL((void*)0)) {
6284 | /* On first pass, update with this response */
6285 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
6286 | request->response_frame_number = pinfo->num;
6287 | request->response_frame_time = pinfo->abs_ts;
6288 | }
6289 |
6290 | /* Show request details */
6291 | show_link_to_acknack_request(section_tree, tvb, pinfo, request);
6292 | }
6293 | else {
6294 | /* Request not found */
6295 | expert_add_info_format(pinfo, ack_ti, &ei_oran_acknack_no_request,
6296 | "Response for ackId=%u received, but no request found",
6297 | ackid);
6298 | }
6299 | }
6300 | }
6301 | for (unsigned int m=1; m <= number_of_nacks; m++) {
6302 | uint32_t nackid;
6303 | proto_item *nack_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_nackid, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &nackid);
6304 | offset += 2;
6305 |
6306 | expert_add_info_format(pinfo, nack_ti, &ei_oran_st8_nackid,
6307 | "Received Nack for ackNackId=%u",
6308 | nackid);
6309 |
6310 | /* Look up request table in state. */
6311 | if (state && state->ack_nack_requests) {
6312 | ack_nack_request_t *request = wmem_tree_lookup32(state->ack_nack_requests, nackid);
6313 | if (request) {
6314 | /* On first pass, update with this response */
6315 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
6316 | request->response_frame_number = pinfo->num;
6317 | request->response_frame_time = pinfo->abs_ts;
6318 | }
6319 |
6320 | /* Show request details */
6321 | show_link_to_acknack_request(section_tree, tvb, pinfo, request);
6322 | }
6323 | else {
6324 | /* Request not found */
6325 | expert_add_info_format(pinfo, nack_ti, &ei_oran_acknack_no_request,
6326 | "Response for nackId=%u received, but no request found",
6327 | nackid);
6328 | }
6329 | }
6330 | }
6331 | break;
6332 |
6333 | case SEC_C_SINR_REPORTING: /* Section Type 9 */
6334 | {
6335 | /* numSinrPerPrb (3 bits) */
6336 | proto_item *nspp_ti;
6337 | nspp_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_num_sinr_per_prb, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &num_sinr_per_prb);
6338 | switch (num_sinr_per_prb) {
6339 | case 0:
6340 | num_sinr_per_prb = 1; break;
6341 | case 1:
6342 | num_sinr_per_prb = 2; break;
6343 | case 2:
6344 | num_sinr_per_prb = 3; break;
6345 | case 3:
6346 | num_sinr_per_prb = 4; break;
6347 | case 4:
6348 | num_sinr_per_prb = 6; break;
6349 | case 5:
6350 | num_sinr_per_prb = 12; break;
6351 |
6352 | default:
6353 | proto_item_append_text(nspp_ti, " (invalid)");
6354 | num_sinr_per_prb = 1;
6355 | expert_add_info_format(pinfo, nspp_ti, &ei_oran_num_sinr_per_prb_unknown,
6356 | "Invalid numSinrPerPrb value (%u)",
6357 | num_sinr_per_prb);
6358 | }
6359 |
6360 | /* oruControlSinrSlotMaskId (5 bits) */
6361 | proto_tree_add_item(section_tree, hf_oran_oru_control_sinr_slot_mask_id, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6362 | offset += 1;
6363 | /* reserved (8 bits) */
6364 | add_reserved_field(section_tree, hf_oran_reserved_8bits, tvb, offset, 1);
6365 | offset += 1;
6366 | break;
6367 | }
6368 |
6369 | case SEC_C_RRM_MEAS_REPORTS: /* Section Type 10 */
6370 | case SEC_C_REQUEST_RRM_MEAS: /* Section Type 11 */
6371 | /* reserved (16 bits) */
6372 | add_reserved_field(section_tree, hf_oran_reserved_16bits, tvb, offset, 2);
6373 | offset += 2;
6374 | break;
6375 | };
6376 |
6377 | /* Update udCompHdr details in state for UL U-Plane */
6378 | if (state && direction==0) {
6379 | switch (sectionType) {
6380 | case SEC_C_NORMAL: /* Section Type 1 */
6381 | case SEC_C_PRACH: /* Section Type 3 */
6382 | case SEC_C_UE_SCHED: /* Section Type 5 */
6383 | state->ul_ud_comp_hdr_set = true1;
6384 | state->ul_ud_comp_hdr_bit_width = bit_width;
6385 | state->ul_ud_comp_hdr_compression = comp_meth;
6386 | state->ul_ud_comp_hdr_frame = pinfo->num;
6387 | break;
6388 | default:
6389 | break;
6390 | }
6391 | }
6392 |
6393 |
6394 | proto_item_append_text(sectionHeading, "%d, %s, frameId: %d, subframeId: %d, slotId: %d, startSymbolId: %d",
6395 | sectionType, val_to_str_const(direction, data_direction_vals, "Unknown"),
6396 | frameId, subframeId, slotId, startSymbolId);
6397 | if (nSections) {
6398 | proto_item_append_text(sectionHeading, ", numberOfSections=%u", nSections);
6399 | }
6400 |
6401 | write_pdu_label_and_info(protocol_item, NULL((void*)0), pinfo, ", Type: %2d %s", sectionType,
6402 | rval_to_str_const(sectionType, section_types_short, "Unknown"));
6403 |
6404 | /* Set actual length of C-Plane section header */
6405 | proto_item_set_len(section_tree, offset - section_tree_offset);
6406 |
6407 | if (sectionType == SEC_C_ACK_NACK_FEEDBACK) {
6408 | write_pdu_label_and_info(oran_tree, section_tree, pinfo,
6409 | (st8_ready) ? " (Ready)" : " (ACK)");
6410 | }
6411 |
6412 |
6413 | /* Section type 4 doesn't have normal sections, so deal with here before normal sections */
6414 | if (sectionType == SEC_C_SLOT_CONTROL) {
6415 | /* numberOfST4Cmds */
6416 | uint32_t no_st4_cmds, st4_cmd_len, num_slots, ack_nack_req_id, st4_cmd_type;
6417 | proto_item *no_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_number_of_st4_cmds,
6418 | tvb, offset, 1, ENC_NA0x00000000, &no_st4_cmds);
6419 | if (no_st4_cmds == 0) {
6420 | expert_add_info(pinfo, no_ti, &ei_oran_st4_no_cmds);
6421 | }
6422 | offset += 1;
6423 |
6424 | /* reserved (1 byte) */
6425 | add_reserved_field(section_tree, hf_oran_reserved_8bits, tvb, offset, 1);
6426 | offset += 1;
6427 |
6428 | /* Loop over commands. Each has 8-byte common header, followed by cmd-specific payload */
6429 | proto_item *len_ti;
6430 | for (uint32_t n=0; n < no_st4_cmds; n++) {
6431 | /* Table 7.4.6-2: Section Type 4 Command common header format */
6432 | proto_item *hdr_ti = proto_tree_add_string_format(section_tree, hf_oran_st4_cmd_header,
6433 | tvb, offset, 8, "",
6434 | "Type 4 Command common header");
6435 | proto_tree *hdr_tree = proto_item_add_subtree(hdr_ti, ett_oran_st4_cmd_header);
6436 |
6437 | /* st4CmdType */
6438 | proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_type, tvb, offset, 1, ENC_NA0x00000000, &st4_cmd_type);
6439 | offset += 1;
6440 |
6441 | /* st4CmdLen */
6442 | len_ti = proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_len, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &st4_cmd_len);
6443 | if (st4_cmd_len == 0) {
6444 | /* Meaning of 0 not yet defined (v15.00) */
6445 | proto_item_append_text(len_ti, " (reserved)");
6446 | expert_add_info(pinfo, len_ti, &ei_oran_st4_zero_len_cmd);
6447 | }
6448 | else {
6449 | proto_item_append_text(len_ti, " (%u bytes)", st4_cmd_len*4);
6450 | }
6451 | offset += 2;
6452 |
6453 | /* numSlots */
6454 | proto_item *slots_ti = proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_num_slots, tvb, offset, 1, ENC_NA0x00000000, &num_slots);
6455 | if (num_slots == 0) {
6456 | proto_item_append_text(slots_ti, " (until changed)");
6457 | }
6458 | offset += 1;
6459 |
6460 | /* ackNackReqId */
6461 | proto_item *ack_nack_req_id_ti;
6462 | ack_nack_req_id_ti = proto_tree_add_item_ret_uint(hdr_tree, hf_oran_st4_cmd_ack_nack_req_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ack_nack_req_id);
6463 | offset += 2;
6464 | if (ack_nack_req_id == 0) {
6465 | proto_item_append_text(ack_nack_req_id_ti, " (no Section type 8 response expected)");
6466 | }
6467 |
6468 | /* reserved (16 bits) */
6469 | add_reserved_field(hdr_tree, hf_oran_reserved_16bits, tvb, offset, 2);
6470 | offset += 2;
6471 |
6472 | /* Set common header summary */
6473 | proto_item_append_text(hdr_ti, " (cmd=%s, len=%u, slots=%u, ackNackReqId=%u)",
6474 | rval_to_str_const(st4_cmd_type, st4_cmd_type_vals, "Unknown"),
6475 | st4_cmd_len, num_slots, ack_nack_req_id);
6476 |
6477 | col_append_fstr(pinfo->cinfo, COL_INFO, " (%s)",
6478 | rval_to_str_const(st4_cmd_type, st4_cmd_type_vals, "Unknown"));
6479 |
6480 |
6481 | /* Subtree for this command body */
6482 | proto_item *command_ti = proto_tree_add_string_format(section_tree, hf_oran_st4_cmd,
6483 | tvb, offset, 0, "",
6484 | "Type 4 Command (%s)", rval_to_str_const(st4_cmd_type, st4_cmd_type_vals, "Unknown"));
6485 | proto_tree *command_tree = proto_item_add_subtree(command_ti, ett_oran_st4_cmd);
6486 |
6487 | unsigned command_start_offset = offset;
6488 |
6489 | /* Check fields compatible with chosen command. */
6490 | if (st4_cmd_type==1) {
6491 | if (num_slots != 0) {
6492 | /* "the value of numSlots should be set to zero for this command type" */
6493 | expert_add_info_format(pinfo, slots_ti, &ei_oran_numslots_not_zero,
6494 | "numSlots should be zero for ST4 command 1 - found %u",
6495 | num_slots);
6496 | }
6497 | }
6498 |
6499 | if (st4_cmd_type==3 || st4_cmd_type==4) {
6500 | if (startSymbolId != 0) {
6501 | /* "expected reception window for the commands is the symbol zero reception window" */
6502 | expert_add_info_format(pinfo, ssid_ti, &ei_oran_start_symbol_id_not_zero,
6503 | "startSymbolId should be zero for ST4 commands 3&4 - found %u",
6504 | startSymbolId);
6505 | }
6506 | }
6507 |
6508 | /* Add format for this command */
6509 | switch (st4_cmd_type) {
6510 | case 1: /* TIME_DOMAIN_BEAM_CONFIG */
6511 | {
6512 | bool_Bool disable_tdbfns;
6513 | uint32_t bfwcomphdr_iq_width, bfwcomphdr_comp_meth;
6514 |
6515 | /* Hidden filter for bf */
6516 | proto_item *bf_ti = proto_tree_add_item(command_tree, hf_oran_bf, tvb, 0, 0, ENC_NA0x00000000);
6517 | PROTO_ITEM_SET_HIDDEN(bf_ti)proto_item_set_hidden((bf_ti));
6518 |
6519 | /* reserved (2 bits) */
6520 | add_reserved_field(command_tree, hf_oran_reserved_2bits, tvb, offset, 1);
6521 | /* symbolMask (14 bits) */
6522 | uint32_t symbol_mask;
6523 | proto_item *symbol_mask_ti;
6524 | offset = dissect_symbolmask(tvb, command_tree, offset, &symbol_mask, &symbol_mask_ti);
6525 | /* Symbol bits before 'startSymbolId' in Section Type 4 common header should be set to 0 by O-DU and shall be ignored by O-RU */
6526 | /* lsb is symbol 0 */
6527 | for (unsigned s=0; s < 14; s++) {
6528 | if ((startSymbolId & (1 << s)) && (startSymbolId > s)) {
6529 | proto_item_append_text(symbol_mask_ti, " (startSymbolId is %u, so some lower symbol bits ignored!)", startSymbolId);
6530 | expert_add_info(pinfo, symbol_mask_ti, &ei_oran_start_symbol_id_bits_ignored);
6531 | break;
6532 | }
6533 | }
6534 |
6535 | /* disableTDBFNs (1 bit) */
6536 | proto_tree_add_item_ret_boolean(command_tree, hf_oran_disable_tdbfns, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disable_tdbfns);
6537 |
6538 | /* tdBeamNum (15 bits) */
6539 | proto_tree_add_item(command_tree, hf_oran_td_beam_num, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6540 | offset += 2;
6541 |
6542 | /* bfwCompHdr (2 subheaders - bfwIqWidth and bfwCompMeth)*/
6543 | offset = dissect_bfwCompHdr(tvb, command_tree, offset,
6544 | &bfwcomphdr_iq_width, &bfwcomphdr_comp_meth, &comp_meth_ti);
6545 | /* reserved (3 bytes) */
6546 | proto_tree_add_bits_item(command_tree, hf_oran_reserved, tvb, offset*8, 24, ENC_BIG_ENDIAN0x00000000);
6547 | offset += 3;
6548 |
6549 | if (disable_tdbfns) {
6550 | /* No beamnum information to show so get out. */
6551 | break;
6552 | }
6553 |
6554 | /* Read beam entries until reach end of command length */
6555 | while ((offset - command_start_offset) < (st4_cmd_len * 4)) {
6556 |
6557 | /* disableTDBFWs (1 bit) */
6558 | bool_Bool disable_tdbfws;
6559 | proto_tree_add_item_ret_boolean(command_tree, hf_oran_disable_tdbfws, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &disable_tdbfws);
6560 |
6561 | /* tdBeamNum (15 bits) */
6562 | proto_tree_add_item(command_tree, hf_oran_td_beam_num, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6563 | offset += 2;
6564 |
6565 | /* Showing BFWs? */
6566 | if (!disable_tdbfws) {
6567 |
6568 | /* bfwCompParam */
6569 | unsigned exponent = 0;
6570 | bool_Bool supported = false0;
6571 | unsigned num_trx_entries;
6572 | uint16_t *trx_entries;
6573 | offset = dissect_bfwCompParam(tvb, command_tree, pinfo, offset, comp_meth_ti,
6574 | &bfwcomphdr_comp_meth, &exponent, &supported,
6575 | &num_trx_entries, &trx_entries);
6576 |
6577 | /* Antenna count from preference */
6578 | unsigned num_trx = pref_num_bf_antennas;
6579 | int bit_offset = offset*8;
6580 |
6581 | for (unsigned trx=0; trx < num_trx; trx++) {
6582 | /* Create antenna subtree */
6583 | int bfw_offset = bit_offset / 8;
6584 | proto_item *bfw_ti = proto_tree_add_string_format(command_tree, hf_oran_bfw,
6585 | tvb, bfw_offset, 0, "", "TRX %3u: (", trx);
6586 | proto_tree *bfw_tree = proto_item_add_subtree(bfw_ti, ett_oran_bfw);
6587 |
6588 | /* I value */
6589 | /* Get bits, and convert to float. */
6590 | uint32_t bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
6591 | float value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent, NULL((void*)0) /* no ModCompr*/, 0 /* RE */);
6592 | /* Add to tree. */
6593 | proto_tree_add_float(bfw_tree, hf_oran_bfw_i, tvb, bit_offset/8,
6594 | (bfwcomphdr_iq_width+7)/8, value);
6595 | bit_offset += bfwcomphdr_iq_width;
6596 | proto_item_append_text(bfw_ti, "I=%f ", value);
6597 |
6598 | /* Leave a gap between I and Q values */
6599 | proto_item_append_text(bfw_ti, " ");
6600 |
6601 | /* Q value */
6602 | /* Get bits, and convert to float. */
6603 | bits = tvb_get_bits32(tvb, bit_offset, bfwcomphdr_iq_width, ENC_BIG_ENDIAN0x00000000);
6604 | value = decompress_value(bits, bfwcomphdr_comp_meth, bfwcomphdr_iq_width, exponent, NULL((void*)0) /* no ModCompr*/, 0 /* RE */);
6605 | /* Add to tree. */
6606 | proto_tree_add_float(bfw_tree, hf_oran_bfw_q, tvb, bit_offset/8,
6607 | (bfwcomphdr_iq_width+7)/8, value);
6608 | bit_offset += bfwcomphdr_iq_width;
6609 | proto_item_append_text(bfw_ti, "Q=%f", value);
6610 |
6611 | proto_item_append_text(bfw_ti, ")");
6612 | proto_item_set_len(bfw_ti, (bit_offset+7)/8 - bfw_offset);
6613 | }
6614 | /* Need to round to next byte */
6615 | offset = (bit_offset+7)/8;
6616 | }
6617 | }
6618 | break;
6619 | }
6620 | case 2: /* TDD_CONFIG_PATTERN */
6621 | /* reserved (2 bits) */
6622 | add_reserved_field(command_tree, hf_oran_reserved_2bits, tvb, offset, 1);
6623 | /* dirPattern (14 bits) */
6624 | proto_tree_add_item(command_tree, hf_oran_dir_pattern, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6625 | offset += 2;
6626 |
6627 | /* reserved (2 bits) */
6628 | add_reserved_field(command_tree, hf_oran_reserved_2bits, tvb, offset, 1);
6629 | /* guardPattern (14 bits) */
6630 | proto_tree_add_item(command_tree, hf_oran_guard_pattern, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6631 | offset += 2;
6632 | break;
6633 |
6634 | case 3: /* TRX_CONTROL */
6635 | case 5: /* TRX_CONTROL_BIDIR */
6636 | {
6637 | /* Only allowed cmdScope is ARRAY-COMMAND */
6638 | if (cmd_scope != 0) {
6639 | expert_add_info(pinfo, command_tree, &ei_oran_trx_control_cmd_scope);
6640 | }
6641 |
6642 | /* reserved (2 bits) */
6643 | add_reserved_field(command_tree, hf_oran_reserved_2bits, tvb, offset, 1);
6644 | /* log2MaskBits (4 bits) */
6645 | unsigned log2maskbits;
6646 | proto_tree_add_item_ret_uint(command_tree, hf_oran_log2maskbits, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &log2maskbits);
6647 | /* sleepMode (2 bits) */
6648 | uint32_t sleep_mode;
6649 | proto_tree_add_item_ret_uint(command_tree, hf_oran_sleepmode_trx, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &sleep_mode);
6650 | offset += 1;
6651 |
6652 | /* reserved (4 bits) */
6653 | add_reserved_field(command_tree, hf_oran_reserved_4bits, tvb, offset, 1);
6654 | /* numSlotsExt (20 bits) */
6655 | uint32_t num_slots_ext;
6656 | proto_item *num_slots_ext_ti = proto_tree_add_item_ret_uint(command_tree, hf_oran_num_slots_ext, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000, &num_slots_ext);
6657 | if (num_slots==0 && num_slots_ext==0) {
6658 | proto_item_append_text(num_slots_ext_ti, " (undefined sleep period)");
6659 | }
6660 | else {
6661 | /* Time should be rounded up according to SCS */
6662 | float total = (float)(num_slots + num_slots_ext);
6663 | /* From table 7.5.2.13-3 */
6664 | const float slot_length_by_scs[16] = { 1000, 500, 250, 125, 62.5, 31.25,
6665 | 0, 0, 0, 0, 0, 0, /* reserved */
6666 | 1000, 1000, 1000, 1000 };
6667 | float slot_length = slot_length_by_scs[scs];
6668 | /* Only using valid SCS. TODO: is this test ok? */
6669 | if (slot_length != 0) {
6670 | /* Round up to next slot */
6671 | total = ((int)(total / slot_length) + 1) * slot_length;
6672 | proto_item_append_text(num_slots_ext_ti, " (defined sleep period of %f us)", total);
6673 | }
6674 | }
6675 | offset += 3;
6676 |
6677 | /* reserved (2 bits) */
6678 | add_reserved_field(command_tree, hf_oran_reserved_2bits, tvb, offset, 1);
6679 |
6680 | /* symbolMask (14 bits) */
6681 | uint32_t symbol_mask;
6682 | proto_item *sm_ti;
6683 | offset = dissect_symbolmask(tvb, command_tree, offset, &symbol_mask, &sm_ti);
6684 | if (symbol_mask == 0x0) {
6685 | proto_item_append_text(sm_ti, " (wake)");
6686 | col_append_str(pinfo->cinfo, COL_INFO, " (wake)");
6687 | }
6688 | else if (symbol_mask == 0x3fff) {
6689 | proto_item_append_text(sm_ti, " (sleep)");
6690 | col_append_str(pinfo->cinfo, COL_INFO, " (sleep)");
6691 | }
6692 | else {
6693 | expert_add_info_format(pinfo, sm_ti, &ei_oran_bad_symbolmask,
6694 | "For non-zero sleepMode (%u), symbolMask should be 0x0 or 0x3fff - found 0x%05x",
6695 | sleep_mode, symbol_mask);
6696 | }
6697 | offset += 2;
6698 |
6699 | /* antMask (16-2048 bits). Size is lookup from log2MaskBits enum.. */
6700 | unsigned antmask_length = 2;
6701 | if (log2maskbits >= 4) {
6702 | antmask_length = (1 << log2maskbits) / 8;
6703 | }
6704 | proto_item *ant_mask_ti = proto_tree_add_item(command_tree, hf_oran_antMask_trx_control, tvb, offset, antmask_length, ENC_NA0x00000000);
6705 | /* show count */
6706 | unsigned antenna_count = 0;
6707 | for (unsigned b=0; b < antmask_length; b++) {
6708 | uint8_t byte = tvb_get_uint8(tvb, offset+b);
6709 | for (unsigned bit=0; bit < 8; bit++) {
6710 | if ((1 << bit) & byte) {
6711 | antenna_count++;
6712 | }
6713 | }
6714 | }
6715 | proto_item_append_text(ant_mask_ti, " (%u antennas)", antenna_count);
6716 | offset += antmask_length;
6717 |
6718 | /* Pad to next 4-byte boundary */
6719 | offset = WS_ROUNDUP_4(offset)(((offset) + ((unsigned)(4U-1U))) & (~((unsigned)(4U-1U)) ));
6720 | break;
6721 | }
6722 |
6723 | case 4: /* ASM (advanced sleep mode) */
6724 | /* reserved (2+4=6 bits) */
6725 | add_reserved_field(command_tree, hf_oran_reserved_6bits, tvb, offset, 1);
6726 | /* sleepMode (2 bits) */
6727 | uint32_t sleep_mode;
6728 | proto_tree_add_item_ret_uint(command_tree, hf_oran_sleepmode_asm, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &sleep_mode);
6729 | offset += 1;
6730 |
6731 | /* reserved (4 bits) */
6732 | add_reserved_field(command_tree, hf_oran_reserved_4bits, tvb, offset, 1);
6733 | /* numSlotsExt (20 bits) */
6734 | proto_tree_add_item(command_tree, hf_oran_num_slots_ext, tvb, offset, 3, ENC_BIG_ENDIAN0x00000000);
6735 | offset += 3;
6736 |
6737 | /* reserved (2 bits) */
6738 | add_reserved_field(command_tree, hf_oran_reserved_2bits, tvb, offset, 1);
6739 | /* symbolMask (14 bits) */
6740 | uint32_t symbol_mask;
6741 | proto_item *sm_ti;
6742 | offset = dissect_symbolmask(tvb, command_tree, offset, &symbol_mask, &sm_ti);
6743 | if (symbol_mask == 0x0) {
6744 | proto_item_append_text(sm_ti, " (wake)");
6745 | col_append_str(pinfo->cinfo, COL_INFO, " (wake)");
6746 | }
6747 | else if (symbol_mask == 0x3fff) {
6748 | proto_item_append_text(sm_ti, " (sleep)");
6749 | col_append_str(pinfo->cinfo, COL_INFO, " (sleep)");
6750 | }
6751 | else {
6752 | expert_add_info_format(pinfo, sm_ti, &ei_oran_bad_symbolmask,
6753 | "For non-zero sleepMode (%u), symbolMask should be 0x0 or 0x3fff - found 0x%05x",
6754 | sleep_mode, symbol_mask);
6755 | }
6756 | offset += 2;
6757 |
6758 | /* reserved (2 bytes) */
6759 | add_reserved_field(command_tree, hf_oran_reserved_16bits, tvb, offset, 2);
6760 | offset += 2;
6761 | break;
6762 |
6763 | default:
6764 | /* Error! */
6765 | expert_add_info_format(pinfo, len_ti, &ei_oran_st4_unknown_cmd,
6766 | "Dissected ST4 command (%u) not recognised",
6767 | st4_cmd_type);
6768 | break;
6769 | }
6770 |
6771 | /* Check apparent size of padding (0-3 bytes ok) */
6772 | long padding_remaining = command_start_offset + (st4_cmd_len * 4) - offset;
6773 | if (padding_remaining > 3) {
6774 | expert_add_info_format(pinfo, len_ti, &ei_oran_st4_wrong_len_cmd,
6775 | "Dissected ST4 command does not match signalled st4CmdLen - set to %u (%u bytes) but dissected %u bytes",
6776 | st4_cmd_len, st4_cmd_len*4, offset-command_start_offset);
6777 | }
6778 |
6779 | /* Advance by signalled length (needs to be aligned on 4-byte boundary) */
6780 | offset = command_start_offset + (st4_cmd_len * 4);
6781 |
6782 | /* Set end of command tree */
6783 | proto_item_set_end(command_ti, tvb, offset);
6784 |
6785 | if (ack_nack_req_id != 0 && state && state->ack_nack_requests) {
6786 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
6787 | /* Add this request into conversation state on first pass */
6788 | ack_nack_request_t *request_details = wmem_new0(wmem_file_scope(), ack_nack_request_t)((ack_nack_request_t*)wmem_alloc0((wmem_file_scope()), sizeof (ack_nack_request_t)));
6789 | request_details->request_frame_number = pinfo->num;
6790 | request_details->request_frame_time = pinfo->abs_ts;
6791 | request_details->requestType = ST4Cmd1+st4_cmd_type-1;
6792 |
6793 | wmem_tree_insert32(state->ack_nack_requests,
6794 | ack_nack_req_id,
6795 | request_details);
6796 | }
6797 | else {
6798 | /* On later passes, try to link forward to ST8 response */
6799 | ack_nack_request_t *response = wmem_tree_lookup32(state->ack_nack_requests,
6800 | ack_nack_req_id);
6801 | if (response) {
6802 | show_link_to_acknack_response(section_tree, tvb, pinfo, response);
6803 | }
6804 | }
6805 | }
6806 | }
6807 | }
6808 | /* LAA doesn't have sections either.. */
6809 | else if (sectionType == SEC_C_LAA) { /* Section Type 7 */
6810 | /* 7.2.5 Table 6.4-6 */
6811 | unsigned mcot;
6812 | proto_item *mcot_ti;
6813 |
6814 | /* laaMsgType */
6815 | uint32_t laa_msg_type;
6816 | proto_item *laa_msg_type_ti;
6817 | laa_msg_type_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_laaMsgType, tvb, offset, 1, ENC_NA0x00000000, &laa_msg_type);
6818 | /* laaMsgLen */
6819 | uint32_t laa_msg_len;
6820 | proto_item *len_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_laaMsgLen, tvb, offset, 1, ENC_NA0x00000000, &laa_msg_len);
6821 | proto_item_append_text(len_ti, " (%u bytes)", 4*laa_msg_len);
6822 | if (laa_msg_len == 0) {
6823 | proto_item_append_text(len_ti, " (reserved)");
6824 | }
6825 | offset += 1;
6826 |
6827 | int payload_offset = offset;
6828 |
6829 | /* Payload */
6830 | switch (laa_msg_type) {
6831 | case 0:
6832 | /* LBT_PDSCH_REQ */
6833 | /* lbtHandle (16 bits) */
6834 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6835 | offset += 2;
6836 | /* lbtOffset (10 bits) */
6837 | proto_tree_add_item(section_tree, hf_oran_lbtOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6838 | offset += 1;
6839 | /* lbtMode (2 bits) */
6840 | proto_tree_add_bits_item(section_tree, hf_oran_lbtMode, tvb, offset*8+2, 2, ENC_BIG_ENDIAN0x00000000);
6841 | /* reserved (1 bit) */
6842 | add_reserved_field(section_tree, hf_oran_reserved_bit4, tvb, offset, 1);
6843 | /* lbtDeferFactor (3 bits) */
6844 | proto_tree_add_item(section_tree, hf_oran_lbtDeferFactor, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6845 | offset += 1;
6846 | /* lbtBackoffCounter (10 bits) */
6847 | proto_tree_add_item(section_tree, hf_oran_lbtBackoffCounter, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6848 | offset += 1;
6849 | /* MCOT (4 bits) */
6850 | mcot_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_MCOT, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000, &mcot);
6851 | if (mcot<1 || mcot>10) {
6852 | proto_item_append_text(mcot_ti, " (should be in range 1-10!)");
6853 | expert_add_info_format(pinfo, mcot_ti, &ei_oran_mcot_out_of_range,
6854 | "MCOT seen with value %u (must be 1-10)", mcot);
6855 |
6856 | }
6857 | /* reserved (10 bits) */
6858 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8)+6, 10, ENC_BIG_ENDIAN0x00000000);
6859 | break;
6860 | case 1:
6861 | /* LBT_DRS_REQ */
6862 | /* lbtHandle (16 bits) */
6863 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6864 | offset += 2;
6865 | /* lbtOffset (10 bits) */
6866 | proto_tree_add_item(section_tree, hf_oran_lbtOffset, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6867 | offset += 1;
6868 | /* lbtMode (2 bits) */
6869 | proto_tree_add_bits_item(section_tree, hf_oran_lbtMode, tvb, offset*8+2, 2, ENC_BIG_ENDIAN0x00000000);
6870 | /* reserved (28 bits) */
6871 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8)+4, 28, ENC_BIG_ENDIAN0x00000000);
6872 | break;
6873 | case 2:
6874 | /* LBT_PDSCH_RSP */
6875 | /* lbtHandle (16 bits) */
6876 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6877 | offset += 2;
6878 | /* lbtPdschRes (2 bits) */
6879 | proto_tree_add_item(section_tree, hf_oran_lbtPdschRes, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6880 | /* inParSF (1 bit) */
6881 | proto_tree_add_item(section_tree, hf_oran_initialPartialSF, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6882 | /* sfStatus (1 bit) */
6883 | proto_tree_add_item(section_tree, hf_oran_sfStatus, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6884 | /* sfnSf (12 bits) */
6885 | proto_tree_add_item(section_tree, hf_oran_sfnSfEnd, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6886 | offset += 2;
6887 | /* reserved (24 bits) */
6888 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8), 24, ENC_BIG_ENDIAN0x00000000);
6889 | break;
6890 | case 3:
6891 | /* LBT_DRS_RSP */
6892 | /* lbtHandle (16 bits) */
6893 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6894 | offset += 2;
6895 | /* lbtDrsRes (1 bit) */
6896 | proto_tree_add_item(section_tree, hf_oran_lbtDrsRes, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6897 | /* reserved (7 bits) */
6898 | add_reserved_field(section_tree, hf_oran_reserved_last_7bits, tvb, offset, 1);
6899 | break;
6900 | case 4:
6901 | /* LBT_Buffer_Error */
6902 | /* lbtHandle (16 bits) */
6903 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6904 | offset += 2;
6905 | /* lbtBufErr (1 bit) */
6906 | proto_tree_add_item(section_tree, hf_oran_lbtBufErr, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6907 | /* reserved (7 bits) */
6908 | add_reserved_field(section_tree, hf_oran_reserved_last_7bits, tvb, offset, 1);
6909 | break;
6910 | case 5:
6911 | /* LBT_CWCONFIG_REQ */
6912 | /* lbtHandle (16 bits) */
6913 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6914 | offset += 2;
6915 | /* lbtCWConfig_H (8 bits) */
6916 | proto_tree_add_item(section_tree, hf_oran_lbtCWConfig_H, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6917 | offset += 1;
6918 | /* lbtCWConfig_T (8 bits) */
6919 | proto_tree_add_item(section_tree, hf_oran_lbtCWConfig_T, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6920 | offset += 1;
6921 | /* lbtMode (2 bits) */
6922 | proto_tree_add_bits_item(section_tree, hf_oran_lbtMode, tvb, offset*8, 2, ENC_BIG_ENDIAN0x00000000);
6923 | /* lbtTrafficClass (3 bits) */
6924 | proto_tree_add_item(section_tree, hf_oran_lbtTrafficClass, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6925 | /* reserved (19 bits) */
6926 | proto_tree_add_bits_item(section_tree, hf_oran_reserved, tvb, (offset*8)+5, 19, ENC_BIG_ENDIAN0x00000000);
6927 | break;
6928 | case 6:
6929 | /* LBT_CWCONFIG_RSP */
6930 | /* lbtHandle (16 bits) */
6931 | proto_tree_add_item(section_tree, hf_oran_lbtHandle, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000);
6932 | offset += 2;
6933 | /* lbtCWR_Rst (1 bit) */
6934 | proto_tree_add_item(section_tree, hf_oran_lbtCWR_Rst, tvb, offset, 1, ENC_BIG_ENDIAN0x00000000);
6935 | /* reserved (7 bits) */
6936 | add_reserved_field(section_tree, hf_oran_reserved_last_7bits, tvb, offset, 1);
6937 | break;
6938 |
6939 | default:
6940 | /* Unhandled! */
6941 | expert_add_info_format(pinfo, laa_msg_type_ti, &ei_oran_laa_msg_type_unsupported,
6942 | "laaMsgType %u not supported by dissector",
6943 | laa_msg_type);
6944 |
6945 | break;
6946 | }
6947 | /* For now just skip indicated length of bytes */
6948 | offset = payload_offset + 4*(laa_msg_len+1);
6949 | }
6950 |
6951 |
6952 | /* Dissect each C section */
6953 | for (uint32_t i = 0; i < nSections; ++i) {
6954 | tvbuff_t *section_tvb = tvb_new_subset_remaining(tvb, offset);
6955 | offset += dissect_oran_c_section(section_tvb, oran_tree, pinfo, state, sectionType, tap_info,
6956 | protocol_item,
6957 | subframeId, frameId, slotId, startSymbolId,
6958 | bit_width, ci_comp_method, ci_comp_opt,
6959 | num_sinr_per_prb);
6960 | }
6961 |
6962 | /* Expert error if we are short of tvb by > 3 bytes */
6963 | if (tvb_reported_length_remaining(tvb, offset) > 3) {
6964 | expert_add_info_format(pinfo, protocol_item, &ei_oran_frame_length,
6965 | "%u bytes remain at end of frame - should be 0-3",
6966 | tvb_reported_length_remaining(tvb, offset));
6967 | }
6968 |
6969 | if (PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited) && result) {
6970 | /* Show list of frames that have corresponding U-plane data */
6971 | wmem_list_frame_t *list_frame;
6972 | for (list_frame = wmem_list_head(result->u_plane_frames); list_frame != NULL((void*)0); list_frame = wmem_list_frame_next(list_frame)) {
6973 | corresponding_uplane_frame *frame = wmem_list_frame_data(list_frame);
6974 | proto_item *uplane_frame_ti = proto_tree_add_uint(oran_tree, hf_oran_corresponding_uplane_frame, tvb, 0, 0,
6975 | frame->frame_number);
6976 | proto_item_append_text(uplane_frame_ti, " sectionId:%2u symbol:%2u PRBs %3u->%3u (in %uus)",
6977 | frame->sectionId, frame->symbol, frame->startPrbu, frame->startPrbu+frame->numPrbu-1, frame->gap_in_usecs);
6978 | proto_item_set_generated(uplane_frame_ti);
6979 | }
6980 | /* Also show total number of corresponding u-plane frames */
6981 | proto_item *uplane_frame_count_ti = proto_tree_add_uint(oran_tree, hf_oran_corresponding_uplane_frames_total, tvb, 0, 0,
6982 | wmem_list_count(result->u_plane_frames));
6983 | proto_item_set_generated(uplane_frame_count_ti);
6984 | }
6985 |
6986 | return tvb_captured_length(tvb);
6987 | }
6988 |
6989 | static int dissect_oran_u_re(tvbuff_t *tvb, proto_tree *tree,
6990 | unsigned sample_number, int samples_offset,
6991 | oran_tap_info *tap_info,
6992 | unsigned sample_bit_width,
6993 | int comp_meth,
6994 | uint32_t exponent,
6995 | section_mod_compr_config_t *mod_compr_params,
6996 | uint8_t re)
6997 | {
6998 | /* I */
6999 | unsigned i_bits = tvb_get_bits32(tvb, samples_offset, sample_bit_width, ENC_BIG_ENDIAN0x00000000);
7000 | float i_value = decompress_value(i_bits, comp_meth, sample_bit_width, exponent, mod_compr_params, re);
7001 | unsigned sample_len_in_bytes = ((samples_offset%8)+sample_bit_width+7)/8;
7002 | proto_item *i_ti = proto_tree_add_float(tree, hf_oran_iSample, tvb, samples_offset/8, sample_len_in_bytes, i_value);
7003 | proto_item_set_text(i_ti, "iSample: % 0.7f 0x%04x (RE-%2u in the PRB)", i_value, i_bits, sample_number);
7004 | samples_offset += sample_bit_width;
7005 | /* Q */
7006 | unsigned q_bits = tvb_get_bits32(tvb, samples_offset, sample_bit_width, ENC_BIG_ENDIAN0x00000000);
7007 | float q_value = decompress_value(q_bits, comp_meth, sample_bit_width, exponent, mod_compr_params, re);
7008 | sample_len_in_bytes = ((samples_offset%8)+sample_bit_width+7)/8;
7009 | proto_item *q_ti = proto_tree_add_float(tree, hf_oran_qSample, tvb, samples_offset/8, sample_len_in_bytes, q_value);
7010 | proto_item_set_text(q_ti, "qSample: % 0.7f 0x%04x (RE-%2u in the PRB)", q_value, q_bits, sample_number);
7011 | samples_offset += sample_bit_width;
7012 |
7013 | /* Update RE stats */
7014 | tap_info->num_res++;
7015 | /* if (i_value == 0.0 && q_value == 0.0) { */
7016 | /* TODO: is just checking bits from frame good enough - assuming this always corresponds to a zero value? */
7017 | if (i_bits == 0 && q_bits == 0) {
7018 | tap_info->num_res_zero++;
7019 | }
7020 | else {
7021 | tap_info->non_zero_re_in_current_prb = true1;
7022 | }
7023 | return samples_offset;
7024 | }
7025 |
7026 |
7027 | static bool_Bool udcomplen_appears_present(bool_Bool udcomphdr_present, tvbuff_t *tvb, int offset)
7028 | {
7029 | if (!udcomplen_heuristic_result_set) {
7030 | /* All sections will start the same way */
7031 | unsigned int section_bytes_before_field = (udcomphdr_present) ? 6 : 4;
7032 |
7033 | /* Move offset back to the start of the section */
7034 | offset -= section_bytes_before_field;
7035 |
7036 | do {
7037 | /* This field appears several bytes into the U-plane section */
7038 | uint32_t length_remaining = tvb_reported_length_remaining(tvb, offset);
7039 | /* Are there enough bytes to still read the length field? */
7040 | if (section_bytes_before_field+2 > length_remaining) {
7041 | udcomplen_heuristic_result = false0;
7042 | udcomplen_heuristic_result_set = true1;
7043 | break;
7044 | }
7045 |
7046 | /* Read the length field */
7047 | uint16_t udcomplen = tvb_get_ntohs(tvb, offset+section_bytes_before_field);
7048 |
7049 | /* Is this less than a valid section? Realistic minimal section will be bigger than this..
7050 | * Could take into account numPrbU, etc */
7051 | if (udcomplen < section_bytes_before_field+2) {
7052 | udcomplen_heuristic_result = false0;
7053 | udcomplen_heuristic_result_set = true1;
7054 | break;
7055 | }
7056 |
7057 | /* Does this section fit into the frame? */
7058 | if (udcomplen > length_remaining) {
7059 | udcomplen_heuristic_result = false0;
7060 | udcomplen_heuristic_result_set = true1;
7061 | break;
7062 | }
7063 |
7064 | /* Move past this section */
7065 | offset += udcomplen;
7066 |
7067 | /* Are we at the end of the frame? */
7068 | /* TODO: if frame is less than 60 bytes, there may be > 4 bytes, likely zeros.. */
7069 | if (tvb_reported_length_remaining(tvb, offset) < 4) {
7070 | udcomplen_heuristic_result = true1;
7071 | udcomplen_heuristic_result_set = true1;
7072 | }
7073 | } while (!udcomplen_heuristic_result_set);
7074 | }
7075 | return udcomplen_heuristic_result;
7076 | }
7077 |
7078 | static bool_Bool at_udcomphdr(tvbuff_t *tvb, int offset)
7079 | {
7080 | if (tvb_captured_length_remaining(tvb, offset) < 2) {
7081 | return false0;
7082 | }
7083 | uint8_t first_byte = tvb_get_uint8(tvb, offset);
7084 | uint8_t reserved_byte = tvb_get_uint8(tvb, offset+1);
7085 |
7086 | /* - iq width could be anything, though unlikely to be signalled as (say) < 1-3? */
7087 | /* - meth should be 0-8 */
7088 | /* - reserved byte should be 0 */
7089 | return (((first_byte & 0x0f) <= MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8) && (reserved_byte == 0));
7090 | }
7091 |
7092 | static bool_Bool udcomphdr_appears_present(flow_state_t *flow, uint32_t direction, tvbuff_t *tvb, int offset)
7093 | {
7094 | /* Should really not happen, but guard against this anyway. */
7095 | if (flow == NULL((void*)0)) {
7096 | /* No state to update. */
7097 | return false0;
7098 | }
7099 |
7100 | if (direction == DIR_UPLINK0) {
7101 | if (flow->udcomphdrUplink_heuristic_result_set) {
7102 | /* Return cached value */
7103 | return flow->udcomphdrUplink_heuristic_result;
7104 | }
7105 | else {
7106 | /* Work it out, and save answer for next time */
7107 | flow->udcomphdrUplink_heuristic_result_set = true1;
7108 | flow->udcomphdrUplink_heuristic_result = at_udcomphdr(tvb, offset);
7109 | return flow->udcomphdrUplink_heuristic_result;
7110 | }
7111 | }
7112 | else {
7113 | /* Downlink */
7114 | if (flow->udcomphdrDownlink_heuristic_result_set) {
7115 | /* Return cached value */
7116 | return flow->udcomphdrDownlink_heuristic_result;
7117 | }
7118 | else {
7119 | /* Work it out, and save answer for next time */
7120 | flow->udcomphdrDownlink_heuristic_result_set = true1;
7121 | flow->udcomphdrDownlink_heuristic_result = at_udcomphdr(tvb, offset);
7122 | return flow->udcomphdrDownlink_heuristic_result;
7123 | }
7124 | }
7125 | }
7126 |
7127 | static bool_Bool copy_section_entry(const void *key, void* value, void *userdata)
7128 | {
7129 | /* Cast parameters to their types */
7130 | uint32_t sectionId = GPOINTER_TO_UINT(key)((guint) (gulong) (key));
7131 | expected_section_data_t *result_value = (expected_section_data_t *)value;
7132 | wmem_tree_t *result_tree = (wmem_tree_t*)userdata;
7133 |
7134 | /* Deep copy of section data */
7135 | expected_section_data_t *copy = wmem_new0(wmem_file_scope(), expected_section_data_t)((expected_section_data_t*)wmem_alloc0((wmem_file_scope()), sizeof (expected_section_data_t)));
7136 | *copy = *result_value;
7137 |
7138 | /* Add into result tree */
7139 | wmem_tree_insert32(result_tree, sectionId, copy);
7140 |
7141 | return false0;
7142 | }
7143 |
7144 | /* User plane dissector (section 8) */
7145 | static int
7146 | dissect_oran_u(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree,
7147 | oran_tap_info *tap_info, void *data _U___attribute__((unused)))
7148 | {
7149 | /* Hidden filter for plane */
7150 | proto_item *plane_ti = proto_tree_add_item(tree, hf_oran_uplane, tvb, 0, 0, ENC_NA0x00000000);
7151 | PROTO_ITEM_SET_HIDDEN(plane_ti)proto_item_set_hidden((plane_ti));
7152 |
7153 | /* Set up structures needed to add the protocol subtree and manage it */
7154 | unsigned offset = 0;
7155 |
7156 | col_set_str(pinfo->cinfo, COL_PROTOCOL, "O-RAN-FH-U");
7157 | col_set_str(pinfo->cinfo, COL_INFO, "U-Plane");
7158 |
7159 | tap_info->userplane = true1;
7160 |
7161 | /* Create display subtree for the protocol */
7162 | proto_item *protocol_item = proto_tree_add_item(tree, proto_oran, tvb, 0, -1, ENC_NA0x00000000);
7163 | proto_item_append_text(protocol_item, "-U");
7164 | proto_tree *oran_tree = proto_item_add_subtree(protocol_item, ett_oran);
7165 |
7166 | /* Transport header */
7167 | /* Real-time control data / IQ data transfer message series identifier */
7168 | uint16_t eAxC;
7169 | addPcOrRtcid(tvb, oran_tree, &offset, hf_oran_ecpri_pcid, &eAxC, tap_info);
7170 | tap_info->eaxc = eAxC;
7171 |
7172 | /* Update/report status of conversation */
7173 | uint32_t key = make_flow_key(pinfo, eAxC, ORAN_U_PLANE1, false0);
7174 | flow_state_t* state = (flow_state_t*)wmem_tree_lookup32(flow_states_table, key);
7175 |
7176 | flow_result_t *result = NULL((void*)0);
7177 |
7178 | /* Message identifier */
7179 | proto_item *seqIdItem;
7180 | uint32_t seqId, subSeqId, e;
7181 | offset = addSeqid(tvb, oran_tree, offset, ORAN_U_PLANE1, &seqId, &seqIdItem, pinfo, &subSeqId, &e);
7182 |
7183 | /* Common header for time reference */
7184 | proto_item *timingHeader = proto_tree_add_string_format(oran_tree, hf_oran_timing_header,
7185 | tvb, offset, 4, "", "Timing Header (");
7186 | proto_tree *timing_header_tree = proto_item_add_subtree(timingHeader, ett_oran_u_timing);
7187 |
7188 | /* dataDirection */
7189 | uint32_t direction;
7190 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_data_direction, tvb, offset, 1, ENC_NA0x00000000, &direction);
7191 | tap_info->uplink = (direction==0);
1 | Assuming 'direction' is not equal to 0 | →
7192 | /* payloadVersion */
7193 | dissect_payload_version(timing_header_tree, tvb, pinfo, offset);
7194 | /* filterIndex */
7195 | proto_tree_add_item(timing_header_tree, hf_oran_filter_index, tvb, offset, 1, ENC_NA0x00000000);
7196 | offset += 1;
7197 |
7198 | int ref_a_offset = offset;
7199 |
7200 | /* frameId */
7201 | uint32_t frameId = 0;
7202 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_frame_id, tvb, offset, 1, ENC_NA0x00000000, &frameId);
7203 | tap_info->frame = frameId;
7204 | offset += 1;
7205 |
7206 | /* subframeId */
7207 | uint32_t subframeId = 0;
7208 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_subframe_id, tvb, offset, 1, ENC_NA0x00000000, &subframeId);
7209 | /* slotId */
7210 | uint32_t slotId = 0;
7211 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_slot_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &slotId);
7212 | tap_info->slot = slotId;
7213 | offset++;
7214 | /* symbolId */
7215 | uint32_t symbolId = 0;
7216 | proto_tree_add_item_ret_uint(timing_header_tree, hf_oran_symbolId, tvb, offset, 1, ENC_NA0x00000000, &symbolId);
7217 | offset++;
7218 |
7219 | char id[16];
7220 | snprintf(id, 16, "%u-%u-%u-%u", frameId, subframeId, slotId, symbolId);
7221 | proto_item *pi = proto_tree_add_string(timing_header_tree, hf_oran_refa, tvb, ref_a_offset, 3, id);
7222 | proto_item_set_generated(pi);
7223 |
7224 | proto_item_append_text(timingHeader, "%s, frameId: %d, subframeId: %d, slotId: %d, symbolId: %d)",
7225 | val_to_str_const(direction, data_direction_vals, "Unknown"), frameId, subframeId, slotId, symbolId);
7226 |
7227 | unsigned sample_bit_width;
7228 | unsigned compression;
7229 | int includeUdCompHeader;
7230 |
7231 | /* Also lookup C-PLANE state (sent in opposite direction for UL) so may check current compression settings */
7232 | uint32_t cplane_key = make_flow_key(pinfo, eAxC, ORAN_C_PLANE0, direction
1.1 | 'direction' is not equal to 0
== 0);
7233 | flow_state_t* cplane_state = (flow_state_t*)wmem_tree_lookup32(flow_states_table, cplane_key);
7234 |
7235 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
2 | ← | Assuming field 'visited' is not equal to 0 | →
3 | ← | Taking false branch | →
7236 | /* Create state/conversation if doesn't exist yet */
7237 | if (!state) {
7238 | /* Allocate new state */
7239 | state = wmem_new0(wmem_file_scope(), flow_state_t)((flow_state_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_state_t )));
7240 | state->ack_nack_requests = wmem_tree_new(wmem_file_scope());
7241 | state->expected_sections[0] = wmem_tree_new(wmem_file_scope());
7242 | state->expected_sections[1] = wmem_tree_new(wmem_file_scope());
7243 | wmem_tree_insert32(flow_states_table, key, state);
7244 | }
7245 |
7246 | result = wmem_new0(wmem_file_scope(), flow_result_t)((flow_result_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_result_t )));
7247 | result->expected_sections = wmem_tree_new(wmem_file_scope());
7248 | result->u_plane_frames = wmem_list_new(wmem_file_scope());
7249 |
7250 | wmem_tree_insert32(flow_results_table, pinfo->num, result);
7251 |
7252 | /* Check sequence analysis status (but not if later part of radio layer fragmentation) */
7253 | if (state->last_frame_seen[direction] && (subSeqId==0) && (seqId != state->next_expected_sequence_number[direction])) {
7254 | /* Store this result */
7255 | result->unexpected_seq_number = true1;
7256 | result->expected_sequence_number = state->next_expected_sequence_number[direction];
7257 | result->previous_frame = state->last_frame[direction];
7258 | }
7259 | /* Update sequence analysis state */
7260 | state->last_frame[direction] = pinfo->num;
7261 | state->last_frame_seen[direction] = true1;
7262 | state->next_expected_sequence_number[direction] = (seqId+1) % 256;
7263 | }
7264 |
7265 | /* Show any issues associated with this frame number */
7266 | result = wmem_tree_lookup32(flow_results_table, pinfo->num);
4 | ← | Value assigned to 'result' | →
7267 | if (result) {
5 | ← | Assuming 'result' is null | →
7268 | if (result->unexpected_seq_number) {
7269 | expert_add_info_format(pinfo, seqIdItem,
7270 | (direction == DIR_UPLINK0) ?
7271 | &ei_oran_uplane_unexpected_sequence_number_ul :
7272 | &ei_oran_uplane_unexpected_sequence_number_dl,
7273 | "Sequence number %u expected, but got %u",
7274 | result->expected_sequence_number, seqId);
7275 | tap_info->missing_sns = (256 + seqId - result->expected_sequence_number) % 256;
7276 | /* TODO: could add previous/next frame (in seqId tree?) ? */
7277 | }
7278 | }
7279 |
7280 | /* Checking UL timing within current slot. Disabled if limit set to 0. */
7281 | /* N.B., timing is relative to first seen frame,
7282 | not some notion of the beginning of the slot from sync, offset by some timing.. */
7283 | if (direction
5.1 | 'direction' is not equal to DIR_UPLINK
== DIR_UPLINK0 && us_allowed_for_ul_in_symbol > 0) {
7284 | uint32_t timing_key = get_timing_key(frameId, subframeId, slotId, symbolId);
7285 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
7286 | /* Set state on first pass */
7287 | ul_timing_for_slot* timing = (ul_timing_for_slot*)wmem_tree_lookup32(ul_symbol_timing, timing_key);
7288 | if (!timing) {
7289 | /* Allocate new state */
7290 | timing = wmem_new0(wmem_file_scope(), ul_timing_for_slot)((ul_timing_for_slot*)wmem_alloc0((wmem_file_scope()), sizeof (ul_timing_for_slot)));
7291 | timing->first_frame = pinfo->num;
7292 | timing->first_frame_time = pinfo->abs_ts;
7293 | timing->frames_seen_in_symbol = 1;
7294 | timing->last_frame_in_symbol = pinfo->num;
7295 | wmem_tree_insert32(ul_symbol_timing, timing_key, timing);
7296 | }
7297 | else {
7298 | /* Update existing state */
7299 | timing->frames_seen_in_symbol++;
7300 | timing->last_frame_in_symbol = pinfo->num;
7301 | }
7302 | }
7303 | else {
7304 | /* Subsequent passes - look up result */
7305 | ul_timing_for_slot* timing = (ul_timing_for_slot*)wmem_tree_lookup32(ul_symbol_timing, timing_key);
7306 | if (timing) { /* Really shouldn't fail! */
7307 | if (timing->frames_seen_in_symbol > 1) {
7308 | /* Work out gap between frames (in microseconds) back to frame carrying first seen symbol */
7309 | int seconds_between_packets = (int)
7310 | (pinfo->abs_ts.secs - timing->first_frame_time.secs);
7311 | int nseconds_between_packets =
7312 | pinfo->abs_ts.nsecs - timing->first_frame_time.nsecs;
7313 |
7314 | /* Round to nearest microsecond. */
7315 | uint32_t total_gap = (seconds_between_packets*1000000) +
7316 | ((nseconds_between_packets+500) / 1000);
7317 |
7318 | /* Show how long it has been */
7319 | proto_item *ti = NULL((void*)0);
7320 | if (pinfo->num != timing->first_frame) {
7321 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_time, tvb, 0, 0, total_gap);
7322 | proto_item_set_generated(ti);
7323 | }
7324 |
7325 | if (total_gap > us_allowed_for_ul_in_symbol) {
7326 | expert_add_info_format(pinfo, ti, &ei_oran_ul_uplane_symbol_too_long,
7327 | "UL U-Plane Tx took longer (%u us) than limit set in preferences (%u us)",
7328 | total_gap, us_allowed_for_ul_in_symbol);
7329 | proto_item_append_text(timingHeader, " (%uus since first frame seen for symbol)", total_gap);
7330 | }
7331 |
7332 | /* Show how many frames were received */
7333 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_frames, tvb, 0, 0, timing->frames_seen_in_symbol);
7334 | proto_item_set_generated(ti);
7335 |
7336 | /* Link to first frame for this symbol */
7337 | if (pinfo->num != timing->first_frame) {
7338 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_first_frame, tvb, 0, 0, timing->first_frame);
7339 | proto_item_set_generated(ti);
7340 | }
7341 |
7342 | /* And also last frame */
7343 | if (pinfo->num != timing->last_frame_in_symbol) {
7344 | ti = proto_tree_add_uint(timingHeader, hf_oran_u_section_ul_symbol_last_frame, tvb, 0, 0, timing->last_frame_in_symbol);
7345 | proto_item_set_generated(ti);
7346 | }
7347 |
7348 | tap_info->ul_delay_in_us = total_gap;
7349 | }
7350 | }
7351 | }
7352 | }
7353 |
7354 |
7355 | /* Look up preferences for samples */
7356 | if (direction
5.2 | 'direction' is not equal to DIR_UPLINK
== DIR_UPLINK0) {
6 | ← | Taking false branch | →
7357 | sample_bit_width = pref_sample_bit_width_uplink;
7358 | compression = pref_iqCompressionUplink;
7359 | includeUdCompHeader = pref_includeUdCompHeaderUplink;
7360 | } else {
7361 | sample_bit_width = pref_sample_bit_width_downlink;
7362 | compression = pref_iqCompressionDownlink;
7363 | includeUdCompHeader = pref_includeUdCompHeaderDownlink;
7364 | }
7365 |
7366 | /* If uplink, load any udCompHdr settings written by C-Plane */
7367 | bool_Bool ud_cmp_hdr_cplane = false0;
7368 | if (cplane_state && direction
7.1 | 'direction' is not equal to 0
== 0) {
7 | ← | Assuming 'cplane_state' is non-null | →
8 | ← | Taking false branch | →
7369 | /* Initialise settings from udpCompHdr from C-Plane */
7370 | if (cplane_state->ul_ud_comp_hdr_set && !pref_override_ul_compression) {
7371 | sample_bit_width = cplane_state->ul_ud_comp_hdr_bit_width;
7372 | compression = cplane_state->ul_ud_comp_hdr_compression;
7373 | ud_cmp_hdr_cplane = true1;
7374 | }
7375 | }
7376 |
7377 | /* Need a valid value (e.g. 9, 14). 0 definitely won't work, as won't progress around loop! */
7378 | /* N.B. may yet be overwritten by udCompHdr settings in sections below! */
7379 | if (sample_bit_width == 0) {
9 | ← | Assuming 'sample_bit_width' is not equal to 0 | →
10 | ← | Taking false branch | →
7380 | expert_add_info_format(pinfo, protocol_item, &ei_oran_invalid_sample_bit_width,
7381 | "%cL Sample bit width from %s (%u) not valid, so can't decode sections",
7382 | (direction == DIR_UPLINK0) ? 'U' : 'D',
7383 | !ud_cmp_hdr_cplane ? "preference" : "C-Plane",
7384 | sample_bit_width);
7385 | return offset;
7386 | }
7387 |
7388 | unsigned bytesLeft;
7389 | unsigned number_of_sections = 0;
7390 | unsigned nBytesPerPrb =0;
7391 |
7392 | if (link_planes_together && !PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited) && cplane_state) {
11 | ← | Assuming 'link_planes_together' is false | →
7393 | /* Take a deep-copy of this state on first pass */
7394 | wmem_tree_foreach(cplane_state->expected_sections[direction], copy_section_entry, result->expected_sections);
7395 | }
7396 |
7397 | /* Add each section (not from count, just keep parsing until payload used) */
7398 | do {
7399 | /* Section subtree */
7400 | unsigned section_start_offset = offset;
7401 | proto_item *sectionHeading = proto_tree_add_string_format(oran_tree, hf_oran_u_section,
7402 | tvb, offset, 0, "", "Section");
7403 | proto_tree *section_tree = proto_item_add_subtree(sectionHeading, ett_oran_u_section);
7404 |
7405 | /* Section Header fields (darker green part) */
7406 |
7407 | /* sectionId */
7408 | uint32_t sectionId = 0;
7409 | proto_item *sectionId_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_section_id, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &sectionId);
7410 | if (sectionId == 4095) {
12 | ← | Assuming 'sectionId' is not equal to 4095 | →
13 | ← | Taking false branch | →
7411 | proto_item_append_text(sectionId_ti, " (not default coupling C/U planes using sectionId)");
7412 | }
7413 | offset++;
7414 |
7415 | if (tap_info->num_section_ids < MAX_SECTION_IDs32) {
14 | ← | Assuming field 'num_section_ids' is >= MAX_SECTION_IDs | →
15 | ← | Taking false branch | →
7416 | tap_info->section_ids[tap_info->num_section_ids++] = sectionId;
7417 | }
7418 |
7419 | section_details_t *section_details = NULL((void*)0);
7420 | corresponding_uplane_frame *details = NULL((void*)0);
7421 |
7422 | /* Lookup corresponding C-plane frame/info */
7423 | if (link_planes_together) {
16 | ← | Assuming 'link_planes_together' is true | →
17 | ← | Taking true branch | →
7424 | if (cplane_state
17.1 | 'cplane_state' is not equal to NULL
!= NULL((void*)0)) {
18 | ← | Taking true branch | →
7425 |
7426 | expected_section_data_t *section_data = NULL((void*)0);
7427 | section_data = wmem_tree_lookup32(result->expected_sections, sectionId);
19 | ← | Access to field 'expected_sections' results in a dereference of a null pointer (loaded from variable 'result')
7428 |
7429 | if (section_data) {
7430 | /* Need to work out which of 2 entries is in use for this data frame */
7431 | unsigned index_to_use = 0;
7432 |
7433 | /* Does the first entry match the timing for this frame? */
7434 | if (section_data->details[0].frame == frameId &&
7435 | section_data->details[0].subframe == subframeId &&
7436 | section_data->details[0].slot == slotId &&
7437 | /* Check that symbolId is in range */
7438 | section_data->details[0].startSymbol <= symbolId &&
7439 | (unsigned)(section_data->details[0].startSymbol + section_data->details[0].numSymbols) <= (unsigned)symbolId) {
7440 |
7441 | index_to_use = 0;
7442 | }
7443 | else if (section_data->details[1].frame == frameId &&
7444 | section_data->details[1].subframe == subframeId &&
7445 | section_data->details[1].slot == slotId &&
7446 | /* Check that symbolId is in range */
7447 | section_data->details[1].startSymbol <= symbolId &&
7448 | (unsigned)(section_data->details[1].startSymbol + section_data->details[1].numSymbols) <= (unsigned)symbolId) {
7449 |
7450 | index_to_use = 1;
7451 | }
7452 | else {
7453 | /* There was a sectionId, but timing header didn't exactly match, so neither index may be used.. */
7454 | index_to_use = 2; /* invalid value */
7455 | /* Expert info */
7456 | expert_add_info_format(NULL((void*)0), sectionId_ti,
7457 | &ei_oran_cplane_entry_not_found,
7458 | "C-plane entry for %s sectionId %u at timing header %u-%u-%u-%u",
7459 | (direction) ? "DL" : "UL", sectionId,
7460 | frameId, subframeId, slotId, symbolId);
7461 | }
7462 |
7463 | if (index_to_use <= 1) {
7464 | section_details = &section_data->details[index_to_use];
7465 |
7466 | /* Cplane frame number */
7467 | proto_item *cplane_frame_ti = proto_tree_add_uint(section_tree, hf_oran_corresponding_cplane_frame, tvb, 0, 0,
7468 | section_details->frame_number);
7469 | proto_item_set_generated(cplane_frame_ti);
7470 |
7471 | /* usecs since cplane frame */
7472 | time_t total_gap = 0;
7473 |
7474 | if ((pinfo->abs_ts.secs == section_details->frame_time.secs) || (pinfo->abs_ts.secs == section_details->frame_time.secs+1)) {
7475 | total_gap = ((pinfo->abs_ts.secs - section_details->frame_time.secs) * 1000000) +
7476 | ((pinfo->abs_ts.nsecs - section_details->frame_time.nsecs)/1000);
7477 | }
7478 |
7479 | if (total_gap > 0) {
7480 | proto_item *cplane_delta_ti = proto_tree_add_uint(section_tree, hf_oran_corresponding_cplane_frame_time_delta, tvb, 0, 0, (uint32_t)total_gap);
7481 | proto_item_set_generated(cplane_delta_ti);
7482 | }
7483 |
7484 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited)) {
7485 | /* Look up 'result' for c-plane frame, and tell it about this frame.. */
7486 | flow_result_t *cplane_result = wmem_tree_lookup32(flow_results_table, section_details->frame_number);
7487 | if (!cplane_result) {
7488 | cplane_result = wmem_new0(wmem_file_scope(), flow_result_t)((flow_result_t*)wmem_alloc0((wmem_file_scope()), sizeof(flow_result_t )));
7489 | cplane_result->u_plane_frames = wmem_list_new(wmem_file_scope());
7490 | wmem_tree_insert32(flow_results_table, section_details->frame_number, cplane_result);
7491 | }
7492 | /* PRB range filled in below.. */
7493 |
7494 | details = wmem_new(wmem_file_scope(), corresponding_uplane_frame)((corresponding_uplane_frame*)wmem_alloc((wmem_file_scope()), sizeof(corresponding_uplane_frame)));
7495 | details->frame_number = pinfo->num;
7496 | details->gap_in_usecs = (uint32_t)total_gap;
7497 | details->sectionId = sectionId;
7498 | details->symbol = symbolId;
7499 |
7500 | wmem_list_append(cplane_result->u_plane_frames, details);
7501 | }
7502 | }
7503 | }
7504 | else {
7505 | /* No section entry at all */
7506 | expert_add_info_format(NULL((void*)0), sectionId_ti,
7507 | &ei_oran_cplane_entry_not_found,
7508 | "C-plane entry for %s sectionId %u not found",
7509 | (direction) ? "DL" : "UL", sectionId);
7510 | }
7511 | }
7512 | }
7513 |
7514 | /* rb */
7515 | uint32_t rb;
7516 | proto_tree_add_item_ret_uint(section_tree, hf_oran_rb, tvb, offset, 1, ENC_NA0x00000000, &rb);
7517 | /* symInc. "use of symInc=1 shall be prohibited in the U-plane" */
7518 | uint8_t syminc;
7519 | proto_item *syminc_ti = proto_tree_add_item_ret_uint8(section_tree, hf_oran_symInc, tvb, offset, 1, ENC_NA0x00000000, &syminc);
7520 | if (syminc) {
7521 | expert_add_info(NULL((void*)0), syminc_ti, &ei_oran_syminc_set_for_uplane);
7522 | }
7523 | /* startPrbu */
7524 | uint32_t startPrbu = 0;
7525 | proto_tree_add_item_ret_uint(section_tree, hf_oran_startPrbu, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &startPrbu);
7526 | offset += 2;
7527 |
7528 | /* numPrbu */
7529 | uint32_t numPrbu = 0;
7530 | proto_tree_add_item_ret_uint(section_tree, hf_oran_numPrbu, tvb, offset, 1, ENC_NA0x00000000, &numPrbu);
7531 | offset += 1;
7532 |
7533 | if (!PINFO_FD_VISITED(pinfo)((pinfo)->fd->visited) && details) {
7534 | details->startPrbu = startPrbu;
7535 | details->numPrbu = (numPrbu) ? numPrbu : 273;
7536 | }
7537 |
7538 | proto_item *ud_comp_meth_item, *ud_comp_len_ti=NULL((void*)0);
7539 | uint32_t ud_comp_len = 0;
7540 |
7541 | /* udCompHdr (if preferences indicate will be present) */
7542 | bool_Bool included = (includeUdCompHeader==1) || /* 1 means present.. */
7543 | (includeUdCompHeader==2 && udcomphdr_appears_present(state, direction, tvb, offset));
7544 | if (included) {
7545 | /* 7.5.2.10 */
7546 | /* Extract these values to inform how wide IQ samples in each PRB will be. */
7547 | offset = dissect_udcomphdr(tvb, pinfo, section_tree, offset, false0, direction == 0, &sample_bit_width,
7548 | &compression, &ud_comp_meth_item, tap_info);
7549 |
7550 | /* Not part of udCompHdr */
7551 | uint32_t reserved;
7552 | proto_item *res_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_reserved_8bits, tvb, offset, 1, ENC_NA0x00000000, &reserved);
7553 | offset += 1;
7554 | if (reserved != 0) {
7555 | expert_add_info_format(pinfo, res_ti, &ei_oran_reserved_not_zero,
7556 | "reserved field (0x%x) not zero - perhaps udCompHdr is not really present?",
7557 | reserved);
7558 | }
7559 | }
7560 | else {
7561 | /* No fields to dissect - just showing comp values from prefs */
7562 | /* iqWidth */
7563 | proto_item *iq_width_item = proto_tree_add_uint(section_tree, hf_oran_udCompHdrIqWidth_pref, tvb, 0, 0, sample_bit_width);
7564 | proto_item_append_text(iq_width_item, (ud_cmp_hdr_cplane) ? " (from c-plane)" : " (from preferences)");
7565 | proto_item_set_generated(iq_width_item);
7566 |
7567 | /* udCompMethod */
7568 | ud_comp_meth_item = proto_tree_add_uint(section_tree, hf_oran_udCompHdrMeth_pref, tvb, 0, 0, compression);
7569 | proto_item_append_text(ud_comp_meth_item, (ud_cmp_hdr_cplane) ? " (from c-plane)" : " (from preferences)");
7570 | proto_item_set_generated(ud_comp_meth_item);
7571 |
7572 | /* Point back to C-Plane, if used */
7573 | /* TODO: doesn't work with multiple port mappings using SE10.. */
7574 | if (ud_cmp_hdr_cplane) {
7575 | proto_item *cplane_ti = proto_tree_add_uint(section_tree, hf_oran_ul_cplane_ud_comp_hdr_frame, tvb, offset, 0, cplane_state->ul_ud_comp_hdr_frame);
7576 | proto_item_set_generated(cplane_ti);
7577 | }
7578 |
7579 | tap_info->compression_methods |= (1 << compression);
7580 | tap_info->compression_width = sample_bit_width;
7581 | }
7582 |
7583 | /* Consider fragmentation after first section header */
7584 | if (do_radio_transport_layer_reassembly && (number_of_sections == 0) && (e !=1 || subSeqId!= 0)) {
7585 |
7586 | /* Set fragmented flag. */
7587 | bool_Bool save_fragmented = pinfo->fragmented;
7588 | pinfo->fragmented = true1;
7589 | fragment_head *fh;
7590 | unsigned frag_data_len = tvb_reported_length_remaining(tvb, offset);
7591 |
7592 | /* Add this fragment into reassembly table */
7593 | uint32_t reassembly_id = make_reassembly_id(seqId, direction, eAxC,
7594 | frameId, subframeId, slotId, symbolId);
7595 | fh = fragment_add_seq(&oran_reassembly_table, tvb, offset, pinfo,
7596 | reassembly_id, /* id */
7597 | GUINT_TO_POINTER(reassembly_id)((gpointer) (gulong) (reassembly_id)), /* data */
7598 | subSeqId, /* frag_number */
7599 | frag_data_len, /* frag_data_len */
7600 | !e, /* more_frags */
7601 | 0);
7602 |
7603 | bool_Bool update_col_info = true1;
7604 |
7605 | /* See if this completes an SDU */
7606 | tvbuff_t *original_tvb = tvb;
7607 | tvbuff_t *next_tvb = process_reassembled_data(tvb, offset, pinfo, "Reassembled O-RAN FH CUS Payload",
7608 | fh, &oran_frag_items,
7609 | &update_col_info, oran_tree);
7610 | if (next_tvb) {
7611 | /* Have reassembled data */
7612 | proto_tree_add_item(oran_tree, hf_oran_payload, next_tvb, 0, -1, ENC_NA0x00000000);
7613 | col_append_fstr(pinfo->cinfo, COL_INFO, " Reassembled Data (%u bytes)", tvb_reported_length(next_tvb));
7614 | /* Dissection should resume at start of reassembled tvb */
7615 | offset = 0;
7616 | }
7617 | /* Will continue with either reassembled tvb or NULL */
7618 | tvb = next_tvb;
7619 |
7620 | /* Restore fragmented flag */
7621 | pinfo->fragmented = save_fragmented;
7622 |
7623 | /* Don't dissect any more if not complete yet.. */
7624 | if (tvb == NULL((void*)0)) {
7625 | return tvb_captured_length(original_tvb);
7626 | }
7627 | }
7628 |
7629 |
7630 | /* Not supported! TODO: other places where comp method is looked up (e.g., bfw?) */
7631 | switch (compression) {
7632 | case COMP_NONE0:
7633 | case COMP_BLOCK_FP1:
7634 | case BFP_AND_SELECTIVE_RE5:
7635 | case COMP_MODULATION4:
7636 | case MOD_COMPR_AND_SELECTIVE_RE6:
7637 | break;
7638 | default:
7639 | expert_add_info_format(pinfo, ud_comp_meth_item, &ei_oran_unsupported_compression_method,
7640 | "Compression method %u (%s) not supported by dissector",
7641 | compression,
7642 | rval_to_str_const(compression, ud_comp_header_meth, "reserved"));
7643 | }
7644 |
7645 | /* udCompLen (when supported, methods 5,6,7,8) */
7646 | if (compression >= BFP_AND_SELECTIVE_RE5) {
7647 | bool_Bool supported = (pref_support_udcompLen==1) || /* supported */
7648 | (pref_support_udcompLen==2 && udcomplen_appears_present(includeUdCompHeader, tvb, offset));
7649 |
7650 | if (supported) {
7651 | ud_comp_len_ti = proto_tree_add_item_ret_uint(section_tree, hf_oran_udCompLen, tvb, offset, 2, ENC_BIG_ENDIAN0x00000000, &ud_comp_len);
7652 | if (ud_comp_len <= 1) {
7653 | proto_item_append_text(ud_comp_len_ti, " (reserved)");
7654 | }
7655 | /* TODO: report if less than a viable section in frame? */
7656 | /* Check that there is this much length left in the frame */
7657 | if (ud_comp_len > tvb_reported_length_remaining(tvb, section_start_offset)) {
7658 | expert_add_info_format(pinfo, ud_comp_len_ti, &ei_oran_ud_comp_len_wrong_size,
7659 | "udCompLen indicates %u bytes in section, but only %u are left in frame",
7660 | ud_comp_len, tvb_reported_length_remaining(tvb, section_start_offset));
7661 | }
7662 | /* Actual length of section will be checked below, at the end of the section */
7663 | offset += 2;
7664 | }
7665 | }
7666 |
7667 | /* sReSMask1 + sReSMask2 (depends upon compression method) */
7668 | uint64_t sresmask1=0, sresmask2=0;
7669 | if (compression == BFP_AND_SELECTIVE_RE_WITH_MASKS7 ||
7670 | compression == MOD_COMPR_AND_SELECTIVE_RE_WITH_MASKS8)
7671 | {
7672 | static int * const sres_mask1_2_flags[] = {
7673 | &hf_oran_sReSMask1_2_re12,
7674 | &hf_oran_sReSMask1_2_re11,
7675 | &hf_oran_sReSMask1_2_re10,
7676 | &hf_oran_sReSMask1_2_re9,
7677 | &hf_oran_sReSMask_re8,
7678 | &hf_oran_sReSMask_re7,
7679 | &hf_oran_sReSMask_re6,
7680 | &hf_oran_sReSMask_re5,
7681 | &hf_oran_sReSMask_re4,
7682 | &hf_oran_sReSMask_re3,
7683 | &hf_oran_sReSMask_re2,
7684 | &hf_oran_sReSMask_re1,
7685 | NULL((void*)0)
7686 | };
7687 |
7688 | /* reserved (4 bits) */
7689 | add_reserved_field(section_tree, hf_oran_reserved_4bits, tvb, offset, 1);
7690 | /* sReSMask1 (12 bits) */
7691 | proto_item *sresmask_ti;
7692 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(section_tree, tvb, offset,
7693 | hf_oran_sReSMask1,
7694 | ett_oran_sresmask,
7695 | sres_mask1_2_flags,
7696 | ENC_NA0x00000000,
7697 | &sresmask1);
7698 | offset += 2;
7699 | /* Count REs present */
7700 | unsigned res = 0;
7701 | for (unsigned n=0; n < 12; n++) {
7702 | if ((sresmask1 >> n) & 0x1) {
7703 | res++;
7704 | }
7705 | }
7706 | proto_item_append_text(sresmask_ti, " (%u REs)", res);
7707 |
7708 |
7709 | /* reserved (4 bits) */
7710 | add_reserved_field(section_tree, hf_oran_reserved_4bits, tvb, offset, 1);
7711 | /* sReSMask2 (12 bits) */
7712 | sresmask_ti = proto_tree_add_bitmask_ret_uint64(section_tree, tvb, offset,
7713 | hf_oran_sReSMask2,
7714 | ett_oran_sresmask,
7715 | sres_mask1_2_flags,
7716 | ENC_NA0x00000000,
7717 | &sresmask2);
7718 | offset += 2;
7719 |
7720 | if (rb == 1) {
7721 | proto_item_append_text(sresmask_ti, " (ignored)");
7722 | if (sresmask2 != 0) {
7723 | expert_add_info(pinfo, ud_comp_len_ti, &ei_oran_sresmask2_not_zero_with_rb);
7724 | }
7725 | }
7726 | else {
7727 | /* Count REs present */
7728 | res = 0;
7729 | for (unsigned n=0; n < 12; n++) {
7730 | if ((sresmask2 >> n) & 0x1) {
7731 | res++;
7732 | }
7733 | }
7734 | proto_item_append_text(sresmask_ti, " (%u REs)", res);
7735 | }
7736 | }
7737 |
7738 | write_section_info(sectionHeading, pinfo, protocol_item, sectionId, startPrbu, numPrbu, rb);
7739 |
7740 | /* TODO: should this use the same pref as c-plane? */
7741 | if (numPrbu == 0) {
7742 | /* Special case for all PRBs (NR: the total number of PRBs may be > 255) */
7743 | numPrbu = pref_data_plane_section_total_rbs;
7744 | startPrbu = 0; /* may already be 0... */
7745 | }
7746 |
7747 | section_mod_compr_config_t* mod_compr_config = get_mod_compr_section_to_read(cplane_state, sectionId);
7748 |
7749 | /* Add each PRB */
7750 | for (unsigned i = 0; i < numPrbu; i++) {
7751 | /* Create subtree */
7752 | proto_item *prbHeading = proto_tree_add_string_format(section_tree, hf_oran_samples_prb,
7753 | tvb, offset, 0,
7754 | "", "PRB");
7755 | proto_tree *rb_tree = proto_item_add_subtree(prbHeading, ett_oran_u_prb);
7756 | uint32_t exponent = 0;
7757 | uint16_t sresmask = 0;
7758 |
7759 | /* udCompParam (depends upon compression method) */
7760 | int before = offset;
7761 | offset = dissect_udcompparam(tvb, pinfo, rb_tree, offset, compression, &exponent, &sresmask, false0);
7762 | int udcompparam_len = offset-before;
7763 |
7764 | /* Show PRB number in root */
7765 | proto_item_append_text(prbHeading, " %3u", startPrbu + i*(1+rb));
7766 |
7767 | /* Work out how many REs / PRB */
7768 | unsigned res_per_prb = 12;
7769 | uint16_t sresmask_to_use = 0x0fff;
7770 |
7771 | if (compression >= BFP_AND_SELECTIVE_RE5) {
7772 | /* Work out which mask should be used */
7773 | if (compression==BFP_AND_SELECTIVE_RE5 || compression==MOD_COMPR_AND_SELECTIVE_RE6) {
7774 | /* Selective RE cases, use value from compModParam */
7775 | sresmask_to_use = (uint16_t)sresmask;
7776 | }
7777 | else {
7778 | /* With masks (in section). Choose between sresmask1 and sresmask2 */
7779 | if (rb==1 || (i%2)==0) {
7780 | /* Even values */
7781 | sresmask_to_use = (uint16_t)sresmask1;
7782 | }
7783 | else {
7784 | /* Odd values */
7785 | sresmask_to_use = (uint16_t)sresmask2;
7786 | }
7787 | }
7788 |
7789 | /* Count REs present using sresmask */
7790 | res_per_prb = 0;
7791 | /* Use sresmask to pick out which REs are present */
7792 | for (unsigned n=0; n<12; n++) {
7793 | if (sresmask_to_use & (1<<n)) {
7794 | res_per_prb++;
7795 | }
7796 | }
7797 | }
7798 |
7799 | /* N.B. bytes for samples need to be padded out to next byte
7800 | (certainly where there aren't 12 REs in PRB..) */
7801 | unsigned nBytesForSamples = (sample_bit_width * res_per_prb * 2 + 7) / 8;
7802 | nBytesPerPrb = nBytesForSamples + udcompparam_len;
7803 |
7804 | proto_tree_add_item(rb_tree, hf_oran_iq_user_data, tvb, offset, nBytesForSamples, ENC_NA0x00000000);
7805 |
7806 | if (section_details) {
7807 | if ((startPrbu + i*(1+rb)) < 273) {
7808 | proto_item *beamid_ti = proto_tree_add_uint(rb_tree, hf_oran_beamId, tvb, 0, 0,
7809 | section_details->beamIds[startPrbu + i*(1+rb)]);
7810 | proto_item_set_generated(beamid_ti);
7811 | }
7812 | }
7813 |
7814 |
7815 | tap_info->non_zero_re_in_current_prb = false0;
7816 |
7817 | /* Optionally trying to show I/Q RE values */
7818 | if (pref_showIQSampleValues) {
7819 | /* Individual values */
7820 | unsigned samples_offset = offset*8;
7821 | unsigned samples_start = offset;
7822 | unsigned samples = 0;
7823 |
7824 | if (compression >= BFP_AND_SELECTIVE_RE5) {
7825 | /* Use sresmask to pick out which REs are present */
7826 | for (unsigned n=1; n<=12; n++) {
7827 | if (sresmask_to_use & (1<<(n-1))) {
7828 | samples_offset = dissect_oran_u_re(tvb, rb_tree,
7829 | n, samples_offset, tap_info, sample_bit_width, compression, exponent, mod_compr_config, n);
7830 | samples++;
7831 | }
7832 | }
7833 | }
7834 | else {
7835 | /* All 12 REs are present */
7836 | for (unsigned n=1; n<=12; n++) {
7837 | samples_offset = dissect_oran_u_re(tvb, rb_tree,
7838 | n, samples_offset, tap_info, sample_bit_width, compression, exponent, mod_compr_config, n);
7839 | samples++;
7840 | }
7841 | }
7842 | proto_item_append_text(prbHeading, " (%u REs)", samples);
7843 | if (section_details) {
7844 | if ((startPrbu + i*(1+rb)) < 273) {
7845 | proto_item_append_text(prbHeading, " [BeamId:%u]", section_details->beamIds[startPrbu + i*(1+rb)]);
7846 | }
7847 | }
7848 |
7849 | /* Was this PRB all zeros? */
7850 | if (!tap_info->non_zero_re_in_current_prb) {
7851 | tap_info->num_prbs_zero++;
7852 | /* Add a filter to make zero-valued PRBs more findable */
7853 | proto_item *zero_ti = proto_tree_add_item(rb_tree, hf_oran_zero_prb, tvb,
7854 | samples_start, nBytesForSamples, ENC_NA0x00000000);
7855 | proto_item_set_hidden(zero_ti);
7856 | proto_item_append_text(prbHeading, " (all zeros)");
7857 | }
7858 | else {
7859 | proto_item *nonzero_ti = proto_tree_add_item(rb_tree, hf_oran_nonzero_prb, tvb, samples_start, nBytesForSamples, ENC_NA0x00000000);
7860 | proto_item_set_hidden(nonzero_ti);
7861 | }
7862 | }
7863 |
7864 | tap_info->num_prbs++;
7865 |
7866 |
7867 | /* Advance past samples */
7868 | offset += nBytesForSamples;
7869 |
7870 | /* Set end of prb subtree */
7871 | proto_item_set_end(prbHeading, tvb, offset);
7872 | }
7873 |
7874 | /* Set extent of section */
7875 | proto_item_set_len(sectionHeading, offset-section_start_offset);
7876 | if (ud_comp_len_ti != NULL((void*)0) && ((offset-section_start_offset != ud_comp_len))) {
7877 | expert_add_info_format(pinfo, ud_comp_len_ti, &ei_oran_ud_comp_len_wrong_size,
7878 | "udCompLen indicates %u bytes in section, but dissected %u instead",
7879 | ud_comp_len, offset-section_start_offset);
7880 | }
7881 |
7882 | bytesLeft = tvb_captured_length(tvb) - offset;
7883 | number_of_sections++;
7884 | } while (bytesLeft >= (4 + nBytesPerPrb)); /* FIXME: bad heuristic */
7885 |
7886 | /* Show number of sections found */
7887 | proto_item *ti = proto_tree_add_uint(oran_tree, hf_oran_numberOfSections, tvb, 0, 0, number_of_sections);
7888 | proto_item_set_generated(ti);
7889 |
7890 | /* Expert error if we are short of tvb by > 3 bytes */
7891 | if (tvb_reported_length_remaining(tvb, offset) > 3) {
7892 | expert_add_info_format(pinfo, protocol_item, &ei_oran_frame_length,
7893 | "%u bytes remain at end of frame - should be 0-3",
7894 | tvb_reported_length_remaining(tvb, offset));
7895 | }
7896 |
7897 | return tvb_captured_length(tvb);
7898 | }
7899 |
7900 |
7901 | /**********************************************************************/
7902 | /* Main dissection function. */
7903 | /* N.B. ecpri message type passed in as 'data' arg by eCPRI dissector */
7904 | static int
7905 | dissect_oran(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, void *data)
7906 | {
7907 | uint32_t ecpri_message_type = *(uint32_t *)data;
7908 | unsigned offset = 0;
7909 |
7910 | /* Allocate and zero tap struct */
7911 | oran_tap_info *tap_info = wmem_new0(wmem_file_scope(), oran_tap_info)((oran_tap_info*)wmem_alloc0((wmem_file_scope()), sizeof(oran_tap_info )));
7912 | tap_info->pdu_size = pinfo->fd->pkt_len;
7913 | tap_info->ul_delay_configured_max = us_allowed_for_ul_in_symbol;
7914 |
7915 | switch (ecpri_message_type) {
7916 | case ECPRI_MT_IQ_DATA0:
7917 | offset = dissect_oran_u(tvb, pinfo, tree, tap_info, data);
7918 | break;
7919 | case ECPRI_MT_RT_CTRL_DATA2:
7920 | offset = dissect_oran_c(tvb, pinfo, tree, tap_info, data);
7921 | break;
7922 | default:
7923 | /* Not dissecting other types - assume these are handled by eCPRI dissector */
7924 | return 0;
7925 | }
7926 |
7927 | tap_queue_packet(oran_tap, pinfo, tap_info);
7928 |
7929 | return offset;
7930 | }
7931 |
7932 | static void oran_init_protocol(void)
7933 | {
7934 | udcomplen_heuristic_result_set = false0;
7935 | udcomplen_heuristic_result = false0;
7936 | }
7937 |
7938 |
7939 | /* Register the protocol with Wireshark. */
7940 | void
7941 | proto_register_oran(void)
7942 | {
7943 | static hf_register_info hf[] = {
7944 |
7945 | /* Section 5.1.3.2.7 */
7946 | { &hf_oran_du_port_id,
7947 | { "DU Port ID", "oran_fh_cus.du_port_id",
7948 | FT_UINT16, BASE_DEC,
7949 | NULL((void*)0), 0x0,
7950 | "Processing unit at O-RU - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7951 | },
7952 |
7953 | /* Section 5.1.3.2.7 */
7954 | { &hf_oran_bandsector_id,
7955 | { "BandSector ID", "oran_fh_cus.bandsector_id",
7956 | FT_UINT16, BASE_DEC,
7957 | NULL((void*)0), 0x0,
7958 | "Aggregated cell identified - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7959 | },
7960 |
7961 | /* Section 5.1.3.2.7 */
7962 | { &hf_oran_cc_id,
7963 | { "CC ID", "oran_fh_cus.cc_id",
7964 | FT_UINT16, BASE_DEC,
7965 | NULL((void*)0), 0x0,
7966 | "Component Carrier - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7967 | },
7968 |
7969 | /* Section 5.1.3.2.7 */
7970 | { &hf_oran_ru_port_id,
7971 | { "RU Port ID", "oran_fh_cus.ru_port_id",
7972 | FT_UINT16, BASE_DEC,
7973 | NULL((void*)0), 0x0,
7974 | "Logical flow - width set in dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7975 | },
7976 |
7977 | /* Section 5.1.3.2.8 */
7978 | { &hf_oran_sequence_id,
7979 | { "Sequence ID", "oran_fh_cus.sequence_id",
7980 | FT_UINT8, BASE_DEC,
7981 | NULL((void*)0), 0x0,
7982 | "The Sequence ID wraps around individually per eAxC", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7983 | },
7984 |
7985 | /* Section 5.1.3.2.8 */
7986 | { &hf_oran_e_bit,
7987 | { "E Bit", "oran_fh_cus.e_bit",
7988 | FT_UINT8, BASE_DEC,
7989 | VALS(e_bit)((0 ? (const struct _value_string*)0 : ((e_bit)))), 0x80,
7990 | "Indicate the last message of a subsequence (U-Plane only)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7991 | },
7992 |
7993 | /* Section 5.1.3.2.8 */
7994 | { &hf_oran_subsequence_id,
7995 | { "Subsequence ID", "oran_fh_cus.subsequence_id",
7996 | FT_UINT8, BASE_DEC,
7997 | NULL((void*)0), 0x7f,
7998 | "The subsequence ID (for eCPRI layer fragmentation)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
7999 | },
8000 |
8001 | { &hf_oran_previous_frame,
8002 | { "Previous frame in stream", "oran_fh_cus.previous-frame",
8003 | FT_FRAMENUM, BASE_NONE,
8004 | FRAMENUM_TYPE(FT_FRAMENUM_NONE)((gpointer) (glong) (FT_FRAMENUM_NONE)), 0x0,
8005 | "Previous frame in sequence", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8006 | },
8007 |
8008 | /* Section 7.5.2.1 */
8009 | { &hf_oran_data_direction,
8010 | { "Data Direction", "oran_fh_cus.data_direction",
8011 | FT_UINT8, BASE_DEC,
8012 | VALS(data_direction_vals)((0 ? (const struct _value_string*)0 : ((data_direction_vals) ))), 0x80,
8013 | "gNB data direction", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8014 | },
8015 |
8016 | /* Section 7.5.2.2 */
8017 | { &hf_oran_payload_version,
8018 | { "Payload Version", "oran_fh_cus.payloadVersion",
8019 | FT_UINT8, BASE_DEC,
8020 | NULL((void*)0), 0x70,
8021 | "Payload protocol version the following IEs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8022 | },
8023 |
8024 | /* Section 7.5.2.3 */
8025 | { &hf_oran_filter_index,
8026 | { "Filter Index", "oran_fh_cus.filterIndex",
8027 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8028 | RVALS(filter_indices)((0 ? (const struct _range_string*)0 : ((filter_indices)))), 0x0f,
8029 | "used between IQ data and air interface, both in DL and UL", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8030 | },
8031 |
8032 | /* Section 7.5.2.4 */
8033 | { &hf_oran_frame_id,
8034 | { "Frame ID", "oran_fh_cus.frameId",
8035 | FT_UINT8, BASE_DEC,
8036 | NULL((void*)0), 0x0,
8037 | "A counter for 10 ms frames (wrapping period 2.56 seconds)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8038 | },
8039 |
8040 | /* Section 7.5.2.5 */
8041 | { &hf_oran_subframe_id,
8042 | { "Subframe ID", "oran_fh_cus.subframe_id",
8043 | FT_UINT8, BASE_DEC,
8044 | NULL((void*)0), 0xf0,
8045 | "A counter for 1 ms sub-frames within 10ms frame", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8046 | },
8047 |
8048 | /* Section 7.5.2.6 */
8049 | { &hf_oran_slot_id,
8050 | { "Slot ID", "oran_fh_cus.slotId",
8051 | FT_UINT16, BASE_DEC,
8052 | NULL((void*)0), 0x0fc0,
8053 | "Slot number within a 1ms sub-frame", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8054 | },
8055 |
8056 | /* Generated for convenience */
8057 | { &hf_oran_slot_within_frame,
8058 | { "Slot within frame", "oran_fh_cus.slot-within-frame",
8059 | FT_UINT16, BASE_DEC,
8060 | NULL((void*)0), 0x0,
8061 | "Slot within frame, to match DCT logs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8062 | },
8063 |
8064 | /* Section 7.5.2.7 */
8065 | { &hf_oran_start_symbol_id,
8066 | { "Start Symbol ID", "oran_fh_cus.startSymbolId",
8067 | FT_UINT8, BASE_DEC,
8068 | NULL((void*)0), 0x3f,
8069 | "The first symbol number within slot affected", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8070 | },
8071 |
8072 | /* Section 7.5.2.8 */
8073 | { &hf_oran_numberOfSections,
8074 | { "Number of Sections", "oran_fh_cus.numberOfSections",
8075 | FT_UINT8, BASE_DEC,
8076 | NULL((void*)0), 0x0,
8077 | "The number of section IDs included in this message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8078 | },
8079 |
8080 | /* Section 7.5.2.9 */
8081 | { &hf_oran_sectionType,
8082 | { "Section Type", "oran_fh_cus.sectionType",
8083 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8084 | RVALS(section_types)((0 ? (const struct _range_string*)0 : ((section_types)))), 0x0,
8085 | "Determines the characteristics of U-plane data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8086 | },
8087 |
8088 | /* Section 7.5.2.10 */
8089 | { &hf_oran_udCompHdr,
8090 | { "udCompHdr", "oran_fh_cus.udCompHdr",
8091 | FT_STRING, BASE_NONE,
8092 | NULL((void*)0), 0x0,
8093 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8094 | },
8095 |
8096 | /* Section 7.5.2.11 */
8097 | { &hf_oran_numberOfUEs,
8098 | { "Number Of UEs", "oran_fh_cus.numberOfUEs",
8099 | FT_UINT8, BASE_DEC,
8100 | NULL((void*)0), 0x0,
8101 | "Indicates number of UEs for which channel info is provided", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8102 | },
8103 |
8104 | /* Section 7.5.2.12 */
8105 | { &hf_oran_timeOffset,
8106 | { "Time Offset", "oran_fh_cus.timeOffset",
8107 | FT_UINT16, BASE_DEC,
8108 | NULL((void*)0), 0x0,
8109 | "from start of the slot to start of CP in samples", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8110 | },
8111 |
8112 | /* Section 7.5.2.13 */
8113 | { &hf_oran_frameStructure_fft,
8114 | { "FFT Size", "oran_fh_cus.frameStructure.fft",
8115 | FT_UINT8, BASE_HEX | BASE_RANGE_STRING0x00000100,
8116 | RVALS(frame_structure_fft)((0 ? (const struct _range_string*)0 : ((frame_structure_fft) ))), 0xf0,
8117 | "The FFT/iFFT size being used for all IQ data processing related to this message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8118 | },
8119 |
8120 | /* Section 7.5.2.13 */
8121 | { &hf_oran_frameStructure_subcarrier_spacing,
8122 | { "Subcarrier Spacing", "oran_fh_cus.frameStructure.spacing",
8123 | FT_UINT8, BASE_HEX | BASE_RANGE_STRING0x00000100,
8124 | RVALS(subcarrier_spacings)((0 ? (const struct _range_string*)0 : ((subcarrier_spacings) ))), 0x0f,
8125 | "The sub carrier spacing as well as the number of slots per 1ms sub-frame",
8126 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
8127 | },
8128 |
8129 | /* Section 7.5.2.14 */
8130 | { &hf_oran_cpLength,
8131 | { "cpLength", "oran_fh_cus.cpLength",
8132 | FT_UINT16, BASE_DEC,
8133 | NULL((void*)0), 0x0,
8134 | "cyclic prefix length", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8135 | },
8136 |
8137 | { &hf_oran_timing_header,
8138 | { "Timing Header", "oran_fh_cus.timingHeader",
8139 | FT_STRING, BASE_NONE,
8140 | NULL((void*)0), 0x0,
8141 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8142 | },
8143 |
8144 | /* Section 7.5.3.1 */
8145 | { &hf_oran_section_id,
8146 | { "sectionId", "oran_fh_cus.sectionId",
8147 | FT_UINT16, BASE_DEC,
8148 | NULL((void*)0), 0xfff0,
8149 | "section identifier of data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8150 | },
8151 |
8152 | /* Section 7.5.3.2 */
8153 | { &hf_oran_rb,
8154 | { "rb", "oran_fh_cus.rb",
8155 | FT_UINT8, BASE_DEC,
8156 | VALS(rb_vals)((0 ? (const struct _value_string*)0 : ((rb_vals)))), 0x08,
8157 | "resource block indicator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8158 | },
8159 |
8160 | /* Section 7.5.5.3 */
8161 | { &hf_oran_symInc,
8162 | { "symInc", "oran_fh_cus.symInc",
8163 | FT_UINT8, BASE_DEC,
8164 | VALS(sym_inc_vals)((0 ? (const struct _value_string*)0 : ((sym_inc_vals)))), 0x04,
8165 | "Symbol Number Increment Command", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8166 | },
8167 |
8168 | /* Section 7.5.3.4 */
8169 | { &hf_oran_startPrbc,
8170 | { "startPrbc", "oran_fh_cus.startPrbc",
8171 | FT_UINT16, BASE_DEC,
8172 | NULL((void*)0), 0x03ff,
8173 | "Starting PRB of Control Plane Section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8174 | },
8175 |
8176 | /* Section 7.5.3.5 */
8177 | { &hf_oran_reMask_re1,
8178 | { "RE 1", "oran_fh_cus.reMask-RE1",
8179 | FT_BOOLEAN, 16,
8180 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x8000,
8181 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8182 | },
8183 | { &hf_oran_reMask_re2,
8184 | { "RE 2", "oran_fh_cus.reMask-RE2",
8185 | FT_BOOLEAN, 16,
8186 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x4000,
8187 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8188 | },
8189 | { &hf_oran_reMask_re3,
8190 | { "RE 3", "oran_fh_cus.reMask-RE3",
8191 | FT_BOOLEAN, 16,
8192 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x2000,
8193 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8194 | },
8195 | { &hf_oran_reMask_re4,
8196 | { "RE 4", "oran_fh_cus.reMask-RE4",
8197 | FT_BOOLEAN, 16,
8198 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x1000,
8199 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8200 | },
8201 | { &hf_oran_reMask_re5,
8202 | { "RE 5", "oran_fh_cus.reMask-RE5",
8203 | FT_BOOLEAN, 16,
8204 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0800,
8205 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8206 | },
8207 | { &hf_oran_reMask_re6,
8208 | { "RE 6", "oran_fh_cus.reMask-RE6",
8209 | FT_BOOLEAN, 16,
8210 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0400,
8211 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8212 | },
8213 | { &hf_oran_reMask_re7,
8214 | { "RE 7", "oran_fh_cus.reMask-RE7",
8215 | FT_BOOLEAN, 16,
8216 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0200,
8217 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8218 | },
8219 | { &hf_oran_reMask_re8,
8220 | { "RE 8", "oran_fh_cus.reMask-RE8",
8221 | FT_BOOLEAN, 16,
8222 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0100,
8223 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8224 | },
8225 | { &hf_oran_reMask_re9,
8226 | { "RE 9", "oran_fh_cus.reMask-RE9",
8227 | FT_BOOLEAN, 16,
8228 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0080,
8229 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8230 | },
8231 | { &hf_oran_reMask_re10,
8232 | { "RE 10", "oran_fh_cus.reMask-RE10",
8233 | FT_BOOLEAN, 16,
8234 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0040,
8235 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8236 | },
8237 | { &hf_oran_reMask_re11,
8238 | { "RE 11", "oran_fh_cus.reMask-RE11",
8239 | FT_BOOLEAN, 16,
8240 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0020,
8241 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8242 | },
8243 | { &hf_oran_reMask_re12,
8244 | { "RE 12", "oran_fh_cus.reMask-RE12",
8245 | FT_BOOLEAN, 16,
8246 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0010,
8247 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8248 | },
8249 | { &hf_oran_reMask,
8250 | { "RE Mask", "oran_fh_cus.reMask",
8251 | FT_UINT16, BASE_HEX,
8252 | NULL((void*)0), 0xfff0,
8253 | "The Resource Element (RE) mask within a PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8254 | },
8255 |
8256 | /* Section 7.5.3.6 */
8257 | { &hf_oran_numPrbc,
8258 | { "numPrbc", "oran_fh_cus.numPrbc",
8259 | FT_UINT8, BASE_DEC,
8260 | NULL((void*)0), 0x0,
8261 | "Number of contiguous PRBs per data section description", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8262 | },
8263 | /* Section 7.5.3.7 */
8264 | { &hf_oran_numSymbol,
8265 | { "Number of Symbols", "oran_fh_cus.numSymbol",
8266 | FT_UINT8, BASE_DEC,
8267 | NULL((void*)0), 0x0f,
8268 | "Defines number of symbols to which the section control is applicable", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8269 | },
8270 | /* Section 7.5.3.8 */
8271 | { &hf_oran_ef,
8272 | { "Extension Flag", "oran_fh_cus.ef",
8273 | FT_BOOLEAN, 8,
8274 | NULL((void*)0), 0x80,
8275 | "Indicates if more section extensions follow", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8276 | },
8277 | /* Section 7.5.3.9 */
8278 | { &hf_oran_beamId,
8279 | { "Beam ID", "oran_fh_cus.beamId",
8280 | FT_UINT16, BASE_DEC,
8281 | NULL((void*)0), 0x7fff,
8282 | "Defines the beam pattern to be applied to the U-Plane data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8283 | },
8284 |
8285 | { &hf_oran_extension,
8286 | { "Extension", "oran_fh_cus.extension",
8287 | FT_STRING, BASE_NONE,
8288 | NULL((void*)0), 0x0,
8289 | "Section extension", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8290 | },
8291 |
8292 | /* Section 7.6.2.1 */
8293 | { &hf_oran_exttype,
8294 | { "extType", "oran_fh_cus.extType",
8295 | FT_UINT8, BASE_DEC|BASE_EXT_STRING0x00000200,
8296 | &exttype_vals_ext, 0x7f,
8297 | "The extension type, which provides additional parameters specific to subject data extension", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8298 | },
8299 |
8300 | /* Section 7.6.2.3 */
8301 | { &hf_oran_extlen,
8302 | { "extLen", "oran_fh_cus.extLen",
8303 | FT_UINT16, BASE_DEC,
8304 | NULL((void*)0), 0x0,
8305 | "Extension length in 32-bit words", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8306 | },
8307 |
8308 | /* Section 7.7.1 */
8309 | { &hf_oran_bfw,
8310 | { "bfw", "oran_fh_cus.bfw",
8311 | FT_STRING, BASE_NONE,
8312 | NULL((void*)0), 0x0,
8313 | "Set of weights for a particular antenna", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8314 | },
8315 | { &hf_oran_bfw_bundle,
8316 | { "Bundle", "oran_fh_cus.bfw.bundle",
8317 | FT_STRING, BASE_NONE,
8318 | NULL((void*)0), 0x0,
8319 | "Bundle of BFWs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8320 | },
8321 | { &hf_oran_bfw_bundle_id,
8322 | { "Bundle Id", "oran_fh_cus.bfw.bundleId",
8323 | FT_UINT32, BASE_DEC,
8324 | NULL((void*)0), 0x0,
8325 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8326 | },
8327 | /* Section 7.7.1.4 */
8328 | { &hf_oran_bfw_i,
8329 | { "bfwI", "oran_fh_cus.bfwI",
8330 | FT_FLOAT, BASE_NONE,
8331 | NULL((void*)0), 0x0,
8332 | "In-phase", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8333 | },
8334 | /* Section 7.7.1.5 */
8335 | { &hf_oran_bfw_q,
8336 | { "bfwQ", "oran_fh_cus.bfwQ",
8337 | FT_FLOAT, BASE_NONE,
8338 | NULL((void*)0), 0x0,
8339 | "Quadrature", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8340 | },
8341 |
8342 | /* Section 7.5.3.10 */
8343 | { &hf_oran_ueId,
8344 | { "UE ID", "oran_fh_cus.ueId",
8345 | FT_UINT16, BASE_DEC,
8346 | NULL((void*)0), 0x7fff,
8347 | "logical identifier for set of channel info", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8348 | },
8349 | /* Section 7.5.3.11 */
8350 | { &hf_oran_freqOffset,
8351 | { "Frequency Offset", "oran_fh_cus.freqOffset",
8352 | FT_UINT24, BASE_DEC,
8353 | NULL((void*)0), 0x0,
8354 | "with respect to the carrier center frequency before additional filtering", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8355 | },
8356 |
8357 | /* Section 7.5.3.12 */
8358 | { &hf_oran_regularizationFactor,
8359 | { "Regularization Factor", "oran_fh_cus.regularizationFactor",
8360 | FT_INT16, BASE_DEC,
8361 | NULL((void*)0), 0x0,
8362 | "Signed value to support MMSE operation within O-RU", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8363 | },
8364 | /* Section 7.5.3.14 */
8365 | { &hf_oran_laaMsgType,
8366 | { "LAA Message Type", "oran_fh_cus.laaMsgType",
8367 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8368 | RVALS(laaMsgTypes)((0 ? (const struct _range_string*)0 : ((laaMsgTypes)))), 0xf0,
8369 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8370 | },
8371 | /* Section 7.5.3.15 */
8372 | { &hf_oran_laaMsgLen,
8373 | { "LAA Message Length", "oran_fh_cus.laaMsgLen",
8374 | FT_UINT8, BASE_DEC,
8375 | NULL((void*)0), 0x0f,
8376 | "number of 32-bit words in the LAA section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8377 | },
8378 | /* Section 7.5.3.16 */
8379 | { &hf_oran_lbtHandle,
8380 | { "LBT Handle", "oran_fh_cus.lbtHandle",
8381 | FT_UINT16, BASE_HEX,
8382 | NULL((void*)0), 0x0,
8383 | "label to identify transaction", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8384 | },
8385 | /* Section 7.5.3.17 */
8386 | { &hf_oran_lbtDeferFactor,
8387 | { "Defer Factor", "oran_fh_cus.lbtDeferFactor",
8388 | FT_UINT8, BASE_DEC,
8389 | NULL((void*)0), 0x07,
8390 | "Defer factor in sensing slots as described in 3GPP TS 36.213 Section 15.1.1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8391 | },
8392 | /* Section 7.5.3.18 */
8393 | { &hf_oran_lbtBackoffCounter,
8394 | { "Backoff Counter", "oran_fh_cus.lbtBackoffCounter",
8395 | FT_UINT16, BASE_DEC,
8396 | NULL((void*)0), 0xffc0,
8397 | "LBT backoff counter in sensing slots as described in 3GPP TS 36.213 Section 15.1.1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8398 | },
8399 | /* Section 7.5.3.19 */
8400 | { &hf_oran_lbtOffset,
8401 | { "LBT Offset", "oran_fh_cus.lbtOffset",
8402 | FT_UINT16, BASE_DEC,
8403 | NULL((void*)0), 0xffc0,
8404 | "LBT start time in microseconds from the beginning of the subframe scheduled by this message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8405 | },
8406 | /* Section 7.5.3.20 */
8407 | { &hf_oran_MCOT,
8408 | { "Maximum Channel Occupancy Time", "oran_fh_cus.MCOT",
8409 | FT_UINT8, BASE_DEC,
8410 | NULL((void*)0), 0x3c,
8411 | "LTE TXOP duration in subframes as described in 3GPP TS 36.213 Section 15.1.1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8412 | },
8413 | /* Section 7.5.3.21 */
8414 | { &hf_oran_lbtMode,
8415 | { "LBT Mode", "oran_fh_cus.lbtMode",
8416 | FT_UINT8, BASE_DEC,
8417 | VALS(lbtMode_vals)((0 ? (const struct _value_string*)0 : ((lbtMode_vals)))), 0x0,
8418 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8419 | },
8420 | /* Section 7.5.3.22 */
8421 | { &hf_oran_lbtPdschRes,
8422 | { "lbtPdschRes", "oran_fh_cus.lbtPdschRes",
8423 | FT_UINT8, BASE_DEC,
8424 | VALS(lbtPdschRes_vals)((0 ? (const struct _value_string*)0 : ((lbtPdschRes_vals)))), 0xc0,
8425 | "LBT result of SFN/SF", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8426 | },
8427 | /* Section 7.5.3.23 */
8428 | { &hf_oran_sfStatus,
8429 | { "sfStatus", "oran_fh_cus.sfStatus",
8430 | FT_BOOLEAN, 8,
8431 | TFS(&tfs_sfStatus)((0 ? (const struct true_false_string*)0 : ((&tfs_sfStatus )))), 0x10,
8432 | "Indicates whether the subframe was dropped or transmitted", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8433 | },
8434 | /* Section 7.5.3.24 */
8435 | { &hf_oran_lbtDrsRes,
8436 | { "lbtDrsRes", "oran_fh_cus.lbtDrsRes",
8437 | FT_BOOLEAN, 8,
8438 | TFS(&tfs_fail_success)((0 ? (const struct true_false_string*)0 : ((&tfs_fail_success )))), 0x80,
8439 | "Indicates whether the subframe was dropped or transmitted", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8440 | },
8441 | /* Section 7.5.3.25 */
8442 | { &hf_oran_initialPartialSF,
8443 | { "Initial partial SF", "oran_fh_cus.initialPartialSF",
8444 | FT_BOOLEAN, 8,
8445 | TFS(&tfs_partial_full_sf)((0 ? (const struct true_false_string*)0 : ((&tfs_partial_full_sf )))), 0x40,
8446 | "Indicates whether the initial SF in the LBT process is full or partial", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8447 | },
8448 | /* Section 7.5.3.26. */
8449 | { &hf_oran_lbtBufErr,
8450 | { "lbtBufErr", "oran_fh_cus.lbtBufErr",
8451 | FT_BOOLEAN, 8,
8452 | TFS(&tfs_lbtBufErr)((0 ? (const struct true_false_string*)0 : ((&tfs_lbtBufErr )))), 0x80,
8453 | "LBT buffer error", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8454 | },
8455 | /* Section 7.5.3.27 */
8456 | { &hf_oran_sfnSfEnd,
8457 | { "SFN/SF End", "oran_fh_cus.sfnSfEnd",
8458 | FT_UINT16, BASE_DEC,
8459 | NULL((void*)0), 0x0fff,
8460 | "SFN/SF by which the DRS window must end", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8461 | },
8462 | /* Section 7.5.3.28 */
8463 | { &hf_oran_lbtCWConfig_H,
8464 | { "lbtCWConfig_H", "oran_fh_cus.lbtCWConfig_H",
8465 | FT_UINT8, BASE_DEC,
8466 | NULL((void*)0), 0x0,
8467 | "HARQ parameters for congestion window management", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8468 | },
8469 | /* Section 7.5.3.29 */
8470 | { &hf_oran_lbtCWConfig_T,
8471 | { "lbtCWConfig_T", "oran_fh_cus.lbtCWConfig_T",
8472 | FT_UINT8, BASE_DEC,
8473 | NULL((void*)0), 0x0,
8474 | "TB parameters for congestion window management", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8475 | },
8476 | /* Section 7.5.3.30 */
8477 | { &hf_oran_lbtTrafficClass,
8478 | { "lbtTrafficClass", "oran_fh_cus.lbtTrafficClass",
8479 | FT_UINT8, BASE_DEC,
8480 | VALS(lbtTrafficClass_vals)((0 ? (const struct _value_string*)0 : ((lbtTrafficClass_vals )))), 0x38,
8481 | "Traffic class priority for congestion window management", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8482 | },
8483 | /* Section 7.5.3.31 */
8484 | { &hf_oran_lbtCWR_Rst,
8485 | { "lbtCWR_Rst", "oran_fh_cus.lbtCWR_Rst",
8486 | FT_BOOLEAN, 8,
8487 | TFS(&tfs_fail_success)((0 ? (const struct true_false_string*)0 : ((&tfs_fail_success )))), 0x80,
8488 | "notification about packet reception successful or not", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8489 | },
8490 |
8491 | /* Reserved fields */
8492 | { &hf_oran_reserved,
8493 | { "reserved", "oran_fh_cus.reserved",
8494 | FT_UINT64, BASE_HEX,
8495 | NULL((void*)0), 0x0,
8496 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8497 | },
8498 | { &hf_oran_reserved_1bit,
8499 | { "reserved", "oran_fh_cus.reserved",
8500 | FT_UINT8, BASE_HEX,
8501 | NULL((void*)0), 0x80,
8502 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8503 | },
8504 | { &hf_oran_reserved_2bits,
8505 | { "reserved", "oran_fh_cus.reserved",
8506 | FT_UINT8, BASE_HEX,
8507 | NULL((void*)0), 0xc0,
8508 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8509 | },
8510 | { &hf_oran_reserved_3bits,
8511 | { "reserved", "oran_fh_cus.reserved",
8512 | FT_UINT8, BASE_HEX,
8513 | NULL((void*)0), 0xe0,
8514 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8515 | },
8516 | { &hf_oran_reserved_4bits,
8517 | { "reserved", "oran_fh_cus.reserved",
8518 | FT_UINT8, BASE_HEX,
8519 | NULL((void*)0), 0xf0,
8520 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8521 | },
8522 | { &hf_oran_reserved_last_4bits,
8523 | { "reserved", "oran_fh_cus.reserved",
8524 | FT_UINT8, BASE_HEX,
8525 | NULL((void*)0), 0x0f,
8526 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8527 | },
8528 | { &hf_oran_reserved_last_5bits,
8529 | { "reserved", "oran_fh_cus.reserved",
8530 | FT_UINT8, BASE_HEX,
8531 | NULL((void*)0), 0x1f,
8532 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8533 | },
8534 | { &hf_oran_reserved_6bits,
8535 | { "reserved", "oran_fh_cus.reserved",
8536 | FT_UINT8, BASE_HEX,
8537 | NULL((void*)0), 0xfc,
8538 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8539 | },
8540 | { &hf_oran_reserved_last_6bits,
8541 | { "reserved", "oran_fh_cus.reserved",
8542 | FT_UINT8, BASE_HEX,
8543 | NULL((void*)0), 0x3f,
8544 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8545 | },
8546 | { &hf_oran_reserved_7bits,
8547 | { "reserved", "oran_fh_cus.reserved",
8548 | FT_UINT8, BASE_HEX,
8549 | NULL((void*)0), 0xfe,
8550 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8551 | },
8552 | { &hf_oran_reserved_last_7bits,
8553 | { "reserved", "oran_fh_cus.reserved",
8554 | FT_UINT8, BASE_HEX,
8555 | NULL((void*)0), 0x7f,
8556 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8557 | },
8558 | { &hf_oran_reserved_8bits,
8559 | { "reserved", "oran_fh_cus.reserved",
8560 | FT_UINT8, BASE_HEX,
8561 | NULL((void*)0), 0x0,
8562 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8563 | },
8564 | { &hf_oran_reserved_16bits,
8565 | { "reserved", "oran_fh_cus.reserved",
8566 | FT_UINT16, BASE_HEX,
8567 | NULL((void*)0), 0x0,
8568 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8569 | },
8570 | { &hf_oran_reserved_15bits,
8571 | { "reserved", "oran_fh_cus.reserved",
8572 | FT_UINT16, BASE_HEX,
8573 | NULL((void*)0), 0x7fff,
8574 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8575 | },
8576 | { &hf_oran_reserved_bit1,
8577 | { "reserved", "oran_fh_cus.reserved",
8578 | FT_UINT8, BASE_HEX,
8579 | NULL((void*)0), 0x40,
8580 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8581 | },
8582 | { &hf_oran_reserved_bit2,
8583 | { "reserved", "oran_fh_cus.reserved",
8584 | FT_UINT8, BASE_HEX,
8585 | NULL((void*)0), 0x20,
8586 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8587 | },
8588 | { &hf_oran_reserved_bit4,
8589 | { "reserved", "oran_fh_cus.reserved",
8590 | FT_UINT8, BASE_HEX,
8591 | NULL((void*)0), 0x08,
8592 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8593 | },
8594 | { &hf_oran_reserved_bit5,
8595 | { "reserved", "oran_fh_cus.reserved",
8596 | FT_UINT8, BASE_HEX,
8597 | NULL((void*)0), 0x04,
8598 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8599 | },
8600 | { &hf_oran_reserved_bits123,
8601 | { "reserved", "oran_fh_cus.reserved",
8602 | FT_UINT8, BASE_HEX,
8603 | NULL((void*)0), 0x70,
8604 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8605 | },
8606 | { &hf_oran_reserved_bits456,
8607 | { "reserved", "oran_fh_cus.reserved",
8608 | FT_UINT8, BASE_HEX,
8609 | NULL((void*)0), 0x0e,
8610 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8611 | },
8612 |
8613 | /* 7.7.11.9 */
8614 | { &hf_oran_cont_ind,
8615 | { "contInd", "oran_fh_cus.contInd",
8616 | FT_BOOLEAN, 8,
8617 | TFS(&continuity_indication_tfs)((0 ? (const struct true_false_string*)0 : ((&continuity_indication_tfs )))), 0x80,
8618 | "PRB region continuity flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8619 | },
8620 | /* 7.7.11.10 */
8621 | { &hf_oran_bundle_offset,
8622 | { "BundleOffset", "oran_fh_cus.bundleOffset",
8623 | FT_UINT8, BASE_DEC,
8624 | NULL((void*)0), 0x3f,
8625 | "offset between start of first PRB bundle and startPrbc", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8626 | },
8627 |
8628 | /* 7.7.1.2 bfwCompHdr (beamforming weight compression header) */
8629 | { &hf_oran_bfwCompHdr,
8630 | { "bfwCompHdr", "oran_fh_cus.bfwCompHdr",
8631 | FT_STRING, BASE_NONE,
8632 | NULL((void*)0), 0x0,
8633 | "Compression method and IQ bit width for beamforming weights", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8634 | },
8635 | { &hf_oran_bfwCompHdr_iqWidth,
8636 | { "IQ Bit Width", "oran_fh_cus.bfwCompHdr_iqWidth",
8637 | FT_UINT8, BASE_HEX,
8638 | VALS(bfw_comp_headers_iq_width)((0 ? (const struct _value_string*)0 : ((bfw_comp_headers_iq_width )))), 0xf0,
8639 | "IQ bit width for the beamforming weights", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8640 | },
8641 | { &hf_oran_bfwCompHdr_compMeth,
8642 | { "Compression Method", "oran_fh_cus.bfwCompHdr_compMeth",
8643 | FT_UINT8, BASE_HEX,
8644 | VALS(bfw_comp_headers_comp_meth)((0 ? (const struct _value_string*)0 : ((bfw_comp_headers_comp_meth )))), 0x0f,
8645 | "compression method for the beamforming weights", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8646 | },
8647 |
8648 | /* 7.5.3.32 */
8649 | { &hf_oran_ciCompParam,
8650 | { "ciCompParam", "oran_fh_cus.ciCompParam",
8651 | FT_STRING, BASE_NONE,
8652 | NULL((void*)0), 0x0,
8653 | "channel information compression parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8654 | },
8655 |
8656 | /* Table 7.5.3.32-1 */
8657 | { &hf_oran_blockScaler,
8658 | { "blockScaler", "oran_fh_cus.blockScaler",
8659 | FT_UINT8, BASE_HEX,
8660 | NULL((void*)0), 0x0,
8661 | "unsigned, 1 integer bit, 7 fractional bits", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8662 | },
8663 | { &hf_oran_compBitWidth,
8664 | { "compBitWidth", "oran_fh_cus.compBitWidth",
8665 | FT_UINT8, BASE_DEC,
8666 | NULL((void*)0), 0xf0,
8667 | "Length of I bits and length of Q bits after compression over entire PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8668 | },
8669 | { &hf_oran_compShift,
8670 | { "compShift", "oran_fh_cus.compShift",
8671 | FT_UINT8, BASE_DEC,
8672 | NULL((void*)0), 0x0f,
8673 | "The shift applied to the entire PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8674 | },
8675 |
8676 | { &hf_oran_active_beamspace_coefficient_n1,
8677 | { "N1", "oran_fh_cus.activeBeamspace_Coefficient_n1",
8678 | FT_BOOLEAN, 8,
8679 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x80,
8680 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8681 | },
8682 | { &hf_oran_active_beamspace_coefficient_n2,
8683 | { "N2", "oran_fh_cus.activeBeamspace_Coefficient_n2",
8684 | FT_BOOLEAN, 8,
8685 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x40,
8686 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8687 | },
8688 | { &hf_oran_active_beamspace_coefficient_n3,
8689 | { "N3", "oran_fh_cus.activeBeamspace_Coefficient_n3",
8690 | FT_BOOLEAN, 8,
8691 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x20,
8692 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8693 | },
8694 | { &hf_oran_active_beamspace_coefficient_n4,
8695 | { "N4", "oran_fh_cus.activeBeamspace_Coefficient_n4",
8696 | FT_BOOLEAN, 8,
8697 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x10,
8698 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8699 | },
8700 | { &hf_oran_active_beamspace_coefficient_n5,
8701 | { "N5", "oran_fh_cus.activeBeamspace_Coefficient_n5",
8702 | FT_BOOLEAN, 8,
8703 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x08,
8704 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8705 | },
8706 | { &hf_oran_active_beamspace_coefficient_n6,
8707 | { "N6", "oran_fh_cus.activeBeamspace_Coefficient_n6",
8708 | FT_BOOLEAN, 8,
8709 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x04,
8710 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8711 | },
8712 | { &hf_oran_active_beamspace_coefficient_n7,
8713 | { "N7", "oran_fh_cus.activeBeamspace_Coefficient_n7",
8714 | FT_BOOLEAN, 8,
8715 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x02,
8716 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8717 | },
8718 | { &hf_oran_active_beamspace_coefficient_n8,
8719 | { "N8", "oran_fh_cus.activeBeamspace_Coefficient_n8",
8720 | FT_BOOLEAN, 8,
8721 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x01,
8722 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8723 | },
8724 |
8725 | { &hf_oran_activeBeamspaceCoefficientMask,
8726 | { "activeBeamspaceCoefficientMask", "oran_fh_cus.activeBeamspaceCoefficientMask",
8727 | FT_UINT8, BASE_HEX,
8728 | NULL((void*)0), 0xff,
8729 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8730 | },
8731 | { &hf_oran_activeBeamspaceCoefficientMask_bits_set,
8732 | { "Array elements set", "oran_fh_cus.activeBeamspaceCoefficientMask.bits-set",
8733 | FT_UINT32, BASE_DEC,
8734 | NULL((void*)0), 0x0,
8735 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8736 | },
8737 |
8738 | /* Section 7.7.6.6 */
8739 | { &hf_oran_se6_repetition,
8740 | { "repetition", "oran_fh_cus.repetition",
8741 | FT_BOOLEAN, BASE_NONE,
8742 | TFS(&repetition_se6_tfs)((0 ? (const struct true_false_string*)0 : ((&repetition_se6_tfs )))), 0x0,
8743 | "Repetition of a highest priority data section for C-Plane", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8744 | },
8745 | /* 7.7.20.9 */
8746 | { &hf_oran_rbgSize,
8747 | { "rbgSize", "oran_fh_cus.rbgSize",
8748 | FT_UINT8, BASE_HEX,
8749 | VALS(rbg_size_vals)((0 ? (const struct _value_string*)0 : ((rbg_size_vals)))), 0x70,
8750 | "Number of PRBs of the resource block groups allocated by the bit mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8751 | },
8752 | /* 7.7.20.10 */
8753 | { &hf_oran_rbgMask,
8754 | { "rbgMask", "oran_fh_cus.rbgMask",
8755 | FT_UINT32, BASE_HEX,
8756 | NULL((void*)0), 0x0fffffff,
8757 | "Each bit indicates whether a corresponding resource block group is present", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8758 | },
8759 | /* 7.7.6.5. Also 7.7.12.3 and 7.7.19.5 */
8760 | { &hf_oran_noncontig_priority,
8761 | { "priority", "oran_fh_cus.priority",
8762 | FT_UINT8, BASE_HEX,
8763 | VALS(priority_vals)((0 ? (const struct _value_string*)0 : ((priority_vals)))), 0xc0,
8764 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8765 | },
8766 |
8767 | /* 7.7.6.4 */
8768 | { &hf_oran_symbol_mask,
8769 | { "symbolMask", "oran_fh_cus.symbolMask",
8770 | FT_UINT16, BASE_HEX,
8771 | NULL((void*)0), 0x3fff,
8772 | "Each bit indicates whether the rbgMask applies to a given symbol in the slot", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8773 | },
8774 | { &hf_oran_symbol_mask_s13,
8775 | { "symbol 13", "oran_fh_cus.symbolMask.symbol-13",
8776 | FT_BOOLEAN, 16,
8777 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x2000,
8778 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8779 | },
8780 | { &hf_oran_symbol_mask_s12,
8781 | { "symbol 12", "oran_fh_cus.symbolMask.symbol-12",
8782 | FT_BOOLEAN, 16,
8783 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x1000,
8784 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8785 | },
8786 | { &hf_oran_symbol_mask_s11,
8787 | { "symbol 11", "oran_fh_cus.symbolMask.symbol-11",
8788 | FT_BOOLEAN, 16,
8789 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0800,
8790 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8791 | },
8792 | { &hf_oran_symbol_mask_s10,
8793 | { "symbol 10", "oran_fh_cus.symbolMask.symbol-10",
8794 | FT_BOOLEAN, 16,
8795 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0400,
8796 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8797 | },
8798 | { &hf_oran_symbol_mask_s9,
8799 | { "symbol 9", "oran_fh_cus.symbolMask.symbol-9",
8800 | FT_BOOLEAN, 16,
8801 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0200,
8802 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8803 | },
8804 | { &hf_oran_symbol_mask_s8,
8805 | { "symbol 8", "oran_fh_cus.symbolMask.symbol-8",
8806 | FT_BOOLEAN, 16,
8807 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0100,
8808 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8809 | },
8810 | { &hf_oran_symbol_mask_s7,
8811 | { "symbol 7", "oran_fh_cus.symbolMask.symbol-7",
8812 | FT_BOOLEAN, 16,
8813 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0080,
8814 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8815 | },
8816 | { &hf_oran_symbol_mask_s6,
8817 | { "symbol 6", "oran_fh_cus.symbolMask.symbol-6",
8818 | FT_BOOLEAN, 16,
8819 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0040,
8820 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8821 | },
8822 | { &hf_oran_symbol_mask_s5,
8823 | { "symbol 5", "oran_fh_cus.symbolMask.symbol-5",
8824 | FT_BOOLEAN, 16,
8825 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0020,
8826 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8827 | },
8828 | { &hf_oran_symbol_mask_s4,
8829 | { "symbol 4", "oran_fh_cus.symbolMask.symbol-4",
8830 | FT_BOOLEAN, 16,
8831 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0010,
8832 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8833 | },
8834 | { &hf_oran_symbol_mask_s3,
8835 | { "symbol 3", "oran_fh_cus.symbolMask.symbol-3",
8836 | FT_BOOLEAN, 16,
8837 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0008,
8838 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8839 | },
8840 | { &hf_oran_symbol_mask_s2,
8841 | { "symbol 2", "oran_fh_cus.symbolMask.symbol-2",
8842 | FT_BOOLEAN, 16,
8843 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0004,
8844 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8845 | },
8846 | { &hf_oran_symbol_mask_s1,
8847 | { "symbol 1", "oran_fh_cus.symbolMask.symbol-1",
8848 | FT_BOOLEAN, 16,
8849 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0002,
8850 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8851 | },
8852 | { &hf_oran_symbol_mask_s0,
8853 | { "symbol 0", "oran_fh_cus.symbolMask.symbol-0",
8854 | FT_BOOLEAN, 16,
8855 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0001,
8856 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8857 | },
8858 |
8859 |
8860 | /* 7.7.22.2 */
8861 | { &hf_oran_ack_nack_req_id,
8862 | { "ackNackReqId", "oran_fh_cus.ackNackReqId",
8863 | FT_UINT16, BASE_HEX,
8864 | NULL((void*)0), 0x0,
8865 | "Indicates the ACK/NACK request ID of a section description", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8866 | },
8867 |
8868 | /* Subtree for next 2 items */
8869 | { &hf_oran_frequency_range,
8870 | { "Frequency Range", "oran_fh_cus.frequencyRange",
8871 | FT_STRING, BASE_NONE,
8872 | NULL((void*)0), 0x0,
8873 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8874 | },
8875 |
8876 | /* 7.7.12.4 */
8877 | { &hf_oran_off_start_prb,
8878 | { "offStartPrb", "oran_fh_cus.offStartPrb",
8879 | FT_UINT8, BASE_DEC,
8880 | NULL((void*)0), 0x0,
8881 | "Offset of PRB range start", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8882 | },
8883 | /* 7.7.12.5 */
8884 | { &hf_oran_num_prb,
8885 | { "numPrb", "oran_fh_cus.numPrb",
8886 | FT_UINT8, BASE_DEC,
8887 | NULL((void*)0), 0x0,
8888 | "Number of PRBs in PRB range", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8889 | },
8890 |
8891 | /* symbolId 8.3.3.7 */
8892 | { &hf_oran_symbolId,
8893 | { "Symbol Identifier", "oran_fh_cus.symbolId",
8894 | FT_UINT8, BASE_DEC,
8895 | NULL((void*)0), 0x3f,
8896 | "Identifies a symbol number within a slot", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8897 | },
8898 |
8899 | /* startPrbu 8.3.3.11 */
8900 | { &hf_oran_startPrbu,
8901 | { "startPrbu", "oran_fh_cus.startPrbu",
8902 | FT_UINT16, BASE_DEC,
8903 | NULL((void*)0), 0x03ff,
8904 | "starting PRB of user plane section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8905 | },
8906 |
8907 | /* numPrbu 8.3.3.12 */
8908 | { &hf_oran_numPrbu,
8909 | { "numPrbu", "oran_fh_cus.numPrbu",
8910 | FT_UINT8, BASE_DEC,
8911 | NULL((void*)0), 0x0,
8912 | "number of PRBs per user plane section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8913 | },
8914 |
8915 | /* 7.7.1.3 */
8916 | { &hf_oran_bfwCompParam,
8917 | { "bfwCompParam", "oran_fh_cus.bfwCompParam",
8918 | FT_STRING, BASE_NONE,
8919 | NULL((void*)0), 0x0,
8920 | "Beamforming weight compression parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8921 | },
8922 |
8923 | /* 6.3.3.13 */
8924 | { &hf_oran_udCompHdrMeth,
8925 | { "User Data Compression Method", "oran_fh_cus.udCompHdrMeth",
8926 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8927 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0f,
8928 | "Defines the compression method for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8929 | },
8930 | { &hf_oran_udCompHdrMeth_pref,
8931 | { "User Data Compression Method", "oran_fh_cus.udCompHdrMeth",
8932 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8933 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0,
8934 | "Defines the compression method for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8935 | },
8936 | /* 8.3.3.18 */
8937 | { &hf_oran_udCompLen,
8938 | { "udCompLen", "oran_fh_cus.udCompLen",
8939 | FT_UINT16, BASE_DEC,
8940 | NULL((void*)0), 0x0,
8941 | "PRB field length in octets", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8942 | },
8943 |
8944 | /* 7.5.2.10 */
8945 | { &hf_oran_udCompHdrIqWidth,
8946 | { "User Data IQ width", "oran_fh_cus.udCompHdrWidth",
8947 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8948 | RVALS(ud_comp_header_width)((0 ? (const struct _range_string*)0 : ((ud_comp_header_width )))), 0xf0,
8949 | "Defines the IQ bit width for the user data in every section in the C-Plane message", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8950 | },
8951 | { &hf_oran_udCompHdrIqWidth_pref,
8952 | { "User Data IQ width", "oran_fh_cus.udCompHdrWidth.pref",
8953 | FT_UINT8, BASE_DEC,
8954 | NULL((void*)0), 0x0,
8955 | "IQ bit width for the user data in every section in the C-Plane message, from preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8956 | },
8957 |
8958 | { &hf_oran_sinrCompHdrIqWidth_pref,
8959 | { "SINR IQ width", "oran_fh_cus.sinrCompHdrWidth",
8960 | FT_UINT8, BASE_DEC,
8961 | NULL((void*)0), 0x0,
8962 | "Defines the IQ bit width for SINR data in section type 9", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8963 | },
8964 | { &hf_oran_sinrCompHdrMeth_pref,
8965 | { "SINR Compression Method", "oran_fh_cus.sinrCompHdrMeth",
8966 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
8967 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0,
8968 | "Defines the compression method for SINR data in section type 9", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8969 | },
8970 |
8971 | /* Section 8.3.3.15 (not always present - depends upon meth) */
8972 | { &hf_oran_udCompParam,
8973 | { "User Data Compression Parameter", "oran_fh_cus.udCompParam",
8974 | FT_STRING, BASE_NONE,
8975 | NULL((void*)0), 0x0,
8976 | "Applies to whatever compression method is specified by the associated sectionID's compMeth value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8977 | },
8978 | /* 8.3.3.18 */
8979 | { &hf_oran_sReSMask,
8980 | { "sReSMask", "oran_fh_cus.sReSMask",
8981 | FT_UINT16, BASE_HEX,
8982 | NULL((void*)0), 0xf0ff,
8983 | "selective RE sending mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8984 | },
8985 |
8986 | { &hf_oran_sReSMask_re12,
8987 | { "RE-12", "oran_fh_cus.sReSMask-re12",
8988 | FT_BOOLEAN, 16,
8989 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x8000,
8990 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8991 | },
8992 | { &hf_oran_sReSMask_re11,
8993 | { "RE-11", "oran_fh_cus.sReSMask-re11",
8994 | FT_BOOLEAN, 16,
8995 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x4000,
8996 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
8997 | },
8998 | { &hf_oran_sReSMask_re10,
8999 | { "RE-10", "oran_fh_cus.sReSMask-re10",
9000 | FT_BOOLEAN, 16,
9001 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x2000,
9002 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9003 | },
9004 | { &hf_oran_sReSMask_re9,
9005 | { "RE-9", "oran_fh_cus.sReSMask-re9",
9006 | FT_BOOLEAN, 16,
9007 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x1000,
9008 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9009 | },
9010 | { &hf_oran_sReSMask_re8,
9011 | { "RE-8", "oran_fh_cus.sReSMask-re8",
9012 | FT_BOOLEAN, 16,
9013 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0080,
9014 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9015 | },
9016 | { &hf_oran_sReSMask_re7,
9017 | { "RE-7", "oran_fh_cus.sReSMask-re7",
9018 | FT_BOOLEAN, 16,
9019 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0040,
9020 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9021 | },
9022 | { &hf_oran_sReSMask_re6,
9023 | { "RE-6", "oran_fh_cus.sReSMask-re6",
9024 | FT_BOOLEAN, 16,
9025 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0020,
9026 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9027 | },
9028 | { &hf_oran_sReSMask_re5,
9029 | { "RE-5", "oran_fh_cus.sReSMask-re5",
9030 | FT_BOOLEAN, 16,
9031 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0010,
9032 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9033 | },
9034 | { &hf_oran_sReSMask_re4,
9035 | { "RE-4", "oran_fh_cus.sReSMask-re4",
9036 | FT_BOOLEAN, 16,
9037 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0008,
9038 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9039 | },
9040 | { &hf_oran_sReSMask_re3,
9041 | { "RE-3", "oran_fh_cus.sReSMask-re3",
9042 | FT_BOOLEAN, 16,
9043 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0004,
9044 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9045 | },
9046 | { &hf_oran_sReSMask_re2,
9047 | { "RE-2", "oran_fh_cus.sReSMask-re2",
9048 | FT_BOOLEAN, 16,
9049 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0002,
9050 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9051 | },
9052 | { &hf_oran_sReSMask_re1,
9053 | { "RE-1", "oran_fh_cus.sReSMask-re1",
9054 | FT_BOOLEAN, 16,
9055 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0001,
9056 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9057 | },
9058 |
9059 | /* 8.3.3.20 */
9060 | { &hf_oran_sReSMask1,
9061 | { "sReSMask1", "oran_fh_cus.sReSMask1",
9062 | FT_UINT16, BASE_HEX,
9063 | NULL((void*)0), 0x0fff,
9064 | "selective RE sending mask 1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9065 | },
9066 | /* 8.3.3.21 */
9067 | { &hf_oran_sReSMask2,
9068 | { "sReSMask2", "oran_fh_cus.sReSMask2",
9069 | FT_UINT16, BASE_HEX,
9070 | NULL((void*)0), 0x0fff,
9071 | "selective RE sending mask 2", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9072 | },
9073 |
9074 | { &hf_oran_sReSMask1_2_re12,
9075 | { "RE-12", "oran_fh_cus.sReSMask-re12",
9076 | FT_BOOLEAN, 16,
9077 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0800,
9078 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9079 | },
9080 | { &hf_oran_sReSMask1_2_re11,
9081 | { "RE-11", "oran_fh_cus.sReSMask-re11",
9082 | FT_BOOLEAN, 16,
9083 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0400,
9084 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9085 | },
9086 | { &hf_oran_sReSMask1_2_re10,
9087 | { "RE-10", "oran_fh_cus.sReSMask-re10",
9088 | FT_BOOLEAN, 16,
9089 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0200,
9090 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9091 | },
9092 | { &hf_oran_sReSMask1_2_re9,
9093 | { "RE-9", "oran_fh_cus.sReSMask-re9",
9094 | FT_BOOLEAN, 16,
9095 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0100,
9096 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9097 | },
9098 |
9099 | /* Section 6.3.3.15 */
9100 | { &hf_oran_iSample,
9101 | { "iSample", "oran_fh_cus.iSample",
9102 | FT_FLOAT, BASE_NONE,
9103 | NULL((void*)0), 0x0,
9104 | "In-phase Sample value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9105 | },
9106 |
9107 | /* Section 6.3.3.16 */
9108 | { &hf_oran_qSample,
9109 | { "qSample", "oran_fh_cus.qSample",
9110 | FT_FLOAT, BASE_NONE,
9111 | NULL((void*)0), 0x0,
9112 | "Quadrature Sample value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9113 | },
9114 |
9115 | { &hf_oran_exponent,
9116 | { "Exponent", "oran_fh_cus.exponent",
9117 | FT_UINT8, BASE_DEC,
9118 | NULL((void*)0), 0x0f,
9119 | "Exponent applicable to the I & Q mantissas", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9120 | },
9121 |
9122 | { &hf_oran_iq_user_data,
9123 | { "IQ User Data", "oran_fh_cus.iq_user_data",
9124 | FT_BYTES, BASE_NONE,
9125 | NULL((void*)0), 0x0,
9126 | "Used for the In-phase and Quadrature sample mantissa", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9127 | },
9128 |
9129 |
9130 | { &hf_oran_u_section_ul_symbol_time,
9131 | { "Microseconds since first UL U-plane frame for this symbol", "oran_fh_cus.us-since-first-ul-frame",
9132 | FT_UINT32, BASE_DEC,
9133 | NULL((void*)0), 0x0,
9134 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9135 | },
9136 | { &hf_oran_u_section_ul_symbol_frames,
9137 | { "Number of UL frames sent for this symbol", "oran_fh_cus.number-ul-frames-in-symbol",
9138 | FT_UINT32, BASE_DEC,
9139 | NULL((void*)0), 0x0,
9140 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9141 | },
9142 | { &hf_oran_u_section_ul_symbol_first_frame,
9143 | { "First UL frame for this symbol", "oran_fh_cus.first-ul-frame-in-symbol",
9144 | FT_FRAMENUM, BASE_NONE,
9145 | FRAMENUM_TYPE(FT_FRAMENUM_NONE)((gpointer) (glong) (FT_FRAMENUM_NONE)), 0x0,
9146 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9147 | },
9148 | { &hf_oran_u_section_ul_symbol_last_frame,
9149 | { "Last UL frame for this symbol", "oran_fh_cus.last-ul-frame-in-symbol",
9150 | FT_FRAMENUM, BASE_NONE,
9151 | FRAMENUM_TYPE(FT_FRAMENUM_NONE)((gpointer) (glong) (FT_FRAMENUM_NONE)), 0x0,
9152 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9153 | },
9154 |
9155 | { &hf_oran_c_eAxC_ID,
9156 | { "c_eAxC_ID", "oran_fh_cus.c_eaxc_id",
9157 | FT_STRING, BASE_NONE,
9158 | NULL((void*)0), 0x0,
9159 | "This is a calculated field for the c_eAxC ID, which identifies the message stream", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9160 | },
9161 |
9162 | { &hf_oran_refa,
9163 | { "RefA", "oran_fh_cus.refa",
9164 | FT_STRING, BASE_NONE,
9165 | NULL((void*)0), 0x0,
9166 | "This is a calculated field for the RefA ID, which provides a reference in time", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9167 | },
9168 |
9169 |
9170 | /* Section 7.5.2.15 */
9171 | { &hf_oran_ciCompHdr,
9172 | { "ciCompHdr", "oran_fh_cus.ciCompHdr",
9173 | FT_STRING, BASE_NONE,
9174 | NULL((void*)0), 0x0,
9175 | "Channel Information Compression Header", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9176 | },
9177 | { &hf_oran_ciCompHdrMeth,
9178 | { "User Data Compression Method", "oran_fh_cus.ciCompHdrMeth",
9179 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
9180 | RVALS(ud_comp_header_meth)((0 ? (const struct _range_string*)0 : ((ud_comp_header_meth) ))), 0x0e,
9181 | "Compression method for Channel Information", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9182 | },
9183 | { &hf_oran_ciCompHdrIqWidth,
9184 | { "User Data IQ width", "oran_fh_cus.ciCompHdrWidth",
9185 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
9186 | RVALS(ud_comp_header_width)((0 ? (const struct _range_string*)0 : ((ud_comp_header_width )))), 0xf0,
9187 | "IQ bit width for Channel Information", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9188 | },
9189 | { &hf_oran_ciCompOpt,
9190 | { "ciCompOpt", "oran_fh_cus.ciCompOpt",
9191 | FT_UINT8, BASE_DEC,
9192 | VALS(ci_comp_opt_vals)((0 ? (const struct _value_string*)0 : ((ci_comp_opt_vals)))), 0x01,
9193 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9194 | },
9195 |
9196 | /* 7.7.11.7 */
9197 | { &hf_oran_disable_bfws,
9198 | { "disableBFWs", "oran_fh_cus.disableBFWs",
9199 | FT_BOOLEAN, 8,
9200 | NULL((void*)0), 0x80,
9201 | "Indicate if BFWs under section extension are disabled", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9202 | },
9203 | /* 7.7.11.8 */
9204 | { &hf_oran_rad,
9205 | { "RAD", "oran_fh_cus.rad",
9206 | FT_BOOLEAN, 8,
9207 | NULL((void*)0), 0x40,
9208 | "Reset After PRB Discontinuity", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9209 | },
9210 | /* 7.7.11.4 */
9211 | { &hf_oran_num_bund_prbs,
9212 | { "numBundPrb", "oran_fh_cus.numBundPrb",
9213 | FT_UINT8, BASE_DEC,
9214 | NULL((void*)0), 0x0,
9215 | "Number of bundled PRBs per BFWs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9216 | },
9217 | { &hf_oran_beam_id,
9218 | { "beamId", "oran_fh_cus.beamId",
9219 | FT_UINT16, BASE_DEC,
9220 | NULL((void*)0), 0x7fff,
9221 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9222 | },
9223 | { &hf_oran_num_weights_per_bundle,
9224 | { "Num weights per bundle", "oran_fh_cus.num_weights_per_bundle",
9225 | FT_UINT16, BASE_DEC,
9226 | NULL((void*)0), 0x0,
9227 | "From dissector preference", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9228 | },
9229 |
9230 | { &hf_oran_samples_prb,
9231 | {"PRB", "oran_fh_cus.prb",
9232 | FT_STRING, BASE_NONE,
9233 | NULL((void*)0), 0x0,
9234 | "Grouping of samples for a particular Physical Resource Block", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9235 | },
9236 |
9237 | /* 7.5.3.13 */
9238 | { &hf_oran_ciSample,
9239 | { "ciSample", "oran_fh_cus.ciSample",
9240 | FT_STRING, BASE_NONE,
9241 | NULL((void*)0), 0x0,
9242 | "Sample (I and Q values)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9243 | },
9244 | { &hf_oran_ciIsample,
9245 | { "ciIsample", "oran_fh_cus.ciISample",
9246 | FT_FLOAT, BASE_NONE,
9247 | NULL((void*)0), 0x0,
9248 | "Channel information complex value - I part", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9249 | },
9250 | { &hf_oran_ciQsample,
9251 | { "ciQsample", "oran_fh_cus.ciQSample",
9252 | FT_FLOAT, BASE_NONE,
9253 | NULL((void*)0), 0x0,
9254 | "Channel information complex value - Q part", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9255 | },
9256 |
9257 | /* 7.7.10.2 */
9258 | { &hf_oran_beamGroupType,
9259 | { "beamGroupType", "oran_fh_cus.beamGroupType",
9260 | FT_UINT8, BASE_DEC,
9261 | VALS(beam_group_type_vals)((0 ? (const struct _value_string*)0 : ((beam_group_type_vals )))), 0xc0,
9262 | "The type of beam grouping", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9263 | },
9264 | /* 7.7.10.3 */
9265 | { &hf_oran_numPortc,
9266 | { "numPortc", "oran_fh_cus.numPortc",
9267 | FT_UINT8, BASE_DEC,
9268 | NULL((void*)0), 0x3f,
9269 | "The number of eAxC ports", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9270 | },
9271 |
9272 | /* 7.7.4.2 (1 bit) */
9273 | { &hf_oran_csf,
9274 | { "csf", "oran_fh_cus.csf",
9275 | FT_BOOLEAN, BASE_NONE,
9276 | NULL((void*)0), 0x0,
9277 | "constellation shift flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9278 | },
9279 | /* 7.7.4.3 */
9280 | { &hf_oran_modcompscaler,
9281 | { "modCompScaler", "oran_fh_cus.modcompscaler",
9282 | FT_UINT16, BASE_DEC,
9283 | NULL((void*)0), 0x7fff,
9284 | "modulation compression scaler value", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9285 | },
9286 |
9287 | /* 7.7.5.1 */
9288 | { &hf_oran_modcomp_param_set,
9289 | { "Set", "oran_fh_cus.modcomp-param-set",
9290 | FT_STRING, BASE_NONE,
9291 | NULL((void*)0), 0x0,
9292 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9293 | },
9294 |
9295 |
9296 |
9297 | /* mcScaleReMask 7.7.5.2 (12 bits) */
9298 |
9299 | /* First entry (starts with msb within byte) */
9300 | { &hf_oran_mc_scale_re_mask_re1,
9301 | { "RE 1", "oran_fh_cus.mcscalermask-RE1",
9302 | FT_BOOLEAN, 16,
9303 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x8000,
9304 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9305 | },
9306 | { &hf_oran_mc_scale_re_mask_re2,
9307 | { "RE 2", "oran_fh_cus.mcscalermask-RE2",
9308 | FT_BOOLEAN, 16,
9309 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x4000,
9310 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9311 | },
9312 | { &hf_oran_mc_scale_re_mask_re3,
9313 | { "RE 3", "oran_fh_cus.mcscalermask-RE3",
9314 | FT_BOOLEAN, 16,
9315 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x2000,
9316 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9317 | },
9318 | { &hf_oran_mc_scale_re_mask_re4,
9319 | { "RE 4", "oran_fh_cus.mcscalermask-RE4",
9320 | FT_BOOLEAN, 16,
9321 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x1000,
9322 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9323 | },
9324 | { &hf_oran_mc_scale_re_mask_re5,
9325 | { "RE 5", "oran_fh_cus.mcscalermask-RE5",
9326 | FT_BOOLEAN, 16,
9327 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0800,
9328 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9329 | },
9330 | { &hf_oran_mc_scale_re_mask_re6,
9331 | { "RE 6", "oran_fh_cus.mcscalermask-RE6",
9332 | FT_BOOLEAN, 16,
9333 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0400,
9334 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9335 | },
9336 | { &hf_oran_mc_scale_re_mask_re7,
9337 | { "RE 7", "oran_fh_cus.mcscalermask-RE7",
9338 | FT_BOOLEAN, 16,
9339 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0200,
9340 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9341 | },
9342 | { &hf_oran_mc_scale_re_mask_re8,
9343 | { "RE 8", "oran_fh_cus.mcscalermask-RE8",
9344 | FT_BOOLEAN, 16,
9345 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0100,
9346 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9347 | },
9348 | { &hf_oran_mc_scale_re_mask_re9,
9349 | { "RE 9", "oran_fh_cus.mcscalermask-RE9",
9350 | FT_BOOLEAN, 16,
9351 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0080,
9352 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9353 | },
9354 | { &hf_oran_mc_scale_re_mask_re10,
9355 | { "RE 10", "oran_fh_cus.mcscalermask-RE10",
9356 | FT_BOOLEAN, 16,
9357 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0040,
9358 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9359 | },
9360 | { &hf_oran_mc_scale_re_mask_re11,
9361 | { "RE 11", "oran_fh_cus.mcscalermask-RE11",
9362 | FT_BOOLEAN, 16,
9363 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0020,
9364 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9365 | },
9366 | { &hf_oran_mc_scale_re_mask_re12,
9367 | { "RE 12", "oran_fh_cus.mcscalermask-RE12",
9368 | FT_BOOLEAN, 16,
9369 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0010,
9370 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9371 | },
9372 |
9373 | /* Even tries entry (starts with 5th bit within byte) */
9374 | { &hf_oran_mc_scale_re_mask_re1_even,
9375 | { "RE 1", "oran_fh_cus.mcscalermask-RE1",
9376 | FT_BOOLEAN, 16,
9377 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0800,
9378 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9379 | },
9380 | { &hf_oran_mc_scale_re_mask_re2_even,
9381 | { "RE 2", "oran_fh_cus.mcscalermask-RE2",
9382 | FT_BOOLEAN, 16,
9383 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0400,
9384 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9385 | },
9386 | { &hf_oran_mc_scale_re_mask_re3_even,
9387 | { "RE 3", "oran_fh_cus.mcscalermask-RE3",
9388 | FT_BOOLEAN, 16,
9389 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0200,
9390 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9391 | },
9392 | { &hf_oran_mc_scale_re_mask_re4_even,
9393 | { "RE 4", "oran_fh_cus.mcscalermask-RE4",
9394 | FT_BOOLEAN, 16,
9395 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0100,
9396 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9397 | },
9398 | { &hf_oran_mc_scale_re_mask_re5_even,
9399 | { "RE 5", "oran_fh_cus.mcscalermask-RE5",
9400 | FT_BOOLEAN, 16,
9401 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0080,
9402 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9403 | },
9404 | { &hf_oran_mc_scale_re_mask_re6_even,
9405 | { "RE 6", "oran_fh_cus.mcscalermask-RE6",
9406 | FT_BOOLEAN, 16,
9407 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0040,
9408 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9409 | },
9410 | { &hf_oran_mc_scale_re_mask_re7_even,
9411 | { "RE 7", "oran_fh_cus.mcscalermask-RE7",
9412 | FT_BOOLEAN, 16,
9413 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0020,
9414 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9415 | },
9416 | { &hf_oran_mc_scale_re_mask_re8_even,
9417 | { "RE 8", "oran_fh_cus.mcscalermask-RE8",
9418 | FT_BOOLEAN, 16,
9419 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0010,
9420 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9421 | },
9422 | { &hf_oran_mc_scale_re_mask_re9_even,
9423 | { "RE 9", "oran_fh_cus.mcscalermask-RE9",
9424 | FT_BOOLEAN, 16,
9425 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0008,
9426 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9427 | },
9428 | { &hf_oran_mc_scale_re_mask_re10_even,
9429 | { "RE 10", "oran_fh_cus.mcscalermask-RE10",
9430 | FT_BOOLEAN, 16,
9431 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0004,
9432 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9433 | },
9434 | { &hf_oran_mc_scale_re_mask_re11_even,
9435 | { "RE 11", "oran_fh_cus.mcscalermask-RE11",
9436 | FT_BOOLEAN, 16,
9437 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0002,
9438 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9439 | },
9440 | { &hf_oran_mc_scale_re_mask_re12_even,
9441 | { "RE 12", "oran_fh_cus.mcscalermask-RE12",
9442 | FT_BOOLEAN, 16,
9443 | TFS(&tfs_applicable_not_applicable)((0 ? (const struct true_false_string*)0 : ((&tfs_applicable_not_applicable )))), 0x0001,
9444 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9445 | },
9446 |
9447 | { &hf_oran_mc_scale_re_mask,
9448 | { "mcScaleReMask", "oran_fh_cus.mcscaleremask",
9449 | FT_UINT16, BASE_HEX,
9450 | NULL((void*)0), 0xfff0,
9451 | "modulation compression power scale RE mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9452 | },
9453 | { &hf_oran_mc_scale_re_mask_even,
9454 | { "mcScaleReMask", "oran_fh_cus.mcscaleremask",
9455 | FT_UINT16, BASE_HEX,
9456 | NULL((void*)0), 0x0fff,
9457 | "modulation compression power scale RE mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9458 | },
9459 |
9460 | /* mcScaleOffset 7.7.5.4 (15 bits) */
9461 | { &hf_oran_mc_scale_offset,
9462 | { "mcScaleOffset", "oran_fh_cus.mcscaleoffset",
9463 | FT_UINT24, BASE_DEC,
9464 | NULL((void*)0), 0x0,
9465 | "scaling value for modulation compression", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9466 | },
9467 | /* eAxCmask (7.7.7.2) */
9468 | { &hf_oran_eAxC_mask,
9469 | { "eAxC Mask", "oran_fh_cus.eaxcmask",
9470 | FT_UINT16, BASE_HEX,
9471 | NULL((void*)0), 0xffff,
9472 | "Which eAxC_ID values the C-Plane message applies to", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9473 | },
9474 | /* technology (interface name) 7.7.9.2 */
9475 | { &hf_oran_technology,
9476 | { "Technology", "oran_fh_cus.technology",
9477 | FT_UINT8, BASE_DEC,
9478 | VALS(interface_name_vals)((0 ? (const struct _value_string*)0 : ((interface_name_vals) ))), 0x0,
9479 | "Interface name (that C-PLane section applies to)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9480 | },
9481 | /* Exttype 14 (7.7.14.2) */
9482 | { &hf_oran_nullLayerInd,
9483 | { "nullLayerInd", "oran_fh_cus.nulllayerind",
9484 | FT_BOOLEAN, BASE_NONE,
9485 | NULL((void*)0), 0x0,
9486 | "Whether corresponding layer is nulling-layer or not", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9487 | },
9488 |
9489 | /* Exttype 19 */
9490 | /* 7.7.19.3 */
9491 | { &hf_oran_se19_repetition,
9492 | { "repetition", "oran_fh_cus.repetition",
9493 | FT_BOOLEAN, BASE_NONE,
9494 | TFS(&repetition_se19_tfs)((0 ? (const struct true_false_string*)0 : ((&repetition_se19_tfs )))), 0x0,
9495 | "repeat port info flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9496 | },
9497 | /* 7.7.19.8 */
9498 | /* TODO: break down into each RE as done for 7.5.3.5 ? */
9499 | { &hf_oran_portReMask,
9500 | { "portReMask", "oran_fh_cus.portReMask",
9501 | FT_BOOLEAN, 16,
9502 | TFS(&tfs_set_notset)((0 ? (const struct true_false_string*)0 : ((&tfs_set_notset )))), 0x0fff,
9503 | "RE bitmask per port", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9504 | },
9505 | /* 7.7.19.9 */
9506 | { &hf_oran_portSymbolMask,
9507 | { "portSymbolMask", "oran_fh_cus.portSymbolMask",
9508 | FT_BOOLEAN, 16,
9509 | TFS(&tfs_set_notset)((0 ? (const struct true_false_string*)0 : ((&tfs_set_notset )))), 0x3fff,
9510 | "Symbol bitmask port port", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9511 | },
9512 |
9513 | { &hf_oran_ext19_port,
9514 | {"Port", "oran_fh_cus.ext19.port",
9515 | FT_STRING, BASE_NONE,
9516 | NULL((void*)0), 0x0,
9517 | "Entry for a given port in ext19", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9518 | },
9519 |
9520 | /* Ext 13 */
9521 | { &hf_oran_prb_allocation,
9522 | {"PRB allocation", "oran_fh_cus.prb-allocation",
9523 | FT_STRING, BASE_NONE,
9524 | NULL((void*)0), 0x0,
9525 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9526 | },
9527 | /* 7.7.13.2 */
9528 | { &hf_oran_nextSymbolId,
9529 | { "nextSymbolId", "oran_fh_cus.nextSymbolId",
9530 | FT_UINT8, BASE_DEC,
9531 | NULL((void*)0), 0x3c,
9532 | "offset of PRB range start", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9533 | },
9534 | /* 7.7.13.3 */
9535 | { &hf_oran_nextStartPrbc,
9536 | { "nextStartPrbc", "oran_fh_cus.nextStartPrbc",
9537 | FT_UINT16, BASE_DEC,
9538 | NULL((void*)0), 0x03ff,
9539 | "number of PRBs in PRB range", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9540 | },
9541 |
9542 | /* Puncturing patters as appears in SE 20 */
9543 | { &hf_oran_puncPattern,
9544 | { "puncPattern", "oran_fh_cus.puncPattern",
9545 | FT_STRING, BASE_NONE,
9546 | NULL((void*)0), 0x0,
9547 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9548 | },
9549 |
9550 | /* 7.7.20.2 numPuncPatterns */
9551 | { &hf_oran_numPuncPatterns,
9552 | { "numPuncPatterns", "oran_fh_cus.numPuncPatterns",
9553 | FT_UINT8, BASE_DEC,
9554 | NULL((void*)0), 0x0,
9555 | "number of puncturing patterns", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }
9556 | },
9557 | /* 7.7.20.3 symbolMask */
9558 | { &hf_oran_symbolMask_ext20,
9559 | { "symbolMask", "oran_fh_cus.symbolMask",
9560 | FT_UINT16, BASE_HEX,
9561 | NULL((void*)0), 0xfffc,
9562 | "Bitmask where each bit indicates the symbols associated with the puncturing pattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9563 | },
9564 | /* 7.7.20.4 startPuncPrb */
9565 | { &hf_oran_startPuncPrb,
9566 | { "startPuncPrb", "oran_fh_cus.startPuncPrb",
9567 | FT_UINT16, BASE_DEC,
9568 | NULL((void*)0), 0x03ff,
9569 | "starting PRB to which one puncturing pattern applies", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9570 | },
9571 | /* 7.7.20.5 numPuncPrb */
9572 | { &hf_oran_numPuncPrb,
9573 | { "numPuncPrb", "oran_fh_cus.numPuncPrb",
9574 | FT_UINT8, BASE_DEC,
9575 | NULL((void*)0), 0x0,
9576 | "the number of PRBs of the puncturing pattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9577 | },
9578 | /* 7.7.20.6 puncReMask */
9579 | { &hf_oran_puncReMask,
9580 | { "puncReMask", "oran_fh_cus.puncReMask",
9581 | FT_UINT16, BASE_DEC,
9582 | NULL((void*)0), 0xffc0,
9583 | "puncturing pattern RE mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9584 | },
9585 | /* 7.7.20.12 multiSDScope */
9586 | { &hf_oran_multiSDScope,
9587 | { "multiSDScope", "oran_fh_cus.multiSDScope",
9588 | FT_BOOLEAN, 8,
9589 | TFS(&multi_sd_scope_tfs)((0 ? (const struct true_false_string*)0 : ((&multi_sd_scope_tfs )))), 0x02,
9590 | "multiple section description scope flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9591 | },
9592 | /* 7.7.20.4 rbgIncl */
9593 | { &hf_oran_RbgIncl,
9594 | { "rbgIncl", "oran_fh_cus.rbgIncl",
9595 | FT_BOOLEAN, 8,
9596 | NULL((void*)0), 0x01,
9597 | "rbg included flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9598 | },
9599 |
9600 | /* 7.7.21.2 ciPrbGroupSize */
9601 | { &hf_oran_ci_prb_group_size,
9602 | { "ciPrbGroupSize", "oran_fh_cus.ciPrbGroupSize",
9603 | FT_UINT8, BASE_DEC,
9604 | NULL((void*)0), 0x0,
9605 | "channel information PRB group size", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9606 | },
9607 | /* 7.21.3 */
9608 | { &hf_oran_prg_size_st5,
9609 | { "prgSize", "oran_fh_cus.prgSize",
9610 | FT_UINT8, BASE_DEC,
9611 | VALS(prg_size_st5_vals)((0 ? (const struct _value_string*)0 : ((prg_size_st5_vals))) ), 0x03,
9612 | "precoding resource block group size", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9613 | },
9614 | { &hf_oran_prg_size_st6,
9615 | { "prgSize", "oran_fh_cus.prgSize",
9616 | FT_UINT8, BASE_DEC,
9617 | VALS(prg_size_st6_vals)((0 ? (const struct _value_string*)0 : ((prg_size_st6_vals))) ), 0x03,
9618 | "precoding resource block group size", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9619 | },
9620 |
9621 | /* 7.7.17.2 numUeID */
9622 | { &hf_oran_num_ueid,
9623 | { "numUeID", "oran_fh_cus.numUeID",
9624 | FT_UINT8, BASE_DEC,
9625 | NULL((void*)0), 0x0,
9626 | "number of ueIDs per user", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9627 | },
9628 |
9629 | /* 7.7.16.2 antMask */
9630 | { &hf_oran_antMask,
9631 | { "antMask", "oran_fh_cus.antMask",
9632 | FT_UINT64, BASE_HEX,
9633 | NULL((void*)0), 0xffffffffffffffff,
9634 | "indices of antennas to be pre-combined per RX endpoint", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9635 | },
9636 |
9637 | /* 7.7.18.2 transmissionWindowOffset */
9638 | { &hf_oran_transmissionWindowOffset,
9639 | { "transmissionWindowOffset", "oran_fh_cus.transmissionWindowOffset",
9640 | FT_UINT16, BASE_DEC,
9641 | NULL((void*)0), 0x0,
9642 | "start of the transmission window as an offset to when the transmission window would have been without this parameter, i.e. (Ta3_max - Ta3_min)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9643 | },
9644 | /* 7.7.18.3 transmissionWindowSize */
9645 | { &hf_oran_transmissionWindowSize,
9646 | { "transmissionWindowSize", "oran_fh_cus.transmissionWindowSize",
9647 | FT_UINT16, BASE_DEC,
9648 | NULL((void*)0), 0x3fff,
9649 | "size of the transmission window in resolution µs", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9650 | },
9651 | /* 7.7.18.4 toT */
9652 | { &hf_oran_toT,
9653 | { "toT", "oran_fh_cus.toT",
9654 | FT_UINT8, BASE_DEC,
9655 | VALS(type_of_transmission_vals)((0 ? (const struct _value_string*)0 : ((type_of_transmission_vals )))), 0x03,
9656 | "type of transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9657 | },
9658 |
9659 | /* 7.7.2.2 bfaCompHdr */
9660 | { &hf_oran_bfaCompHdr,
9661 | { "bfaCompHdr", "oran_fh_cus.bfaCompHdr",
9662 | FT_STRING, BASE_NONE,
9663 | NULL((void*)0), 0x0,
9664 | "beamforming attributes compression header", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9665 | },
9666 | /* 7.7.2.2-2: bfAzPtWidth */
9667 | { &hf_oran_bfAzPtWidth,
9668 | { "bfAzPtWidth", "oran_fh_cus.bfAzPtWidth",
9669 | FT_UINT8, BASE_DEC,
9670 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x38,
9671 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9672 | },
9673 | /* 7.7.2.2-3: bfZePtWidth */
9674 | { &hf_oran_bfZePtWidth,
9675 | { "bfZePtWidth", "oran_fh_cus.bfZePtWidth",
9676 | FT_UINT8, BASE_DEC,
9677 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x07,
9678 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9679 | },
9680 | /* 7.7.2.2-4: bfAz3ddWidth */
9681 | { &hf_oran_bfAz3ddWidth,
9682 | { "bfAz3ddWidth", "oran_fh_cus.bfAz3ddWidth",
9683 | FT_UINT8, BASE_DEC,
9684 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x38,
9685 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9686 | },
9687 | /* 7.7.2.2-5: bfZe3ddWidth */
9688 | { &hf_oran_bfZe3ddWidth,
9689 | { "bfZe3ddWidth", "oran_fh_cus.bfZe3ddWidth",
9690 | FT_UINT8, BASE_DEC,
9691 | VALS(bfa_bw_vals)((0 ? (const struct _value_string*)0 : ((bfa_bw_vals)))), 0x07,
9692 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9693 | },
9694 |
9695 | /* 7.7.2.3 bfAzPt */
9696 | { &hf_oran_bfAzPt,
9697 | { "bfAzPt", "oran_fh_cus.bfAzPt",
9698 | FT_UINT8, BASE_DEC,
9699 | NULL((void*)0), 0x0,
9700 | "beamforming azimuth pointing parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9701 | },
9702 | /* 7.7.2.4 bfZePt */
9703 | { &hf_oran_bfZePt,
9704 | { "bfZePt", "oran_fh_cus.bfZePt",
9705 | FT_UINT8, BASE_DEC,
9706 | NULL((void*)0), 0x0,
9707 | "beamforming zenith pointing parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9708 | },
9709 | /* 7.7.2.5 bfAz3dd */
9710 | { &hf_oran_bfAz3dd,
9711 | { "bfAz3dd", "oran_fh_cus.bfAz3dd",
9712 | FT_UINT8, BASE_DEC,
9713 | NULL((void*)0), 0x0,
9714 | "beamforming azimuth beamwidth parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9715 | },
9716 | /* 7.7.2.6 bfZe3dd */
9717 | { &hf_oran_bfZe3dd,
9718 | { "bfZe3dd", "oran_fh_cus.bfZe3dd",
9719 | FT_UINT8, BASE_DEC,
9720 | NULL((void*)0), 0x0,
9721 | "beamforming zenith beamwidth parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9722 | },
9723 |
9724 | /* 7.7.2.7 bfAzSl */
9725 | { &hf_oran_bfAzSl,
9726 | { "bfAzSl", "oran_fh_cus.bfAzSl",
9727 | FT_UINT8, BASE_DEC,
9728 | VALS(sidelobe_suppression_vals)((0 ? (const struct _value_string*)0 : ((sidelobe_suppression_vals )))), 0x38,
9729 | "beamforming azimuth sidelobe parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9730 | },
9731 | /* 7.7.2.8 bfZeSl */
9732 | { &hf_oran_bfZeSl,
9733 | { "bfZeSl", "oran_fh_cus.bfZeSl",
9734 | FT_UINT8, BASE_DEC,
9735 | VALS(sidelobe_suppression_vals)((0 ? (const struct _value_string*)0 : ((sidelobe_suppression_vals )))), 0x07,
9736 | "beamforming zenith sidelobe parameter", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9737 | },
9738 |
9739 | /* 7.5.2.17 */
9740 | { &hf_oran_cmd_scope,
9741 | { "cmdScope", "oran_fh_cus.cmdScope",
9742 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
9743 | RVALS(cmd_scope_vals)((0 ? (const struct _range_string*)0 : ((cmd_scope_vals)))), 0x0f,
9744 | "command scope", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9745 | },
9746 | /* 7.5.2.18 */
9747 | { &hf_oran_number_of_st4_cmds,
9748 | { "numberOfST4Cmds", "oran_fh_cus.numberOfST4Cmds",
9749 | FT_UINT8, BASE_DEC,
9750 | NULL((void*)0), 0x0,
9751 | "Number of Section Type 4 commands", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9752 | },
9753 |
9754 | { &hf_oran_st4_cmd_header,
9755 | { "Command common header", "oran_fh_cus.st4CmdCommonHeader",
9756 | FT_STRING, BASE_NONE,
9757 | NULL((void*)0), 0x0,
9758 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9759 | },
9760 |
9761 | /* 7.5.3.38 */
9762 | { &hf_oran_st4_cmd_type,
9763 | { "st4CmdType", "oran_fh_cus.st4CmdType",
9764 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
9765 | RVALS(st4_cmd_type_vals)((0 ? (const struct _range_string*)0 : ((st4_cmd_type_vals))) ), 0x0,
9766 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9767 | },
9768 | /* 7.5.3.39 */
9769 | { &hf_oran_st4_cmd_len,
9770 | { "st4CmdLen", "oran_fh_cus.st4CmdLen",
9771 | FT_UINT16, BASE_DEC,
9772 | NULL((void*)0), 0x0,
9773 | "Length of command in 32-bit words", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9774 | },
9775 | /* 7.5.3.40 */
9776 | { &hf_oran_st4_cmd_num_slots,
9777 | { "numSlots", "oran_fh_cus.st4NumSlots",
9778 | FT_UINT8, BASE_DEC,
9779 | NULL((void*)0), 0x0,
9780 | "Contiguous slots for which command is applicable", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9781 | },
9782 | /* 7.5.3.41 */
9783 | { &hf_oran_st4_cmd_ack_nack_req_id,
9784 | { "ackNackReqId", "oran_fh_cus.ackNackReqId",
9785 | FT_UINT16, BASE_DEC,
9786 | NULL((void*)0), 0x0,
9787 | "ACK/NACK Request Id", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9788 | },
9789 |
9790 | { &hf_oran_st4_cmd,
9791 | { "Command", "oran_fh_cus.st4Cmd",
9792 | FT_STRING, BASE_NONE,
9793 | NULL((void*)0), 0x0,
9794 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9795 | },
9796 |
9797 | /* 7.5.3.52 */
9798 | { &hf_oran_sleepmode_trx,
9799 | { "sleepMode", "oran_fh_cus.sleepMode",
9800 | FT_UINT8, BASE_HEX,
9801 | VALS(sleep_mode_trx_vals)((0 ? (const struct _value_string*)0 : ((sleep_mode_trx_vals) ))), 0x03,
9802 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9803 | },
9804 | { &hf_oran_sleepmode_asm,
9805 | { "sleepMode", "oran_fh_cus.sleepMode",
9806 | FT_UINT8, BASE_HEX,
9807 | VALS(sleep_mode_asm_vals)((0 ? (const struct _value_string*)0 : ((sleep_mode_asm_vals) ))), 0x03,
9808 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9809 | },
9810 |
9811 | /* 7.5.3.51 */
9812 | { &hf_oran_log2maskbits,
9813 | { "log2MaskBits", "oran_fh_cus.log2MaskBits",
9814 | FT_UINT8, BASE_HEX,
9815 | VALS(log2maskbits_vals)((0 ? (const struct _value_string*)0 : ((log2maskbits_vals))) ), 0x3c,
9816 | "Number of bits to appear in antMask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9817 | },
9818 | /* 7.5.3.53 */
9819 | { &hf_oran_num_slots_ext,
9820 | { "numSlotsExt", "oran_fh_cus.numSlotsExt",
9821 | FT_UINT24, BASE_HEX,
9822 | NULL((void*)0), 0x0fffff,
9823 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9824 | },
9825 | /* 7.5.3.54 */
9826 | { &hf_oran_antMask_trx_control,
9827 | { "antMask", "oran_fh_cus.trxControl.antMask",
9828 | FT_BYTES, BASE_NONE,
9829 | NULL((void*)0), 0x0,
9830 | "which antennas should sleep or wake-up", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9831 | },
9832 | /* 7.5.3.55 */
9833 | { &hf_oran_ready,
9834 | { "ready", "oran_fh_cus.ready",
9835 | FT_BOOLEAN, 8,
9836 | TFS(&ready_tfs)((0 ? (const struct true_false_string*)0 : ((&ready_tfs)) )), 0x01,
9837 | "wake-up ready indicator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9838 | },
9839 | /* 7.5.3.34 */
9840 | { &hf_oran_number_of_acks,
9841 | { "numberOfAcks", "oran_fh_cus.numberOfAcks",
9842 | FT_UINT8, BASE_DEC,
9843 | NULL((void*)0), 0x0,
9844 | "number of ACKs for one eAxC_ID", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9845 | },
9846 | /* 7.5.3.35 */
9847 | { &hf_oran_number_of_nacks,
9848 | { "numberOfNacks", "oran_fh_cus.numberOfNacks",
9849 | FT_UINT8, BASE_DEC,
9850 | NULL((void*)0), 0x0,
9851 | "number of NACKs for one eAxC_ID", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9852 | },
9853 | /* 7.5.3.36 */
9854 | { &hf_oran_ackid,
9855 | { "ackId", "oran_fh_cus.ackId",
9856 | FT_UINT16, BASE_DEC,
9857 | NULL((void*)0), 0x0,
9858 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9859 | },
9860 | /* 7.5.3.37 */
9861 | { &hf_oran_nackid,
9862 | { "nackId", "oran_fh_cus.nackId",
9863 | FT_UINT16, BASE_DEC,
9864 | NULL((void*)0), 0x0,
9865 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9866 | },
9867 |
9868 | /* Links between acknack requests & responses */
9869 | { &hf_oran_acknack_request_frame,
9870 | { "Request Frame", "oran_fh_cus.ackNackId.request-frame",
9871 | FT_FRAMENUM, BASE_NONE,
9872 | FRAMENUM_TYPE(FT_FRAMENUM_REQUEST)((gpointer) (glong) (FT_FRAMENUM_REQUEST)), 0x0,
9873 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9874 | },
9875 | { &hf_oran_acknack_request_time,
9876 | { "Time since request in ms", "oran_fh_cus.ackNackId.time-since-request",
9877 | FT_UINT32, BASE_DEC,
9878 | NULL((void*)0), 0x0,
9879 | "Time between request and response", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9880 | },
9881 | { &hf_oran_acknack_request_type,
9882 | { "Request Type", "oran_fh_cus.ackNackId.request-type",
9883 | FT_UINT32, BASE_DEC,
9884 | VALS(acknack_type_vals)((0 ? (const struct _value_string*)0 : ((acknack_type_vals))) ), 0x0,
9885 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9886 | },
9887 | { &hf_oran_acknack_response_frame,
9888 | { "Response Frame", "oran_fh_cus.ackNackId.response-frame",
9889 | FT_FRAMENUM, BASE_NONE,
9890 | FRAMENUM_TYPE(FT_FRAMENUM_RESPONSE)((gpointer) (glong) (FT_FRAMENUM_RESPONSE)), 0x0,
9891 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9892 | },
9893 | { &hf_oran_acknack_response_time,
9894 | { "Time to response in ms", "oran_fh_cus.ackNackId.time-to-response",
9895 | FT_UINT32, BASE_DEC,
9896 | NULL((void*)0), 0x0,
9897 | "Time between request and response", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9898 | },
9899 |
9900 | /* 7.5.3.43 */
9901 | { &hf_oran_disable_tdbfns,
9902 | { "disableTDBFNs", "oran_fh_cus.disableTDBFNs",
9903 | FT_BOOLEAN, 8,
9904 | TFS(&disable_tdbfns_tfs)((0 ? (const struct true_false_string*)0 : ((&disable_tdbfns_tfs )))), 0x80,
9905 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9906 | },
9907 |
9908 | /* 7.5.3.44 */
9909 | { &hf_oran_td_beam_group,
9910 | { "tdBeamGrp", "oran_fh_cus.tdBeamGrp",
9911 | FT_UINT16, BASE_HEX,
9912 | NULL((void*)0), 0x7fff,
9913 | "Applies to symbolMask in command header", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9914 | },
9915 | /* 7.5.3.43 */
9916 | { &hf_oran_disable_tdbfws,
9917 | { "disableTDBFWs", "oran_fh_cus.disableTDBFWs",
9918 | FT_BOOLEAN, 8,
9919 | TFS(&beam_numbers_included_tfs)((0 ? (const struct true_false_string*)0 : ((&beam_numbers_included_tfs )))), 0x80,
9920 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9921 | },
9922 |
9923 | /* 7.5.3.56 */
9924 | { &hf_oran_td_beam_num,
9925 | { "tdBeamNum", "oran_fh_cus.tdBeamNum",
9926 | FT_UINT16, BASE_HEX,
9927 | NULL((void*)0), 0x7fff,
9928 | "time-domain beam number", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9929 | },
9930 |
9931 | /* 7.5.3.49 */
9932 | { &hf_oran_dir_pattern,
9933 | { "dirPattern", "oran_fh_cus.dirPattern",
9934 | FT_BOOLEAN, 16,
9935 | TFS(&symbol_direction_tfs)((0 ? (const struct true_false_string*)0 : ((&symbol_direction_tfs )))), 0x3fff,
9936 | "symbol data direction (gNB Tx/Rx) pattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9937 | },
9938 | /* 7.5.3.50 */
9939 | { &hf_oran_guard_pattern,
9940 | { "guardPattern", "oran_fh_cus.guardPattern",
9941 | FT_BOOLEAN, 16,
9942 | TFS(&symbol_guard_tfs)((0 ? (const struct true_false_string*)0 : ((&symbol_guard_tfs )))), 0x3fff,
9943 | "guard pattern bitmask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9944 | },
9945 |
9946 | /* For convenient filtering */
9947 | { &hf_oran_cplane,
9948 | { "C-Plane", "oran_fh_cus.c-plane",
9949 | FT_NONE, BASE_NONE,
9950 | NULL((void*)0), 0x0,
9951 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9952 | },
9953 | { &hf_oran_uplane,
9954 | { "U-Plane", "oran_fh_cus.u-plane",
9955 | FT_NONE, BASE_NONE,
9956 | NULL((void*)0), 0x0,
9957 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9958 | },
9959 | { &hf_oran_bf,
9960 | { "BeamForming", "oran_fh_cus.bf",
9961 | FT_NONE, BASE_NONE,
9962 | NULL((void*)0), 0x0,
9963 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9964 | },
9965 | { &hf_oran_zero_prb,
9966 | { "Zero PRB", "oran_fh_cus.zero-prb",
9967 | FT_NONE, BASE_NONE,
9968 | NULL((void*)0), 0x0,
9969 | "All of the REs in this PRB are zero", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9970 | },
9971 | { &hf_oran_nonzero_prb,
9972 | { "Non-Zero PRB", "oran_fh_cus.nonzero-prb",
9973 | FT_NONE, BASE_NONE,
9974 | NULL((void*)0), 0x0,
9975 | "Not all of the REs in this PRB are zero", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9976 | },
9977 | { &hf_oran_bundle_weights_all_zero,
9978 | { "Bundle Weights all zero", "oran_fh_cus.zero-bundle",
9979 | FT_NONE, BASE_NONE,
9980 | NULL((void*)0), 0x0,
9981 | "All of the weights in a bundle are zero", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9982 | },
9983 |
9984 |
9985 | /* 5.1.3.2.7 */
9986 | { &hf_oran_ecpri_pcid,
9987 | { "ecpriPcid", "oran_fh_cus.ecpriPcid",
9988 | FT_NONE, BASE_NONE,
9989 | NULL((void*)0), 0x0,
9990 | "IQ data transfer message series identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9991 | },
9992 | { &hf_oran_ecpri_rtcid,
9993 | { "ecpriRtcid", "oran_fh_cus.ecpriRtcid",
9994 | FT_NONE, BASE_NONE,
9995 | NULL((void*)0), 0x0,
9996 | "Real time control data identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
9997 | },
9998 | /* 5.1.3.2.8 */
9999 | { &hf_oran_ecpri_seqid,
10000 | { "ecpriSeqid", "oran_fh_cus.ecpriSeqid",
10001 | FT_NONE, BASE_NONE,
10002 | NULL((void*)0), 0x0,
10003 | "message identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10004 | },
10005 |
10006 | /* 7.7.23.2 */
10007 | { &hf_oran_num_sym_prb_pattern,
10008 | { "numSymPrbPattern", "oran_fh_cus.numSymPrbPattern",
10009 | FT_UINT8, BASE_DEC,
10010 | NULL((void*)0), 0xf0,
10011 | "number of symbol and resource block patterns", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10012 | },
10013 | /* 7.7.23.9 */
10014 | { &hf_oran_prb_mode,
10015 | { "prbMode", "oran_fh_cus.prbMode",
10016 | FT_BOOLEAN, 8,
10017 | TFS(&prb_mode_tfs)((0 ? (const struct true_false_string*)0 : ((&prb_mode_tfs )))), 0x01,
10018 | "PRB Mode", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10019 | },
10020 | /* 7.7.23.4 */
10021 | { &hf_oran_sym_prb_pattern,
10022 | { "symPrbPattern", "oran_fh_cus.symPrbPattern",
10023 | FT_STRING, BASE_NONE,
10024 | NULL((void*)0), 0x0,
10025 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10026 | },
10027 | /* 7.7.23.3 */
10028 | { &hf_oran_sym_mask,
10029 | { "symMask", "oran_fh_cus.symMask",
10030 | FT_UINT16, BASE_HEX,
10031 | NULL((void*)0), 0x3fff,
10032 | "symbol mask part of symPrbPattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10033 | },
10034 | /* 7.7.23.5 */
10035 | {&hf_oran_num_mc_scale_offset,
10036 | {"numMcScaleOffset", "oran_fh_cus.numMcScaleOffset",
10037 | FT_UINT8, BASE_DEC,
10038 | NULL((void*)0), 0xf0,
10039 | "number of modulation compression scaling value per symPrbPattern",
10040 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10041 | },
10042 | /* 7.7.23.4 */
10043 | { &hf_oran_prb_pattern,
10044 | { "prbPattern", "oran_fh_cus.prbPattern",
10045 | FT_UINT8, BASE_DEC,
10046 | NULL((void*)0), 0x0f,
10047 | "size of one PRB block of one SymPrbPattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10048 | },
10049 | /* 7.7.23.10 */
10050 | { &hf_oran_prb_blk_offset,
10051 | { "prbBlkOffset", "oran_fh_cus.prbBlkOffset",
10052 | FT_UINT16, BASE_DEC,
10053 | NULL((void*)0), 0x0ff0,
10054 | "offset to start of PRB block", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10055 | },
10056 |
10057 | /* 7.7.23.11 */
10058 | { &hf_oran_prb_blk_size,
10059 | { "prbBlkSize", "oran_fh_cus.prbBlkSize",
10060 | FT_UINT16, BASE_DEC,
10061 | NULL((void*)0), 0x0ff0,
10062 | "size of one PRB block of one SymPrbPattern", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10063 | },
10064 |
10065 | /* 7.7.3.2 */
10066 | { &hf_oran_codebook_index,
10067 | { "codebookIndex", "oran_fh_cus.codebookIndex",
10068 | FT_UINT8, BASE_DEC,
10069 | NULL((void*)0), 0x0,
10070 | "precoder codebook used for transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10071 | },
10072 | /* 7.7.3.3 */
10073 | { &hf_oran_layerid,
10074 | { "layerID", "oran_fh_cus.layerID",
10075 | FT_UINT8, BASE_DEC,
10076 | NULL((void*)0), 0xf0,
10077 | "Layer ID for DL transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10078 | },
10079 | /* 7.7.3.5 */
10080 | { &hf_oran_numlayers,
10081 | { "numLayers", "oran_fh_cus.numLayers",
10082 | FT_UINT8, BASE_DEC,
10083 | NULL((void*)0), 0x0f,
10084 | "number of layers for DL transmission", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10085 | },
10086 | /* 7.7.3.4 */
10087 | { &hf_oran_txscheme,
10088 | { "txScheme", "oran_fh_cus.txScheme",
10089 | FT_UINT8, BASE_DEC,
10090 | NULL((void*)0), 0xf0,
10091 | "transmission scheme", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10092 | },
10093 | /* 7.7.3.6 */
10094 | { &hf_oran_crs_remask,
10095 | { "crsReMask", "oran_fh_cus.crsReMask",
10096 | FT_UINT16, BASE_HEX,
10097 | NULL((void*)0), 0x0fff,
10098 | "CRS resource element mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10099 | },
10100 | /* 7.7.3.8 */
10101 | { &hf_oran_crs_shift,
10102 | { "crsShift", "oran_fh_cus.crsShift",
10103 | FT_UINT8, BASE_HEX,
10104 | NULL((void*)0), 0x80,
10105 | "CRS resource element mask", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10106 | },
10107 | /* 7.7.3.7 */
10108 | { &hf_oran_crs_symnum,
10109 | { "crsSymNum", "oran_fh_cus.crsSymNum",
10110 | FT_UINT8, BASE_DEC,
10111 | NULL((void*)0), 0x0f,
10112 | "CRS symbol number indication", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10113 | },
10114 | /* 7.7.3.9 */
10115 | { &hf_oran_beamid_ap1,
10116 | { "beamIdAP1", "oran_fh_cus.beamIdAP1",
10117 | FT_UINT16, BASE_DEC,
10118 | NULL((void*)0), 0x7f,
10119 | "beam id to be used for antenna port 1", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10120 | },
10121 | /* 7.7.3.10 */
10122 | { &hf_oran_beamid_ap2,
10123 | { "beamIdAP2", "oran_fh_cus.beamIdAP2",
10124 | FT_UINT16, BASE_DEC,
10125 | NULL((void*)0), 0x7f,
10126 | "beam id to be used for antenna port 2", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10127 | },
10128 | /* 7.7.3.11 */
10129 | { &hf_oran_beamid_ap3,
10130 | { "beamIdAP3", "oran_fh_cus.beamIdAP3",
10131 | FT_UINT16, BASE_DEC,
10132 | NULL((void*)0), 0x7f,
10133 | "beam id to be used for antenna port 3", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10134 | },
10135 |
10136 | /* 7.7.10.3a */
10137 | { &hf_oran_port_list_index,
10138 | { "portListIndex", "oran_fh_cus.portListIndex",
10139 | FT_UINT8, BASE_DEC,
10140 | NULL((void*)0), 0x0,
10141 | "the index of an eAxC_ID in the port-list", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10142 | },
10143 |
10144 | { &hf_oran_alpn_per_sym,
10145 | { "alpnPerSym", "oran_fh_cus.alpnPerSym",
10146 | FT_UINT8, BASE_HEX,
10147 | VALS(alpn_per_sym_vals)((0 ? (const struct _value_string*)0 : ((alpn_per_sym_vals))) ), 0x80,
10148 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10149 | },
10150 | { &hf_oran_ant_dmrs_snr,
10151 | { "antDmrsSnr", "oran_fh_cus.antDmrsSnr",
10152 | FT_UINT8, BASE_HEX,
10153 | VALS(ant_dmrs_snr_vals)((0 ? (const struct _value_string*)0 : ((ant_dmrs_snr_vals))) ), 0x40,
10154 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10155 | },
10156 |
10157 | /* 7.7.24.6 */
10158 | { &hf_oran_user_group_size,
10159 | { "userGroupSize", "oran_fh_cus.userGroupSize",
10160 | FT_UINT8, BASE_DEC,
10161 | NULL((void*)0), 0x1f,
10162 | "number of UE data layers in the user group identified by userGroupId", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10163 | },
10164 | /* 7.7.24.7 */
10165 | { &hf_oran_user_group_id,
10166 | { "userGroupId", "oran_fh_cus.userGroupId",
10167 | FT_UINT8, BASE_DEC,
10168 | NULL((void*)0), 0x0,
10169 | "indicates user group described by the section", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10170 | },
10171 | /* 7.7.24.8 */
10172 | { &hf_oran_entry_type,
10173 | { "entryType", "oran_fh_cus.entryType",
10174 | FT_UINT8, BASE_DEC,
10175 | VALS(entry_type_vals)((0 ? (const struct _value_string*)0 : ((entry_type_vals)))), 0xe0,
10176 | "indicates format of the entry", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10177 | },
10178 | /* 7.7.24.9 */
10179 | { &hf_oran_dmrs_port_number,
10180 | { "dmrsPortNumber", "oran_fh_cus.dmrsPortNumber",
10181 | FT_UINT8, BASE_DEC,
10182 | NULL((void*)0), 0x1f,
10183 | "DMRS antenna port number for the associated ueId", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10184 | },
10185 | /* 7.7.24.10 */
10186 | { &hf_oran_ueid_reset,
10187 | { "ueidReset", "oran_fh_cus.ueidReset",
10188 | FT_BOOLEAN, 8,
10189 | TFS(&tfs_ueid_reset)((0 ? (const struct true_false_string*)0 : ((&tfs_ueid_reset )))), 0x80,
10190 | "same UEID as the previous slot", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10191 | },
10192 | /* 7.7.24.11 */
10193 | { &hf_oran_dmrs_symbol_mask,
10194 | { "dmrsSymbolMask", "oran_fh_cus.dmrsSymbolMask",
10195 | FT_UINT16, BASE_HEX,
10196 | NULL((void*)0), 0x3fff,
10197 | "symbols within the slot containing DMRS", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10198 | },
10199 | { &hf_oran_dmrs_symbol_mask_s13,
10200 | { "symbol 13", "oran_fh_cus.dmrsSymbolMask.symbol-13",
10201 | FT_BOOLEAN, 16,
10202 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x2000,
10203 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10204 | },
10205 | { &hf_oran_dmrs_symbol_mask_s12,
10206 | { "symbol 12", "oran_fh_cus.dmrsSymbolMask.symbol-12",
10207 | FT_BOOLEAN, 16,
10208 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x1000,
10209 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10210 | },
10211 | { &hf_oran_dmrs_symbol_mask_s11,
10212 | { "symbol 11", "oran_fh_cus.dmrsSymbolMask.symbol-11",
10213 | FT_BOOLEAN, 16,
10214 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0800,
10215 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10216 | },
10217 | { &hf_oran_dmrs_symbol_mask_s10,
10218 | { "symbol 10", "oran_fh_cus.dmrsSymbolMask.symbol-10",
10219 | FT_BOOLEAN, 16,
10220 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0400,
10221 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10222 | },
10223 | { &hf_oran_dmrs_symbol_mask_s9,
10224 | { "symbol 9", "oran_fh_cus.dmrsSymbolMask.symbol-9",
10225 | FT_BOOLEAN, 16,
10226 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0200,
10227 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10228 | },
10229 | { &hf_oran_dmrs_symbol_mask_s8,
10230 | { "symbol 8", "oran_fh_cus.dmrsSymbolMask.symbol-8",
10231 | FT_BOOLEAN, 16,
10232 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0100,
10233 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10234 | },
10235 | { &hf_oran_dmrs_symbol_mask_s7,
10236 | { "symbol 7", "oran_fh_cus.dmrsSymbolMask.symbol-7",
10237 | FT_BOOLEAN, 16,
10238 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0080,
10239 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10240 | },
10241 | { &hf_oran_dmrs_symbol_mask_s6,
10242 | { "symbol 6", "oran_fh_cus.dmrsSymbolMask.symbol-6",
10243 | FT_BOOLEAN, 16,
10244 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0040,
10245 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10246 | },
10247 | { &hf_oran_dmrs_symbol_mask_s5,
10248 | { "symbol 5", "oran_fh_cus.dmrsSymbolMask.symbol-5",
10249 | FT_BOOLEAN, 16,
10250 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0020,
10251 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10252 | },
10253 | { &hf_oran_dmrs_symbol_mask_s4,
10254 | { "symbol 4", "oran_fh_cus.dmrsSymbolMask.symbol-4",
10255 | FT_BOOLEAN, 16,
10256 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0010,
10257 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10258 | },
10259 | { &hf_oran_dmrs_symbol_mask_s3,
10260 | { "symbol 3", "oran_fh_cus.dmrsSymbolMask.symbol-3",
10261 | FT_BOOLEAN, 16,
10262 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0008,
10263 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10264 | },
10265 | { &hf_oran_dmrs_symbol_mask_s2,
10266 | { "symbol 2", "oran_fh_cus.dmrsSymbolMask.symbol-2",
10267 | FT_BOOLEAN, 16,
10268 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0004,
10269 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10270 | },
10271 | { &hf_oran_dmrs_symbol_mask_s1,
10272 | { "symbol 1", "oran_fh_cus.dmrsSymbolMask.symbol-1",
10273 | FT_BOOLEAN, 16,
10274 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0002,
10275 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10276 | },
10277 | { &hf_oran_dmrs_symbol_mask_s0,
10278 | { "symbol 0", "oran_fh_cus.dmrsSymbolMask.symbol-0",
10279 | FT_BOOLEAN, 16,
10280 | TFS(&tfs_present_not_present)((0 ? (const struct true_false_string*)0 : ((&tfs_present_not_present )))), 0x0001,
10281 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10282 | },
10283 |
10284 | /* 7.7.24.12 */
10285 | { &hf_oran_scrambling,
10286 | { "scrambling", "oran_fh_cus.scrambling",
10287 | FT_UINT16, BASE_HEX,
10288 | NULL((void*)0), 0x0,
10289 | "used to calculate the seed value required to initialize pseudo-random generator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10290 | },
10291 | /* 7.7.24.13 */
10292 | { &hf_oran_nscid,
10293 | { "nscid", "oran_fh_cus.nscid",
10294 | FT_UINT8, BASE_HEX,
10295 | NULL((void*)0), 0x80,
10296 | "used to calculate the seed value for pseudo-random generator", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10297 | },
10298 | /* 7.7.24.14 */
10299 | { &hf_oran_dtype,
10300 | { "dType", "oran_fh_cus.dType",
10301 | FT_UINT8, BASE_HEX,
10302 | VALS(dtype_vals)((0 ? (const struct _value_string*)0 : ((dtype_vals)))), 0x40,
10303 | "PUSCH DMRS configuration type", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10304 | },
10305 | /* 7.7.24.15 */
10306 | { &hf_oran_cmd_without_data,
10307 | { "cmdWithoutData", "oran_fh_cus.cmdWithoutData",
10308 | FT_UINT8, BASE_HEX,
10309 | NULL((void*)0), 0x30,
10310 | "number of DMRS CDM groups without data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10311 | },
10312 | /* 7.7.24.16 */
10313 | { &hf_oran_lambda,
10314 | { "lambda", "oran_fh_cus.lambda",
10315 | FT_UINT8, BASE_HEX,
10316 | NULL((void*)0), 0x0c,
10317 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10318 | },
10319 | /* 7.7.24.19 */
10320 | { &hf_oran_first_prb,
10321 | { "firstPrb", "oran_fh_cus.firstPrb",
10322 | FT_UINT16, BASE_DEC,
10323 | NULL((void*)0), 0x03fe,
10324 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10325 | },
10326 | /* 7.7.24.20 */
10327 | { &hf_oran_last_prb,
10328 | { "lastPrb", "oran_fh_cus.lastPrb",
10329 | FT_UINT16, BASE_DEC,
10330 | NULL((void*)0), 0x01ff,
10331 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10332 | },
10333 |
10334 | /* 7.7.24.17 */
10335 | /* TODO: add value_string */
10336 | { &hf_oran_low_papr_type,
10337 | { "lowPaprType", "oran_fh_cus.lowPaprType",
10338 | FT_UINT8, BASE_HEX,
10339 | VALS(papr_type_vals)((0 ? (const struct _value_string*)0 : ((papr_type_vals)))), 0x30,
10340 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10341 | },
10342 | /* 7.7.24.18 */
10343 | { &hf_oran_hopping_mode,
10344 | { "hoppingMode", "oran_fh_cus.hoppingMode",
10345 | FT_UINT8, BASE_HEX,
10346 | VALS(hopping_mode_vals)((0 ? (const struct _value_string*)0 : ((hopping_mode_vals))) ), 0x0c,
10347 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10348 | },
10349 |
10350 | { &hf_oran_tx_win_for_on_air_symbol_l,
10351 | { "txWinForOnAirSymbol", "oran_fh_cus.txWinForOnAirSymbol",
10352 | FT_UINT8, BASE_DEC,
10353 | NULL((void*)0), 0xf0,
10354 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10355 | },
10356 | { &hf_oran_tx_win_for_on_air_symbol_r,
10357 | { "txWinForOnAirSymbol", "oran_fh_cus.txWinForOnAirSymbol",
10358 | FT_UINT8, BASE_DEC,
10359 | NULL((void*)0), 0x0f,
10360 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10361 | },
10362 | /* 7.7.26.2 */
10363 | { &hf_oran_num_fo_fb,
10364 | { "numFoFb", "oran_fh_cus.numFoFb",
10365 | FT_UINT8, BASE_DEC,
10366 | NULL((void*)0), 0x7f,
10367 | "number of frequency offset feedback", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10368 | },
10369 | /* 7.7.26.3 */
10370 | { &hf_oran_freq_offset_fb,
10371 | { "freqOffsetFb", "oran_fh_cus.freqOffsetFb",
10372 | FT_UINT16, BASE_HEX_DEC | BASE_RANGE_STRING0x00000100,
10373 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
10374 | "UE frequency offset feedback", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10375 | },
10376 |
10377 | /* 7.7.28.2 */
10378 | { &hf_oran_num_ue_sinr_rpt,
10379 | { "numUeSinrRpt", "oran_fh_cus.numUeSinrRpt",
10380 | FT_UINT8, BASE_DEC,
10381 | NULL((void*)0), 0x1f,
10382 | "number of sinr reported UEs {1 - 12}", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10383 | },
10384 |
10385 | /* 7.5.2.19 */
10386 | { &hf_oran_num_sinr_per_prb,
10387 | { "numSinrPerPrb", "oran_fh_cus.numSinrPerPrb",
10388 | FT_UINT8, BASE_DEC,
10389 | VALS(num_sinr_per_prb_vals)((0 ? (const struct _value_string*)0 : ((num_sinr_per_prb_vals )))), 0x70,
10390 | "number of SINR values per PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10391 | },
10392 | { &hf_oran_num_sinr_per_prb_right,
10393 | { "numSinrPerPrb", "oran_fh_cus.numSinrPerPrb",
10394 | FT_UINT8, BASE_DEC,
10395 | VALS(num_sinr_per_prb_vals)((0 ? (const struct _value_string*)0 : ((num_sinr_per_prb_vals )))), 0x07,
10396 | "number of SINR values per PRB", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10397 | },
10398 |
10399 | /* 7.5.3.68 */
10400 | { &hf_oran_sinr_value,
10401 | { "sinrValue", "oran_fh_cus.sinrValue",
10402 | FT_FLOAT, BASE_NONE,
10403 | NULL((void*)0), 0x0,
10404 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10405 | },
10406 |
10407 | { &hf_oran_measurement_report,
10408 | { "Measurement Report", "oran_fh_cus.measurement-report",
10409 | FT_STRING, BASE_NONE,
10410 | NULL((void*)0), 0x0,
10411 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10412 | },
10413 | /* 7.5.3.57 */
10414 | { &hf_oran_mf,
10415 | { "mf", "oran_fh_cus.mf",
10416 | FT_BOOLEAN, 8,
10417 | TFS(&measurement_flag_tfs)((0 ? (const struct true_false_string*)0 : ((&measurement_flag_tfs )))), 0x80,
10418 | "measurement flag", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10419 | },
10420 | /* 7.5.3.59 */
10421 | { &hf_oran_meas_data_size,
10422 | { "measDataSize", "oran_fh_cus.measDataSize",
10423 | FT_UINT16, BASE_DEC,
10424 | NULL((void*)0), 0x0,
10425 | "measurement data size (in words)", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10426 | },
10427 |
10428 | /* 7.5.3.58 */
10429 | { &hf_oran_meas_type_id,
10430 | { "measTypeId", "oran_fh_cus.measTypeId",
10431 | FT_UINT8, BASE_DEC,
10432 | VALS(meas_type_id_vals)((0 ? (const struct _value_string*)0 : ((meas_type_id_vals))) ), 0x7F,
10433 | "measurement report type identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10434 | },
10435 | /* 7.5.3.66 */
10436 | { &hf_oran_num_elements,
10437 | { "numElements", "oran_fh_cus.numElements",
10438 | FT_UINT8, BASE_DEC,
10439 | NULL((void*)0), 0x0,
10440 | "measurement report type identifier", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10441 | },
10442 | /* 7.5.3.60 */
10443 | { &hf_oran_ue_tae,
10444 | { "ueTae", "oran_fh_cus.ueTae",
10445 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
10446 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
10447 | "UE Timing Advance Error", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10448 | },
10449 | /* 7.5.3.61 */
10450 | { &hf_oran_ue_layer_power,
10451 | { "ueLayerPower", "oran_fh_cus.ueLayerPower",
10452 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
10453 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
10454 | "UE Layer Power", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10455 | },
10456 |
10457 | /* 7.5.3.62 */
10458 | { &hf_oran_ue_freq_offset,
10459 | { "ueFreqOffset", "oran_fh_cus.ueFreqOffset",
10460 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
10461 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
10462 | "UE frequency offset", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10463 | },
10464 | /* 7.5.3.63 */
10465 | { &hf_oran_ipn_power,
10466 | { "ipnPower", "oran_fh_cus.ipnPower",
10467 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
10468 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
10469 | "Interference plus Noise power", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10470 | },
10471 | /* 7.5.3.64 */
10472 | { &hf_oran_ant_dmrs_snr_val,
10473 | { "antDmrsSnrVal", "oran_fh_cus.antDmrsSnrVal",
10474 | FT_UINT16, BASE_DEC | BASE_RANGE_STRING0x00000100,
10475 | RVALS(freq_offset_fb_values)((0 ? (const struct _range_string*)0 : ((freq_offset_fb_values )))), 0x0,
10476 | "antenna DMRS-SNR", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10477 | },
10478 |
10479 | { &hf_oran_measurement_command,
10480 | { "Measurement Command", "oran_fh_cus.measurement-command",
10481 | FT_STRING, BASE_NONE,
10482 | NULL((void*)0), 0x0,
10483 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10484 | },
10485 |
10486 | /* 7.5.27.2 */
10487 | { &hf_oran_beam_type,
10488 | {"beamType", "oran_fh_cus.beamType",
10489 | FT_UINT16, BASE_DEC,
10490 | VALS(beam_type_vals)((0 ? (const struct _value_string*)0 : ((beam_type_vals)))), 0xc0,
10491 | NULL((void*)0),
10492 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10493 | },
10494 | /* 7.5.3.65 */
10495 | { &hf_oran_meas_cmd_size,
10496 | {"measCmdSize", "oran_fh_cus.measCmdSize",
10497 | FT_UINT16, BASE_DEC,
10498 | NULL((void*)0), 0x0,
10499 | "measurement command size in words",
10500 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10501 | },
10502 |
10503 | { &hf_oran_symbol_reordering_layer,
10504 | { "Layer", "oran_fh_cus.layer",
10505 | FT_STRING, BASE_NONE,
10506 | NULL((void*)0), 0x0,
10507 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10508 | },
10509 | { &hf_oran_dmrs_entry,
10510 | { "Entry", "oran_fh_cus.dmrs-entry",
10511 | FT_STRING, BASE_NONE,
10512 | NULL((void*)0), 0x0,
10513 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10514 | },
10515 |
10516 | /* 7.7.29.3 */
10517 | { &hf_oran_cd_scg_size,
10518 | {"cdScgSize", "oran_fh_cus.cdScgSize",
10519 | FT_UINT8, BASE_DEC | BASE_RANGE_STRING0x00000100,
10520 | RVALS(cd_scg_size_vals)((0 ? (const struct _range_string*)0 : ((cd_scg_size_vals)))), 0x0f,
10521 | "Cyclic delay subcarrier group size",
10522 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10523 | },
10524 | /* 7.7.29.4 */
10525 | { &hf_oran_cd_scg_phase_step,
10526 | {"cdScgPhaseStep", "oran_fh_cus.cdScgPhaseStep",
10527 | FT_INT8, BASE_DEC,
10528 | NULL((void*)0), 0x0,
10529 | "Cyclic delay subcarrier group phase step",
10530 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10531 | },
10532 |
10533 | { &hf_oran_sinr_prb,
10534 | { "PRB", "oran_fh_cus.sinr.prb",
10535 | FT_STRING, BASE_NONE,
10536 | NULL((void*)0), 0x0,
10537 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10538 | },
10539 | /* 7.5.2.20 */
10540 | { &hf_oran_oru_control_sinr_slot_mask_id,
10541 | {"oruControlSinrSlotMaskId", "oran_fh_cus.oruControlSinrSlotMaskId",
10542 | FT_UINT8, BASE_DEC,
10543 | NULL((void*)0), 0x1f,
10544 | "SINR time resolution",
10545 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10546 | },
10547 | /* 7.7.24.21 */
10548 | { &hf_oran_pos_meas,
10549 | {"posMeas", "oran_fh_cus.posMeas",
10550 | FT_BOOLEAN, 8,
10551 | TFS(&tfs_report_no_report_pos_meas)((0 ? (const struct true_false_string*)0 : ((&tfs_report_no_report_pos_meas )))), 0x40,
10552 | "Positioning measurement report request",
10553 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10554 | },
10555 |
10556 | /* 7.5.3.69 */
10557 | { &hf_oran_ue_radial_speed,
10558 | {"ueRadialSpeed", "oran_fh_cus.ueRadialSpeed",
10559 | FT_UINT16, BASE_DEC,
10560 | NULL((void*)0), 0x0,
10561 | "UE radial speed",
10562 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10563 | },
10564 | /* 7.5.3.70 */
10565 | { &hf_oran_ue_az_aoa,
10566 | {"ueAzAoa", "oran_fh_cus.ueAzAoa",
10567 | FT_UINT16, BASE_DEC,
10568 | NULL((void*)0), 0x0,
10569 | "UE azimuth angle of arrival",
10570 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10571 | },
10572 | /* 7.5.3.71 */
10573 | { &hf_oran_ue_ze_aoa,
10574 | {"ueZeAoa", "oran_fh_cus.ueZeAoa",
10575 | FT_UINT16, BASE_DEC,
10576 | NULL((void*)0), 0x0,
10577 | "UE zenith angle of arrival",
10578 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10579 | },
10580 | /* 7.5.3.72 */
10581 | { &hf_oran_ue_pos_toa_offset,
10582 | {"uePosToaOffset", "oran_fh_cus.uePosToaOffset",
10583 | FT_UINT16, BASE_DEC,
10584 | NULL((void*)0), 0x0,
10585 | "UE positioning time of arrival offset",
10586 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10587 | },
10588 |
10589 | /* 7.7.30.2 */
10590 | { &hf_oran_num_rep_ue,
10591 | {"numRepUe", "oran_fh_cus.numRepUe",
10592 | FT_UINT8, BASE_DEC,
10593 | NULL((void*)0), 0x0f,
10594 | "Number of UEs with PUSCH repetition",
10595 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10596 | },
10597 | /* 7.7.30.3 */
10598 | { &hf_oran_rep_ueid,
10599 | {"repUeId", "oran_fh_cus.repUeId",
10600 | FT_UINT16, BASE_DEC,
10601 | NULL((void*)0), 0x7fff,
10602 | "UEId the PUSCH is part of",
10603 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10604 | },
10605 | /* 7.7.30.4 */
10606 | { &hf_oran_is_last_rep,
10607 | {"isLastRep", "oran_fh_cus.isLastRep",
10608 | FT_BOOLEAN, 8,
10609 | NULL((void*)0), 0x40,
10610 | "Last transmission in the repetition",
10611 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10612 | },
10613 | /* 7.7.30.5 */
10614 | { &hf_oran_rep_index,
10615 | {"repIndex", "oran_fh_cus.repIndex",
10616 | FT_UINT8, BASE_DEC,
10617 | NULL((void*)0), 0x3f,
10618 | "Repetition index of the PUSCH transmission",
10619 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10620 | },
10621 | /* 7.7.30.6 */
10622 | { &hf_oran_num_reps,
10623 | {"numReps", "oran_fh_cus.numReps",
10624 | FT_UINT8, BASE_DEC,
10625 | NULL((void*)0), 0x3f,
10626 | "The number of total PUSCH repetitions",
10627 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10628 | },
10629 |
10630 | /* 7.7.31.2 */
10631 | { &hf_oran_mcs_table,
10632 | {"mcsTable", "oran_fh_cus.mcsTable",
10633 | FT_UINT8, BASE_DEC,
10634 | VALS(mcs_table_vals)((0 ? (const struct _value_string*)0 : ((mcs_table_vals)))), 0x0f,
10635 | "MCS index table",
10636 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10637 | },
10638 | /* 7.7.31.3 */
10639 | { &hf_oran_mcs_index,
10640 | {"mcsIndex", "oran_fh_cus.mcsIndex",
10641 | FT_UINT8, BASE_DEC,
10642 | NULL((void*)0), 0x3f,
10643 | "MCS index value",
10644 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10645 | },
10646 |
10647 | /* 7.7.33.3 */
10648 | { &hf_oran_num_meas_req,
10649 | {"numMeasReq", "oran_fh_cus.numMeasReq",
10650 | FT_UINT8, BASE_DEC,
10651 | NULL((void*)0), 0x1f,
10652 | "Number of UEs for which meas is requested",
10653 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10654 | },
10655 | /* 7.7.32.5 */
10656 | { &hf_oran_ue_rank,
10657 | {"ueRank", "oran_fh_cus.ueRank",
10658 | FT_UINT8, BASE_DEC,
10659 | VALS(ue_rank_vals)((0 ? (const struct _value_string*)0 : ((ue_rank_vals)))), 0x0f,
10660 | "Number of UE layers under evaluation",
10661 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10662 | },
10663 | /* 7.7.32.6 */
10664 | { &hf_oran_num_of_ue_ant_ports,
10665 | {"numOfUeAntPorts", "oran_fh_cus.numofUeAntPorts",
10666 | FT_UINT8, BASE_DEC,
10667 | VALS(num_of_ue_ant_ports_vals)((0 ? (const struct _value_string*)0 : ((num_of_ue_ant_ports_vals )))), 0xf0,
10668 | "Used for the PUSCH tx under evaluation",
10669 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10670 | },
10671 | /* 7.7.32.8 */
10672 | { &hf_oran_codebook_subset,
10673 | {"codebookSubset", "oran_fh_cus.codebookSubset",
10674 | FT_UINT8, BASE_DEC,
10675 | VALS(codebook_subset_vals)((0 ? (const struct _value_string*)0 : ((codebook_subset_vals )))), 0xc0,
10676 | "UE capability wrt ULTPMI sets",
10677 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10678 | },
10679 | /* 7.7.32.9 */
10680 | { &hf_oran_full_pwr_mode,
10681 | {"fullPwrMode", "oran_fh_cus.fullPwrMode",
10682 | FT_UINT8, BASE_DEC,
10683 | VALS(full_pwr_mode_vals)((0 ? (const struct _value_string*)0 : ((full_pwr_mode_vals)) )), 0xc0,
10684 | "Transmission mode",
10685 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10686 | },
10687 | /* 7.7.32.10 */
10688 | { &hf_oran_full_pwr_mode_2_tpmi_group,
10689 | {"fullPwrMode2TpmiGroup", "oran_fh_cus.fullPwrMode2TpmiGroup",
10690 | FT_UINT16, BASE_HEX,
10691 | NULL((void*)0), 0x3fff,
10692 | "Capabilities",
10693 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10694 | },
10695 |
10696 | /* 7.5.3.75 */
10697 | { &hf_oran_num_cand_ranks,
10698 | {"numCandRanks", "oran_fh_cus.numCandRanks",
10699 | FT_UINT8, BASE_DEC,
10700 | NULL((void*)0), 0xf0,
10701 | NULL((void*)0),
10702 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10703 | },
10704 | /* 7.5.3.76 */
10705 | { &hf_oran_ue_pref_rank,
10706 | {"uePrefRank", "oran_fh_cus.uePrefRank",
10707 | FT_UINT8, BASE_DEC,
10708 | NULL((void*)0), 0x0f,
10709 | "Most optimal UL Tx rank for UE",
10710 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10711 | },
10712 | /* 7.5.3.77 */
10713 | { &hf_oran_ue_tpmi_rank_y,
10714 | {"ueTpmiRankY", "oran_fh_cus.ueTpmiRankY",
10715 | FT_UINT8, BASE_DEC,
10716 | NULL((void*)0), 0x0,
10717 | "TPMI index for codebook-based PUSCH tx",
10718 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10719 | },
10720 | /* 7.5.3.78 */
10721 | { &hf_oran_ue_tpmi_rank_y_sinr_lx,
10722 | {"ueTpmiRankYSinrLX", "oran_fh_cus.ueTpmiRankYSinrLX",
10723 | FT_UINT16, BASE_HEX | BASE_RANGE_STRING0x00000100,
10724 | RVALS(ue_tmpi_rank_sinr_vals)((0 ? (const struct _range_string*)0 : ((ue_tmpi_rank_sinr_vals )))), 0x0,
10725 | "Estimation of post-equalization SINR",
10726 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10727 | },
10728 | /* 7.5.3.79 */
10729 | { &hf_oran_ue_layer_pre_eq_sinr,
10730 | {"ueLayerPreEqSinr", "oran_fh_cus.ueLayerPreEqSinr",
10731 | FT_UINT16, BASE_HEX,
10732 | NULL((void*)0), 0x0,
10733 | "Pre-equalization SINR of a UE layer",
10734 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10735 | },
10736 |
10737 | { &hf_oran_c_section_common,
10738 | { "Common Section", "oran_fh_cus.c-plane.section.common",
10739 | FT_STRING, BASE_NONE,
10740 | NULL((void*)0), 0x0,
10741 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10742 | },
10743 | { &hf_oran_c_section,
10744 | { "Section", "oran_fh_cus.c-plane.section",
10745 | FT_STRING, BASE_NONE,
10746 | NULL((void*)0), 0x0,
10747 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10748 | },
10749 | { &hf_oran_u_section,
10750 | { "Section", "oran_fh_cus.u-plane.section",
10751 | FT_STRING, BASE_NONE,
10752 | NULL((void*)0), 0x0,
10753 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10754 | },
10755 |
10756 | /* Link back to UL C-plane where udCompHdr was recorded */
10757 | { &hf_oran_ul_cplane_ud_comp_hdr_frame,
10758 | { "C-Plane UL udCompHdr frame", "oran_fh_cus.ul-cplane.udCompHdr",
10759 | FT_FRAMENUM, BASE_NONE,
10760 | FRAMENUM_TYPE(FT_FRAMENUM_REQUEST)((gpointer) (glong) (FT_FRAMENUM_REQUEST)), 0x0,
10761 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10762 | },
10763 |
10764 | /* For ext11, where was a beamId (last) defined? */
10765 | { &hf_oran_bfws_frame_defined,
10766 | { "Beam defined in frame", "oran_fh_cus.bfw-defined",
10767 | FT_FRAMENUM, BASE_NONE,
10768 | FRAMENUM_TYPE(FT_FRAMENUM_RETRANS_PREV)((gpointer) (glong) (FT_FRAMENUM_RETRANS_PREV)), 0x0,
10769 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10770 | },
10771 | { &hf_oran_bfws_symbols_since_defined,
10772 | { "Symbols since BFWs defined", "oran_fh_cus.symbols-since-bfw-defined",
10773 | FT_UINT32, BASE_DEC,
10774 | NULL((void*)0), 0x0,
10775 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10776 | },
10777 |
10778 | /* Corresponding C-plane frame for DL U-plane */
10779 | { &hf_oran_corresponding_cplane_frame,
10780 | { "C-plane frame", "oran_fh_cus.cplane-frame",
10781 | FT_FRAMENUM, BASE_NONE,
10782 | FRAMENUM_TYPE(FT_FRAMENUM_REQUEST)((gpointer) (glong) (FT_FRAMENUM_REQUEST)), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10783 | },
10784 | /* Time since corresponding C-plane frame for U-plane */
10785 | { &hf_oran_corresponding_cplane_frame_time_delta,
10786 | { "Time since C-plane frame", "oran_fh_cus.cplane-frame-time-delta",
10787 | FT_UINT32, BASE_DEC, NULL((void*)0), 0x0,
10788 | "Microseconds since C-plane frame", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10789 | },
10790 | /* Corresponding U-plane frame for C-plane */
10791 | { &hf_oran_corresponding_uplane_frame,
10792 | { "U-plane frame", "oran_fh_cus.uplane-frame",
10793 | FT_FRAMENUM, BASE_NONE,
10794 | FRAMENUM_TYPE(FT_FRAMENUM_RESPONSE)((gpointer) (glong) (FT_FRAMENUM_RESPONSE)), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10795 | },
10796 | { &hf_oran_corresponding_uplane_frames_total,
10797 | { "U-plane frames total", "oran_fh_cus.u-plane-frames-total",
10798 | FT_UINT32, BASE_DEC, NULL((void*)0), 0x0,
10799 | "Number of corresponding U-plane frames", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0)}
10800 | },
10801 |
10802 | /* Reassembly */
10803 | { &hf_oran_fragment,
10804 | { "Fragment", "oran_fh_cus.fragment", FT_FRAMENUM, BASE_NONE,
10805 | NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10806 | { &hf_oran_fragments,
10807 | { "Fragments", "oran_fh_cus.fragments", FT_BYTES, BASE_NONE,
10808 | NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10809 | { &hf_oran_fragment_overlap,
10810 | { "Fragment overlap", "oran_fh_cus.fragment.overlap", FT_BOOLEAN, BASE_NONE,
10811 | NULL((void*)0), 0x0, "Fragment overlaps with other fragments", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10812 | { &hf_oran_fragment_overlap_conflict,
10813 | { "Conflicting data in fragment overlap", "oran_fh_cus.fragment.overlap.conflict",
10814 | FT_BOOLEAN, BASE_NONE, NULL((void*)0), 0x0,
10815 | "Overlapping fragments contained conflicting data", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10816 | { &hf_oran_fragment_multiple_tails,
10817 | { "Multiple tail fragments found", "oran_fh_cus.fragment.multipletails",
10818 | FT_BOOLEAN, BASE_NONE, NULL((void*)0), 0x0,
10819 | "Several tails were found when defragmenting the packet", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10820 | { &hf_oran_fragment_too_long_fragment,
10821 | { "Fragment too long", "oran_fh_cus.fragment.toolongfragment",
10822 | FT_BOOLEAN, BASE_NONE, NULL((void*)0), 0x0,
10823 | "Fragment contained data past end of packet", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10824 | { &hf_oran_fragment_error,
10825 | { "Defragmentation error", "oran_fh_cus.fragment.error", FT_FRAMENUM, BASE_NONE,
10826 | NULL((void*)0), 0x0, "Defragmentation error due to illegal fragments", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10827 | { &hf_oran_fragment_count,
10828 | { "Fragment count", "oran_fh_cus.fragment.count", FT_UINT32, BASE_DEC,
10829 | NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10830 | { &hf_oran_reassembled_in,
10831 | { "Reassembled payload in frame", "oran_fh_cus.reassembled_in", FT_FRAMENUM, BASE_NONE,
10832 | NULL((void*)0), 0x0, "This payload packet is reassembled in this frame", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10833 | { &hf_oran_reassembled_length,
10834 | { "Reassembled payload length", "oran_fh_cus.reassembled.length", FT_UINT32, BASE_DEC,
10835 | NULL((void*)0), 0x0, "The total length of the reassembled payload", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10836 | { &hf_oran_reassembled_data,
10837 | { "Reassembled data", "oran_fh_cus.reassembled.data", FT_BYTES, BASE_NONE,
10838 | NULL((void*)0), 0x0, "The reassembled payload", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10839 |
10840 | { &hf_oran_payload,
10841 | { "Payload", "oran_fh_cus.payload", FT_BYTES, BASE_SHOW_ASCII_PRINTABLE0x00010000,
10842 | NULL((void*)0), 0x0, "Complete or reassembled payload", HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
10843 | };
10844 |
10845 | /* Setup protocol subtree array */
10846 | static int *ett[] = {
10847 | &ett_oran,
10848 | &ett_oran_ecpri_pcid,
10849 | &ett_oran_ecpri_rtcid,
10850 | &ett_oran_ecpri_seqid,
10851 | &ett_oran_section_type,
10852 | &ett_oran_u_timing,
10853 | &ett_oran_u_section,
10854 | &ett_oran_u_prb,
10855 | &ett_oran_section,
10856 | &ett_oran_iq,
10857 | &ett_oran_bfw_bundle,
10858 | &ett_oran_bfw,
10859 | &ett_oran_frequency_range,
10860 | &ett_oran_prb_cisamples,
10861 | &ett_oran_cisample,
10862 | &ett_oran_udcomphdr,
10863 | &ett_oran_udcompparam,
10864 | &ett_oran_cicomphdr,
10865 | &ett_oran_cicompparam,
10866 | &ett_oran_bfwcomphdr,
10867 | &ett_oran_bfwcompparam,
10868 | &ett_oran_ext19_port,
10869 | &ett_oran_prb_allocation,
10870 | &ett_oran_punc_pattern,
10871 | &ett_oran_bfacomphdr,
10872 | &ett_oran_modcomp_param_set,
10873 | &ett_oran_st4_cmd_header,
10874 | &ett_oran_st4_cmd,
10875 | &ett_oran_sym_prb_pattern,
10876 | &ett_oran_measurement_report,
10877 | &ett_oran_measurement_command,
10878 | &ett_oran_sresmask,
10879 | &ett_oran_c_section_common,
10880 | &ett_oran_c_section,
10881 | &ett_oran_remask,
10882 | &ett_oran_mc_scale_remask,
10883 | &ett_oran_symbol_reordering_layer,
10884 | &ett_oran_dmrs_entry,
10885 | &ett_oran_dmrs_symbol_mask,
10886 | &ett_oran_symbol_mask,
10887 | &ett_oran_active_beamspace_coefficient_mask,
10888 | &ett_oran_sinr_prb,
10889 |
10890 | &ett_oran_fragment,
10891 | &ett_oran_fragments
10892 | };
10893 |
10894 | /* Separate subtree array for extensions. Used with [ext-1] */
10895 | static int *ext_ett[HIGHEST_EXTTYPE32];
10896 | for (unsigned extno=0; extno<HIGHEST_EXTTYPE32; extno++) {
10897 | ext_ett[extno] = &ett_oran_c_section_extension[extno];
10898 | }
10899 |
10900 | expert_module_t* expert_oran;
10901 |
10902 | static ei_register_info ei[] = {
10903 | { &ei_oran_unsupported_bfw_compression_method, { "oran_fh_cus.unsupported_bfw_compression_method", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Unsupported BFW Compression Method", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10904 | { &ei_oran_invalid_sample_bit_width, { "oran_fh_cus.invalid_sample_bit_width", PI_UNDECODED0x05000000, PI_ERROR0x00800000, "Unsupported sample bit width", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10905 | { &ei_oran_reserved_numBundPrb, { "oran_fh_cus.reserved_numBundPrb", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "Reserved value 0 for numBundPrb seen - not valid", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10906 | { &ei_oran_extlen_wrong, { "oran_fh_cus.extlen_wrong", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "extlen doesn't match number of dissected bytes", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10907 | { &ei_oran_invalid_eaxc_bit_width, { "oran_fh_cus.invalid_eaxc_bit_width", PI_UNDECODED0x05000000, PI_ERROR0x00800000, "Inconsistent eAxC bit width", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10908 | { &ei_oran_extlen_zero, { "oran_fh_cus.extlen_zero", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "extlen value of 0 is reserved", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10909 | { &ei_oran_rbg_size_reserved, { "oran_fh_cus.rbg_size_reserved", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "rbgSize value of 0 is reserved", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10910 | { &ei_oran_frame_length, { "oran_fh_cus.frame_length", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "there should be 0-3 bytes remaining after PDU in frame", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10911 | { &ei_oran_numprbc_ext21_zero, { "oran_fh_cus.numprbc_ext21_zero", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "numPrbc shall not be set to 0 when ciPrbGroupSize is configured", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10912 | { &ei_oran_ci_prb_group_size_reserved, { "oran_fh_cus.ci_prb_group_size_reserved", PI_MALFORMED0x07000000, PI_WARN0x00600000, "ciPrbGroupSize should be 2-254", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10913 | { &ei_oran_st8_nackid, { "oran_fh_cus.st8_nackid", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "operation for this ackId failed", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10914 | { &ei_oran_st4_no_cmds, { "oran_fh_cus.st4_nackid", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "Not valid for ST4 to carry no commands", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10915 | { &ei_oran_st4_zero_len_cmd, { "oran_fh_cus.st4_zero_len_cmd", PI_MALFORMED0x07000000, PI_WARN0x00600000, "ST4 cmd with length 0 is reserved", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10916 | { &ei_oran_st4_wrong_len_cmd, { "oran_fh_cus.st4_wrong_len_cmd", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "ST4 cmd with length not matching contents", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10917 | { &ei_oran_st4_unknown_cmd, { "oran_fh_cus.st4_unknown_cmd", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "ST4 cmd with unknown command code", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10918 | { &ei_oran_mcot_out_of_range, { "oran_fh_cus.mcot_out_of_range", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "MCOT should be 1-10", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10919 | { &ei_oran_se10_unknown_beamgrouptype, { "oran_fh_cus.se10_unknown_beamgrouptype", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE10 - unknown BeamGroupType value", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10920 | { &ei_oran_se10_not_allowed, { "oran_fh_cus.se10_not_allowed", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE10 - type not allowed for sectionType", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10921 | { &ei_oran_start_symbol_id_not_zero, { "oran_fh_cus.startsymbolid_shall_be_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "For ST4 commands 3&4, startSymbolId shall be 0", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10922 | { &ei_oran_trx_control_cmd_scope, { "oran_fh_cus.trx_command.bad_cmdscope", PI_MALFORMED0x07000000, PI_WARN0x00600000, "TRX command must have cmdScope of ARRAY-COMMAND", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10923 | { &ei_oran_unhandled_se, { "oran_fh_cus.se_not_handled", PI_UNDECODED0x05000000, PI_WARN0x00600000, "SE not recognised/handled by dissector", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10924 | { &ei_oran_bad_symbolmask, { "oran_fh_cus.bad_symbol_mask", PI_MALFORMED0x07000000, PI_WARN0x00600000, "For non-zero sleepMode, symbolMask must be 0x0 or 0x3ffff", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10925 | { &ei_oran_numslots_not_zero, { "oran_fh_cus.numslots_not_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "For ST4 TIME_DOMAIN_BEAM_WEIGHTS, numSlots should be 0", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10926 | { &ei_oran_version_unsupported, { "oran_fh_cus.version_unsupported", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Protocol version unsupported", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10927 | { &ei_oran_laa_msg_type_unsupported, { "oran_fh_cus.laa_msg_type_unsupported", PI_UNDECODED0x05000000, PI_WARN0x00600000, "laaMsgType unsupported", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10928 | { &ei_oran_se_on_unsupported_st, { "oran_fh_cus.se_on_unsupported_st", PI_MALFORMED0x07000000, PI_WARN0x00600000, "Section Extension should not appear on this Section Type", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10929 | { &ei_oran_cplane_unexpected_sequence_number_ul, { "oran_fh_cus.unexpected_seq_no_cplane.ul", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in C-Plane UL", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10930 | { &ei_oran_cplane_unexpected_sequence_number_dl, { "oran_fh_cus.unexpected_seq_no_cplane.dl", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in C-Plane DL", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10931 | { &ei_oran_uplane_unexpected_sequence_number_ul, { "oran_fh_cus.unexpected_seq_no_uplane.ul", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in U-Plane UL", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10932 | { &ei_oran_uplane_unexpected_sequence_number_dl, { "oran_fh_cus.unexpected_seq_no_uplane.dl", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Unexpected sequence number seen in U-Plane DL", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10933 | { &ei_oran_acknack_no_request, { "oran_fh_cus.acknack_no_request", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Have ackNackId response, but no request", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10934 | { &ei_oran_udpcomphdr_should_be_zero, { "oran_fh_cus.udcomphdr_should_be_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "C-Plane udCompHdr in DL should be set to 0", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10935 | { &ei_oran_radio_fragmentation_c_plane, { "oran_fh_cus.radio_fragmentation_c_plane", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "Radio fragmentation not allowed in C-PLane", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10936 | { &ei_oran_lastRbdid_out_of_range, { "oran_fh_cus.lastrbdid_out_of_range", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE 6 has bad rbgSize", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10937 | { &ei_oran_rbgMask_beyond_last_rbdid, { "oran_fh_cus.rbgmask_beyond_lastrbdid", PI_MALFORMED0x07000000, PI_WARN0x00600000, "rbgMask has bits set beyond lastRbgId", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10938 | { &ei_oran_unexpected_measTypeId, { "oran_fh_cus.unexpected_meastypeid", PI_MALFORMED0x07000000, PI_WARN0x00600000, "unexpected measTypeId", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10939 | { &ei_oran_unsupported_compression_method, { "oran_fh_cus.compression_type_unsupported", PI_UNDECODED0x05000000, PI_WARN0x00600000, "Unsupported compression type", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10940 | { &ei_oran_ud_comp_len_wrong_size, { "oran_fh_cus.ud_comp_len_wrong_size", PI_MALFORMED0x07000000, PI_WARN0x00600000, "udCompLen does not match length of U-Plane section", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10941 | { &ei_oran_sresmask2_not_zero_with_rb, { "oran_fh_cus.sresmask2_not_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "sReSMask2 should be zero when rb set", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10942 | { &ei_oran_st6_rb_shall_be_0, { "oran_fh_cus.st6_rb_set", PI_MALFORMED0x07000000, PI_WARN0x00600000, "rb should not be set for Section Type 6", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10943 | { &ei_oran_st9_not_ul, { "oran_fh_cus.st9_not_ul", PI_MALFORMED0x07000000, PI_WARN0x00600000, "Section Type 9 should only be sent in uplink direction", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10944 | { &ei_oran_st10_numsymbol_not_14, { "oran_fh_cus.st10_numsymbol_not_14", PI_MALFORMED0x07000000, PI_WARN0x00600000, "numSymbol should be 14 for Section Type 10", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10945 | { &ei_oran_st10_startsymbolid_not_0, { "oran_fh_cus.st10_startsymbolid_not_0", PI_MALFORMED0x07000000, PI_WARN0x00600000, "startSymbolId should be 0 for Section Type 10", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10946 | { &ei_oran_st10_not_ul, { "oran_fh_cus.st10_not_ul", PI_MALFORMED0x07000000, PI_WARN0x00600000, "Section Type 10 should only be sent in uplink direction", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10947 | { &ei_oran_se24_nothing_to_inherit, { "oran_fh_cus.se24_nothing_to_inherit", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE10 doesn't have type 2 or 3 before trying to inherit", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10948 | { &ei_oran_num_sinr_per_prb_unknown, { "oran_fh_cus.unexpected_num_sinr_per_prb", PI_MALFORMED0x07000000, PI_WARN0x00600000, "invalid numSinrPerPrb value", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10949 | { &ei_oran_start_symbol_id_bits_ignored, { "oran_fh_cus.start_symbol_id_bits_ignored", PI_MALFORMED0x07000000, PI_WARN0x00600000, "some startSymbolId lower bits ignored", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10950 | { &ei_oran_user_group_id_reserved_value, { "oran_fh_cus.user_group_id.reserved_value", PI_MALFORMED0x07000000, PI_WARN0x00600000, "userGroupId value 255 is reserved", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10951 | { &ei_oran_port_list_index_zero, { "oran_fh_cus.port_list_index.zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "portListIndex should not be zero", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10952 | { &ei_oran_ul_uplane_symbol_too_long, { "oran_fh_cus.ul_uplane_symbol_tx_too_slow", PI_RECEIVE0x0f000000, PI_WARN0x00600000, "UL U-Plane Tx took too long for symbol (limit set in preference)", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10953 | { &ei_oran_reserved_not_zero, { "oran_fh_cus.reserved_not_zero", PI_MALFORMED0x07000000, PI_WARN0x00600000, "Reserved field is not zero", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10954 | { &ei_oran_too_many_symbols, { "oran_fh_cus.too_many_symbols", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "Range of symbols in slot exceeds 14", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10955 | { &ei_oran_se30_not_ul, { "oran_fh_cus.se30_not_ul", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE30 should only be sent in uplink direction", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10956 | { &ei_oran_se30_unknown_ueid, { "oran_fh_cus.se30_unknown_ue", PI_MALFORMED0x07000000, PI_WARN0x00600000, "SE30 UEId not recognised from SE10", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10957 | { &ei_oran_beamid_bfws_not_found, { "oran_fh_cus.beamid_bfws_not_found", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "Have bundle with disableBFWs but no definition found", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10958 | { &ei_oran_syminc_set_for_uplane, { "oran_fh_cus.syminc_set_for_uplane", PI_MALFORMED0x07000000, PI_ERROR0x00800000, "symcInc is prohibited in the U-Plane", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10959 | { &ei_oran_cplane_entry_not_found, { "oran_fh_cus.cplane_entry_not_found", PI_SEQUENCE0x02000000, PI_WARN0x00600000, "C-plane for this U-plane section not found", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
10960 | };
10961 |
10962 |
10963 | /* Register the protocol name and description */
10964 | proto_oran = proto_register_protocol("O-RAN Fronthaul CUS", "O-RAN FH CUS", "oran_fh_cus");
10965 |
10966 | /* Allow dissector to find be found by name. */
10967 | register_dissector("oran_fh_cus", dissect_oran, proto_oran);
10968 |
10969 | /* Register the tap name. */
10970 | oran_tap = register_tap("oran-fh-cus");
10971 |
10972 | /* Required function calls to register the header fields and subtrees */
10973 | proto_register_field_array(proto_oran, hf, array_length(hf)(sizeof (hf) / sizeof (hf)[0]));
10974 | proto_register_subtree_array(ett, array_length(ett)(sizeof (ett) / sizeof (ett)[0]));
10975 | proto_register_subtree_array(ext_ett, array_length(ext_ett)(sizeof (ext_ett) / sizeof (ext_ett)[0]));
10976 |
10977 | expert_oran = expert_register_protocol(proto_oran);
10978 | expert_register_field_array(expert_oran, ei, array_length(ei)(sizeof (ei) / sizeof (ei)[0]));
10979 |
10980 |
10981 | /* Preferences */
10982 | module_t * oran_module = prefs_register_protocol(proto_oran, NULL((void*)0));
10983 |
10984 | /* Register bit width/compression preferences separately by direction. */
10985 | prefs_register_uint_preference(oran_module, "oran.du_port_id_bits", "DU Port ID bits [a]",
10986 | "The bit width of DU Port ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_du_port_id_bits);
10987 | prefs_register_uint_preference(oran_module, "oran.bandsector_id_bits", "BandSector ID bits [b]",
10988 | "The bit width of BandSector ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_bandsector_id_bits);
10989 | prefs_register_uint_preference(oran_module, "oran.cc_id_bits", "CC ID bits [c]",
10990 | "The bit width of CC ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_cc_id_bits);
10991 | prefs_register_uint_preference(oran_module, "oran.ru_port_id_bits", "RU Port ID bits [d]",
10992 | "The bit width of RU Port ID - sum of a,b,c&d (eAxC) must be 16", 10, &pref_ru_port_id_bits);
10993 |
10994 | /* Uplink userplane */
10995 | prefs_register_static_text_preference(oran_module, "oran.ul", "", "");
10996 | prefs_register_uint_preference(oran_module, "oran.iq_bitwidth_up", "IQ Bitwidth Uplink",
10997 | "The bit width of a sample in the Uplink (if no udcompHdr and no C-Plane)", 10, &pref_sample_bit_width_uplink);
10998 | prefs_register_enum_preference(oran_module, "oran.ud_comp_up", "Uplink User Data Compression",
10999 | "Uplink User Data Compression (if no udcompHdr and no C-Plane)", &pref_iqCompressionUplink, ul_compression_options, false0);
11000 | prefs_register_enum_preference(oran_module, "oran.ud_comp_hdr_up", "udCompHdr field is present for uplink",
11001 | "The udCompHdr field in U-Plane messages may or may not be present, depending on the "
11002 | "configuration of the O-RU. This preference instructs the dissector to expect "
11003 | "this field to be present in uplink messages",
11004 | &pref_includeUdCompHeaderUplink, udcomphdr_present_options, false0);
11005 | prefs_register_bool_preference(oran_module, "oran.ignore_cplane_ul_udcomphdr", "Ignore UL compression settings from C-plane",
11006 | "When set, override udCompHdr from UL C-Plane with compression method and width configured here", &pref_override_ul_compression);
11007 | prefs_register_uint_preference(oran_module, "oran.ul_slot_us_limit", "Microseconds allowed for UL tx in symbol",
11008 | "Maximum number of microseconds allowed for UL slot transmission before expert warning (zero to disable). N.B. timing relative to first frame seen for same symbol",
11009 | 10, &us_allowed_for_ul_in_symbol);
11010 |
11011 | /* Downlink userplane */
11012 | prefs_register_static_text_preference(oran_module, "oran.dl", "", "");
11013 | prefs_register_uint_preference(oran_module, "oran.iq_bitwidth_down", "IQ Bitwidth Downlink",
11014 | "The bit width of a sample in the Downlink (if no udcompHdr)", 10, &pref_sample_bit_width_downlink);
11015 | prefs_register_enum_preference(oran_module, "oran.ud_comp_down", "Downlink User Data Compression",
11016 | "Downlink User Data Compression", &pref_iqCompressionDownlink, dl_compression_options, false0);
11017 | prefs_register_enum_preference(oran_module, "oran.ud_comp_hdr_down", "udCompHdr field is present for downlink",
11018 | "The udCompHdr field in U-Plane messages may or may not be present, depending on the "
11019 | "configuration of the O-RU. This preference instructs the dissector to expect "
11020 | "this field to be present in downlink messages",
11021 | &pref_includeUdCompHeaderDownlink, udcomphdr_present_options, false0);
11022 |
11023 | /* SINR */
11024 | prefs_register_static_text_preference(oran_module, "oran.sinr", "", "");
11025 | prefs_register_uint_preference(oran_module, "oran.iq_bitwidth_sinr", "IQ Bitwidth SINR",
11026 | "The bit width of a sample in SINR", 10, &pref_sample_bit_width_sinr);
11027 | prefs_register_enum_preference(oran_module, "oran.ud_comp_sinr", "SINR Compression",
11028 | "SINR Compression", &pref_iqCompressionSINR, ul_compression_options, false0);
11029 |
11030 | /* BF-related */
11031 | prefs_register_static_text_preference(oran_module, "oran.bf", "", "");
11032 | prefs_register_uint_preference(oran_module, "oran.num_bf_antennas", "Number of beam weights",
11033 | "Number of array elements that BF weights will be provided for", 10, &pref_num_bf_antennas);
11034 | prefs_register_obsolete_preference(oran_module, "oran.num_weights_per_bundle");
11035 | prefs_register_obsolete_preference(oran_module, "oran.num_bf_weights");
11036 | prefs_register_bool_preference(oran_module, "oran.st6_4byte_alignment_required", "Use 4-byte alignment for ST6 sections",
11037 | "Default is 1-byte alignment", &st6_4byte_alignment);
11038 |
11039 | /* Misc (and will seldom need to be accessed) */
11040 | prefs_register_static_text_preference(oran_module, "oran.misc", "", "");
11041 | prefs_register_bool_preference(oran_module, "oran.show_iq_samples", "Show IQ Sample values",
11042 | "When enabled, for U-Plane frames show each I and Q value in PRB", &pref_showIQSampleValues);
11043 | prefs_register_enum_preference(oran_module, "oran.support_udcomplen", "udCompLen supported",
11044 | "When enabled, U-Plane messages with relevant compression schemes will include udCompLen",
11045 | &pref_support_udcompLen, udcomplen_support_options, false0);
11046 | prefs_register_uint_preference(oran_module, "oran.rbs_in_uplane_section", "Total RBs in User-Plane data section",
11047 | "This is used if numPrbu is signalled as 0", 10, &pref_data_plane_section_total_rbs);
11048 | prefs_register_bool_preference(oran_module, "oran.unscaled_iq", "Show unscaled I/Q values",
11049 | "", &show_unscaled_values);
11050 | prefs_register_bool_preference(oran_module, "oran.attempt_reassembly",
11051 | "Attempt Radio Transport layer reassembly", "",
11052 | &do_radio_transport_layer_reassembly);
11053 | prefs_register_obsolete_preference(oran_module, "oran.k_antenna_ports");
11054 |
11055 | prefs_register_bool_preference(oran_module, "oran.link_planes",
11056 | "Link C-plane and U-plane using sectionId", "",
11057 | &link_planes_together);
11058 |
11059 |
11060 | flow_states_table = wmem_tree_new_autoreset(wmem_epan_scope(), wmem_file_scope());
11061 | flow_results_table = wmem_tree_new_autoreset(wmem_epan_scope(), wmem_file_scope());
11062 | ul_symbol_timing = wmem_tree_new_autoreset(wmem_epan_scope(), wmem_file_scope());
11063 |
11064 | dl_beam_ids_defined = wmem_tree_new_autoreset(wmem_epan_scope(), wmem_file_scope());
11065 | dl_beam_ids_results = wmem_tree_new_autoreset(wmem_epan_scope(), wmem_file_scope());
11066 |
11067 | register_init_routine(&oran_init_protocol);
11068 |
11069 | /* Register reassembly table. */
11070 | reassembly_table_register(&oran_reassembly_table,
11071 | &oran_reassembly_table_functions);
11072 | }
11073 |
11074 | /*
11075 | * Editor modelines - http://www.wireshark.org/tools/modelines.html
11076 | *
11077 | * Local Variables:
11078 | * c-basic-offset: 4
11079 | * tab-width: 8
11080 | * indent-tabs-mode: nil
11081 | * End:
11082 | *
11083 | * ex: set shiftwidth=4 tabstop=8 expandtab:
11084 | * :indentSize=4:tabSize=8:noTabs=true:
11085 | */