### Bug Summary

File: | builds/wireshark/wireshark/epan/dissectors/packet-zbee-nwk-gp.c
Warning: | line 1175, column 13 Value stored to 'offset' is never read

### Annotated Source Code

Press '?' to see keyboard shortcuts

Show analyzer invocation
clang -cc1 -cc1 -triple x86_64-pc-linux-gnu -analyze -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name packet-zbee-nwk-gp.c -analyzer-checker=core -analyzer-checker=apiModeling -analyzer-checker=unix -analyzer-checker=deadcode -analyzer-checker=security.insecureAPI.UncheckedReturn -analyzer-checker=security.insecureAPI.getpw -analyzer-checker=security.insecureAPI.gets -analyzer-checker=security.insecureAPI.mktemp -analyzer-checker=security.insecureAPI.mkstemp -analyzer-checker=security.insecureAPI.vfork -analyzer-checker=nullability.NullPassedToNonnull -analyzer-checker=nullability.NullReturnedFromNonnull -analyzer-output plist -w -setup-static-analyzer -mrelocation-model pic -pic-level 2 -fhalf-no-semantic-interposition -fno-delete-null-pointer-checks -mframe-pointer=all -relaxed-aliasing -fmath-errno -ffp-contract=on -fno-rounding-math -ffloat16-excess-precision=fast -fbfloat16-excess-precision=fast -mconstructor-aliases -funwind-tables=2 -target-cpu x86-64 -tune-cpu generic -debugger-tuning=gdb -fdebug-compilation-dir=/builds/wireshark/wireshark/build -fcoverage-compilation-dir=/builds/wireshark/wireshark/build -resource-dir /usr/lib/llvm-22/lib/clang/22 -isystem /usr/include/glib-2.0 -isystem /usr/lib/x86_64-linux-gnu/glib-2.0/include -isystem /builds/wireshark/wireshark/epan/dissectors -isystem /builds/wireshark/wireshark/build/epan/dissectors -isystem /usr/include/mit-krb5 -isystem /usr/include/libxml2 -isystem /builds/wireshark/wireshark/epan -D CARES_NO_DEPRECATED -D G_DISABLE_DEPRECATED -D G_DISABLE_SINGLE_INCLUDES -D WS_BUILD_DLL -D WS_DEBUG -D WS_DEBUG_UTF_8 -I /builds/wireshark/wireshark/build -I /builds/wireshark/wireshark -I /builds/wireshark/wireshark/include -D _GLIBCXX_ASSERTIONS -internal-isystem /usr/lib/llvm-22/lib/clang/22/include -internal-isystem /usr/local/include -internal-isystem /usr/lib/gcc/x86_64-linux-gnu/16/../../../../x86_64-linux-gnu/include -internal-externc-isystem /usr/include/x86_64-linux-gnu -internal-externc-isystem /include -internal-externc-isystem /usr/include -fmacro-prefix-map=/builds/wireshark/wireshark/= -fmacro-prefix-map=/builds/wireshark/wireshark/build/= -fmacro-prefix-map=../= -Wno-format-nonliteral -std=gnu17 -ferror-limit 19 -fvisibility=hidden -fwrapv -fwrapv-pointer -fstrict-flex-arrays=3 -stack-protector 2 -fstack-clash-protection -fcf-protection=full -fgnuc-version=4.2.1 -fskip-odr-check-in-gmf -fexceptions -fcolor-diagnostics -analyzer-output=html -faddrsig -fdwarf2-cfi-asm -o /builds/wireshark/wireshark/sbout/2026-08-26-100403-3659-1 -x c /builds/wireshark/wireshark/epan/dissectors/packet-zbee-nwk-gp.c

Keyboard shortcuts:

- Use 'j/k' keys for keyboard navigation
- Use 'Shift+S' to show/hide relevant lines
- Use '?' to toggle this window

Close
Show only relevant lines Show control flow arrows

1 | /* packet-zbee-nwk-gp.c
2 | * Dissector routines for the ZigBee Green Power profile (GP)
3 | * Copyright 2013 DSR Corporation, http://dsr-wireless.com/
4 | *
5 | * Wireshark - Network traffic analyzer
6 | * By Gerald Combs <gerald@wireshark.org>
7 | * Copyright 1998 Gerald Combs
8 | *
9 | * Used Owen Kirby's packet-zbee-aps module as a template. Based
10 | * on ZigBee Cluster Library Specification document 075123r02ZB
11 | *
12 | * SPDX-License-Identifier: GPL-2.0-or-later
13 | */
14 |
15 | /* Include files. */
16 | #include "config.h"
17 |
18 | #include <epan/packet.h>
19 | #include <epan/exceptions.h>
20 | #include <epan/expert.h>
21 | #include <epan/prefs.h>
22 | #include <epan/uat.h>
23 | #include <wsutil/bits_ctz.h>
24 | #include <wsutil/pint.h>
25 | #include "packet-zbee.h"
26 | #include "packet-zbee-nwk.h"
27 | #include "packet-zbee-security.h"
28 | #include "packet-zbee-aps.h"
29 | #include "packet-zbee-zcl.h"
30 |
31 | void proto_register_zbee_nwk_gp(void);
32 | void proto_reg_handoff_zbee_nwk_gp(void);
33 |
34 | /**************************/
35 | /* Defines. */
36 | /**************************/
37 |
38 | /* ZigBee NWK GP FCF frame types. */
39 | #define ZBEE_NWK_GP_FCF_DATA0x00 0x00
40 | #define ZBEE_NWK_GP_FCF_MAINTENANCE0x01 0x01
41 |
42 | /* ZigBee NWK GP FCF fields. */
43 | #define ZBEE_NWK_GP_FCF_AUTO_COMMISSIONING0x40 0x40
44 | #define ZBEE_NWK_GP_FCF_CONTROL_EXTENSION0x80 0x80
45 | #define ZBEE_NWK_GP_FCF_FRAME_TYPE0x03 0x03
46 | #define ZBEE_NWK_GP_FCF_VERSION0x3C 0x3C
47 |
48 | /* Extended NWK Frame Control field. */
49 | #define ZBEE_NWK_GP_FCF_EXT_APP_ID0x07 0x07 /* 0 - 2 b. */
50 | #define ZBEE_NWK_GP_FCF_EXT_SECURITY_LEVEL0x18 0x18 /* 3 - 4 b. */
51 | #define ZBEE_NWK_GP_FCF_EXT_SECURITY_KEY0x20 0x20 /* 5 b. */
52 | #define ZBEE_NWK_GP_FCF_EXT_RX_AFTER_TX0x40 0x40 /* 6 b. */
53 | #define ZBEE_NWK_GP_FCF_EXT_DIRECTION0x80 0x80 /* 7 b. */
54 |
55 | /* Definitions for application IDs. */
56 | #define ZBEE_NWK_GP_APP_ID_DEFAULT0x00 0x00
57 | #define ZBEE_NWK_GP_APP_ID_LPED0x01 0x01
58 | #define ZBEE_NWK_GP_APP_ID_ZGP0x02 0x02
59 |
60 | /* Definitions for GP directions. */
61 | #define ZBEE_NWK_GP_FC_EXT_DIRECTION_DEFAULT0x00 0x00
62 | #define ZBEE_NWK_GP_FC_EXT_DIRECTION_FROM_ZGPD0x00 0x00
63 | #define ZBEE_NWK_GP_FC_EXT_DIRECTION_FROM_ZGPP0x01 0x01
64 |
65 | /* Definitions for ZGPD Source IDs. */
66 | #define ZBEE_NWK_GP_ZGPD_SRCID_ALL0xFFFFFFFF 0xFFFFFFFF
67 | #define ZBEE_NWK_GP_ZGPD_SRCID_UNKNOWN0x00000000 0x00000000
68 |
69 | /* Security level values. */
70 | #define ZBEE_NWK_GP_SECURITY_LEVEL_NO0x00 0x00
71 | #define ZBEE_NWK_GP_SECURITY_LEVEL_1LSB0x01 0x01
72 | #define ZBEE_NWK_GP_SECURITY_LEVEL_FULL0x02 0x02
73 | #define ZBEE_NWK_GP_SECURITY_LEVEL_FULLENCR0x03 0x03
74 |
75 | /* GP Security key types. */
76 | #define ZBEE_NWK_GP_SECURITY_KEY_TYPE_NO_KEY0x00 0x00
77 | #define ZBEE_NWK_GP_SECURITY_KEY_TYPE_ZB_NWK_KEY0x01 0x01
78 | #define ZBEE_NWK_GP_SECURITY_KEY_TYPE_GPD_GROUP_KEY0x02 0x02
79 | #define ZBEE_NWK_GP_SECURITY_KEY_TYPE_NWK_KEY_DERIVED_GPD_KEY_GROUP_KEY0x03 0x03
80 | #define ZBEE_NWK_GP_SECURITY_KEY_TYPE_PRECONFIGURED_INDIVIDUAL_GPD_KEY0x04 0x04
81 | #define ZBEE_NWK_GP_SECURITY_KEY_TYPE_DERIVED_INDIVIDUAL_GPD_KEY0x07 0x07
82 |
83 | typedef struct {
84 | /* FCF Data. */
85 | uint8_t frame_type;
86 | bool_Bool nwk_frame_control_extension;
87 |
88 | /* Ext FCF Data. */
89 | uint8_t application_id;
90 | uint8_t security_level;
91 | uint8_t direction;
92 |
93 | /* Src ID. */
94 | uint32_t source_id;
95 |
96 | /* GPD Endpoint */
97 | uint8_t endpoint;
98 |
99 | /* Security Frame Counter. */
100 | uint32_t security_frame_counter;
101 |
102 | /* MIC. */
103 | uint8_t mic_size;
104 | uint32_t mic;
105 |
106 | /* Application Payload. */
107 | uint8_t payload_len;
108 |
109 | /* Source IEEE address from parent */
110 | uint64_t ieee_packet_src64;
111 | } zbee_nwk_green_power_packet;
112 |
113 | /* Definitions for GP Commissioning command opt field (bitmask). */
114 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_MAC_SEQ0x01 0x01
115 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_RX_ON_CAP0x02 0x02
116 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_APPLICATION_INFO0x04 0x04
117 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_PAN_ID_REQ0x10 0x10
118 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_GP_SEC_KEY_REQ0x20 0x20
119 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_FIXED_LOCATION0x40 0x40
120 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_EXT_OPTIONS0x80 0x80
121 |
122 | /* Definitions for GP Commissioning command ext_opt field (bitmask). */
123 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_SEC_LEVEL_CAP0x03 0x03
124 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_KEY_TYPE0x1C 0x1C
125 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_GPD_KEY_PRESENT0x20 0x20
126 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_GPD_KEY_ENCR0x40 0x40
127 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_OUT_COUNTER0x80 0x80
128 |
129 | /* Definitions for GP Commissioning command application information field (bitmask). */
130 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_MIP0x01 0x01
131 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_MMIP0x02 0x02
132 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_GCLP0x04 0x04
133 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_CRP0x08 0x08
134 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_SIP0x10 0x10
135 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_ADCF0x20 0x20
136 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_RES0xC0 0xC0
137 |
138 | /* Definitions for GP Commissioning command switch information field. */
139 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_SWITCH_INFO_LEN0x02 0x02
140 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_SWITCH_CONF_NUM_CONTACTS0x0F 0x0F
141 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_SWITCH_CONF_SWITCH_TYPE0x30 0x30
142 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_SWITCH_CONF_RES0xC0 0xC0
143 |
144 | /* Definitions for GP Commissioning command Number of server ClusterIDs (bitmask) */
145 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_CLID_LIST_LEN_SRV0x0F 0x0F
146 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_CLID_LIST_LEN_CLI0xF0 0xF0
147 |
148 | /* Definitions for GP Decommissioning command opt field (bitmask). */
149 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_PAN_ID_PRESENT0x01 0x01
150 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_SEC_KEY_PRESENT0x02 0x02
151 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_KEY_ENCR0x04 0x04
152 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_SEC_LEVEL0x18 0x18
153 | #define ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_KEY_TYPE0xE0 0xE0
154 |
155 | /* Definition for GP read attributes command opt field (bitmask). */
156 | #define ZBEE_NWK_GP_CMD_READ_ATTRIBUTE_OPT_MULTI_RECORD0x01 0x01
157 | #define ZBEE_NWK_GP_CMD_READ_ATTRIBUTE_OPT_MAN_FIELD_PRESENT0x02 0x02
158 |
159 | #define ZBEE_NWK_GP_CMD_ZCL_TUNNEL_OPT_FRAME_TYPE0x03 0x03
160 | #define ZBEE_NWK_GP_CMD_ZCL_TUNNEL_OPT_MAN_FIELD_PRESENT0x04 0x04
161 | #define ZBEE_NWK_GP_CMD_ZCL_TUNNEL_OPT_DIRECTION0x08 0x08
162 |
163 | /* Definition for GP Application Description command opt fields bitmasks */
164 | #define ZBEE_NWK_GP_CMD_APP_DESC_REPORT_DESC_OPT_TIMEOUT_PRESENT0x01 0x01
165 | #define ZBEE_NWK_GP_CMD_APP_DESC_DATA_PT_DESC_OPT_ATTR_NUM0x07 0x07
166 | #define ZBEE_NWK_GP_CMD_APP_DESC_DATA_PT_DESC_OPT_SERVER0x08 0x08
167 | #define ZBEE_NWK_GP_CMD_APP_DESC_DATA_PT_DESC_OPT_MANU_ID_PRESENT0x10 0x10
168 | #define ZBEE_NWK_GP_CMD_APP_DESC_ATTR_REC_OPT_LEN_REMAIN0x0F 0x0F
169 | #define ZBEE_NWK_GP_CMD_APP_DESC_ATTR_REC_OPT_REPORTED0x10 0x10
170 | #define ZBEE_NWK_GP_CMD_APP_DESC_ATTR_REC_OPT_VAL_PRESENT0x20 0x20
171 |
172 | /* Definitions for GP Channel Request command. */
173 | #define ZBEE_NWK_GP_CMD_CHANNEL_REQUEST_1ST0x0F 0x0F
174 | #define ZBEE_NWK_GP_CMD_CHANNEL_REQUEST_2ND0xF0 0xF0
175 |
176 | /* GP Channel Configuration command. */
177 | #define ZBEE_NWK_GP_CMD_CHANNEL_CONFIGURATION_OPERATION_CH0x0F 0x0F
178 |
179 | /* GP GENERIC IDS. */
180 | #define GPD_DEVICE_ID_GENERIC_GP_SIMPLE_GENERIC_1STATE_SWITCH0x00 0x00
181 | #define GPD_DEVICE_ID_GENERIC_GP_SIMPLE_GENERIC_2STATE_SWITCH0x01 0x01
182 | #define GPD_DEVICE_ID_GENERIC_GP_ON_OFF_SWITCH0x02 0x02
183 | #define GPD_DEVICE_ID_GENERIC_GP_LEVEL_CONTROL_SWITCH0x03 0x03
184 | #define GPD_DEVICE_ID_GENERIC_GP_SIMPLE_SENSOR0x04 0x04
185 | #define GPD_DEVICE_ID_GENERIC_GP_ADVANCED_GENERIC_1STATE_SWITCH0x05 0x05
186 | #define GPD_DEVICE_ID_GENERIC_GP_ADVANCED_GENERIC_2STATE_SWITCH0x06 0x06
187 |
188 | /* GP LIGHTING IDS. */
189 | #define GPD_DEVICE_ID_LIGHTING_GP_COLOR_DIMMER_SWITCH0x10 0x10
190 | #define GPD_DEVICE_ID_LIGHTING_GP_LIGHT_SENSOR0x11 0x11
191 | #define GPD_DEVICE_ID_LIGHTING_GP_OCCUPANCY_SENSOR0x12 0x12
192 |
193 | /* GP CLOSURES IDS. */
194 | #define GPD_DEVICE_ID_CLOSURES_GP_DOOR_LOCK_CONTROLLER0x20 0x20
195 |
196 | /* HVAC IDS. */
197 | #define GPD_DEVICE_ID_HVAC_GP_TEMPERATURE_SENSOR0x30 0x30
198 | #define GPD_DEVICE_ID_HVAC_GP_PRESSURE_SENSOR0x31 0x31
199 | #define GPD_DEVICE_ID_HVAC_GP_FLOW_SENSOR0x32 0x32
200 | #define GPD_DEVICE_ID_HVAC_GP_INDOOR_ENVIRONMENT_SENSOR0x33 0x33
201 |
202 | /* Manufacturer specific device. */
203 | #define GPD_DEVICE_ID_MANUFACTURER_SPECIFIC0xFE 0xFE
204 |
205 | /* GPD manufacturers. */
206 | #define ZBEE_NWK_GP_MANUF_ID_GREENPEAK0x10D0 0x10D0
207 |
208 | /* GPD devices by GreenPeak. */
209 | #define ZBEE_NWK_GP_MANUF_GREENPEAK_IZDS0x0000 0x0000
210 | #define ZBEE_NWK_GP_MANUF_GREENPEAK_IZDWS0x0001 0x0001
211 | #define ZBEE_NWK_GP_MANUF_GREENPEAK_IZLS0x0002 0x0002
212 | #define ZBEE_NWK_GP_MANUF_GREENPEAK_IZRHS0x0003 0x0003
213 |
214 | /*********************/
215 | /* Global variables. */
216 | /*********************/
217 |
218 | /* GP proto handle. */
219 | static int proto_zbee_nwk_gp;
220 |
221 | /* GP NWK FC. */
222 | static int hf_zbee_nwk_gp_auto_commissioning;
223 | static int hf_zbee_nwk_gp_fc_ext;
224 | static int hf_zbee_nwk_gp_fcf;
225 | static int hf_zbee_nwk_gp_frame_type;
226 | static int hf_zbee_nwk_gp_proto_version;
227 |
228 | /* GP NWK FC extension. */
229 | static int hf_zbee_nwk_gp_fc_ext_field;
230 | static int hf_zbee_nwk_gp_fc_ext_app_id;
231 | static int hf_zbee_nwk_gp_fc_ext_direction;
232 | static int hf_zbee_nwk_gp_fc_ext_rx_after_tx;
233 | static int hf_zbee_nwk_gp_fc_ext_sec_key;
234 | static int hf_zbee_nwk_gp_fc_ext_sec_level;
235 |
236 | /* ZGPD Src ID. */
237 | static int hf_zbee_nwk_gp_zgpd_src_id;
238 |
239 | /* ZGPD Endpoint */
240 | static int hf_zbee_nwk_gp_zgpd_endpoint;
241 |
242 | /* Security frame counter. */
243 | static int hf_zbee_nwk_gp_security_frame_counter;
244 |
245 | /* Security MIC. */
246 | static int hf_zbee_nwk_gp_security_mic_2b;
247 | static int hf_zbee_nwk_gp_security_mic_4b;
248 |
249 | /* Payload subframe. */
250 | static int hf_zbee_nwk_gp_command_id;
251 |
252 | /* Commissioning. */
253 | static int hf_zbee_nwk_gp_cmd_comm_device_id;
254 | static int hf_zbee_nwk_gp_cmd_comm_ext_opt;
255 | static int hf_zbee_nwk_gp_cmd_comm_ext_opt_gpd_key_encr;
256 | static int hf_zbee_nwk_gp_cmd_comm_ext_opt_gpd_key_present;
257 | static int hf_zbee_nwk_gp_cmd_comm_ext_opt_key_type;
258 | static int hf_zbee_nwk_gp_cmd_comm_ext_opt_outgoing_counter;
259 | static int hf_zbee_nwk_gp_cmd_comm_ext_opt_sec_level_cap;
260 | static int hf_zbee_nwk_gp_cmd_comm_security_key;
261 | static int hf_zbee_nwk_gp_cmd_comm_gpd_sec_key_mic;
262 | static int hf_zbee_nwk_gp_cmd_comm_opt_ext_opt;
263 | static int hf_zbee_nwk_gp_cmd_comm_opt;
264 | static int hf_zbee_nwk_gp_cmd_comm_opt_fixed_location;
265 | static int hf_zbee_nwk_gp_cmd_comm_opt_mac_sec_num_cap;
266 | static int hf_zbee_nwk_gp_cmd_comm_opt_appli_info_present;
267 | static int hf_zbee_nwk_gp_cmd_comm_opt_panid_req;
268 | static int hf_zbee_nwk_gp_cmd_comm_opt_rx_on_cap;
269 | static int hf_zbee_nwk_gp_cmd_comm_opt_sec_key_req;
270 | static int hf_zbee_nwk_gp_cmd_comm_outgoing_counter;
271 | static int hf_zbee_nwk_gp_cmd_comm_manufacturer_greenpeak_dev_id;
272 | static int hf_zbee_nwk_gp_cmd_comm_manufacturer_dev_id;
273 | static int hf_zbee_nwk_gp_cmd_comm_manufacturer_id;
274 | static int hf_zbee_nwk_gp_cmd_comm_appli_info;
275 | static int hf_zbee_nwk_gp_cmd_comm_appli_info_crp;
276 | static int hf_zbee_nwk_gp_cmd_comm_appli_info_gclp;
277 | static int hf_zbee_nwk_gp_cmd_comm_appli_info_mip;
278 | static int hf_zbee_nwk_gp_cmd_comm_appli_info_mmip;
279 | static int hf_zbee_nwk_gp_cmd_comm_appli_info_sip;
280 | static int hf_zbee_nwk_gp_cmd_comm_appli_info_adcf;
281 | static int hf_zbee_nwk_gp_cmd_comm_appli_info_res;
282 | static int hf_zbee_nwk_gp_cmd_comm_gpd_cmd_num;
283 | static int hf_zbee_nwk_gp_cmd_comm_gpd_cmd_id_list;
284 | static int hf_zbee_nwk_gp_cmd_comm_length_of_clid_list;
285 | static int hf_zbee_nwk_gp_cmd_comm_length_of_clid_list_server;
286 | static int hf_zbee_nwk_gp_cmd_comm_length_of_clid_list_client;
287 | static int hf_zbee_nwk_cmd_comm_clid_list_server;
288 | static int hf_zbee_nwk_cmd_comm_clid_list_client;
289 | static int hf_zbee_nwk_cmd_comm_cluster_id;
290 | static int hf_zbee_nwk_gp_cmd_comm_switch_info;
291 | static int hf_zbee_nwk_gp_cmd_comm_switch_info_length;
292 | static int hf_zbee_nwk_gp_cmd_comm_switch_info_generic_switch_config;
293 | static int hf_zbee_nwk_gp_cmd_comm_switch_info_num_contacts;
294 | static int hf_zbee_nwk_gp_cmd_comm_switch_info_switch_type;
295 | static int hf_zbee_nwk_gp_cmd_comm_switch_info_reserved;
296 | static int hf_zbee_nwk_gp_cmd_comm_switch_info_current_contact_status;
297 |
298 | /* Commissioning reply. */
299 | static int hf_zbee_nwk_gp_cmd_comm_rep_opt;
300 | static int hf_zbee_nwk_gp_cmd_comm_rep_opt_key_encr;
301 | static int hf_zbee_nwk_gp_cmd_comm_rep_opt_panid_present;
302 | static int hf_zbee_nwk_gp_cmd_comm_rep_opt_sec_key_present;
303 | static int hf_zbee_nwk_gp_cmd_comm_rep_opt_sec_level;
304 | static int hf_zbee_nwk_gp_cmd_comm_rep_opt_sec_type;
305 | static int hf_zbee_nwk_gp_cmd_comm_rep_pan_id;
306 | static int hf_zbee_nwk_gp_cmd_comm_rep_frame_counter;
307 |
308 | /* Read attribute and read attribute response. */
309 | static int hf_zbee_nwk_gp_cmd_read_att_opt_multi_rec;
310 | static int hf_zbee_nwk_gp_cmd_read_att_opt_man_field_present;
311 | static int hf_zbee_nwk_gp_cmd_read_att_opt;
312 | static int hf_zbee_nwk_gp_cmd_read_att_record_len;
313 |
314 | /* ZCL Tunnel */
315 | static int hf_zbee_nwk_gp_cmd_zcl_tunnel_opt_frame_type;
316 | static int hf_zbee_nwk_gp_cmd_zcl_tunnel_opt_man_field_present;
317 | static int hf_zbee_nwk_gp_cmd_zcl_tunnel_opt_direction;
318 | static int hf_zbee_nwk_gp_cmd_zcl_tunnel_opt;
319 | static int hf_zbee_nwk_gp_cmd_zcl_tunnel_command_id;
320 | static int hf_zbee_nwk_gp_cmd_zcl_tunnel_payload_len;
321 |
322 | /* Compact Attribute Reporting */
323 | static int hf_zbee_nwk_gp_cmd_compact_attr_report_report_id;
324 | static int hf_zbee_nwk_gp_cmd_compact_attr_report_data_points;
325 |
326 | /* Application Description */
327 | static int hf_zbee_nwk_gp_cmd_app_desc_total_report;
328 | static int hf_zbee_nwk_gp_cmd_app_desc_num_report;
329 | static int hf_zbee_nwk_gp_cmd_app_desc_report_desc_id;
330 | static int hf_zbee_nwk_gp_cmd_app_desc_report_desc_opt;
331 | static int hf_zbee_nwk_gp_cmd_app_desc_report_desc_opt_timeout_present;
332 | static int hf_zbee_nwk_gp_cmd_app_desc_report_desc_timeout;
333 | static int hf_zbee_nwk_gp_cmd_app_desc_report_desc_len_remain;
334 | static int hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt;
335 | static int hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt_num_recs;
336 | static int hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt_server;
337 | static int hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt_manu_id_present;
338 | static int hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_cluster_id;
339 | static int hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_manu_id;
340 | static int hf_zbee_nwk_gp_cmd_app_desc_attr_rec_id;
341 | static int hf_zbee_nwk_gp_cmd_app_desc_attr_rec_data_type;
342 | static int hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt;
343 | static int hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt_len_remain;
344 | static int hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt_reported;
345 | static int hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt_val_present;
346 | static int hf_zbee_nwk_gp_cmd_app_desc_attr_rec_offset;
347 | static int hf_zbee_nwk_gp_cmd_app_desc_attr_rec_val;
348 |
349 | /* Common to commands returning data */
350 | static int hf_zbee_nwk_gp_zcl_attr_status;
351 | static int hf_zbee_nwk_gp_zcl_attr_data_type;
352 | static int hf_zbee_nwk_gp_zcl_attr_cluster_id;
353 |
354 | /* Common to all manufacturer specific commands */
355 | static int hf_zbee_zcl_gp_cmd_ms_manufacturer_code;
356 |
357 | /* Channel request. */
358 | static int hf_zbee_nwk_gp_cmd_channel_request_toggling_behaviour;
359 | static int hf_zbee_nwk_gp_cmd_channel_request_toggling_behaviour_1st;
360 | static int hf_zbee_nwk_gp_cmd_channel_request_toggling_behaviour_2nd;
361 |
362 | /* Channel Configuration command. */
363 | static int hf_zbee_nwk_gp_cmd_operational_channel;
364 | static int hf_zbee_nwk_gp_cmd_channel_configuration;
365 |
366 | /* Move Color command. */
367 | static int hf_zbee_nwk_gp_cmd_move_color_ratex;
368 | static int hf_zbee_nwk_gp_cmd_move_color_ratey;
369 |
370 | /* Move Up/Down command. */
371 | static int hf_zbee_nwk_gp_cmd_move_up_down_rate;
372 |
373 | /* Step Color command. */
374 | static int hf_zbee_nwk_gp_cmd_step_color_stepx;
375 | static int hf_zbee_nwk_gp_cmd_step_color_stepy;
376 | static int hf_zbee_nwk_gp_cmd_step_color_transition_time;
377 |
378 | /* Step Up/Down command. */
379 | static int hf_zbee_nwk_gp_cmd_step_up_down_step_size;
380 | static int hf_zbee_nwk_gp_cmd_step_up_down_transition_time;
381 |
382 | static expert_field ei_zbee_nwk_gp_no_payload;
383 | static expert_field ei_zbee_nwk_gp_inval_residual_data;
384 | static expert_field ei_zbee_nwk_gp_com_rep_no_out_cnt;
385 |
386 | /* Proto tree elements. */
387 | static int ett_zbee_nwk;
388 | static int ett_zbee_nwk_cmd;
389 | static int ett_zbee_nwk_cmd_cinfo;
390 | static int ett_zbee_nwk_cmd_appli_info;
391 | static int ett_zbee_nwk_cmd_options;
392 | static int ett_zbee_nwk_fcf;
393 | static int ett_zbee_nwk_fcf_ext;
394 | static int ett_zbee_nwk_clu_rec;
395 | static int ett_zbee_nwk_att_rec;
396 | static int ett_zbee_nwk_cmd_app_desc_report_desc;
397 | static int ett_zbee_nwk_cmd_app_desc_data_pt_desc;
398 | static int ett_zbee_nwk_cmd_app_desc_data_pt_options;
399 | static int ett_zbee_nwk_cmd_app_desc_att_rec;
400 | static int ett_zbee_nwk_cmd_comm_gpd_cmd_id_list;
401 | static int ett_zbee_nwk_cmd_comm_length_of_clid_list;
402 | static int ett_zbee_nwk_cmd_comm_clid_list_server;
403 | static int ett_zbee_nwk_cmd_comm_clid_list_client;
404 | static int ett_zbee_nwk_cmd_comm_switch_info;
405 | static int ett_zbee_nwk_cmd_comm_switch_info_generic_switch_config;
406 |
407 | /* Common. */
408 | static GSList *zbee_gp_keyring;
409 | static unsigned num_uat_key_records;
410 |
411 | typedef struct {
412 | char *string;
413 | uint8_t byte_order;
414 | char *label;
415 | uint8_t key[ZBEE_SEC_CONST_KEYSIZE16];
416 | } uat_key_record_t;
417 |
418 | static const uint8_t empty_key[ZBEE_SEC_CONST_KEYSIZE16] = {
419 | 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,
420 | 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00
421 | };
422 | static uat_key_record_t *gp_uat_key_records;
423 | static uat_t *zbee_gp_sec_key_table_uat;
424 |
425 | /* UAT. */
426 | UAT_CSTRING_CB_DEF(gp_uat_key_records, string, uat_key_record_t)static void gp_uat_key_records_string_set_cb(void* rec, const char* buf, unsigned len, const void* u1 __attribute__((unused )), const void* u2 __attribute__((unused))) { char* new_buf = g_strndup(buf,len); (__builtin_object_size (((((uat_key_record_t *)rec)->string)), 0) != ((size_t) - 1)) ? g_free_sized ((( (uat_key_record_t*)rec)->string), __builtin_object_size (( (((uat_key_record_t*)rec)->string)), 0)) : (g_free) ((((uat_key_record_t *)rec)->string)); (((uat_key_record_t*)rec)->string) = new_buf ; } static void gp_uat_key_records_string_tostr_cb(void* rec, char** out_ptr, unsigned* out_len, const void* u1 __attribute__ ((unused)), const void* u2 __attribute__((unused))) { if (((uat_key_record_t *)rec)->string ) { *out_ptr = g_strdup_inline ((((uat_key_record_t *)rec)->string)); *out_len = (unsigned)strlen((((uat_key_record_t *)rec)->string)); } else { *out_ptr = g_strdup_inline ("") ; *out_len = 0; } }
427 | UAT_VS_DEF(gp_uat_key_records, byte_order, uat_key_record_t, uint8_t, 0, "Normal")static void gp_uat_key_records_byte_order_set_cb(void* rec, const char* buf, unsigned len, const void* vs, const void* u2 __attribute__ ((unused))) { unsigned i; char* str = g_strndup(buf,len); const char* cstr; ((uat_key_record_t*)rec)->byte_order = 0; for (i=0; ( cstr = ((const value_string*)vs)[i].strptr ) ;i++) { if ((strcmp ((const char *) (cstr), (const char *) (str)) == 0) ) { ((uat_key_record_t*)rec)->byte_order = (uint8_t)((const value_string*)vs)[i].value; (__builtin_object_size ((str), 0 ) != ((size_t) - 1)) ? g_free_sized (str, __builtin_object_size ((str), 0)) : (g_free) (str); return; } } (__builtin_object_size ((str), 0) != ((size_t) - 1)) ? g_free_sized (str, __builtin_object_size ((str), 0)) : (g_free) (str); } static void gp_uat_key_records_byte_order_tostr_cb (void* rec, char** out_ptr, unsigned* out_len, const void* vs , const void* u2 __attribute__((unused))) { unsigned i; for(i =0;((const value_string*)vs)[i].strptr;i++) { if ( ((const value_string *)vs)[i].value == ((uat_key_record_t*)rec)->byte_order ) { *out_ptr = g_strdup_inline (((const value_string*)vs)[i].strptr ); *out_len = (unsigned)strlen(*out_ptr); return; } } *out_ptr = g_strdup_inline ("Normal"); *out_len = (unsigned)strlen("Normal" ); }
428 | UAT_CSTRING_CB_DEF(gp_uat_key_records, label, uat_key_record_t)static void gp_uat_key_records_label_set_cb(void* rec, const char * buf, unsigned len, const void* u1 __attribute__((unused)), const void* u2 __attribute__((unused))) { char* new_buf = g_strndup (buf,len); (__builtin_object_size (((((uat_key_record_t*)rec) ->label)), 0) != ((size_t) - 1)) ? g_free_sized ((((uat_key_record_t *)rec)->label), __builtin_object_size (((((uat_key_record_t *)rec)->label)), 0)) : (g_free) ((((uat_key_record_t*)rec) ->label)); (((uat_key_record_t*)rec)->label) = new_buf; } static void gp_uat_key_records_label_tostr_cb(void* rec, char ** out_ptr, unsigned* out_len, const void* u1 __attribute__(( unused)), const void* u2 __attribute__((unused))) { if (((uat_key_record_t *)rec)->label ) { *out_ptr = g_strdup_inline ((((uat_key_record_t *)rec)->label)); *out_len = (unsigned)strlen((((uat_key_record_t *)rec)->label)); } else { *out_ptr = g_strdup_inline (""); *out_len = 0; } }
429 |
430 | /****************/
431 | /* Field names. */
432 | /****************/
433 |
434 | /* Byte order. */
435 | static const value_string byte_order_vals[] = {
436 | { 0, "Normal"},
437 | { 1, "Reverse"},
438 |
439 | { 0, NULL((void*)0) }
440 | };
441 |
442 | /* Application ID names. */
443 | static const value_string zbee_nwk_gp_app_id_names[] = {
444 | { ZBEE_NWK_GP_APP_ID_LPED0x01, "LPED" },
445 | { ZBEE_NWK_GP_APP_ID_ZGP0x02, "ZGP" },
446 |
447 | { 0, NULL((void*)0) }
448 | };
449 |
450 | /* Green Power commands. */
451 |
452 | /* Abbreviations:
453 | * GPDF commands sent:
454 | * From GPD w/o payload: "F "
455 | * From GPD w payload: "FP"
456 | * To GPD: "T "
457 | */
458 |
459 | #define zbee_nwk_gp_cmd_names_VALUE_STRING_LIST(XXX)XXX( ZB_GP_CMD_ID_IDENTIFY , 0x00, "Identify" ) XXX( ZB_GP_CMD_ID_RECALL_SCENE0 , 0x10, "Recall Scene 0" ) XXX( ZB_GP_CMD_ID_RECALL_SCENE1 , 0x11, "Recall Scene 1" ) XXX( ZB_GP_CMD_ID_RECALL_SCENE2 , 0x12 , "Recall Scene 2" ) XXX( ZB_GP_CMD_ID_RECALL_SCENE3 , 0x13, "Recall Scene 3" ) XXX( ZB_GP_CMD_ID_RECALL_SCENE4 , 0x14, "Recall Scene 4" ) XXX( ZB_GP_CMD_ID_RECALL_SCENE5 , 0x15, "Recall Scene 5" ) XXX ( ZB_GP_CMD_ID_RECALL_SCENE6 , 0x16, "Recall Scene 6" ) XXX( ZB_GP_CMD_ID_RECALL_SCENE7 , 0x17, "Recall Scene 7" ) XXX( ZB_GP_CMD_ID_STORE_SCENE0 , 0x18 , "Store Scene 0" ) XXX( ZB_GP_CMD_ID_STORE_SCENE1 , 0x19, "Store Scene 1" ) XXX( ZB_GP_CMD_ID_STORE_SCENE2 , 0x1A, "Store Scene 2" ) XXX ( ZB_GP_CMD_ID_STORE_SCENE3 , 0x1B, "Store Scene 3" ) XXX( ZB_GP_CMD_ID_STORE_SCENE4 , 0x1C, "Store Scene 4" ) XXX( ZB_GP_CMD_ID_STORE_SCENE5 , 0x1D , "Store Scene 5" ) XXX( ZB_GP_CMD_ID_STORE_SCENE6 , 0x1E, "Store Scene 6" ) XXX( ZB_GP_CMD_ID_STORE_SCENE7 , 0x1F, "Store Scene 7" ) XXX ( ZB_GP_CMD_ID_OFF , 0x20, "Off" ) XXX( ZB_GP_CMD_ID_ON , 0x21 , "On" ) XXX( ZB_GP_CMD_ID_TOGGLE , 0x22, "Toggle" ) XXX( ZB_GP_CMD_ID_RELEASE , 0x23, "Release" ) XXX( ZB_GP_CMD_ID_MOVE_UP , 0x30, "Move Up" ) XXX( ZB_GP_CMD_ID_MOVE_DOWN , 0x31, "Move Down" ) XXX( ZB_GP_CMD_ID_STEP_UP , 0x32, "Step Up" ) XXX( ZB_GP_CMD_ID_STEP_DOWN , 0x33, "Step Down" ) XXX( ZB_GP_CMD_ID_LEVEL_CONTROL_STOP , 0x34, "Level Control/Stop" ) XXX( ZB_GP_CMD_ID_MOVE_UP_WITH_ON_OFF , 0x35, "Move Up (with On/Off)" ) XXX( ZB_GP_CMD_ID_MOVE_DOWN_WITH_ON_OFF , 0x36, "Move Down (with On/Off)" ) XXX( ZB_GP_CMD_ID_STEP_UP_WITH_ON_OFF , 0x37, "Step Up (with On/Off)" ) XXX( ZB_GP_CMD_ID_STEP_DOWN_WITH_ON_OFF , 0x38, "Step Down (with On/Off)" ) XXX( ZB_GP_CMD_ID_MOVE_HUE_STOP , 0x40, "Move Hue Stop" ) XXX ( ZB_GP_CMD_ID_MOVE_HUE_UP , 0x41, "Move Hue Up" ) XXX( ZB_GP_CMD_ID_MOVE_HUE_DOWN , 0x42, "Move Hue Down" ) XXX( ZB_GP_CMD_ID_STEP_HUE_UP , 0x43 , "Step Hue Up" ) XXX( ZB_GP_CMD_ID_STEP_HUW_DOWN , 0x44, "Step Hue Down" ) XXX( ZB_GP_CMD_ID_MOVE_SATURATION_STOP , 0x45, "Move Saturation Stop" ) XXX( ZB_GP_CMD_ID_MOVE_SATURATION_UP , 0x46, "Move Saturation Up" ) XXX( ZB_GP_CMD_ID_MOVE_SATURATION_DOWN , 0x47, "Move Saturation Down" ) XXX( ZB_GP_CMD_ID_STEP_SATURATION_UP , 0x48, "Step Saturation Up" ) XXX( ZB_GP_CMD_ID_STEP_SATURATION_DOWN , 0x49, "Step Saturation Down" ) XXX( ZB_GP_CMD_ID_MOVE_COLOR , 0x4A, "Move Color" ) XXX( ZB_GP_CMD_ID_STEP_COLOR , 0x4B, "Step Color" ) XXX( ZB_GP_CMD_ID_LOCK_DOOR , 0x50, "Lock Door" ) XXX( ZB_GP_CMD_ID_UNLOCK_DOOR , 0x51, "Unlock Door" ) XXX( ZB_GP_CMD_ID_PRESS11 , 0x60, "Press 1 of 1" ) XXX( ZB_GP_CMD_ID_RELEASE11 , 0x61, "Release 1 of 1" ) XXX( ZB_GP_CMD_ID_PRESS12 , 0x62, "Press 1 of 2" ) XXX( ZB_GP_CMD_ID_RELEASE12 , 0x63, "Release 1 of 2" ) XXX( ZB_GP_CMD_ID_PRESS22 , 0x64, "Press 2 of 2" ) XXX( ZB_GP_CMD_ID_RELEASE22 , 0x65, "Release 2 of 2" ) XXX( ZB_GP_CMD_ID_SHORT_PRESS11 , 0x66, "Short press 1 of 1" ) XXX( ZB_GP_CMD_ID_SHORT_PRESS12 , 0x67, "Short press 1 of 2" ) XXX( ZB_GP_CMD_ID_SHORT_PRESS22 , 0x68, "Short press 2 of 2" ) XXX( ZB_GP_CMD_ID_ATTRIBUTE_REPORTING , 0xA0, "Attribute reporting" ) XXX( ZB_GP_CMD_ID_MANUFACTURE_SPECIFIC_ATTR_REPORTING , 0xA1, "Manufacturer-specific attribute reporting" ) XXX( ZB_GP_CMD_ID_MULTI_CLUSTER_REPORTING , 0xA2, "Multi-cluster reporting" ) XXX( ZB_GP_CMD_ID_MANUFACTURER_SPECIFIC_MCLUSTER_REPORTING , 0xA3, "Manufacturer-specific multi-cluster reporting" ) XXX ( ZB_GP_CMD_ID_REQUEST_ATTRIBUTES , 0xA4, "Request Attributes" ) XXX( ZB_GP_CMD_ID_READ_ATTRIBUTES_RESPONSE , 0xA5, "Read Attributes Response" ) XXX( ZB_GP_CMD_ID_ZCL_TUNNELING , 0xA6, "ZCL Tunneling" ) XXX ( ZB_GP_CMD_ID_COMPACT_ATTR_REPORT , 0xA8, "Compact Attribute Reporting" ) XXX( ZB_GP_CMD_ID_ANY_SENSOR_COMMAND_A0_A3 , 0xAF, "Any GPD sensor command (0xA0 - 0xA3)" ) XXX( ZB_GP_CMD_ID_COMMISSIONING , 0xE0, "Commissioning" ) XXX ( ZB_GP_CMD_ID_DECOMMISSIONING , 0xE1, "Decommissioning" ) XXX ( ZB_GP_CMD_ID_SUCCESS , 0xE2, "Success" ) XXX( ZB_GP_CMD_ID_CHANNEL_REQUEST , 0xE3, "Channel Request" ) XXX( ZB_GP_CMD_ID_APPLICATION_DESC , 0xE4, "Application Description" ) XXX( ZB_GP_CMD_ID_COMMISSIONING_REPLY , 0xF0, "Commissioning Reply" ) XXX( ZB_GP_CMD_ID_WRITE_ATTRIBUTES , 0xF1, "Write Attributes" ) XXX( ZB_GP_CMD_ID_READ_ATTRIBUTES , 0xF2, "Read Attributes" ) XXX( ZB_GP_CMD_ID_CHANNEL_CONFIGURATION , 0xF3, "Channel Configuration" ) \
460 | XXX( /*F */ ZB_GP_CMD_ID_IDENTIFY , 0x00, "Identify" ) \
461 | XXX( /*F */ ZB_GP_CMD_ID_RECALL_SCENE0 , 0x10, "Recall Scene 0" ) \
462 | XXX( /*F */ ZB_GP_CMD_ID_RECALL_SCENE1 , 0x11, "Recall Scene 1" ) \
463 | XXX( /*F */ ZB_GP_CMD_ID_RECALL_SCENE2 , 0x12, "Recall Scene 2" ) \
464 | XXX( /*F */ ZB_GP_CMD_ID_RECALL_SCENE3 , 0x13, "Recall Scene 3" ) \
465 | XXX( /*F */ ZB_GP_CMD_ID_RECALL_SCENE4 , 0x14, "Recall Scene 4" ) \
466 | XXX( /*F */ ZB_GP_CMD_ID_RECALL_SCENE5 , 0x15, "Recall Scene 5" ) \
467 | XXX( /*F */ ZB_GP_CMD_ID_RECALL_SCENE6 , 0x16, "Recall Scene 6" ) \
468 | XXX( /*F */ ZB_GP_CMD_ID_RECALL_SCENE7 , 0x17, "Recall Scene 7" ) \
469 | XXX( /*F */ ZB_GP_CMD_ID_STORE_SCENE0 , 0x18, "Store Scene 0" ) \
470 | XXX( /*F */ ZB_GP_CMD_ID_STORE_SCENE1 , 0x19, "Store Scene 1" ) \
471 | XXX( /*F */ ZB_GP_CMD_ID_STORE_SCENE2 , 0x1A, "Store Scene 2" ) \
472 | XXX( /*F */ ZB_GP_CMD_ID_STORE_SCENE3 , 0x1B, "Store Scene 3" ) \
473 | XXX( /*F */ ZB_GP_CMD_ID_STORE_SCENE4 , 0x1C, "Store Scene 4" ) \
474 | XXX( /*F */ ZB_GP_CMD_ID_STORE_SCENE5 , 0x1D, "Store Scene 5" ) \
475 | XXX( /*F */ ZB_GP_CMD_ID_STORE_SCENE6 , 0x1E, "Store Scene 6" ) \
476 | XXX( /*F */ ZB_GP_CMD_ID_STORE_SCENE7 , 0x1F, "Store Scene 7" ) \
477 | XXX( /*F */ ZB_GP_CMD_ID_OFF , 0x20, "Off" ) \
478 | XXX( /*F */ ZB_GP_CMD_ID_ON , 0x21, "On" ) \
479 | XXX( /*F */ ZB_GP_CMD_ID_TOGGLE , 0x22, "Toggle" ) \
480 | XXX( /*F */ ZB_GP_CMD_ID_RELEASE , 0x23, "Release" ) \
481 | XXX( /*FP*/ ZB_GP_CMD_ID_MOVE_UP , 0x30, "Move Up" ) \
482 | XXX( /*FP*/ ZB_GP_CMD_ID_MOVE_DOWN , 0x31, "Move Down" ) \
483 | XXX( /*FP*/ ZB_GP_CMD_ID_STEP_UP , 0x32, "Step Up" ) \
484 | XXX( /*FP*/ ZB_GP_CMD_ID_STEP_DOWN , 0x33, "Step Down" ) \
485 | XXX( /*F */ ZB_GP_CMD_ID_LEVEL_CONTROL_STOP , 0x34, "Level Control/Stop" ) \
486 | XXX( /*FP*/ ZB_GP_CMD_ID_MOVE_UP_WITH_ON_OFF , 0x35, "Move Up (with On/Off)" ) \
487 | XXX( /*FP*/ ZB_GP_CMD_ID_MOVE_DOWN_WITH_ON_OFF , 0x36, "Move Down (with On/Off)" ) \
488 | XXX( /*FP*/ ZB_GP_CMD_ID_STEP_UP_WITH_ON_OFF , 0x37, "Step Up (with On/Off)" ) \
489 | XXX( /*FP*/ ZB_GP_CMD_ID_STEP_DOWN_WITH_ON_OFF , 0x38, "Step Down (with On/Off)" ) \
490 | XXX( /*F */ ZB_GP_CMD_ID_MOVE_HUE_STOP , 0x40, "Move Hue Stop" ) \
491 | XXX( /*FP*/ ZB_GP_CMD_ID_MOVE_HUE_UP , 0x41, "Move Hue Up" ) \
492 | XXX( /*FP*/ ZB_GP_CMD_ID_MOVE_HUE_DOWN , 0x42, "Move Hue Down" ) \
493 | XXX( /*FP*/ ZB_GP_CMD_ID_STEP_HUE_UP , 0x43, "Step Hue Up" ) \
494 | XXX( /*FP*/ ZB_GP_CMD_ID_STEP_HUW_DOWN , 0x44, "Step Hue Down" ) \
495 | XXX( /*F */ ZB_GP_CMD_ID_MOVE_SATURATION_STOP , 0x45, "Move Saturation Stop" ) \
496 | XXX( /*FP*/ ZB_GP_CMD_ID_MOVE_SATURATION_UP , 0x46, "Move Saturation Up" ) \
497 | XXX( /*FP*/ ZB_GP_CMD_ID_MOVE_SATURATION_DOWN , 0x47, "Move Saturation Down" ) \
498 | XXX( /*FP*/ ZB_GP_CMD_ID_STEP_SATURATION_UP , 0x48, "Step Saturation Up" ) \
499 | XXX( /*FP*/ ZB_GP_CMD_ID_STEP_SATURATION_DOWN , 0x49, "Step Saturation Down" ) \
500 | XXX( /*FP*/ ZB_GP_CMD_ID_MOVE_COLOR , 0x4A, "Move Color" ) \
501 | XXX( /*FP*/ ZB_GP_CMD_ID_STEP_COLOR , 0x4B, "Step Color" ) \
502 | XXX( /*F */ ZB_GP_CMD_ID_LOCK_DOOR , 0x50, "Lock Door" ) \
503 | XXX( /*F */ ZB_GP_CMD_ID_UNLOCK_DOOR , 0x51, "Unlock Door" ) \
504 | XXX( /*F */ ZB_GP_CMD_ID_PRESS11 , 0x60, "Press 1 of 1" ) \
505 | XXX( /*F */ ZB_GP_CMD_ID_RELEASE11 , 0x61, "Release 1 of 1" ) \
506 | XXX( /*F */ ZB_GP_CMD_ID_PRESS12 , 0x62, "Press 1 of 2" ) \
507 | XXX( /*F */ ZB_GP_CMD_ID_RELEASE12 , 0x63, "Release 1 of 2" ) \
508 | XXX( /*F */ ZB_GP_CMD_ID_PRESS22 , 0x64, "Press 2 of 2" ) \
509 | XXX( /*F */ ZB_GP_CMD_ID_RELEASE22 , 0x65, "Release 2 of 2" ) \
510 | XXX( /*F */ ZB_GP_CMD_ID_SHORT_PRESS11 , 0x66, "Short press 1 of 1" ) \
511 | XXX( /*F */ ZB_GP_CMD_ID_SHORT_PRESS12 , 0x67, "Short press 1 of 2" ) \
512 | XXX( /*F */ ZB_GP_CMD_ID_SHORT_PRESS22 , 0x68, "Short press 2 of 2" ) \
513 | XXX( /*FP*/ ZB_GP_CMD_ID_ATTRIBUTE_REPORTING , 0xA0, "Attribute reporting" ) \
514 | XXX( /*FP*/ ZB_GP_CMD_ID_MANUFACTURE_SPECIFIC_ATTR_REPORTING , 0xA1, "Manufacturer-specific attribute reporting" ) \
515 | XXX( /*FP*/ ZB_GP_CMD_ID_MULTI_CLUSTER_REPORTING , 0xA2, "Multi-cluster reporting" ) \
516 | XXX( /*FP*/ ZB_GP_CMD_ID_MANUFACTURER_SPECIFIC_MCLUSTER_REPORTING , 0xA3, "Manufacturer-specific multi-cluster reporting" ) \
517 | XXX( /*FP*/ ZB_GP_CMD_ID_REQUEST_ATTRIBUTES , 0xA4, "Request Attributes" ) \
518 | XXX( /*FP*/ ZB_GP_CMD_ID_READ_ATTRIBUTES_RESPONSE , 0xA5, "Read Attributes Response" ) \
519 | XXX( /*FP*/ ZB_GP_CMD_ID_ZCL_TUNNELING , 0xA6, "ZCL Tunneling" ) \
520 | XXX( /*FP*/ ZB_GP_CMD_ID_COMPACT_ATTR_REPORT , 0xA8, "Compact Attribute Reporting" ) \
521 | XXX( /*FP*/ ZB_GP_CMD_ID_ANY_SENSOR_COMMAND_A0_A3 , 0xAF, "Any GPD sensor command (0xA0 - 0xA3)" ) \
522 | XXX( /*FP*/ ZB_GP_CMD_ID_COMMISSIONING , 0xE0, "Commissioning" ) \
523 | XXX( /*F */ ZB_GP_CMD_ID_DECOMMISSIONING , 0xE1, "Decommissioning" ) \
524 | XXX( /*F */ ZB_GP_CMD_ID_SUCCESS , 0xE2, "Success" ) \
525 | XXX( /*FP*/ ZB_GP_CMD_ID_CHANNEL_REQUEST , 0xE3, "Channel Request" ) \
526 | XXX( /*FP*/ ZB_GP_CMD_ID_APPLICATION_DESC , 0xE4, "Application Description" ) \
527 | XXX( /*T */ ZB_GP_CMD_ID_COMMISSIONING_REPLY , 0xF0, "Commissioning Reply" ) \
528 | XXX( /*T */ ZB_GP_CMD_ID_WRITE_ATTRIBUTES , 0xF1, "Write Attributes" ) \
529 | XXX( /*T */ ZB_GP_CMD_ID_READ_ATTRIBUTES , 0xF2, "Read Attributes" ) \
530 | XXX( /*T */ ZB_GP_CMD_ID_CHANNEL_CONFIGURATION , 0xF3, "Channel Configuration" )
531 |
532 | VALUE_STRING_ENUM(zbee_nwk_gp_cmd_names)enum { ZB_GP_CMD_ID_IDENTIFY = 0x00, ZB_GP_CMD_ID_RECALL_SCENE0 = 0x10, ZB_GP_CMD_ID_RECALL_SCENE1 = 0x11, ZB_GP_CMD_ID_RECALL_SCENE2 = 0x12, ZB_GP_CMD_ID_RECALL_SCENE3 = 0x13, ZB_GP_CMD_ID_RECALL_SCENE4 = 0x14, ZB_GP_CMD_ID_RECALL_SCENE5 = 0x15, ZB_GP_CMD_ID_RECALL_SCENE6 = 0x16, ZB_GP_CMD_ID_RECALL_SCENE7 = 0x17, ZB_GP_CMD_ID_STORE_SCENE0 = 0x18, ZB_GP_CMD_ID_STORE_SCENE1 = 0x19, ZB_GP_CMD_ID_STORE_SCENE2 = 0x1A, ZB_GP_CMD_ID_STORE_SCENE3 = 0x1B, ZB_GP_CMD_ID_STORE_SCENE4 = 0x1C, ZB_GP_CMD_ID_STORE_SCENE5 = 0x1D, ZB_GP_CMD_ID_STORE_SCENE6 = 0x1E, ZB_GP_CMD_ID_STORE_SCENE7 = 0x1F, ZB_GP_CMD_ID_OFF = 0x20, ZB_GP_CMD_ID_ON = 0x21, ZB_GP_CMD_ID_TOGGLE = 0x22, ZB_GP_CMD_ID_RELEASE = 0x23, ZB_GP_CMD_ID_MOVE_UP = 0x30, ZB_GP_CMD_ID_MOVE_DOWN = 0x31, ZB_GP_CMD_ID_STEP_UP = 0x32, ZB_GP_CMD_ID_STEP_DOWN = 0x33 , ZB_GP_CMD_ID_LEVEL_CONTROL_STOP = 0x34, ZB_GP_CMD_ID_MOVE_UP_WITH_ON_OFF = 0x35, ZB_GP_CMD_ID_MOVE_DOWN_WITH_ON_OFF = 0x36, ZB_GP_CMD_ID_STEP_UP_WITH_ON_OFF = 0x37, ZB_GP_CMD_ID_STEP_DOWN_WITH_ON_OFF = 0x38, ZB_GP_CMD_ID_MOVE_HUE_STOP = 0x40, ZB_GP_CMD_ID_MOVE_HUE_UP = 0x41, ZB_GP_CMD_ID_MOVE_HUE_DOWN = 0x42, ZB_GP_CMD_ID_STEP_HUE_UP = 0x43, ZB_GP_CMD_ID_STEP_HUW_DOWN = 0x44, ZB_GP_CMD_ID_MOVE_SATURATION_STOP = 0x45, ZB_GP_CMD_ID_MOVE_SATURATION_UP = 0x46, ZB_GP_CMD_ID_MOVE_SATURATION_DOWN = 0x47, ZB_GP_CMD_ID_STEP_SATURATION_UP = 0x48, ZB_GP_CMD_ID_STEP_SATURATION_DOWN = 0x49, ZB_GP_CMD_ID_MOVE_COLOR = 0x4A, ZB_GP_CMD_ID_STEP_COLOR = 0x4B, ZB_GP_CMD_ID_LOCK_DOOR = 0x50, ZB_GP_CMD_ID_UNLOCK_DOOR = 0x51, ZB_GP_CMD_ID_PRESS11 = 0x60, ZB_GP_CMD_ID_RELEASE11 = 0x61, ZB_GP_CMD_ID_PRESS12 = 0x62, ZB_GP_CMD_ID_RELEASE12 = 0x63, ZB_GP_CMD_ID_PRESS22 = 0x64 , ZB_GP_CMD_ID_RELEASE22 = 0x65, ZB_GP_CMD_ID_SHORT_PRESS11 = 0x66, ZB_GP_CMD_ID_SHORT_PRESS12 = 0x67, ZB_GP_CMD_ID_SHORT_PRESS22 = 0x68, ZB_GP_CMD_ID_ATTRIBUTE_REPORTING = 0xA0, ZB_GP_CMD_ID_MANUFACTURE_SPECIFIC_ATTR_REPORTING = 0xA1, ZB_GP_CMD_ID_MULTI_CLUSTER_REPORTING = 0xA2, ZB_GP_CMD_ID_MANUFACTURER_SPECIFIC_MCLUSTER_REPORTING = 0xA3, ZB_GP_CMD_ID_REQUEST_ATTRIBUTES = 0xA4, ZB_GP_CMD_ID_READ_ATTRIBUTES_RESPONSE = 0xA5, ZB_GP_CMD_ID_ZCL_TUNNELING = 0xA6, ZB_GP_CMD_ID_COMPACT_ATTR_REPORT = 0xA8, ZB_GP_CMD_ID_ANY_SENSOR_COMMAND_A0_A3 = 0xAF, ZB_GP_CMD_ID_COMMISSIONING = 0xE0, ZB_GP_CMD_ID_DECOMMISSIONING = 0xE1, ZB_GP_CMD_ID_SUCCESS = 0xE2, ZB_GP_CMD_ID_CHANNEL_REQUEST = 0xE3, ZB_GP_CMD_ID_APPLICATION_DESC = 0xE4, ZB_GP_CMD_ID_COMMISSIONING_REPLY = 0xF0, ZB_GP_CMD_ID_WRITE_ATTRIBUTES = 0xF1, ZB_GP_CMD_ID_READ_ATTRIBUTES = 0xF2, ZB_GP_CMD_ID_CHANNEL_CONFIGURATION = 0xF3, _zbee_nwk_gp_cmd_names_ENUM_DUMMY = 0 };
533 |
534 | VALUE_STRING_ARRAY(zbee_nwk_gp_cmd_names)static const value_string zbee_nwk_gp_cmd_names[] = { { 0x00, "Identify" }, { 0x10, "Recall Scene 0" }, { 0x11, "Recall Scene 1" }, { 0x12, "Recall Scene 2" }, { 0x13, "Recall Scene 3" }, { 0x14, "Recall Scene 4" }, { 0x15, "Recall Scene 5" }, { 0x16 , "Recall Scene 6" }, { 0x17, "Recall Scene 7" }, { 0x18, "Store Scene 0" }, { 0x19, "Store Scene 1" }, { 0x1A, "Store Scene 2" }, { 0x1B , "Store Scene 3" }, { 0x1C, "Store Scene 4" }, { 0x1D, "Store Scene 5" }, { 0x1E, "Store Scene 6" }, { 0x1F, "Store Scene 7" }, { 0x20 , "Off" }, { 0x21, "On" }, { 0x22, "Toggle" }, { 0x23, "Release" }, { 0x30, "Move Up" }, { 0x31, "Move Down" }, { 0x32, "Step Up" }, { 0x33, "Step Down" }, { 0x34, "Level Control/Stop" }, { 0x35 , "Move Up (with On/Off)" }, { 0x36, "Move Down (with On/Off)" }, { 0x37, "Step Up (with On/Off)" }, { 0x38, "Step Down (with On/Off)" }, { 0x40, "Move Hue Stop" }, { 0x41, "Move Hue Up" }, { 0x42 , "Move Hue Down" }, { 0x43, "Step Hue Up" }, { 0x44, "Step Hue Down" }, { 0x45, "Move Saturation Stop" }, { 0x46, "Move Saturation Up" }, { 0x47, "Move Saturation Down" }, { 0x48, "Step Saturation Up" }, { 0x49, "Step Saturation Down" }, { 0x4A, "Move Color" }, { 0x4B, "Step Color" }, { 0x50, "Lock Door" }, { 0x51, "Unlock Door" }, { 0x60, "Press 1 of 1" }, { 0x61, "Release 1 of 1" }, { 0x62 , "Press 1 of 2" }, { 0x63, "Release 1 of 2" }, { 0x64, "Press 2 of 2" }, { 0x65, "Release 2 of 2" }, { 0x66, "Short press 1 of 1" } , { 0x67, "Short press 1 of 2" }, { 0x68, "Short press 2 of 2" }, { 0xA0, "Attribute reporting" }, { 0xA1, "Manufacturer-specific attribute reporting" }, { 0xA2, "Multi-cluster reporting" }, { 0xA3, "Manufacturer-specific multi-cluster reporting" }, { 0xA4, "Request Attributes" }, { 0xA5, "Read Attributes Response" }, { 0xA6, "ZCL Tunneling" }, { 0xA8, "Compact Attribute Reporting" }, { 0xAF, "Any GPD sensor command (0xA0 - 0xA3)" }, { 0xE0, "Commissioning" }, { 0xE1, "Decommissioning" }, { 0xE2, "Success" }, { 0xE3, "Channel Request" }, { 0xE4, "Application Description" }, { 0xF0, "Commissioning Reply" }, { 0xF1, "Write Attributes" }, { 0xF2, "Read Attributes" }, { 0xF3, "Channel Configuration" }, { 0, ((void*)0) } };
535 | value_string_ext zbee_nwk_gp_cmd_names_ext = VALUE_STRING_EXT_INIT(zbee_nwk_gp_cmd_names){ _try_val_to_str_ext_init, 0, (sizeof (zbee_nwk_gp_cmd_names ) / sizeof ((zbee_nwk_gp_cmd_names)[0]))-1, zbee_nwk_gp_cmd_names , "zbee_nwk_gp_cmd_names", ((void*)0) };
536 |
537 |
538 | /* Green Power devices. */
539 | const value_string zbee_nwk_gp_device_ids_names[] = {
540 |
541 | /* GP GENERIC */
542 | { GPD_DEVICE_ID_GENERIC_GP_SIMPLE_GENERIC_1STATE_SWITCH0x00, "Generic: GP Simple Generic 1-state Switch" },
543 | { GPD_DEVICE_ID_GENERIC_GP_SIMPLE_GENERIC_2STATE_SWITCH0x01, "Generic: GP Simple Generic 2-state Switch" },
544 | { GPD_DEVICE_ID_GENERIC_GP_ON_OFF_SWITCH0x02, "Generic: GP On/Off Switch" },
545 | { GPD_DEVICE_ID_GENERIC_GP_LEVEL_CONTROL_SWITCH0x03, "Generic: GP Level Control Switch" },
546 | { GPD_DEVICE_ID_GENERIC_GP_SIMPLE_SENSOR0x04, "Generic: GP Simple Sensor" },
547 | { GPD_DEVICE_ID_GENERIC_GP_ADVANCED_GENERIC_1STATE_SWITCH0x05, "Generic: GP Advanced Generic 1-state Switch" },
548 | { GPD_DEVICE_ID_GENERIC_GP_ADVANCED_GENERIC_2STATE_SWITCH0x06, "Generic: GP Advanced Generic 2-state Switch" },
549 |
550 | /* GP LIGHTING */
551 | { GPD_DEVICE_ID_LIGHTING_GP_COLOR_DIMMER_SWITCH0x10, "Lighting: GP Color Dimmer Switch" },
552 | { GPD_DEVICE_ID_LIGHTING_GP_LIGHT_SENSOR0x11, "Lighting: GP Light Sensor" },
553 | { GPD_DEVICE_ID_LIGHTING_GP_OCCUPANCY_SENSOR0x12, "Lighting: GP Occupancy Sensor" },
554 |
555 | /* GP CLOSURES */
556 | { GPD_DEVICE_ID_CLOSURES_GP_DOOR_LOCK_CONTROLLER0x20, "Closures: GP Door Lock Controller" },
557 |
558 | /* HVAC */
559 | { GPD_DEVICE_ID_HVAC_GP_TEMPERATURE_SENSOR0x30, "HVAC: GP Temperature Sensor" },
560 | { GPD_DEVICE_ID_HVAC_GP_PRESSURE_SENSOR0x31, "HVAC: GP Pressure Sensor" },
561 | { GPD_DEVICE_ID_HVAC_GP_FLOW_SENSOR0x32, "HVAC: GP Flow Sensor" },
562 | { GPD_DEVICE_ID_HVAC_GP_INDOOR_ENVIRONMENT_SENSOR0x33, "HVAC: GP Indoor Environment Sensor" },
563 |
564 | /* CUSTOM */
565 | { GPD_DEVICE_ID_MANUFACTURER_SPECIFIC0xFE, "Manufacturer Specific" },
566 |
567 | { 0, NULL((void*)0) }
568 | };
569 | static value_string_ext zbee_nwk_gp_device_ids_names_ext = VALUE_STRING_EXT_INIT(zbee_nwk_gp_device_ids_names){ _try_val_to_str_ext_init, 0, (sizeof (zbee_nwk_gp_device_ids_names ) / sizeof ((zbee_nwk_gp_device_ids_names)[0]))-1, zbee_nwk_gp_device_ids_names , "zbee_nwk_gp_device_ids_names", ((void*)0) };
570 |
571 | /* GP directions. */
572 | static const value_string zbee_nwk_gp_directions[] = {
573 | { ZBEE_NWK_GP_FC_EXT_DIRECTION_FROM_ZGPD0x00, "From ZGPD" },
574 | { ZBEE_NWK_GP_FC_EXT_DIRECTION_FROM_ZGPP0x01, "From ZGPP" },
575 |
576 | { 0, NULL((void*)0) }
577 | };
578 |
579 | /* Frame types for Green Power profile. */
580 | static const value_string zbee_nwk_gp_frame_types[] = {
581 | { ZBEE_NWK_GP_FCF_DATA0x00, "Data" },
582 | { ZBEE_NWK_GP_FCF_MAINTENANCE0x01, "Maintenance" },
583 |
584 | { 0, NULL((void*)0) }
585 | };
586 |
587 | /* GreenPeak Green Power devices. */
588 | static const value_string zbee_nwk_gp_manufacturer_greenpeak_dev_names[] = {
589 | { ZBEE_NWK_GP_MANUF_GREENPEAK_IZDS0x0000, "IAS Zone Door Sensor" },
590 | { ZBEE_NWK_GP_MANUF_GREENPEAK_IZDWS0x0001, "IAS Zone Door/Window Sensor" },
591 | { ZBEE_NWK_GP_MANUF_GREENPEAK_IZLS0x0002, "IAS Zone Leakage Sensor" },
592 | { ZBEE_NWK_GP_MANUF_GREENPEAK_IZRHS0x0003, "IAS Zone Relative Humidity Sensor" },
593 |
594 | { 0, NULL((void*)0) }
595 | };
596 |
597 | /* GP Generic switch type names. */
598 | static const value_string zbee_nwk_gp_switch_type_names[] = {
599 | { 0x00, "Unknown: exact configuration apart from number of contacts unknown" },
600 | { 0x01, "Button switch" },
601 | { 0x02, "Rocker switch" },
602 | { 0x03, "Reserved" },
603 |
604 | { 0, NULL((void*)0) }
605 | };
606 |
607 | /* GP Src ID names. */
608 | static const value_string zbee_nwk_gp_src_id_names[] = {
609 | { ZBEE_NWK_GP_ZGPD_SRCID_ALL0xFFFFFFFF, "All" },
610 | { ZBEE_NWK_GP_ZGPD_SRCID_UNKNOWN0x00000000, "Unspecified" },
611 |
612 | { 0, NULL((void*)0) }
613 | };
614 |
615 | /* GP security key type names. */
616 | static const value_string zbee_nwk_gp_src_sec_keys_type_names[] = {
617 | { ZBEE_NWK_GP_SECURITY_KEY_TYPE_NO_KEY0x00, "No key" },
618 | { ZBEE_NWK_GP_SECURITY_KEY_TYPE_ZB_NWK_KEY0x01, "ZigBee NWK key" },
619 | { ZBEE_NWK_GP_SECURITY_KEY_TYPE_GPD_GROUP_KEY0x02, "GPD group key" },
620 | { ZBEE_NWK_GP_SECURITY_KEY_TYPE_NWK_KEY_DERIVED_GPD_KEY_GROUP_KEY0x03, "NWK key derived GPD group key" },
621 | { ZBEE_NWK_GP_SECURITY_KEY_TYPE_PRECONFIGURED_INDIVIDUAL_GPD_KEY0x04, "Individual, out of the box GPD key" },
622 | { ZBEE_NWK_GP_SECURITY_KEY_TYPE_DERIVED_INDIVIDUAL_GPD_KEY0x07, "Derived individual GPD key" },
623 |
624 | { 0, NULL((void*)0) }
625 | };
626 |
627 | /* GP security levels. */
628 | static const value_string zbee_nwk_gp_src_sec_levels_names[] = {
629 | { ZBEE_NWK_GP_SECURITY_LEVEL_NO0x00, "No security" },
630 | { ZBEE_NWK_GP_SECURITY_LEVEL_1LSB0x01, "1 LSB of frame counter and short MIC only" },
631 | { ZBEE_NWK_GP_SECURITY_LEVEL_FULL0x02, "Full frame counter and full MIC only" },
632 | { ZBEE_NWK_GP_SECURITY_LEVEL_FULLENCR0x03, "Encryption with full frame counter and full MIC" },
633 |
634 | { 0, NULL((void*)0) }
635 | };
636 |
637 | /*************************/
638 | /* Function definitions. */
639 | /*************************/
640 |
641 | /* UAT record copy callback. */
642 | static void *
643 | uat_key_record_copy_cb(void *n, const void *o, size_t siz _U___attribute__((unused)))
644 | {
645 | uat_key_record_t *new_key = (uat_key_record_t *)n;
646 | const uat_key_record_t *old_key = (const uat_key_record_t *)o;
647 |
648 | new_key->string = g_strdup(old_key->string)g_strdup_inline (old_key->string);
649 | new_key->label = g_strdup(old_key->label)g_strdup_inline (old_key->label);
650 |
651 | return new_key;
652 | }
653 |
654 | /* UAT record free callback. */
655 | static void
656 | uat_key_record_free_cb(void *r)
657 | {
658 | uat_key_record_t *key = (uat_key_record_t *)r;
659 | g_free(key->string)(__builtin_object_size ((key->string), 0) != ((size_t) - 1 )) ? g_free_sized (key->string, __builtin_object_size ((key ->string), 0)) : (g_free) (key->string);
660 | g_free(key->label)(__builtin_object_size ((key->label), 0) != ((size_t) - 1) ) ? g_free_sized (key->label, __builtin_object_size ((key-> label), 0)) : (g_free) (key->label);
661 | }
662 |
663 | /**
664 | *Parses a key string from left to right into a buffer with increasing (normal byte order) or decreasing (reverse
665 | *
666 | *@param key_str pointer to the string
667 | *@param key_buf destination buffer in memory
668 | *@param byte_order byte order
669 | */
670 | static bool_Bool
671 | zbee_gp_security_parse_key(const char *key_str, uint8_t *key_buf, bool_Bool byte_order)
672 | {
673 | bool_Bool string_mode = false0;
674 | char temp;
675 | int i, j;
676 |
677 | memset(key_buf, 0, ZBEE_SEC_CONST_KEYSIZE16);
678 | if (key_str == NULL((void*)0)) {
679 | return false0;
680 | }
681 | if ((temp = *key_str++) == '"') {
682 | string_mode = true1;
683 | temp = *key_str++;
684 | }
685 | j = byte_order ? ZBEE_SEC_CONST_KEYSIZE16 - 1 : 0;
686 | for (i = ZBEE_SEC_CONST_KEYSIZE16 - 1; i >= 0; i--) {
687 | if (string_mode) {
688 | if (g_ascii_isprint(temp)((g_ascii_table[(guchar) (temp)] & G_ASCII_PRINT) != 0)) {
689 | key_buf[j] = temp;
690 | temp = *key_str++;
691 | } else {
692 | return false0;
693 | }
694 | } else {
695 | if ((temp == ':') || (temp == '-') || (temp == ' ')) {
696 | temp = *(key_str++);
697 | }
698 | if (g_ascii_isxdigit(temp)((g_ascii_table[(guchar) (temp)] & G_ASCII_XDIGIT) != 0)) {
699 | key_buf[j] = g_ascii_xdigit_value(temp) << 4;
700 | } else {
701 | return false0;
702 | }
703 | temp = *(key_str++);
704 | if (g_ascii_isxdigit(temp)((g_ascii_table[(guchar) (temp)] & G_ASCII_XDIGIT) != 0)) {
705 | key_buf[j] |= g_ascii_xdigit_value(temp);
706 | } else {
707 | return false0;
708 | }
709 | temp = *(key_str++);
710 | }
711 | if (byte_order) {
712 | j--;
713 | } else {
714 | j++;
715 | }
716 | }
717 | return true1;
718 | }
719 |
720 | /* UAT record update callback. */
721 | static bool_Bool
722 | uat_key_record_update_cb(void *r, char **err)
723 | {
724 | uat_key_record_t *rec = (uat_key_record_t *)r;
725 |
726 | if (rec->string == NULL((void*)0)) {
727 | *err = g_strdup("Key can't be blank.")g_strdup_inline ("Key can't be blank.");
728 | return false0;
729 | } else {
730 | g_strstrip(rec->string)g_strchomp (g_strchug (rec->string));
731 | if (rec->string[0] != 0) {
732 | *err = NULL((void*)0);
733 | if (!zbee_gp_security_parse_key(rec->string, rec->key, rec->byte_order)) {
734 | *err = ws_strdup_printf("Expecting %d hexadecimal bytes or a %d character double-quoted string",wmem_strdup_printf(((void*)0), "Expecting %d hexadecimal bytes or a %d character double-quoted string" , 16, 16)
735 | ZBEE_SEC_CONST_KEYSIZE, ZBEE_SEC_CONST_KEYSIZE)wmem_strdup_printf(((void*)0), "Expecting %d hexadecimal bytes or a %d character double-quoted string" , 16, 16);
736 | return false0;
737 | }
738 | } else {
739 | *err = g_strdup("Key can't be blank.")g_strdup_inline ("Key can't be blank.");
740 | return false0;
741 | }
742 | }
743 | return true1;
744 | }
745 |
746 | static void uat_key_record_post_update_cb(void) {
747 | unsigned i;
748 |
749 | for (i = 0; i < num_uat_key_records; i++) {
750 | if (memcmp(gp_uat_key_records[i].key, empty_key, ZBEE_SEC_CONST_KEYSIZE16) == 0) {
751 | /* key was not loaded from string yet */
752 | zbee_gp_security_parse_key(gp_uat_key_records[i].string, gp_uat_key_records[i].key,
753 | gp_uat_key_records[i].byte_order);
754 | }
755 | }
756 | }
757 |
758 | /**
759 | *Fills in ZigBee GP security nonce from the provided packet structure.
760 | *
761 | *@param packet ZigBee NWK packet.
762 | *@param nonce nonce buffer.
763 | */
764 | static void
765 | zbee_gp_make_nonce(zbee_nwk_green_power_packet *packet, uint8_t *nonce)
766 | {
767 | memset(nonce, 0, ZBEE_SEC_CONST_NONCE_LEN(16 -2 -1));
768 |
769 | /* Source address */
770 | if (packet->application_id == ZBEE_NWK_GP_APP_ID_DEFAULT0x00)
771 | {
772 | if (packet->direction == ZBEE_NWK_GP_FC_EXT_DIRECTION_FROM_ZGPD0x00) {
773 | phtoleu32(nonce, packet->source_id);
774 | }
775 | phtoleu32(nonce+4, packet->source_id);
776 | }
777 | else if (packet->application_id == ZBEE_NWK_GP_APP_ID_ZGP0x02)
778 | {
779 | phtoleu64(nonce, packet->ieee_packet_src64);
780 | }
781 |
782 | /* Frame counter */
783 | phtoleu32(nonce+8, packet->security_frame_counter);
784 |
785 | /* Security control */
786 | if ((packet->application_id == ZBEE_NWK_GP_APP_ID_ZGP0x02) &&
787 | (packet->direction != ZBEE_NWK_GP_FC_EXT_DIRECTION_FROM_ZGPD0x00)) {
788 | nonce[12] = (char)0xc5; /* Security level = 0b101, Key Identifier = 0x00,
789 | Extended nonce = 0b0, Reserved = 0b00 */
790 | } else {
791 | nonce[12] = (char)0x05; /* Security level = 0b101, Key Identifier = 0x00,
792 | Extended nonce = 0b0, Reserved = 0b11 */
793 | }
794 | }
795 |
796 | /**
797 | *Creates a nonce and decrypts secured ZigBee GP payload.
798 | *
799 | *@param packet ZigBee NWK packet.
800 | *@param enc_buffer encoded payload buffer.
801 | *@param offset payload offset.
802 | *@param dec_buffer decoded payload buffer.
803 | *@param payload_len payload length.
804 | *@param mic_len MIC length.
805 | *@param key key.
806 | */
807 | static bool_Bool
808 | zbee_gp_decrypt_payload(zbee_nwk_green_power_packet *packet, const uint8_t *enc_buffer, const unsigned offset, uint8_t
809 | *dec_buffer, unsigned payload_len, unsigned mic_len, uint8_t *key)
810 | {
811 | uint8_t *key_buffer = key;
812 | uint8_t nonce[ZBEE_SEC_CONST_NONCE_LEN(16 -2 -1)];
813 |
814 | zbee_gp_make_nonce(packet, nonce);
815 | if (zbee_sec_ccm_decrypt(key_buffer, nonce, enc_buffer, enc_buffer + offset, dec_buffer, offset, payload_len,
816 | mic_len)) {
817 | return true1;
818 | }
819 |
820 | return false0;
821 | }
822 |
823 | /**
824 | *Dissector for ZigBee Green Power commissioning.
825 | *
826 | *@param tvb pointer to buffer containing raw packet.
827 | *@param pinfo pointer to packet information fields.
828 | *@param tree pointer to data tree Wireshark uses to display packet.
829 | *@param packet packet data.
830 | *@param offset current payload offset.
831 | *@return payload processed offset.
832 | */
833 | static unsigned
834 | dissect_zbee_nwk_gp_cmd_commissioning(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree,
835 | zbee_nwk_green_power_packet *packet, unsigned offset)
836 | {
837 | uint8_t comm_options;
838 | uint8_t comm_ext_options = 0;
839 | uint8_t appli_info_options = 0;
840 | uint16_t manufacturer_id = 0;
841 |
842 | uint8_t i;
843 | uint8_t gpd_cmd_num = 0;
844 | proto_item *gpd_cmd_list;
845 | proto_tree *gpd_cmd_list_tree;
846 |
847 | uint8_t length_of_clid_list_bm;
848 | uint8_t server_clid_num;
849 | uint8_t client_clid_num;
850 | proto_item *server_clid_list, *client_clid_list;
851 | proto_tree *server_clid_list_tree, *client_clid_list_tree;
852 | uint8_t switch_info_length;
853 | proto_item *switch_info;
854 | proto_tree *switch_info_tree;
855 |
856 | void *enc_buffer;
857 | uint8_t *enc_buffer_withA;
858 | uint8_t *dec_buffer;
859 | bool_Bool gp_decrypted;
860 | GSList *GSList_i;
861 | tvbuff_t *payload_tvb;
862 |
863 | static int * const options[] = {
864 | &hf_zbee_nwk_gp_cmd_comm_opt_mac_sec_num_cap,
865 | &hf_zbee_nwk_gp_cmd_comm_opt_rx_on_cap,
866 | &hf_zbee_nwk_gp_cmd_comm_opt_appli_info_present,
867 | &hf_zbee_nwk_gp_cmd_comm_opt_panid_req,
868 | &hf_zbee_nwk_gp_cmd_comm_opt_sec_key_req,
869 | &hf_zbee_nwk_gp_cmd_comm_opt_fixed_location,
870 | &hf_zbee_nwk_gp_cmd_comm_opt_ext_opt,
871 | NULL((void*)0)
872 | };
873 | static int * const ext_options[] = {
874 | &hf_zbee_nwk_gp_cmd_comm_ext_opt_sec_level_cap,
875 | &hf_zbee_nwk_gp_cmd_comm_ext_opt_key_type,
876 | &hf_zbee_nwk_gp_cmd_comm_ext_opt_gpd_key_present,
877 | &hf_zbee_nwk_gp_cmd_comm_ext_opt_gpd_key_encr,
878 | &hf_zbee_nwk_gp_cmd_comm_ext_opt_outgoing_counter,
879 | NULL((void*)0)
880 | };
881 | static int * const appli_info[] = {
882 | &hf_zbee_nwk_gp_cmd_comm_appli_info_mip,
883 | &hf_zbee_nwk_gp_cmd_comm_appli_info_mmip,
884 | &hf_zbee_nwk_gp_cmd_comm_appli_info_gclp,
885 | &hf_zbee_nwk_gp_cmd_comm_appli_info_crp,
886 | &hf_zbee_nwk_gp_cmd_comm_appli_info_sip,
887 | &hf_zbee_nwk_gp_cmd_comm_appli_info_adcf,
888 | &hf_zbee_nwk_gp_cmd_comm_appli_info_res,
889 | NULL((void*)0)
890 | };
891 | static int * const length_of_clid_list[] = {
892 | &hf_zbee_nwk_gp_cmd_comm_length_of_clid_list_server,
893 | &hf_zbee_nwk_gp_cmd_comm_length_of_clid_list_client,
894 | NULL((void*)0)
895 | };
896 | static int * const generic_switch_config[] = {
897 | &hf_zbee_nwk_gp_cmd_comm_switch_info_num_contacts,
898 | &hf_zbee_nwk_gp_cmd_comm_switch_info_switch_type,
899 | &hf_zbee_nwk_gp_cmd_comm_switch_info_reserved,
900 | NULL((void*)0)
901 | };
902 |
903 | /* Get Device ID and display it. */
904 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_device_id, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
905 | offset += 1;
906 | /* Get Options Field, build subtree and display the results. */
907 | comm_options = tvb_get_uint8(tvb, offset);
908 | proto_tree_add_bitmask(tree, tvb, offset, hf_zbee_nwk_gp_cmd_comm_opt, ett_zbee_nwk_cmd_options, options, ENC_NA0x00000000);
909 | offset += 1;
910 |
911 | if (comm_options & ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_EXT_OPTIONS0x80) {
912 | /* Get extended Options Field, build subtree and display the results. */
913 | comm_ext_options = tvb_get_uint8(tvb, offset);
914 | proto_tree_add_bitmask(tree, tvb, offset, hf_zbee_nwk_gp_cmd_comm_ext_opt, ett_zbee_nwk_cmd_options, ext_options, ENC_NA0x00000000);
915 | offset += 1;
916 | if (comm_ext_options & ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_GPD_KEY_PRESENT0x20) {
917 | /* Get security key and display it. */
918 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_security_key, tvb, offset, ZBEE_SEC_CONST_KEYSIZE16, ENC_NA0x00000000);
919 | offset += ZBEE_SEC_CONST_KEYSIZE16;
920 |
921 | /* Key is encrypted */
922 | if (comm_ext_options & ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_GPD_KEY_ENCR0x40) {
923 | /* Get Security MIC and display it. */
924 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_gpd_sec_key_mic, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
925 | offset += 4;
926 |
927 | if (packet != NULL((void*)0))
928 | {
929 | /* Decrypt the security key */
930 | dec_buffer = (uint8_t *)wmem_alloc(pinfo->pool, ZBEE_SEC_CONST_KEYSIZE16);
931 | enc_buffer_withA = (uint8_t *)wmem_alloc(pinfo->pool, 4 + ZBEE_SEC_CONST_KEYSIZE16 + 4); /* CCM* a (this is SrcID) + encKey + MIC */
932 | enc_buffer = tvb_memdup(pinfo->pool, tvb, offset - ZBEE_SEC_CONST_KEYSIZE16 - 4, ZBEE_SEC_CONST_KEYSIZE16 + 4);
933 | phtoleu32(enc_buffer_withA, packet->source_id);
934 | memcpy(enc_buffer_withA+4, enc_buffer, ZBEE_SEC_CONST_KEYSIZE16 + 4);
935 | gp_decrypted = false0;
936 |
937 | for (GSList_i = zbee_gp_keyring; GSList_i && !gp_decrypted; GSList_i = g_slist_next(GSList_i)((GSList_i) ? (((GSList *)(GSList_i))->next) : ((void*)0))) {
938 | packet->security_frame_counter = packet->source_id; /* for Nonce creation*/
939 | gp_decrypted = zbee_gp_decrypt_payload(packet, enc_buffer_withA, 4
940 | , dec_buffer, ZBEE_SEC_CONST_KEYSIZE16, 4, ((key_record_t *)(GSList_i->data))->key);
941 | }
942 |
943 | if (gp_decrypted) {
944 | key_record_t key_record;
945 |
946 | key_record.frame_num = 0;
947 | key_record.label = NULL((void*)0);
948 | memcpy(key_record.key, dec_buffer, ZBEE_SEC_CONST_KEYSIZE16);
949 | zbee_gp_keyring = g_slist_prepend(zbee_gp_keyring, g_memdup2(&key_record, sizeof(key_record_t)));
950 |
951 | payload_tvb = tvb_new_child_real_data(tvb, dec_buffer, ZBEE_SEC_CONST_KEYSIZE16, ZBEE_SEC_CONST_KEYSIZE16);
952 | add_new_data_source(pinfo, payload_tvb, "Decrypted security key");
953 | }
954 | }
955 | }
956 | else
957 | {
958 | key_record_t key_record;
959 | void *key;
960 |
961 | key_record.frame_num = 0;
962 | key_record.label = NULL((void*)0);
963 | key = tvb_memdup(pinfo->pool, tvb, offset - ZBEE_SEC_CONST_KEYSIZE16, ZBEE_SEC_CONST_KEYSIZE16);
964 | memcpy(key_record.key, key, ZBEE_SEC_CONST_KEYSIZE16);
965 | zbee_gp_keyring = g_slist_prepend(zbee_gp_keyring, g_memdup2(&key_record, sizeof(key_record_t)));
966 | }
967 | }
968 |
969 | if (comm_ext_options & ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_OUT_COUNTER0x80) {
970 | /* Get GPD Outgoing Frame Counter and display it. */
971 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_outgoing_counter, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
972 | offset += 4;
973 | }
974 | }
975 | /* Display manufacturer specific data. */
976 | if (comm_options & ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_APPLICATION_INFO0x04) {
977 | /* Display application information. */
978 | appli_info_options = tvb_get_uint8(tvb, offset);
979 | proto_tree_add_bitmask(tree, tvb, offset, hf_zbee_nwk_gp_cmd_comm_appli_info, ett_zbee_nwk_cmd_appli_info, appli_info, ENC_NA0x00000000);
980 | offset += 1;
981 | if (appli_info_options & ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_MIP0x01) {
982 | /* Get Manufacturer ID. */
983 | proto_tree_add_item_ret_uint16(tree, hf_zbee_nwk_gp_cmd_comm_manufacturer_id, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &manufacturer_id);
984 | offset += 2;
985 | }
986 | if (appli_info_options & ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_MMIP0x02) {
987 | /* Get Manufacturer Device ID. */
988 | switch (manufacturer_id) {
989 | case ZBEE_NWK_GP_MANUF_ID_GREENPEAK0x10D0:
990 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_manufacturer_greenpeak_dev_id, tvb, offset, 2,
991 | ENC_LITTLE_ENDIAN0x80000000);
992 | offset += 2;
993 | break;
994 | default:
995 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_manufacturer_dev_id, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
996 | offset += 2;
997 | break;
998 | }
999 | }
1000 | if (appli_info_options & ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_GCLP0x04) {
1001 | /* Get and display number of GPD commands */
1002 | proto_tree_add_item_ret_uint8(tree, hf_zbee_nwk_gp_cmd_comm_gpd_cmd_num, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000, &gpd_cmd_num);
1003 | offset += 1;
1004 | /* Display GPD command list */
1005 | if (gpd_cmd_num > 0) {
1006 | gpd_cmd_list = proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_gpd_cmd_id_list,
1007 | tvb, offset, gpd_cmd_num, ENC_NA0x00000000);
1008 | gpd_cmd_list_tree = proto_item_add_subtree(gpd_cmd_list, ett_zbee_nwk_cmd_comm_gpd_cmd_id_list);
1009 | for (i = 0; i < gpd_cmd_num; i++, offset++) {
1010 | /* Display command id */
1011 | proto_tree_add_item(gpd_cmd_list_tree, hf_zbee_nwk_gp_command_id,
1012 | tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1013 | }
1014 | }
1015 | }
1016 | if (appli_info_options & ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_CRP0x08) {
1017 | /* Get and display Cluster List */
1018 | length_of_clid_list_bm = tvb_get_uint8(tvb, offset);
1019 | server_clid_num = (length_of_clid_list_bm & ZBEE_NWK_GP_CMD_COMMISSIONING_CLID_LIST_LEN_SRV0x0F) >>
1020 | ws_ctz(ZBEE_NWK_GP_CMD_COMMISSIONING_CLID_LIST_LEN_SRV0x0F);
1021 | client_clid_num = (length_of_clid_list_bm & ZBEE_NWK_GP_CMD_COMMISSIONING_CLID_LIST_LEN_CLI0xF0 ) >>
1022 | ws_ctz(ZBEE_NWK_GP_CMD_COMMISSIONING_CLID_LIST_LEN_CLI0xF0);
1023 |
1024 | proto_tree_add_bitmask(tree, tvb, offset, hf_zbee_nwk_gp_cmd_comm_length_of_clid_list,
1025 | ett_zbee_nwk_cmd_comm_length_of_clid_list, length_of_clid_list, ENC_NA0x00000000);
1026 | offset += 1;
1027 |
1028 | if (server_clid_num > 0) {
1029 | /* Display server cluster list */
1030 | server_clid_list = proto_tree_add_item(tree, hf_zbee_nwk_cmd_comm_clid_list_server,
1031 | tvb, offset, 2*server_clid_num, ENC_NA0x00000000);
1032 | server_clid_list_tree = proto_item_add_subtree(server_clid_list, ett_zbee_nwk_cmd_comm_clid_list_server);
1033 | /* Retrieve server clusters */
1034 | for (i = 0; i < server_clid_num; i++, offset += 2) {
1035 | proto_tree_add_item(server_clid_list_tree, hf_zbee_nwk_cmd_comm_cluster_id,
1036 | tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1037 | }
1038 | }
1039 | if (client_clid_num > 0) {
1040 | /* Display client cluster list */
1041 | client_clid_list = proto_tree_add_item(tree, hf_zbee_nwk_cmd_comm_clid_list_client,
1042 | tvb, offset, 2*client_clid_num, ENC_NA0x00000000);
1043 | client_clid_list_tree = proto_item_add_subtree(client_clid_list, ett_zbee_nwk_cmd_comm_clid_list_client);
1044 | /* Retrieve client clusters */
1045 | for (i = 0; i < client_clid_num; i++, offset += 2) {
1046 | proto_tree_add_item(client_clid_list_tree, hf_zbee_nwk_cmd_comm_cluster_id,
1047 | tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1048 | }
1049 | }
1050 | }
1051 | if (appli_info_options & ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_SIP0x10) {
1052 | /* Get and display Switch Information. */
1053 | switch_info_length = tvb_get_uint8(tvb, offset);
1054 | switch_info = proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_switch_info,
1055 | tvb, offset, 1 + switch_info_length, ENC_NA0x00000000);
1056 | switch_info_tree = proto_item_add_subtree(switch_info, ett_zbee_nwk_cmd_comm_switch_info);
1057 | proto_tree_add_item(switch_info_tree, hf_zbee_nwk_gp_cmd_comm_switch_info_length,
1058 | tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1059 | offset += 1;
1060 |
1061 | if (switch_info_length >= 1) {
1062 | proto_tree_add_bitmask(switch_info_tree, tvb, offset,
1063 | hf_zbee_nwk_gp_cmd_comm_switch_info_generic_switch_config,
1064 | ett_zbee_nwk_cmd_comm_switch_info_generic_switch_config, generic_switch_config, ENC_NA0x00000000);
1065 | offset += 1;
1066 | }
1067 |
1068 | if (switch_info_length >= ZBEE_NWK_GP_CMD_COMMISSIONING_SWITCH_INFO_LEN0x02) {
1069 | proto_tree_add_item(switch_info_tree,
1070 | hf_zbee_nwk_gp_cmd_comm_switch_info_current_contact_status,
1071 | tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1072 | offset += 1;
1073 | }
1074 |
1075 | /* Guard against future spec revisions that may increase Switch info length beyond the currently defined value of 0x02. */
1076 | if (switch_info_length > ZBEE_NWK_GP_CMD_COMMISSIONING_SWITCH_INFO_LEN0x02) {
1077 | offset += switch_info_length - ZBEE_NWK_GP_CMD_COMMISSIONING_SWITCH_INFO_LEN0x02;
1078 | }
1079 | }
1080 | }
1081 | return offset;
1082 | } /* dissect_zbee_nwk_gp_cmd_commissioning */
1083 |
1084 | /**
1085 | *Dissector for ZigBee Green Power channel request.
1086 | *
1087 | *@param tvb pointer to buffer containing raw packet.
1088 | *@param pinfo pointer to packet information fields.
1089 | *@param tree pointer to data tree Wireshark uses to display packet.
1090 | *@param packet packet data.
1091 | *@param offset current payload offset.
1092 | *@return payload processed offset.
1093 | */
1094 | static unsigned
1095 | dissect_zbee_nwk_gp_cmd_channel_request(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1096 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1097 | {
1098 | static int * const channels[] = {
1099 | &hf_zbee_nwk_gp_cmd_channel_request_toggling_behaviour_1st,
1100 | &hf_zbee_nwk_gp_cmd_channel_request_toggling_behaviour_2nd,
1101 | NULL((void*)0)
1102 | };
1103 |
1104 | /* Get Command Options Field, build subtree and display the results. */
1105 | proto_tree_add_bitmask(tree, tvb, offset, hf_zbee_nwk_gp_cmd_channel_request_toggling_behaviour, ett_zbee_nwk_cmd_options, channels, ENC_NA0x00000000);
1106 | offset += 1;
1107 | return offset;
1108 | } /* dissect_zbee_nwk_gp_cmd_channel_request */
1109 |
1110 | /**
1111 | * Dissector for ZigBee Green Power Application Description Attribute Records.
1112 | *
1113 | *@param tvb pointer to buffer containing raw packet.
1114 | *@param pinfo pointer to packet information fields.
1115 | *@param tree pointer to data tree Wireshark uses to display packet.
1116 | *@param packet packet data.
1117 | *@param offset current payload offset.
1118 | *@param num_attr_recs number of attribute records to parse.
1119 | *@return payload processed offset.
1120 | */
1121 | static unsigned
1122 | dissect_zbee_nwk_gp_report_desc_attr_rec(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1123 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset, unsigned num_attr_recs)
1124 | {
1125 | uint8_t attr_rec_opt, len_remain;
1126 | proto_tree *subtree = NULL((void*)0);
1127 | unsigned i, end;
1128 |
1129 | static int * const options[] = {
1130 | &hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt_len_remain,
1131 | &hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt_reported,
1132 | &hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt_val_present,
1133 | NULL((void*)0)
1134 | };
1135 |
1136 | for (i = 0; i < num_attr_recs; i++) {
1137 | subtree = proto_tree_add_subtree_format(tree, tvb, offset, -1, ett_zbee_nwk_cmd_app_desc_att_rec,
1138 | NULL((void*)0), "Attribute Record %u", i);
1139 |
1140 | /* Attribute ID */
1141 | proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_app_desc_attr_rec_id, tvb, offset,
1142 | 2, ENC_LITTLE_ENDIAN0x80000000);
1143 | offset += 2;
1144 |
1145 | /* Attribute Data Type */
1146 | proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_app_desc_attr_rec_data_type, tvb,
1147 | offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1148 | offset++;
1149 |
1150 | /* Attribute Options */
1151 | attr_rec_opt = tvb_get_uint8(tvb, offset);
1152 | proto_tree_add_bitmask(subtree, tvb, offset, hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt,
1153 | ett_zbee_nwk_cmd_options, options, ENC_NA0x00000000);
1154 |
1155 | /* Extract remaining attribute record length (add 1 since stored value is decremented by 1) */
1156 | len_remain = (attr_rec_opt & ZBEE_NWK_GP_CMD_APP_DESC_ATTR_REC_OPT_LEN_REMAIN0x0F) + 1;
1157 | offset++;
1158 |
1159 | /* Determine the offset at the end of the packet so we can calculate the attribute value length later */
1160 | end = offset + len_remain;
1161 |
1162 | /* Attribute Offset within Report */
1163 | if (attr_rec_opt & ZBEE_NWK_GP_CMD_APP_DESC_ATTR_REC_OPT_REPORTED0x10) {
1164 | proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_app_desc_attr_rec_offset,
1165 | tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1166 | offset++;
1167 | }
1168 |
1169 | /* Optional Attribute Value */
1170 | if (attr_rec_opt & ZBEE_NWK_GP_CMD_APP_DESC_ATTR_REC_OPT_VAL_PRESENT0x20) {
1171 | unsigned val_len = end - offset;
1172 |
1173 | proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_app_desc_attr_rec_val,
1174 | tvb, offset, val_len, ENC_NA0x00000000);
1175 | offset += val_len;
| Value stored to 'offset' is never read
1176 | }
1177 | offset = end;
1178 | }
1179 |
1180 | return offset;
1181 | } /* dissect_zbee_nwk_gp_report_desc_attr_rec */
1182 |
1183 | /**
1184 | * Dissector for ZigBee Green Power Application Description Data Point Descriptors.
1185 | *
1186 | *@param tvb pointer to buffer containing raw packet.
1187 | *@param pinfo pointer to packet information fields.
1188 | *@param tree pointer to data tree Wireshark uses to display packet.
1189 | *@param packet packet data.
1190 | *@param offset current payload offset.
1191 | *@param len_remain remaining length of report descriptor containing data point descriptors
1192 | *@return payload processed offset.
1193 | */
1194 | static unsigned
1195 | dissect_zbee_nwk_gp_report_desc_data_pt_desc(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1196 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset, uint8_t len_remain)
1197 | {
1198 | uint8_t data_pt_opt, raw_recs;
1199 | proto_item *ti, *opt_item;
1200 | proto_tree *subtree, *mask_tree;
1201 | unsigned i = 0;
1202 | unsigned end = offset + len_remain;
1203 | static int * const options[] = {
1204 | /* We are manually adding the 'number of attribute records' field */
1205 | &hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt_server,
1206 | &hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt_manu_id_present,
1207 | NULL((void*)0)
1208 | };
1209 |
1210 | while (offset < end)
1211 | {
1212 | unsigned start_offset = offset;
1213 |
1214 | /* Create the container for this descriptor */
1215 | subtree = proto_tree_add_subtree_format(tree, tvb, offset, -1, ett_zbee_nwk_cmd_app_desc_data_pt_desc,
1216 | &ti, "Data Point Descriptor %u", i++);
1217 |
1218 | data_pt_opt = tvb_get_uint8(tvb, offset);
1219 | raw_recs = data_pt_opt & ZBEE_NWK_GP_CMD_APP_DESC_DATA_PT_DESC_OPT_ATTR_NUM0x07;
1220 |
1221 | /** Options */
1222 | opt_item = proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt,
1223 | tvb, offset, 1, ENC_NA0x00000000);
1224 |
1225 | mask_tree = proto_item_add_subtree(opt_item, ett_zbee_nwk_cmd_app_desc_data_pt_options);
1226 |
1227 | proto_tree_add_uint_format_value(mask_tree, hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt_num_recs,
1228 | tvb, offset, 1, raw_recs, "%u", raw_recs + 1);
1229 |
1230 | proto_tree_add_bitmask_list(mask_tree, tvb, offset, 1, options, ENC_NA0x00000000);
1231 |
1232 | offset++;
1233 |
1234 | /* Cluster ID */
1235 | proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_cluster_id,
1236 | tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1237 | offset += 2;
1238 |
1239 | /* Optional Manufacturer ID */
1240 | if (data_pt_opt & ZBEE_NWK_GP_CMD_APP_DESC_DATA_PT_DESC_OPT_MANU_ID_PRESENT0x10) {
1241 | proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_manu_id,
1242 | tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1243 | offset += 2;
1244 | }
1245 |
1246 | /* Logic for the next function call remains the same */
1247 | offset = dissect_zbee_nwk_gp_report_desc_attr_rec(tvb, pinfo, subtree, packet, offset, raw_recs + 1);
1248 |
1249 | if (ti) {
1250 | proto_item_set_len(ti, offset - start_offset);
1251 | }
1252 | }
1253 |
1254 | return offset;
1255 | } /* dissect_zbee_nwk_gp_report_desc_data_pt_desc */
1256 |
1257 | /**
1258 | * Dissector for ZigBee Green Power Application Description Report Descriptors.
1259 | *
1260 | *@param tvb pointer to buffer containing raw packet.
1261 | *@param pinfo pointer to packet information fields.
1262 | *@param tree pointer to data tree Wireshark uses to display packet.
1263 | *@param packet packet data.
1264 | *@param offset current payload offset.
1265 | *@param num_reports number of report descriptors to parse.
1266 | *@return payload processed offset.
1267 | */
1268 | static unsigned
1269 | dissect_zbee_nwk_gp_report_desc(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1270 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset, unsigned num_reports)
1271 | {
1272 | uint8_t report_opt, len_remain;
1273 | proto_tree *subtree = NULL((void*)0);
1274 | unsigned i;
1275 |
1276 | static int * const options[] = {
1277 | &hf_zbee_nwk_gp_cmd_app_desc_report_desc_opt_timeout_present,
1278 | NULL((void*)0)
1279 | };
1280 |
1281 | for (i = 0; i < num_reports; i++) {
1282 | subtree = proto_tree_add_subtree_format(tree, tvb, offset, -1, ett_zbee_nwk_cmd_app_desc_report_desc,
1283 | NULL((void*)0), "Report Descriptor %u", i);
1284 |
1285 | /* Report Identifier */
1286 | proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_app_desc_report_desc_id, tvb,
1287 | offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1288 | offset++;
1289 |
1290 | /* Report Options */
1291 | report_opt = tvb_get_uint8(tvb, offset);
1292 | proto_tree_add_bitmask(subtree, tvb, offset, hf_zbee_nwk_gp_cmd_app_desc_report_desc_opt,
1293 | ett_zbee_nwk_cmd_options, options, ENC_NA0x00000000);
1294 | offset++;
1295 |
1296 | /* Optional Timeout Period */
1297 | if (report_opt & ZBEE_NWK_GP_CMD_APP_DESC_REPORT_DESC_OPT_TIMEOUT_PRESENT0x01) {
1298 | proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_app_desc_report_desc_timeout,
1299 | tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1300 | offset += 2;
1301 | }
1302 |
1303 | /* Remaining Length */
1304 | len_remain = tvb_get_uint8(tvb, offset);
1305 | proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_app_desc_report_desc_len_remain,
1306 | tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1307 | offset++;
1308 |
1309 | /* Dissect the data point descriptors */
1310 | offset = dissect_zbee_nwk_gp_report_desc_data_pt_desc(tvb, pinfo, subtree, packet, offset, len_remain);
1311 | }
1312 |
1313 | return offset;
1314 | } /* dissect_zbee_nwk_gp_report_desc */
1315 |
1316 |
1317 | /**
1318 | * Dissector for ZigBee Green Power Application Description.
1319 | *
1320 | *@param tvb pointer to buffer containing raw packet.
1321 | *@param pinfo pointer to packet information fields.
1322 | *@param tree pointer to data tree Wireshark uses to display packet.
1323 | *@param packet packet data.
1324 | *@param offset current payload offset.
1325 | *@return payload processed offset.
1326 | */
1327 | static unsigned
1328 | dissect_zbee_nwk_gp_cmd_application_desc(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1329 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1330 | {
1331 | uint8_t num_reports;
1332 |
1333 | /* Total number of reports */
1334 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_app_desc_total_report, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1335 | offset++;
1336 |
1337 | /* Number of reports */
1338 | num_reports = tvb_get_uint8(tvb, offset);
1339 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_app_desc_num_report, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1340 | offset++;
1341 |
1342 | /* Dissect the report descriptors */
1343 | offset = dissect_zbee_nwk_gp_report_desc(tvb, pinfo, tree, packet, offset, num_reports);
1344 |
1345 | return offset;
1346 | } /* dissect_zbee_nwk_gp_cmd_application_desc */
1347 |
1348 | /**
1349 | *Dissector for ZigBee Green Power channel configuration.
1350 | *
1351 | *@param tvb pointer to buffer containing raw packet.
1352 | *@param pinfo pointer to packet information fields.
1353 | *@param tree pointer to data tree Wireshark uses to display packet.
1354 | *@param packet packet data.
1355 | *@param offset current payload offset.
1356 | *@return payload processed offset.
1357 | */
1358 | static unsigned
1359 | dissect_zbee_nwk_gp_cmd_channel_configuration(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1360 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1361 | {
1362 | static int * const channels[] = {
1363 | &hf_zbee_nwk_gp_cmd_channel_configuration,
1364 | NULL((void*)0)
1365 | };
1366 |
1367 | /* Get Command Options Field, build subtree and display the results. */
1368 | proto_tree_add_bitmask(tree, tvb, offset, hf_zbee_nwk_gp_cmd_operational_channel, ett_zbee_nwk_cmd_options, channels, ENC_NA0x00000000);
1369 |
1370 | offset += 1;
1371 | return offset;
1372 | } /* dissect_zbee_nwk_gp_cmd_channel_configuration */
1373 |
1374 | /**
1375 | *Dissector for ZigBee Green Power commands attrib reporting.
1376 | *
1377 | *@param tvb pointer to buffer containing raw packet.
1378 | *@param pinfo pointer to packet information fields.
1379 | *@param tree pointer to data tree Wireshark uses to display packet.
1380 | *@param packet packet data.
1381 | *@param offset current payload offset.
1382 | *@param mfr_code manufacturer code.
1383 | *@return payload processed offset.
1384 | */
1385 | static unsigned
1386 | dissect_zbee_nwk_gp_cmd_attr_reporting(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1387 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset, uint16_t mfr_code)
1388 | {
1389 | uint16_t cluster_id;
1390 | proto_tree *field_tree;
1391 |
1392 | /* Get cluster ID and add it into the tree. */
1393 | proto_tree_add_item_ret_uint16(tree, hf_zbee_nwk_gp_zcl_attr_cluster_id, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &cluster_id);
1394 |
1395 | offset += 2;
1396 | /* Create subtree and parse ZCL Write Attribute Payload. */
1397 | field_tree = proto_tree_add_subtree_format(tree, tvb, offset, 2, ett_zbee_nwk_cmd_options, NULL((void*)0),
1398 | "Attribute reporting command for cluster: 0x%04X", cluster_id);
1399 |
1400 | dissect_zcl_report_attr(tvb, pinfo, field_tree, &offset, cluster_id, mfr_code, ZBEE_ZCL_FCF_TO_CLIENT0x01);
1401 |
1402 | return offset;
1403 | } /* dissect_zbee_nwk_gp_cmd_attr_reporting */
1404 |
1405 |
1406 | /**
1407 | * Dissector for ZigBee Green Power manufacturer specific attribute reporting.
1408 | *
1409 | *@param tvb pointer to buffer containing raw packet.
1410 | *@param pinfo pointer to packet information fields.
1411 | *@param tree pointer to data tree Wireshark uses to display packet.
1412 | *@param packet packet data.
1413 | *@param offset current payload offset.
1414 | *@return payload processed offset.
1415 | */
1416 | static unsigned
1417 | dissect_zbee_nwk_gp_cmd_MS_attr_reporting(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1418 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1419 | {
1420 | uint16_t mfr_code;
1421 |
1422 | /*dissect manufacturer ID*/
1423 | proto_tree_add_item_ret_uint16(tree, hf_zbee_zcl_gp_cmd_ms_manufacturer_code, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &mfr_code);
1424 | offset += 2;
1425 |
1426 | offset = dissect_zbee_nwk_gp_cmd_attr_reporting(tvb, pinfo, tree, packet, offset, mfr_code);
1427 |
1428 | return offset;
1429 | }/*dissect_zbee_nwk_gp_cmd_MS_attr_reporting*/
1430 |
1431 |
1432 |
1433 |
1434 | /**
1435 | *Dissector for ZigBee Green Power commissioning reply.
1436 | *
1437 | *@param tvb pointer to buffer containing raw packet.
1438 | *@param pinfo pointer to packet information fields.
1439 | *@param tree pointer to data tree Wireshark uses to display packet.
1440 | *@param packet packet data.
1441 | *@param offset current payload offset.
1442 | *@return payload processed offset.
1443 | */
1444 | static unsigned
1445 | dissect_zbee_nwk_gp_cmd_commissioning_reply(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree,
1446 | zbee_nwk_green_power_packet *packet, unsigned offset)
1447 | {
1448 | uint8_t cr_options;
1449 | uint8_t cr_sec_level;
1450 |
1451 | void *enc_buffer;
1452 | uint8_t *enc_buffer_withA;
1453 | uint8_t *dec_buffer;
1454 | bool_Bool gp_decrypted;
1455 | GSList *GSList_i;
1456 | tvbuff_t *payload_tvb;
1457 |
1458 | static int * const options[] = {
1459 | &hf_zbee_nwk_gp_cmd_comm_rep_opt_panid_present,
1460 | &hf_zbee_nwk_gp_cmd_comm_rep_opt_sec_key_present,
1461 | &hf_zbee_nwk_gp_cmd_comm_rep_opt_key_encr,
1462 | &hf_zbee_nwk_gp_cmd_comm_rep_opt_sec_level,
1463 | &hf_zbee_nwk_gp_cmd_comm_rep_opt_sec_type,
1464 | NULL((void*)0)
1465 | };
1466 |
1467 | /* Get Options Field, build subtree and display the results. */
1468 | cr_options = tvb_get_uint8(tvb, offset);
1469 | proto_tree_add_bitmask(tree, tvb, offset, hf_zbee_nwk_gp_cmd_comm_rep_opt, ett_zbee_nwk_cmd_options, options, ENC_NA0x00000000);
1470 | offset += 1;
1471 |
1472 | /* Parse and display security Pan ID value. */
1473 | if (cr_options & ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_PAN_ID_PRESENT0x01) {
1474 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_rep_pan_id, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1475 | offset += 2;
1476 | }
1477 |
1478 | cr_sec_level = (cr_options & ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_SEC_LEVEL0x18) >>
1479 | ws_ctz(ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_SEC_LEVEL0x18);
1480 |
1481 | /* Parse and display security key. */
1482 | if (cr_options & ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_SEC_KEY_PRESENT0x02) {
1483 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_security_key, tvb, offset, ZBEE_SEC_CONST_KEYSIZE16, ENC_NA0x00000000);
1484 | offset += ZBEE_SEC_CONST_KEYSIZE16;
1485 |
1486 | /* Key is present clear, add to the key ring */
1487 | if (!(cr_options & ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_KEY_ENCR0x04)) {
1488 | key_record_t key_record;
1489 | void *key;
1490 |
1491 | key_record.frame_num = 0;
1492 | key_record.label = NULL((void*)0);
1493 | key = tvb_memdup(pinfo->pool, tvb, offset - ZBEE_SEC_CONST_KEYSIZE16, ZBEE_SEC_CONST_KEYSIZE16);
1494 | memcpy(key_record.key, key, ZBEE_SEC_CONST_KEYSIZE16);
1495 | zbee_gp_keyring = g_slist_prepend(zbee_gp_keyring, g_memdup2(&key_record, sizeof(key_record_t)));
1496 | }
1497 | }
1498 | /* Parse and display security MIC. */
1499 | if ((cr_options & ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_KEY_ENCR0x04) &&
1500 | (cr_options & ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_SEC_KEY_PRESENT0x02)) {
1501 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_gpd_sec_key_mic, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
1502 | offset += 4;
1503 | }
1504 |
1505 | /* Parse and display Frame Counter and decrypt key */
1506 | if ((cr_options & ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_KEY_ENCR0x04) &&
1507 | (cr_options & ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_SEC_KEY_PRESENT0x02) &&
1508 | ((cr_sec_level == ZBEE_NWK_GP_SECURITY_LEVEL_FULL0x02) ||
1509 | (cr_sec_level == ZBEE_NWK_GP_SECURITY_LEVEL_FULLENCR0x03))) {
1510 | if (offset + 4 <= tvb_captured_length(tvb)){
1511 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_comm_rep_frame_counter, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
1512 | offset += 4;
1513 |
1514 | if (packet != NULL((void*)0))
1515 | {
1516 | /* decrypt the security key*/
1517 | dec_buffer = (uint8_t *)wmem_alloc(pinfo->pool, ZBEE_SEC_CONST_KEYSIZE16);
1518 | enc_buffer_withA = (uint8_t *)wmem_alloc(pinfo->pool, 4 + ZBEE_SEC_CONST_KEYSIZE16 + 4); /* CCM* a (this is SrcID) + encKey + MIC */
1519 | enc_buffer = tvb_memdup(pinfo->pool, tvb, offset - ZBEE_SEC_CONST_KEYSIZE16 - 4 - 4, ZBEE_SEC_CONST_KEYSIZE16 + 4);
1520 | phtoleu32(enc_buffer_withA, packet->source_id); /* enc_buffer_withA = CCM* a (srcID) | enc_buffer */
1521 | memcpy(enc_buffer_withA+4, enc_buffer, ZBEE_SEC_CONST_KEYSIZE16 + 4);
1522 | gp_decrypted = false0;
1523 |
1524 | for (GSList_i = zbee_gp_keyring; GSList_i && !gp_decrypted; GSList_i = g_slist_next(GSList_i)((GSList_i) ? (((GSList *)(GSList_i))->next) : ((void*)0))) {
1525 | packet->security_frame_counter = tvb_get_uint32(tvb, offset - 4, ENC_LITTLE_ENDIAN0x80000000); /*for Nonce creation */
1526 | gp_decrypted = zbee_gp_decrypt_payload(packet, enc_buffer_withA, 4
1527 | , dec_buffer, ZBEE_SEC_CONST_KEYSIZE16, 4, ((key_record_t *)(GSList_i->data))->key);
1528 | }
1529 |
1530 | if (gp_decrypted) {
1531 | key_record_t key_record;
1532 |
1533 | key_record.frame_num = 0;
1534 | key_record.label = NULL((void*)0);
1535 | memcpy(key_record.key, dec_buffer, ZBEE_SEC_CONST_KEYSIZE16);
1536 | zbee_gp_keyring = g_slist_prepend(zbee_gp_keyring, g_memdup2(&key_record, sizeof(key_record_t)));
1537 |
1538 | payload_tvb = tvb_new_child_real_data(tvb, dec_buffer, ZBEE_SEC_CONST_KEYSIZE16, ZBEE_SEC_CONST_KEYSIZE16);
1539 | add_new_data_source(pinfo, payload_tvb, "Decrypted security key");
1540 | }
1541 | }
1542 | }
1543 | else{
1544 | /* This field is new in 2016 specification, older implementation may exist without it */
1545 | proto_tree_add_expert_remaining(tree, pinfo, &ei_zbee_nwk_gp_com_rep_no_out_cnt, tvb, 0);
1546 | }
1547 | }
1548 | return offset;
1549 | } /* dissect_zbee_nwk_gp_cmd_commissioning_reply */
1550 |
1551 | /**
1552 | * Dissector for ZigBee Green Power read attributes and request attributes commands.
1553 | *
1554 | *@param tvb pointer to buffer containing raw packet.
1555 | *@param pinfo pointer to packet information fields.
1556 | *@param tree pointer to data tree Wireshark uses to display packet.
1557 | *@param packet packet data.
1558 | *@param offset current payload offset.
1559 | *@return payload processed offset.
1560 | */
1561 | static unsigned
1562 | dissect_zbee_nwk_gp_cmd_read_attributes(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1563 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1564 | {
1565 | uint8_t cr_options = 0;
1566 | proto_tree *subtree = NULL((void*)0);
1567 | uint16_t cluster_id;
1568 | uint16_t mfr_code = ZBEE_MFG_CODE_NONE0x0000;
1569 | uint8_t record_list_len;
1570 | unsigned tvb_len;
1571 | uint8_t i;
1572 |
1573 | static int * const options[] = {
1574 | &hf_zbee_nwk_gp_cmd_read_att_opt_multi_rec,
1575 | &hf_zbee_nwk_gp_cmd_read_att_opt_man_field_present,
1576 | NULL((void*)0)
1577 | };
1578 |
1579 | /* Get Options Field, build subtree and display the results. */
1580 | cr_options = tvb_get_uint8(tvb, offset);
1581 | proto_tree_add_bitmask(tree, tvb, offset, hf_zbee_nwk_gp_cmd_read_att_opt, ett_zbee_nwk_cmd_options, options, ENC_NA0x00000000);
1582 |
1583 | offset += 1;
1584 | /* Parse and display manufacturer ID value. */
1585 | if (cr_options & ZBEE_NWK_GP_CMD_READ_ATTRIBUTE_OPT_MAN_FIELD_PRESENT0x02) {
1586 | proto_tree_add_item_ret_uint16(tree, hf_zbee_zcl_gp_cmd_ms_manufacturer_code, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &mfr_code);
1587 | offset += 2;
1588 | }
1589 |
1590 | tvb_len = tvb_captured_length(tvb);
1591 | while (offset < tvb_len)
1592 | {
1593 | /* Create subtree and parse attributes list. */
1594 | subtree = proto_tree_add_subtree_format(tree, tvb, offset, -1, ett_zbee_nwk_clu_rec, NULL((void*)0), "Cluster Record Request");
1595 |
1596 | /* Get cluster ID and add it into the subtree. */
1597 | proto_tree_add_item_ret_uint16(subtree, hf_zbee_nwk_gp_zcl_attr_cluster_id, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &cluster_id);
1598 | offset += 2;
1599 | /* Get length of record list (number of attributes * 2). */
1600 | proto_tree_add_item_ret_uint8(subtree, hf_zbee_nwk_gp_cmd_read_att_record_len, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000, &record_list_len);
1601 | offset += 1;
1602 |
1603 | for(i=0 ; i<record_list_len ; i+=2)
1604 | {
1605 | /* Dissect the attribute identifier */
1606 | dissect_zcl_attr_id(tvb, subtree, &offset, cluster_id, mfr_code, ZBEE_ZCL_FCF_TO_CLIENT0x01);
1607 | }
1608 | }
1609 | return offset;
1610 | } /* dissect_zbee_nwk_gp_cmd_read_attributes */
1611 | /**
1612 | * Dissector for ZigBee Green Power write attributes commands.
1613 | *
1614 | *@param tvb pointer to buffer containing raw packet.
1615 | *@param pinfo pointer to packet information fields.
1616 | *@param tree pointer to data tree Wireshark uses to display packet.
1617 | *@param packet packet data.
1618 | *@param offset current payload offset.
1619 | *@return payload processed offset.
1620 | */
1621 | static unsigned
1622 | dissect_zbee_nwk_gp_cmd_write_attributes(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree,
1623 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1624 | {
1625 | uint8_t cr_options = 0;
1626 | proto_tree *subtree = NULL((void*)0);
1627 | proto_tree *att_tree = NULL((void*)0);
1628 | uint16_t mfr_code = ZBEE_MFG_CODE_NONE0x0000;
1629 | uint16_t cluster_id;
1630 | uint8_t record_list_len;
1631 | unsigned tvb_len;
1632 | uint16_t attr_id;
1633 | unsigned end_byte;
1634 | //uint8_t i;
1635 |
1636 | static int * const options[] = {
1637 | &hf_zbee_nwk_gp_cmd_read_att_opt_multi_rec,
1638 | &hf_zbee_nwk_gp_cmd_read_att_opt_man_field_present,
1639 | NULL((void*)0)
1640 | };
1641 |
1642 | /* Get Options Field, build subtree and display the results. */
1643 | cr_options = tvb_get_uint8(tvb, offset);
1644 | proto_tree_add_bitmask(tree, tvb, offset, hf_zbee_nwk_gp_cmd_read_att_opt, ett_zbee_nwk_cmd_options, options, ENC_NA0x00000000);
1645 |
1646 | offset += 1;
1647 | /* Parse and display manufacturer ID value. */
1648 | if (cr_options & ZBEE_NWK_GP_CMD_READ_ATTRIBUTE_OPT_MAN_FIELD_PRESENT0x02) {
1649 | proto_tree_add_item_ret_uint16(tree, hf_zbee_zcl_gp_cmd_ms_manufacturer_code, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &mfr_code);
1650 | offset += 2;
1651 | }
1652 |
1653 | tvb_len = tvb_captured_length(tvb);
1654 | while (offset < tvb_len)
1655 | {
1656 | /* Create subtree and parse attributes list. */
1657 | subtree = proto_tree_add_subtree_format(tree, tvb, offset, -1, ett_zbee_nwk_clu_rec, NULL((void*)0), "Write Cluster Record");
1658 |
1659 | /* Get cluster ID and add it into the subtree. */
1660 | proto_tree_add_item_ret_uint16(subtree, hf_zbee_nwk_gp_zcl_attr_cluster_id, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &cluster_id);
1661 | offset += 2;
1662 | /* Get length of record list. */
1663 | record_list_len = tvb_get_uint8(tvb, offset);
1664 | proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_read_att_record_len, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1665 | offset += 1;
1666 |
1667 | end_byte = offset + record_list_len;
1668 | while ( offset < end_byte)
1669 | {
1670 | /* Create subtree for attribute status field */
1671 | att_tree = proto_tree_add_subtree_format(subtree, tvb, offset, 0, ett_zbee_nwk_att_rec, NULL((void*)0), "Write Attribute record");
1672 |
1673 | /* Dissect the attribute identifier */
1674 | attr_id = tvb_get_letohs(tvb, offset);
1675 | dissect_zcl_attr_id(tvb, att_tree, &offset, cluster_id, mfr_code, ZBEE_ZCL_FCF_TO_CLIENT0x01);
1676 |
1677 | /* Dissect the attribute data type and data */
1678 | dissect_zcl_attr_data_type_val(tvb, pinfo, att_tree, &offset, attr_id, cluster_id, mfr_code, ZBEE_ZCL_FCF_TO_CLIENT0x01);
1679 | }
1680 | }
1681 | return offset;
1682 | } /* dissect_zbee_nwk_gp_cmd_write_attributes */
1683 |
1684 |
1685 | /**
1686 | * Dissector for ZigBee Green Power read attribute response command.
1687 | *
1688 | *@param tvb pointer to buffer containing raw packet.
1689 | *@param pinfo pointer to packet information fields.
1690 | *@param tree pointer to data tree Wireshark uses to display packet.
1691 | *@param packet packet data.
1692 | *@param offset current payload offset.
1693 | *@return payload processed offset.
1694 | */
1695 | static unsigned
1696 | dissect_zbee_nwk_gp_cmd_read_attributes_response(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree,
1697 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1698 | {
1699 | uint8_t cr_options;
1700 | proto_tree *subtree = NULL((void*)0);
1701 | proto_tree *att_tree = NULL((void*)0);
1702 | uint16_t cluster_id;
1703 | uint16_t attr_id;
1704 | uint16_t mfr_code = ZBEE_MFG_CODE_NONE0x0000;
1705 | uint8_t record_list_len;
1706 | unsigned tvb_len;
1707 | unsigned end_byte;
1708 |
1709 | static int * const options[] = {
1710 | &hf_zbee_nwk_gp_cmd_read_att_opt_multi_rec,
1711 | &hf_zbee_nwk_gp_cmd_read_att_opt_man_field_present,
1712 | NULL((void*)0)
1713 | };
1714 |
1715 | /* Get Options Field, build subtree and display the results. */
1716 | cr_options = tvb_get_uint8(tvb, offset);
1717 | proto_tree_add_bitmask(tree, tvb, offset, hf_zbee_nwk_gp_cmd_read_att_opt, ett_zbee_nwk_cmd_options, options, ENC_NA0x00000000);
1718 | offset += 1;
1719 |
1720 | /* Parse and display manufacturer ID value. */
1721 | if (cr_options & ZBEE_NWK_GP_CMD_READ_ATTRIBUTE_OPT_MAN_FIELD_PRESENT0x02) {
1722 | proto_tree_add_item_ret_uint16(tree, hf_zbee_zcl_gp_cmd_ms_manufacturer_code, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &mfr_code);
1723 | offset += 2;
1724 | }
1725 |
1726 | tvb_len = tvb_captured_length(tvb);
1727 | while (offset < tvb_len)
1728 | {
1729 | /* Create subtree and parse attributes list. */
1730 | subtree = proto_tree_add_subtree_format(tree, tvb, offset,0, ett_zbee_nwk_clu_rec, NULL((void*)0), "Cluster record");
1731 |
1732 | /* Get cluster ID and add it into the subtree. */
1733 | proto_tree_add_item_ret_uint16(subtree, hf_zbee_nwk_gp_zcl_attr_cluster_id, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &cluster_id);
1734 | offset += 2;
1735 | /* Get length of record list in bytes. */
1736 | record_list_len = tvb_get_uint8(tvb, offset);
1737 | proto_tree_add_item(subtree, hf_zbee_nwk_gp_cmd_read_att_record_len, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1738 | offset += 1;
1739 |
1740 | end_byte = offset + record_list_len;
1741 | while ( offset < end_byte)
1742 | {
1743 | /* Create subtree for attribute status field */
1744 | /* TODO ett_ could be an array to permit not to unroll all always */
1745 | att_tree = proto_tree_add_subtree_format(subtree, tvb, offset, 0, ett_zbee_nwk_att_rec, NULL((void*)0), "Read Attribute record");
1746 |
1747 | /* Dissect the attribute identifier */
1748 | attr_id = tvb_get_letohs(tvb, offset);
1749 | dissect_zcl_attr_id(tvb, att_tree, &offset, cluster_id, mfr_code, ZBEE_ZCL_FCF_TO_CLIENT0x01);
1750 |
1751 | /* Dissect the status and optionally the data type and value */
1752 | if (dissect_zcl_attr_uint8(tvb, att_tree, &offset, &hf_zbee_nwk_gp_zcl_attr_status)
1753 | == ZBEE_ZCL_STAT_SUCCESS0x00)
1754 | {
1755 | /* Dissect the attribute data type and data */
1756 | dissect_zcl_attr_data_type_val(tvb, pinfo, att_tree, &offset, attr_id, cluster_id, mfr_code, ZBEE_ZCL_FCF_TO_CLIENT0x01);
1757 | }
1758 | else
1759 | {
1760 | /* Data type field is always present (not like in ZCL read attribute response command) */
1761 | dissect_zcl_attr_data(tvb, pinfo, att_tree, &offset,
1762 | dissect_zcl_attr_uint8(tvb, att_tree, &offset, &hf_zbee_nwk_gp_zcl_attr_data_type), ZBEE_ZCL_FCF_TO_CLIENT0x01 );
1763 | }
1764 | }
1765 | }
1766 | return offset;
1767 | } /* dissect_zbee_nwk_gp_cmd_read_attributes_response */
1768 |
1769 | /**
1770 | * Dissector for ZigBee Green Power ZCL tunneling command.
1771 | *
1772 | *@param tvb pointer to buffer containing raw packet.
1773 | *@param pinfo pointer to packet information fields.
1774 | *@param tree pointer to data tree Wireshark uses to display packet.
1775 | *@param packet packet data.
1776 | *@param offset current payload offset.
1777 | *@return payload processed offset.
1778 | */
1779 | static unsigned
1780 | dissect_zbee_nwk_gp_cmd_zcl_tunneling(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1781 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1782 | {
1783 | uint8_t tun_options;
1784 |
1785 | static int * const options[] = {
1786 | &hf_zbee_nwk_gp_cmd_zcl_tunnel_opt_frame_type,
1787 | &hf_zbee_nwk_gp_cmd_zcl_tunnel_opt_man_field_present,
1788 | &hf_zbee_nwk_gp_cmd_zcl_tunnel_opt_direction,
1789 | NULL((void*)0)
1790 | };
1791 |
1792 | /* Get Options Field, build subtree and display the results. */
1793 | tun_options = tvb_get_uint8(tvb, offset);
1794 | proto_tree_add_bitmask(tree, tvb, offset, hf_zbee_nwk_gp_cmd_zcl_tunnel_opt, ett_zbee_nwk_cmd_options, options, ENC_NA0x00000000);
1795 | offset += 1;
1796 |
1797 | /* Parse and display manufacturer ID value. */
1798 | if (tun_options & ZBEE_NWK_GP_CMD_ZCL_TUNNEL_OPT_MAN_FIELD_PRESENT0x04) {
1799 | proto_tree_add_item(tree, hf_zbee_zcl_gp_cmd_ms_manufacturer_code, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1800 | offset += 2;
1801 | }
1802 |
1803 | proto_tree_add_item(tree, hf_zbee_nwk_gp_zcl_attr_cluster_id, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1804 | offset += 2;
1805 |
1806 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_zcl_tunnel_command_id, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1807 | offset += 1;
1808 |
1809 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_zcl_tunnel_payload_len, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1810 | offset += 1;
1811 |
1812 | /* We're not parsing the ZCL payload, as it's non-trivial and will require a lot of refactoring of the
1813 | * ZCL data parsers to make work. For now, let it just show up as raw data. */
1814 |
1815 | return offset;
1816 | } /* dissect_zbee_nwk_gp_cmd_zcl_tunneling */
1817 |
1818 | /**
1819 | * Dissector for ZigBee Green Power Compact Attribute Reporting command.
1820 | *
1821 | *@param tvb pointer to buffer containing raw packet.
1822 | *@param pinfo pointer to packet information fields.
1823 | *@param tree pointer to data tree Wireshark uses to display packet.
1824 | *@param packet packet data.
1825 | *@param offset current payload offset.
1826 | *@return payload processed offset.
1827 | */
1828 | static unsigned
1829 | dissect_zbee_nwk_gp_cmd_compact_attr_report(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1830 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1831 | {
1832 | int len_remaining;
1833 |
1834 | /* Report Identifier */
1835 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_compact_attr_report_report_id, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1836 | offset++;
1837 |
1838 | /* Data points */
1839 | len_remaining = tvb_reported_length_remaining(tvb, offset);
1840 | if (len_remaining > 0) {
1841 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_compact_attr_report_data_points,
1842 | tvb, offset, len_remaining, ENC_NA0x00000000);
1843 | offset += len_remaining;
1844 | }
1845 |
1846 | return offset;
1847 | } /* dissect_zbee_nwk_gp_cmd_compact_attr_report */
1848 |
1849 | /**
1850 | *Dissector for ZigBee Green Power multi-cluster reporting command.
1851 | *
1852 | *@param tvb pointer to buffer containing raw packet.
1853 | *@param pinfo pointer to packet information fields.
1854 | *@param tree pointer to data tree Wireshark uses to display packet.
1855 | *@param packet packet data.
1856 | *@param offset current payload offset.
1857 | *@param mfr_code manufacturer code.
1858 | *@return payload processed offset.
1859 | */
1860 | static unsigned
1861 | dissect_zbee_nwk_gp_cmd_multi_cluster_reporting(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1862 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset, uint16_t mfr_code)
1863 | {
1864 | proto_tree *subtree = NULL((void*)0);
1865 | uint16_t cluster_id;
1866 | uint16_t attr_id;
1867 | unsigned tvb_len;
1868 |
1869 | tvb_len = tvb_captured_length(tvb);
1870 | while (offset < tvb_len)
1871 | {
1872 | /* Create subtree and parse attributes list. */
1873 | subtree = proto_tree_add_subtree_format(tree, tvb, offset, 0, ett_zbee_nwk_clu_rec, NULL((void*)0), "Cluster record"); //TODO for cluster %% blabla
1874 |
1875 | /* Get cluster ID and add it into the subtree. */
1876 | proto_tree_add_item_ret_uint16(subtree, hf_zbee_nwk_gp_zcl_attr_cluster_id, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &cluster_id);
1877 | offset += 2;
1878 |
1879 | /* Dissect the attribute identifier */
1880 | attr_id = tvb_get_letohs(tvb, offset);
1881 | dissect_zcl_attr_id(tvb, subtree, &offset, cluster_id, mfr_code, ZBEE_ZCL_FCF_TO_CLIENT0x01);
1882 |
1883 | /* Dissect the attribute data type and data */
1884 | dissect_zcl_attr_data_type_val(tvb, pinfo, subtree, &offset, attr_id, cluster_id, mfr_code, ZBEE_ZCL_FCF_TO_CLIENT0x01);
1885 | // TODO how to dissect when data type is different from expected one for this attribute ? this shouldn't happen
1886 | }
1887 | return offset;
1888 | } /* dissect_zbee_nwk_gp_cmd_multi_cluster_reporting */
1889 |
1890 |
1891 | /**
1892 | *Dissector for ZigBee Green Power commands manufacturer specific attrib reporting.
1893 | *
1894 | *@param tvb pointer to buffer containing raw packet.
1895 | *@param pinfo pointer to packet information fields.
1896 | *@param tree pointer to data tree Wireshark uses to display packet.
1897 | *@param packet packet data.
1898 | *@param offset current payload offset.
1899 | *@return payload processed offset.
1900 | */
1901 | static unsigned
1902 | dissect_zbee_nwk_gp_cmd_MS_multi_cluster_reporting(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1903 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1904 | {
1905 | uint16_t mfr_code;
1906 |
1907 | /*dissect manufacturer ID*/
1908 | proto_tree_add_item_ret_uint16(tree, hf_zbee_zcl_gp_cmd_ms_manufacturer_code, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000, &mfr_code);
1909 | offset += 2;
1910 |
1911 | offset = dissect_zbee_nwk_gp_cmd_multi_cluster_reporting(tvb, pinfo, tree, packet, offset, mfr_code);
1912 |
1913 | return offset;
1914 | }/*dissect_zbee_nwk_gp_cmd_MS_multi_cluster_reporting*/
1915 |
1916 | /**
1917 | *Dissector for ZigBee Green Power Move Color.
1918 | *
1919 | *@param tvb pointer to buffer containing raw packet.
1920 | *@param pinfo pointer to packet information fields.
1921 | *@param tree pointer to data tree Wireshark uses to display packet.
1922 | *@param packet packet data.
1923 | *@param offset current payload offset.
1924 | *@return payload processed offset.
1925 | */
1926 | static unsigned
1927 | dissect_zbee_nwk_gp_cmd_move_color(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1928 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1929 | {
1930 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_move_color_ratex, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1931 | offset += 2;
1932 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_move_color_ratey, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1933 | offset += 2;
1934 | return offset;
1935 | } /* dissect_zbee_nwk_gp_cmd_move_color */
1936 |
1937 | /**
1938 | *Dissector for ZigBee Green Power Move Up/Down.
1939 | *
1940 | *@param tvb pointer to buffer containing raw packet.
1941 | *@param pinfo pointer to packet information fields.
1942 | *@param tree pointer to data tree Wireshark uses to display packet.
1943 | *@param packet packet data.
1944 | *@param offset current payload offset.
1945 | *@return payload processed offset.
1946 | */
1947 | static unsigned
1948 | dissect_zbee_nwk_gp_cmd_move_up_down(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1949 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1950 | {
1951 | /* Optional rate field. */
1952 | if (tvb_reported_length(tvb) - offset >= 1) {
1953 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_move_up_down_rate, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
1954 | offset += 1;
1955 | }
1956 | return offset;
1957 | } /* dissect_zbee_nwk_gp_cmd_move_up_down */
1958 |
1959 | /**
1960 | *Dissector for ZigBee Green Power Step Color.
1961 | *
1962 | *@param tvb pointer to buffer containing raw packet.
1963 | *@param pinfo pointer to packet information fields.
1964 | *@param tree pointer to data tree Wireshark uses to display packet.
1965 | *@param packet packet data.
1966 | *@param offset current payload offset.
1967 | *@return payload processed offset.
1968 | */
1969 | static unsigned
1970 | dissect_zbee_nwk_gp_cmd_step_color(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1971 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1972 | {
1973 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_step_color_stepx, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1974 | offset += 2;
1975 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_step_color_stepy, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1976 | offset += 2;
1977 | /* Optional time field. */
1978 | if (tvb_reported_length(tvb) - offset >= 2) {
1979 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_step_color_transition_time, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
1980 | offset += 2;
1981 | }
1982 | return offset;
1983 | } /* dissect_zbee_nwk_gp_cmd_step_color */
1984 |
1985 | /**
1986 | *Dissector for ZigBee Green Power Step Up/Down.
1987 | *
1988 | *@param tvb pointer to buffer containing raw packet.
1989 | *@param pinfo pointer to packet information fields.
1990 | *@param tree pointer to data tree Wireshark uses to display packet.
1991 | *@param packet packet data.
1992 | *@param offset current payload offset.
1993 | *@return payload processed offset.
1994 | */
1995 | static unsigned
1996 | dissect_zbee_nwk_gp_cmd_step_up_down(tvbuff_t *tvb, packet_info *pinfo _U___attribute__((unused)), proto_tree *tree,
1997 | zbee_nwk_green_power_packet *packet _U___attribute__((unused)), unsigned offset)
1998 | {
1999 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_step_up_down_step_size, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
2000 | offset += 1;
2001 | /* Optional time field. */
2002 | if (tvb_reported_length(tvb) - offset >= 2) {
2003 | proto_tree_add_item(tree, hf_zbee_nwk_gp_cmd_step_up_down_transition_time, tvb, offset, 2, ENC_LITTLE_ENDIAN0x80000000);
2004 | offset += 2;
2005 | }
2006 | return offset;
2007 | } /* dissect_zbee_nwk_gp_cmd_step_up_down */
2008 |
2009 | /**
2010 | *Dissector for ZigBee Green Power commands.
2011 | *
2012 | *@param tvb pointer to buffer containing raw packet.
2013 | *@param pinfo pointer to packet information fields.
2014 | *@param tree pointer to data tree Wireshark uses to display packet.
2015 | *@param data raw packet private data.
2016 | *@return payload processed offset
2017 | */
2018 | static int
2019 | dissect_zbee_nwk_gp_cmd(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, void *data)
2020 | {
2021 | unsigned offset = 0;
2022 | uint8_t cmd_id = tvb_get_uint8(tvb, offset);
2023 | proto_item *cmd_root;
2024 | proto_tree *cmd_tree;
2025 | zbee_nwk_green_power_packet *packet = (zbee_nwk_green_power_packet *)data;
2026 |
2027 | /* Create a subtree for the command. */
2028 | cmd_tree = proto_tree_add_subtree_format(tree, tvb, offset, -1, ett_zbee_nwk_cmd, &cmd_root,
2029 | "Command Frame: %s", val_to_str_ext_const(cmd_id,
2030 | &zbee_nwk_gp_cmd_names_ext,
2031 | "Unknown Command Frame"));
2032 | /* Add the command ID. */
2033 | proto_tree_add_uint(cmd_tree, hf_zbee_nwk_gp_command_id, tvb, offset, 1, cmd_id);
2034 |
2035 | offset += 1;
2036 | /* Add the command name to the info column. */
2037 | col_set_str(pinfo->cinfo, COL_INFO, val_to_str_ext_const(cmd_id, &zbee_nwk_gp_cmd_names_ext, "Unknown command"));
2038 | /* Handle the command for one of the following devices:
2039 | * - Door Lock Controller (IDs: 0x50 - 0x51);
2040 | * - GP Flow Sensor (IDs: 0xE0, 0xA0 - 0xA3);
2041 | * - GP Temperature Sensor (IDs: 0xE0, 0xA0 - 0xA3); */
2042 | switch(cmd_id) {
2043 | /* Payloadless GPDF commands sent by GPD. */
2044 | case ZB_GP_CMD_ID_IDENTIFY:
2045 | case ZB_GP_CMD_ID_RECALL_SCENE0:
2046 | case ZB_GP_CMD_ID_RECALL_SCENE1:
2047 | case ZB_GP_CMD_ID_RECALL_SCENE2:
2048 | case ZB_GP_CMD_ID_RECALL_SCENE3:
2049 | case ZB_GP_CMD_ID_RECALL_SCENE4:
2050 | case ZB_GP_CMD_ID_RECALL_SCENE5:
2051 | case ZB_GP_CMD_ID_RECALL_SCENE6:
2052 | case ZB_GP_CMD_ID_RECALL_SCENE7:
2053 | case ZB_GP_CMD_ID_STORE_SCENE0:
2054 | case ZB_GP_CMD_ID_STORE_SCENE1:
2055 | case ZB_GP_CMD_ID_STORE_SCENE2:
2056 | case ZB_GP_CMD_ID_STORE_SCENE3:
2057 | case ZB_GP_CMD_ID_STORE_SCENE4:
2058 | case ZB_GP_CMD_ID_STORE_SCENE5:
2059 | case ZB_GP_CMD_ID_STORE_SCENE6:
2060 | case ZB_GP_CMD_ID_STORE_SCENE7:
2061 | case ZB_GP_CMD_ID_OFF:
2062 | case ZB_GP_CMD_ID_ON:
2063 | case ZB_GP_CMD_ID_TOGGLE:
2064 | case ZB_GP_CMD_ID_RELEASE:
2065 | case ZB_GP_CMD_ID_LEVEL_CONTROL_STOP:
2066 | case ZB_GP_CMD_ID_MOVE_HUE_STOP:
2067 | case ZB_GP_CMD_ID_MOVE_SATURATION_STOP:
2068 | case ZB_GP_CMD_ID_LOCK_DOOR:
2069 | case ZB_GP_CMD_ID_UNLOCK_DOOR:
2070 | case ZB_GP_CMD_ID_PRESS11:
2071 | case ZB_GP_CMD_ID_RELEASE11:
2072 | case ZB_GP_CMD_ID_PRESS12:
2073 | case ZB_GP_CMD_ID_RELEASE12:
2074 | case ZB_GP_CMD_ID_PRESS22:
2075 | case ZB_GP_CMD_ID_RELEASE22:
2076 | case ZB_GP_CMD_ID_SHORT_PRESS11:
2077 | case ZB_GP_CMD_ID_SHORT_PRESS12:
2078 | case ZB_GP_CMD_ID_SHORT_PRESS22:
2079 | case ZB_GP_CMD_ID_DECOMMISSIONING:
2080 | case ZB_GP_CMD_ID_SUCCESS:
2081 | break;
2082 | /* GPDF commands with payload sent by GPD. */
2083 | case ZB_GP_CMD_ID_MOVE_UP:
2084 | case ZB_GP_CMD_ID_MOVE_DOWN:
2085 | case ZB_GP_CMD_ID_MOVE_UP_WITH_ON_OFF:
2086 | case ZB_GP_CMD_ID_MOVE_DOWN_WITH_ON_OFF:
2087 | case ZB_GP_CMD_ID_MOVE_HUE_UP:
2088 | case ZB_GP_CMD_ID_MOVE_HUE_DOWN:
2089 | case ZB_GP_CMD_ID_MOVE_SATURATION_UP:
2090 | case ZB_GP_CMD_ID_MOVE_SATURATION_DOWN:
2091 | offset = dissect_zbee_nwk_gp_cmd_move_up_down(tvb, pinfo, cmd_tree, packet, offset);
2092 | break;
2093 | case ZB_GP_CMD_ID_STEP_UP:
2094 | case ZB_GP_CMD_ID_STEP_DOWN:
2095 | case ZB_GP_CMD_ID_STEP_UP_WITH_ON_OFF:
2096 | case ZB_GP_CMD_ID_STEP_DOWN_WITH_ON_OFF:
2097 | case ZB_GP_CMD_ID_STEP_HUE_UP:
2098 | case ZB_GP_CMD_ID_STEP_HUW_DOWN:
2099 | case ZB_GP_CMD_ID_STEP_SATURATION_UP:
2100 | case ZB_GP_CMD_ID_STEP_SATURATION_DOWN:
2101 | offset = dissect_zbee_nwk_gp_cmd_step_up_down(tvb, pinfo, cmd_tree, packet, offset);
2102 | break;
2103 | case ZB_GP_CMD_ID_MOVE_COLOR:
2104 | offset = dissect_zbee_nwk_gp_cmd_move_color(tvb, pinfo, cmd_tree, packet, offset);
2105 | break;
2106 | case ZB_GP_CMD_ID_STEP_COLOR:
2107 | offset = dissect_zbee_nwk_gp_cmd_step_color(tvb, pinfo, cmd_tree, packet, offset);
2108 | break;
2109 | case ZB_GP_CMD_ID_ATTRIBUTE_REPORTING:
2110 | offset = dissect_zbee_nwk_gp_cmd_attr_reporting(tvb, pinfo, cmd_tree, packet, offset, ZBEE_MFG_CODE_NONE0x0000);
2111 | break;
2112 | case ZB_GP_CMD_ID_MANUFACTURE_SPECIFIC_ATTR_REPORTING:
2113 | offset = dissect_zbee_nwk_gp_cmd_MS_attr_reporting(tvb, pinfo, cmd_tree, packet, offset);
2114 | break;
2115 | case ZB_GP_CMD_ID_MULTI_CLUSTER_REPORTING:
2116 | offset = dissect_zbee_nwk_gp_cmd_multi_cluster_reporting(tvb, pinfo, cmd_tree, packet, offset, ZBEE_MFG_CODE_NONE0x0000);
2117 | break;
2118 | case ZB_GP_CMD_ID_MANUFACTURER_SPECIFIC_MCLUSTER_REPORTING:
2119 | offset = dissect_zbee_nwk_gp_cmd_MS_multi_cluster_reporting(tvb, pinfo, cmd_tree, packet, offset);
2120 | break;
2121 | case ZB_GP_CMD_ID_READ_ATTRIBUTES_RESPONSE:
2122 | offset = dissect_zbee_nwk_gp_cmd_read_attributes_response(tvb, pinfo, cmd_tree, packet, offset);
2123 | break;
2124 | case ZB_GP_CMD_ID_ZCL_TUNNELING:
2125 | offset = dissect_zbee_nwk_gp_cmd_zcl_tunneling(tvb, pinfo, cmd_tree, packet, offset);
2126 | break;
2127 | case ZB_GP_CMD_ID_COMPACT_ATTR_REPORT:
2128 | offset = dissect_zbee_nwk_gp_cmd_compact_attr_report(tvb, pinfo, cmd_tree, packet, offset);
2129 | break;
2130 | case ZB_GP_CMD_ID_ANY_SENSOR_COMMAND_A0_A3:
2131 | /* TODO: implement it. */
2132 | break;
2133 | case ZB_GP_CMD_ID_COMMISSIONING:
2134 | offset = dissect_zbee_nwk_gp_cmd_commissioning(tvb, pinfo, cmd_tree, packet, offset);
2135 | break;
2136 | case ZB_GP_CMD_ID_CHANNEL_REQUEST:
2137 | offset = dissect_zbee_nwk_gp_cmd_channel_request(tvb, pinfo, cmd_tree, packet, offset);
2138 | break;
2139 | case ZB_GP_CMD_ID_APPLICATION_DESC:
2140 | offset = dissect_zbee_nwk_gp_cmd_application_desc(tvb, pinfo, cmd_tree, packet, offset);
2141 | break;
2142 | case ZB_GP_CMD_ID_REQUEST_ATTRIBUTES:
2143 | /* GPDF commands sent to GPD. */
2144 | case ZB_GP_CMD_ID_READ_ATTRIBUTES:
2145 | offset = dissect_zbee_nwk_gp_cmd_read_attributes(tvb, pinfo, cmd_tree, packet, offset);
2146 | break;
2147 | case ZB_GP_CMD_ID_COMMISSIONING_REPLY:
2148 | offset = dissect_zbee_nwk_gp_cmd_commissioning_reply(tvb, pinfo, cmd_tree, packet, offset);
2149 | break;
2150 | case ZB_GP_CMD_ID_WRITE_ATTRIBUTES:
2151 | offset = dissect_zbee_nwk_gp_cmd_write_attributes(tvb, pinfo, cmd_tree, packet, offset);
2152 | break;
2153 | case ZB_GP_CMD_ID_CHANNEL_CONFIGURATION:
2154 | offset = dissect_zbee_nwk_gp_cmd_channel_configuration(tvb, pinfo, cmd_tree, packet, offset);
2155 | break;
2156 | }
2157 | if (offset < tvb_reported_length(tvb)) {
2158 | /* There are leftover bytes! */
2159 | proto_tree *root;
2160 | tvbuff_t *leftover_tvb = tvb_new_subset_remaining(tvb, offset);
2161 |
2162 | /* Correct the length of the command tree. */
2163 | root = proto_tree_get_root(tree);
2164 | proto_item_set_len(cmd_root, offset);
2165 |
2166 | /* Dump the tail. */
2167 | call_data_dissector(leftover_tvb, pinfo, root);
2168 | }
2169 | return offset;
2170 | } /* dissect_zbee_nwk_gp_cmd */
2171 |
2172 | /**
2173 | *ZigBee NWK packet dissection routine for Green Power profile.
2174 | *
2175 | *@param tvb pointer to buffer containing raw packet.
2176 | *@param pinfo pointer to packet information fields.
2177 | *@param tree pointer to data tree Wireshark uses to display packet.
2178 | *@param data raw packet private data.
2179 | */
2180 | static int
2181 | dissect_zbee_nwk_gp(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, void *data)
2182 | {
2183 | ieee802154_packet *ieee_packet = (ieee802154_packet *)data;
2184 | bool_Bool gp_decrypted;
2185 | GSList *GSList_i;
2186 | unsigned offset = 0;
2187 | uint8_t *dec_buffer;
2188 | uint8_t *enc_buffer;
2189 | uint8_t fcf;
2190 | proto_tree *nwk_tree;
2191 | proto_item *proto_root;
2192 | proto_item *ti = NULL((void*)0);
2193 | tvbuff_t *payload_tvb;
2194 | zbee_nwk_green_power_packet packet;
2195 | static int * const fields[] = {
2196 | &hf_zbee_nwk_gp_frame_type,
2197 | &hf_zbee_nwk_gp_proto_version,
2198 | &hf_zbee_nwk_gp_auto_commissioning,
2199 | &hf_zbee_nwk_gp_fc_ext,
2200 | NULL((void*)0)
2201 | };
2202 | static int * const ext_fields[] = {
2203 | &hf_zbee_nwk_gp_fc_ext_app_id,
2204 | &hf_zbee_nwk_gp_fc_ext_sec_level,
2205 | &hf_zbee_nwk_gp_fc_ext_sec_key,
2206 | &hf_zbee_nwk_gp_fc_ext_rx_after_tx,
2207 | &hf_zbee_nwk_gp_fc_ext_direction,
2208 | NULL((void*)0)
2209 | };
2210 |
2211 | if (data == NULL((void*)0))
2212 | return 0;
2213 |
2214 | memset(&packet, 0, sizeof(packet));
2215 | packet.ieee_packet_src64 = ieee_packet->src64;
2216 | /* Add ourself to the protocol column, clear the info column and create the protocol tree. */
2217 | col_set_str(pinfo->cinfo, COL_PROTOCOL, "ZigBee Green Power");
2218 | col_clear(pinfo->cinfo, COL_INFO);
2219 |
2220 | proto_root = proto_tree_add_protocol_format(tree, proto_zbee_nwk_gp, tvb, offset, tvb_captured_length(tvb),
2221 | "ZGP stub NWK header");
2222 | nwk_tree = proto_item_add_subtree(proto_root, ett_zbee_nwk);
2223 |
2224 | enc_buffer = (uint8_t *)tvb_memdup(pinfo->pool, tvb, 0, tvb_captured_length(tvb));
2225 | /* Get and parse the FCF. */
2226 | fcf = tvb_get_uint8(tvb, offset);
2227 | packet.frame_type = zbee_get_bit_field(fcf, ZBEE_NWK_GP_FCF_FRAME_TYPE0x03);
2228 | packet.nwk_frame_control_extension = zbee_get_bit_field(fcf, ZBEE_NWK_GP_FCF_CONTROL_EXTENSION0x80);
2229 |
2230 | /* Display the FCF. */
2231 | ti = proto_tree_add_bitmask(nwk_tree, tvb, offset, hf_zbee_nwk_gp_fcf, ett_zbee_nwk_fcf, fields, ENC_NA0x00000000);
2232 | proto_item_append_text(ti, " %s", val_to_str_const(packet.frame_type, zbee_nwk_gp_frame_types, "Unknown Frame Type"));
2233 | offset += 1;
2234 |
2235 | /* Add the frame type to the info column and protocol root. */
2236 | proto_item_append_text(proto_root, " %s", val_to_str_const(packet.frame_type, zbee_nwk_gp_frame_types, "Unknown type"));
2237 | col_set_str(pinfo->cinfo, COL_INFO, val_to_str_const(packet.frame_type, zbee_nwk_gp_frame_types, "Reserved frame type"));
2238 |
2239 | if (packet.nwk_frame_control_extension) {
2240 | /* Display ext FCF. */
2241 | fcf = tvb_get_uint8(tvb, offset);
2242 | packet.application_id = zbee_get_bit_field(fcf, ZBEE_NWK_GP_FCF_EXT_APP_ID0x07);
2243 | packet.security_level = zbee_get_bit_field(fcf, ZBEE_NWK_GP_FCF_EXT_SECURITY_LEVEL0x18);
2244 | packet.direction = zbee_get_bit_field(fcf, ZBEE_NWK_GP_FCF_EXT_DIRECTION0x80);
2245 |
2246 | /* Create a subtree for the extended FCF. */
2247 | proto_tree_add_bitmask(nwk_tree, tvb, offset, hf_zbee_nwk_gp_fc_ext_field, ett_zbee_nwk_fcf_ext, ext_fields, ENC_NA0x00000000);
2248 | offset += 1;
2249 | }
2250 | if ((packet.frame_type == ZBEE_NWK_GP_FCF_DATA0x00 && !packet.nwk_frame_control_extension) || (packet.frame_type ==
2251 | ZBEE_NWK_GP_FCF_DATA0x00 && packet.nwk_frame_control_extension && packet.application_id ==
2252 | ZBEE_NWK_GP_APP_ID_DEFAULT0x00) || (packet.frame_type == ZBEE_NWK_GP_FCF_MAINTENANCE0x01 &&
2253 | packet.nwk_frame_control_extension && packet.application_id == ZBEE_NWK_GP_APP_ID_DEFAULT0x00 && tvb_get_uint8(tvb,
2254 | offset) != ZB_GP_CMD_ID_CHANNEL_CONFIGURATION)) {
2255 | /* Display GPD Src ID. */
2256 | packet.source_id = tvb_get_letohl(tvb, offset);
2257 | proto_tree_add_item(nwk_tree, hf_zbee_nwk_gp_zgpd_src_id, tvb, offset, 4, ENC_LITTLE_ENDIAN0x80000000);
2258 | proto_item_append_text(proto_root, ", GPD Src ID: 0x%08x", packet.source_id);
2259 |
2260 | col_append_fstr(pinfo->cinfo, COL_INFO, ", GPD Src ID: 0x%08x", packet.source_id);
2261 |
2262 | col_clear(pinfo->cinfo, COL_DEF_SRC);
2263 | col_append_fstr(pinfo->cinfo, COL_DEF_SRC, "0x%08x", packet.source_id);
2264 |
2265 | offset += 4;
2266 | }
2267 | if (packet.application_id == ZBEE_NWK_GP_APP_ID_ZGP0x02) {
2268 | /* Display GPD endpoint */
2269 | packet.endpoint = tvb_get_uint8(tvb, offset);
2270 | proto_tree_add_item(nwk_tree, hf_zbee_nwk_gp_zgpd_endpoint, tvb, offset, 1, ENC_LITTLE_ENDIAN0x80000000);
2271 | proto_item_append_text(proto_root, ", Endpoint: %d", packet.endpoint);
2272 |
2273 | col_append_fstr(pinfo->cinfo, COL_INFO, ", Endpoint: %d", packet.endpoint);
2274 | offset += 1;
2275 | }
2276 | /* Display Security Frame Counter. */
2277 | packet.mic_size = 0;
2278 | if (packet.nwk_frame_control_extension) {
2279 | if (packet.application_id == ZBEE_NWK_GP_APP_ID_DEFAULT0x00 || packet.application_id == ZBEE_NWK_GP_APP_ID_ZGP0x02
2280 | || packet.application_id == ZBEE_NWK_GP_APP_ID_LPED0x01) {
2281 | if (packet.security_level == ZBEE_NWK_GP_SECURITY_LEVEL_1LSB0x01
2282 | && packet.application_id != ZBEE_NWK_GP_APP_ID_LPED0x01) {
2283 | packet.mic_size = 2;
2284 | } else if (packet.security_level == ZBEE_NWK_GP_SECURITY_LEVEL_FULL0x02 || packet.security_level ==
2285 | ZBEE_NWK_GP_SECURITY_LEVEL_FULLENCR0x03) {
2286 | /* Get Security Frame Counter and display it. */
2287 | packet.mic_size = 4;
2288 | packet.security_frame_counter = tvb_get_letohl(tvb, offset);
2289 | proto_tree_add_item(nwk_tree, hf_zbee_nwk_gp_security_frame_counter, tvb, offset, 4,
2290 | ENC_LITTLE_ENDIAN0x80000000);
2291 | offset += 4;
2292 | }
2293 | }
2294 | }
2295 | /* Parse application payload. */
2296 | /* This is a uint8_t, but tvb_reported_length might be larger; e.g.,
2297 | * SCOP over TCP, presumably with errors. It's bogus either way; perhaps
2298 | * we should warn.
2299 | */
2300 | packet.payload_len = tvb_reported_length(tvb) - offset - packet.mic_size;
2301 | /* Ensure that the payload exists. */
2302 | if (packet.payload_len <= 0) {
2303 | proto_tree_add_expert_remaining(nwk_tree, pinfo, &ei_zbee_nwk_gp_no_payload, tvb, 0);
2304 | return offset;
2305 | }
2306 | /* OK, payload exists. Parse MIC field if needed. */
2307 | if (packet.mic_size == 2) {
2308 | packet.mic = tvb_get_letohs(tvb, offset + packet.payload_len);
2309 | } else if (packet.mic_size == 4) {
2310 | packet.mic = tvb_get_letohl(tvb, offset + packet.payload_len);
2311 | }
2312 | /* Save packet private data. */
2313 | data = (void *)&packet;
2314 | payload_tvb = tvb_new_subset_length(tvb, offset, packet.payload_len);
2315 | if (packet.security_level != ZBEE_NWK_GP_SECURITY_LEVEL_FULLENCR0x03) {
2316 | dissect_zbee_nwk_gp_cmd(payload_tvb, pinfo, nwk_tree, data);
2317 | }
2318 | offset += packet.payload_len;
2319 | /* Display MIC field. */
2320 | if (packet.mic_size) {
2321 | proto_tree_add_uint(nwk_tree, packet.mic_size == 4 ? hf_zbee_nwk_gp_security_mic_4b :
2322 | hf_zbee_nwk_gp_security_mic_2b, tvb, offset, packet.mic_size, packet.mic);
2323 | offset += packet.mic_size;
2324 | }
2325 | if ((offset < tvb_captured_length(tvb)) && (packet.security_level != ZBEE_NWK_GP_SECURITY_LEVEL_FULLENCR0x03)) {
2326 | proto_tree_add_expert_remaining(nwk_tree, pinfo, &ei_zbee_nwk_gp_inval_residual_data, tvb, offset);
2327 | return offset;
2328 | }
2329 | if (packet.security_level == ZBEE_NWK_GP_SECURITY_LEVEL_FULLENCR0x03) {
2330 | gp_decrypted = false0;
2331 |
2332 | if (tvb_captured_length(tvb) >= tvb_reported_length(tvb)) {
2333 | dec_buffer = (uint8_t *)wmem_alloc(pinfo->pool, packet.payload_len);
2334 | for (GSList_i = zbee_gp_keyring; GSList_i && !gp_decrypted; GSList_i = g_slist_next(GSList_i)((GSList_i) ? (((GSList *)(GSList_i))->next) : ((void*)0))) {
2335 | gp_decrypted = zbee_gp_decrypt_payload(&packet, enc_buffer, offset - packet.payload_len -
2336 | packet.mic_size, dec_buffer, packet.payload_len, packet.mic_size,
2337 | ((key_record_t *)(GSList_i->data))->key);
2338 | }
2339 | }
2340 |
2341 | if (gp_decrypted) {
2342 | payload_tvb = tvb_new_child_real_data(tvb, dec_buffer, packet.payload_len, packet.payload_len);
2343 | add_new_data_source(pinfo, payload_tvb, "Decrypted GP Payload");
2344 | dissect_zbee_nwk_gp_cmd(payload_tvb, pinfo, nwk_tree, data);
2345 | } else {
2346 | payload_tvb = tvb_new_subset_length(tvb, offset - packet.payload_len - packet.mic_size, packet.payload_len);
2347 | call_data_dissector(payload_tvb, pinfo, tree);
2348 | }
2349 | }
2350 | return tvb_captured_length(tvb);
2351 | } /* dissect_zbee_nwk_gp */
2352 |
2353 | /**
2354 | *Heuristic interpreter for the ZigBee Green Power dissectors.
2355 | *
2356 | *@param tvb pointer to buffer containing raw packet.
2357 | *@param pinfo pointer to packet information fields.
2358 | *@param tree pointer to data tree Wireshark uses to display packet.
2359 | *@param data raw packet private data.
2360 | */
2361 | static bool_Bool
2362 | dissect_zbee_nwk_heur_gp(tvbuff_t *tvb, packet_info *pinfo, proto_tree *tree, void *data)
2363 | {
2364 | ieee802154_packet *packet = (ieee802154_packet *)data;
2365 | uint8_t fcf;
2366 |
2367 | /* We must have the IEEE 802.15.4 headers. */
2368 | if (packet == NULL((void*)0)) return false0;
2369 |
2370 | /* If the frame type and version are not sane, then it's probably not ZGP. */
2371 | fcf = tvb_get_uint8(tvb, 0);
2372 | if (zbee_get_bit_field(fcf, ZBEE_NWK_GP_FCF_VERSION0x3C) != ZBEE_VERSION_GREEN_POWER3) return false0;
2373 | if (!try_val_to_str(zbee_get_bit_field(fcf, ZBEE_NWK_FCF_FRAME_TYPE0x0003), zbee_nwk_gp_frame_types)) return false0;
2374 |
2375 | /* ZigBee greenpower frames are either sent to broadcast or the extended address. */
2376 | if (packet->dst_addr_mode == IEEE802154_FCF_ADDR_SHORT0x2 && packet->dst16 == IEEE802154_BCAST_ADDR0xFFFF) {
2377 | dissect_zbee_nwk_gp(tvb, pinfo, tree, data);
2378 | return true1;
2379 | }
2380 | /* 64-bit destination addressing mode support. */
2381 | if (packet->dst_addr_mode == IEEE802154_FCF_ADDR_EXT0x3) {
2382 | dissect_zbee_nwk_gp(tvb, pinfo, tree, data);
2383 | return true1;
2384 | }
2385 |
2386 | return false0;
2387 | } /* dissect_zbee_nwk_heur_gp */
2388 |
2389 | /**
2390 | *Init routine for the ZigBee GP profile security.
2391 | *
2392 | */
2393 | static void
2394 | gp_init_zbee_security(void)
2395 | {
2396 | unsigned i;
2397 | key_record_t key_record;
2398 |
2399 | for (i = 0; gp_uat_key_records && (i < num_uat_key_records); i++) {
2400 | key_record.frame_num = 0;
2401 | key_record.label = g_strdup(gp_uat_key_records[i].label)g_strdup_inline (gp_uat_key_records[i].label);
2402 | memcpy(key_record.key, gp_uat_key_records[i].key, ZBEE_SEC_CONST_KEYSIZE16);
2403 | zbee_gp_keyring = g_slist_prepend(zbee_gp_keyring, g_memdup2(&key_record, sizeof(key_record_t)));
2404 | }
2405 | }
2406 |
2407 | static void zbee_free_key_record(void *ptr)
2408 | {
2409 | key_record_t *k;
2410 |
2411 | k = (key_record_t *)ptr;
2412 | if (!k)
2413 | return;
2414 |
2415 | g_free(k->label)(__builtin_object_size ((k->label), 0) != ((size_t) - 1)) ? g_free_sized (k->label, __builtin_object_size ((k->label ), 0)) : (g_free) (k->label);
2416 | g_free(k)(__builtin_object_size ((k), 0) != ((size_t) - 1)) ? g_free_sized (k, __builtin_object_size ((k), 0)) : (g_free) (k);
2417 | }
2418 |
2419 | static void
2420 | gp_cleanup_zbee_security(void)
2421 | {
2422 | if (!zbee_gp_keyring)
2423 | return;
2424 |
2425 | g_slist_free_full(zbee_gp_keyring, zbee_free_key_record);
2426 | zbee_gp_keyring = NULL((void*)0);
2427 | }
2428 |
2429 | /**
2430 | *ZigBee NWK GP protocol registration routine.
2431 | *
2432 | */
2433 | void
2434 | proto_register_zbee_nwk_gp(void)
2435 | {
2436 | module_t *gp_zbee_prefs;
2437 | expert_module_t* expert_zbee_nwk_gp;
2438 |
2439 | static hf_register_info hf[] = {
2440 | { &hf_zbee_nwk_gp_auto_commissioning,
2441 | { "Auto Commissioning", "zbee_nwk_gp.auto_commissioning", FT_BOOLEAN, 8, NULL((void*)0),
2442 | ZBEE_NWK_GP_FCF_AUTO_COMMISSIONING0x40, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2443 |
2444 | { &hf_zbee_nwk_gp_fc_ext,
2445 | { "NWK Frame Extension", "zbee_nwk_gp.fc_extension", FT_BOOLEAN, 8, NULL((void*)0), ZBEE_NWK_GP_FCF_CONTROL_EXTENSION0x80,
2446 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2447 |
2448 | { &hf_zbee_nwk_gp_fcf,
2449 | { "Frame Control Field", "zbee_nwk_gp.fcf", FT_UINT8, BASE_HEX, NULL((void*)0),
2450 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2451 |
2452 | { &hf_zbee_nwk_gp_frame_type,
2453 | { "Frame Type", "zbee_nwk_gp.frame_type", FT_UINT8, BASE_HEX, VALS(zbee_nwk_gp_frame_types)((0 ? (const struct _value_string*)0 : ((zbee_nwk_gp_frame_types )))),
2454 | ZBEE_NWK_GP_FCF_FRAME_TYPE0x03, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2455 |
2456 | { &hf_zbee_nwk_gp_proto_version,
2457 | { "Protocol Version", "zbee_nwk_gp.proto_version", FT_UINT8, BASE_DEC, NULL((void*)0), ZBEE_NWK_GP_FCF_VERSION0x3C, NULL((void*)0),
2458 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2459 |
2460 | { &hf_zbee_nwk_gp_fc_ext_field,
2461 | { "Extended NWK Frame Control Field", "zbee_nwk_gp.fc_ext", FT_UINT8, BASE_HEX, NULL((void*)0),
2462 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2463 |
2464 | { &hf_zbee_nwk_gp_fc_ext_app_id,
2465 | { "Application ID", "zbee_nwk_gp.fc_ext_app_id", FT_UINT8, BASE_HEX, VALS(zbee_nwk_gp_app_id_names)((0 ? (const struct _value_string*)0 : ((zbee_nwk_gp_app_id_names )))),
2466 | ZBEE_NWK_GP_FCF_EXT_APP_ID0x07, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2467 |
2468 | { &hf_zbee_nwk_gp_fc_ext_direction,
2469 | { "Direction", "zbee_nwk_gp.fc_ext_direction", FT_UINT8, BASE_HEX, VALS(zbee_nwk_gp_directions)((0 ? (const struct _value_string*)0 : ((zbee_nwk_gp_directions )))),
2470 | ZBEE_NWK_GP_FCF_EXT_DIRECTION0x80, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2471 |
2472 | { &hf_zbee_nwk_gp_fc_ext_rx_after_tx,
2473 | { "Rx After Tx", "zbee_nwk_gp.fc_ext_rxaftertx", FT_BOOLEAN, 8, NULL((void*)0), ZBEE_NWK_GP_FCF_EXT_RX_AFTER_TX0x40, NULL((void*)0),
2474 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2475 |
2476 | { &hf_zbee_nwk_gp_fc_ext_sec_key,
2477 | { "Security Key", "zbee_nwk_gp.fc_ext_security_key", FT_BOOLEAN, 8, NULL((void*)0), ZBEE_NWK_GP_FCF_EXT_SECURITY_KEY0x20,
2478 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2479 |
2480 | { &hf_zbee_nwk_gp_fc_ext_sec_level,
2481 | { "Security Level", "zbee_nwk_gp.fc_ext_security_level", FT_UINT8, BASE_HEX,
2482 | VALS(zbee_nwk_gp_src_sec_levels_names)((0 ? (const struct _value_string*)0 : ((zbee_nwk_gp_src_sec_levels_names )))), ZBEE_NWK_GP_FCF_EXT_SECURITY_LEVEL0x18, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2483 |
2484 | { &hf_zbee_nwk_gp_zgpd_src_id,
2485 | { "Src ID", "zbee_nwk_gp.source_id", FT_UINT32, BASE_HEX, VALS(zbee_nwk_gp_src_id_names)((0 ? (const struct _value_string*)0 : ((zbee_nwk_gp_src_id_names )))), 0x0, NULL((void*)0),
2486 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2487 |
2488 | { &hf_zbee_nwk_gp_zgpd_endpoint,
2489 | { "Endpoint", "zbee_nwk_gp.endpoint", FT_UINT8, BASE_DEC, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2490 |
2491 | { &hf_zbee_nwk_gp_security_frame_counter,
2492 | { "Security Frame Counter", "zbee_nwk_gp.security_frame_counter", FT_UINT32, BASE_DEC, NULL((void*)0), 0x0, NULL((void*)0),
2493 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2494 |
2495 | { &hf_zbee_nwk_gp_security_mic_2b,
2496 | { "Security MIC", "zbee_nwk_gp.security_mic2", FT_UINT16, BASE_HEX, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2497 |
2498 | { &hf_zbee_nwk_gp_security_mic_4b,
2499 | { "Security MIC", "zbee_nwk_gp.security_mic4", FT_UINT32, BASE_HEX, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2500 |
2501 | { &hf_zbee_nwk_gp_command_id,
2502 | { "ZGPD Command ID", "zbee_nwk_gp.command_id", FT_UINT8, BASE_HEX | BASE_EXT_STRING0x00000200, &zbee_nwk_gp_cmd_names_ext, 0x0, NULL((void*)0),
2503 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2504 |
2505 | { &hf_zbee_nwk_gp_cmd_comm_device_id,
2506 | { "ZGPD Device ID", "zbee_nwk_gp.cmd.comm.dev_id", FT_UINT8, BASE_HEX | BASE_EXT_STRING0x00000200, &zbee_nwk_gp_device_ids_names_ext,
2507 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2508 |
2509 | { &hf_zbee_nwk_gp_cmd_comm_ext_opt_gpd_key_encr,
2510 | { "GPD Key Encryption", "zbee_nwk_gp.cmd.comm.ext_opt.gpd_key_encr", FT_BOOLEAN, 8, NULL((void*)0),
2511 | ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_GPD_KEY_ENCR0x40, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2512 |
2513 | { &hf_zbee_nwk_gp_cmd_comm_ext_opt_gpd_key_present,
2514 | { "GPD Key Present", "zbee_nwk_gp.cmd.comm.ext_opt.gpd_key_present", FT_BOOLEAN, 8, NULL((void*)0),
2515 | ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_GPD_KEY_PRESENT0x20, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2516 |
2517 | { &hf_zbee_nwk_gp_cmd_comm_ext_opt_key_type,
2518 | { "Key Type", "zbee_nwk_gp.cmd.comm.ext_opt.key_type", FT_UINT8, BASE_HEX,
2519 | VALS(zbee_nwk_gp_src_sec_keys_type_names)((0 ? (const struct _value_string*)0 : ((zbee_nwk_gp_src_sec_keys_type_names )))), ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_KEY_TYPE0x1C, NULL((void*)0),
2520 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2521 |
2522 | { &hf_zbee_nwk_gp_cmd_comm_outgoing_counter,
2523 | { "GPD Outgoing Counter", "zbee_nwk_gp.cmd.comm.out_counter", FT_UINT32, BASE_HEX, NULL((void*)0), 0x0, NULL((void*)0),
2524 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2525 |
2526 | { &hf_zbee_nwk_gp_cmd_comm_ext_opt_sec_level_cap,
2527 | { "Security Level Capabilities", "zbee_nwk_gp.cmd.comm.ext_opt.seclevel_cap", FT_UINT8, BASE_HEX, NULL((void*)0),
2528 | ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_SEC_LEVEL_CAP0x03, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2529 |
2530 | { &hf_zbee_nwk_gp_cmd_comm_security_key,
2531 | { "Security Key", "zbee_nwk_gp.cmd.comm.security_key", FT_BYTES, BASE_NONE, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2532 |
2533 | { &hf_zbee_nwk_gp_cmd_comm_gpd_sec_key_mic,
2534 | { "GPD Key MIC", "zbee_nwk_gp.cmd.comm.gpd_key_mic", FT_UINT32, BASE_HEX, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2535 |
2536 | { &hf_zbee_nwk_gp_cmd_comm_opt_ext_opt,
2537 | { "Extended Option Field", "zbee_nwk_gp.cmd.comm.opt.ext_opt_field", FT_BOOLEAN, 8, NULL((void*)0),
2538 | ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_EXT_OPTIONS0x80, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2539 |
2540 | { &hf_zbee_nwk_gp_cmd_comm_opt,
2541 | { "Options Field", "zbee_nwk_gp.cmd.comm.opt", FT_UINT8, BASE_HEX, NULL((void*)0),
2542 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2543 |
2544 | { &hf_zbee_nwk_gp_cmd_comm_opt_fixed_location,
2545 | { "Fixed Location", "zbee_nwk_gp.cmd.comm.opt.fixed_location", FT_BOOLEAN, 8, NULL((void*)0),
2546 | ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_FIXED_LOCATION0x40, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2547 |
2548 | { &hf_zbee_nwk_gp_cmd_comm_opt_mac_sec_num_cap,
2549 | { "MAC Sequence number capability", "zbee_nwk_gp.cmd.comm.opt.mac_seq_num_cap", FT_BOOLEAN, 8, NULL((void*)0),
2550 | ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_MAC_SEQ0x01, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2551 |
2552 | { &hf_zbee_nwk_gp_cmd_comm_opt_appli_info_present,
2553 | { "Application information present", "zbee_nwk_gp.cmd.comm.opt.appli_info_present", FT_BOOLEAN, 8, NULL((void*)0),
2554 | ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_APPLICATION_INFO0x04, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2555 |
2556 | { &hf_zbee_nwk_gp_cmd_comm_opt_panid_req,
2557 | { "PANId request", "zbee_nwk_gp.cmd.comm.opt.panid_req", FT_BOOLEAN, 8, NULL((void*)0),
2558 | ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_PAN_ID_REQ0x10, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2559 |
2560 | { &hf_zbee_nwk_gp_cmd_comm_opt_rx_on_cap,
2561 | { "RxOnCapability", "zbee_nwk_gp.cmd.comm.opt.rxon_cap", FT_BOOLEAN, 8, NULL((void*)0),
2562 | ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_RX_ON_CAP0x02, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2563 |
2564 | { &hf_zbee_nwk_gp_cmd_comm_opt_sec_key_req,
2565 | { "GP Security Key Request", "zbee_nwk_gp.cmd.comm.opt.seq_key_req", FT_BOOLEAN, 8, NULL((void*)0),
2566 | ZBEE_NWK_GP_CMD_COMMISSIONING_OPT_GP_SEC_KEY_REQ0x20, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2567 |
2568 | { &hf_zbee_nwk_gp_cmd_comm_ext_opt,
2569 | { "Extended Options Field", "zbee_nwk_gp.cmd.comm.ext_opt", FT_UINT8, BASE_HEX, NULL((void*)0),
2570 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2571 |
2572 | { &hf_zbee_nwk_gp_cmd_comm_ext_opt_outgoing_counter,
2573 | { "GPD Outgoing present", "zbee_nwk_gp.cmd.comm.ext_opt.outgoing_counter", FT_BOOLEAN, 8, NULL((void*)0),
2574 | ZBEE_NWK_GP_CMD_COMMISSIONING_EXT_OPT_OUT_COUNTER0x80, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2575 |
2576 | { &hf_zbee_nwk_gp_cmd_comm_manufacturer_greenpeak_dev_id,
2577 | { "Manufacturer Model ID", "zbee_nwk_gp.cmd.comm.manufacturer_model_id", FT_UINT16, BASE_HEX,
2578 | VALS(zbee_nwk_gp_manufacturer_greenpeak_dev_names)((0 ? (const struct _value_string*)0 : ((zbee_nwk_gp_manufacturer_greenpeak_dev_names )))), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2579 |
2580 | { &hf_zbee_nwk_gp_cmd_comm_manufacturer_dev_id,
2581 | { "Manufacturer Model ID", "zbee_nwk_gp.cmd.comm.manufacturer_model_id", FT_UINT16, BASE_HEX,
2582 | NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2583 |
2584 | { &hf_zbee_nwk_gp_cmd_comm_manufacturer_id,
2585 | { "Manufacturer ID", "zbee_nwk_gp.cmd.comm.manufacturer_id", FT_UINT16, BASE_HEX,
2586 | VALS(zbee_mfr_code_names)((0 ? (const struct _value_string*)0 : ((zbee_mfr_code_names) ))), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2587 |
2588 | { &hf_zbee_nwk_gp_cmd_comm_appli_info_crp,
2589 | { "Cluster reports present", "zbee_nwk_gp.cmd.comm.appli_info.crp", FT_BOOLEAN, 8, NULL((void*)0),
2590 | ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_CRP0x08 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2591 |
2592 | { &hf_zbee_nwk_gp_cmd_comm_appli_info_gclp,
2593 | { "GP commands list present", "zbee_nwk_gp.cmd.comm.appli_info.gclp", FT_BOOLEAN, 8, NULL((void*)0),
2594 | ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_GCLP0x04 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2595 |
2596 | { &hf_zbee_nwk_gp_cmd_comm_appli_info,
2597 | { "Application information Field", "zbee_nwk_gp.cmd.comm.appli_info", FT_UINT8, BASE_HEX, NULL((void*)0),
2598 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2599 |
2600 | { &hf_zbee_nwk_gp_cmd_comm_appli_info_mip,
2601 | { "Manufacturer ID present", "zbee_nwk_gp.cmd.comm.appli_info.mip", FT_BOOLEAN, 8, NULL((void*)0),
2602 | ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_MIP0x01 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2603 |
2604 | { &hf_zbee_nwk_gp_cmd_comm_appli_info_mmip,
2605 | { "Manufacturer Model ID present", "zbee_nwk_gp.cmd.comm.appli_info.mmip", FT_BOOLEAN, 8, NULL((void*)0),
2606 | ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_MMIP0x02 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2607 |
2608 | { &hf_zbee_nwk_gp_cmd_comm_appli_info_sip,
2609 | { "Switch information present", "zbee_nwk_gp.cmd.comm.appli_info.sip", FT_BOOLEAN, 8, NULL((void*)0),
2610 | ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_SIP0x10 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2611 |
2612 | { &hf_zbee_nwk_gp_cmd_comm_appli_info_adcf,
2613 | { "GPD Application Description command follows", "zbee_nwk_gp.cmd.comm.appli_info.adcf", FT_BOOLEAN, 8, NULL((void*)0),
2614 | ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_ADCF0x20 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2615 |
2616 | { &hf_zbee_nwk_gp_cmd_comm_appli_info_res,
2617 | { "Reserved", "zbee_nwk_gp.cmd.comm.appli_info.reserved", FT_UINT8, BASE_HEX, NULL((void*)0),
2618 | ZBEE_NWK_GP_CMD_COMMISSIONING_APPLI_INFO_RES0xC0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2619 |
2620 | { &hf_zbee_nwk_gp_cmd_comm_gpd_cmd_num,
2621 | { "Number of GPD commands", "zbee_nwk_gp.cmd.comm.gpd_cmd_num", FT_UINT8, BASE_DEC, NULL((void*)0),
2622 | 0x0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2623 |
2624 | { &hf_zbee_nwk_gp_cmd_comm_gpd_cmd_id_list,
2625 | { "GPD CommandID list", "zbee_nwk_gp.cmd.comm.gpd_cmd_id_list", FT_NONE, BASE_NONE, NULL((void*)0),
2626 | 0x0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2627 |
2628 | { &hf_zbee_nwk_gp_cmd_comm_length_of_clid_list,
2629 | { "Length of ClusterID list", "zbee_nwk_gp.cmd.comm.length_of_clid_list", FT_UINT8, BASE_HEX, NULL((void*)0),
2630 | 0x0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2631 |
2632 | { &hf_zbee_nwk_gp_cmd_comm_length_of_clid_list_server,
2633 | { "Number of server ClusterIDs", "zbee_nwk_gp.cmd.comm.length_of_clid_list_srv", FT_UINT8, BASE_DEC, NULL((void*)0),
2634 | ZBEE_NWK_GP_CMD_COMMISSIONING_CLID_LIST_LEN_SRV0x0F, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2635 |
2636 | { &hf_zbee_nwk_gp_cmd_comm_length_of_clid_list_client,
2637 | { "Number of client ClusterIDs", "zbee_nwk_gp.cmd.comm.length_of_clid_list_cli", FT_UINT8, BASE_DEC, NULL((void*)0),
2638 | ZBEE_NWK_GP_CMD_COMMISSIONING_CLID_LIST_LEN_CLI0xF0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2639 |
2640 | { &hf_zbee_nwk_cmd_comm_clid_list_server,
2641 | { "Cluster ID List Server", "zbee_nwk_gp.cmd.comm.clid_list_server", FT_NONE, BASE_NONE, NULL((void*)0),
2642 | 0x0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2643 |
2644 | { &hf_zbee_nwk_cmd_comm_clid_list_client,
2645 | { "ClusterID List Client", "zbee_nwk_gp.cmd.comm.clid_list_client", FT_NONE, BASE_NONE, NULL((void*)0),
2646 | 0x0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2647 |
2648 | { &hf_zbee_nwk_cmd_comm_cluster_id,
2649 | { "Cluster ID", "zbee_nwk_gp.cmd.comm.cluster_id", FT_UINT16, BASE_HEX | BASE_RANGE_STRING0x00000100, RVALS(zbee_aps_cid_names)((0 ? (const struct _range_string*)0 : ((zbee_aps_cid_names)) )),
2650 | 0x0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2651 |
2652 | { &hf_zbee_nwk_gp_cmd_comm_switch_info,
2653 | { "Switch information", "zbee_nwk_gp.cmd.comm.switch_info", FT_NONE, BASE_NONE, NULL((void*)0),
2654 | 0x0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2655 |
2656 | { &hf_zbee_nwk_gp_cmd_comm_switch_info_length,
2657 | { "Switch info length", "zbee_nwk_gp.cmd.comm.switch_info.length", FT_UINT8, BASE_DEC, NULL((void*)0),
2658 | 0x0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2659 |
2660 | { &hf_zbee_nwk_gp_cmd_comm_switch_info_generic_switch_config,
2661 | { "Generic switch configuration", "zbee_nwk_gp.cmd.comm.switch_info.generic_switch_config", FT_UINT8, BASE_HEX, NULL((void*)0),
2662 | 0x0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2663 |
2664 | { &hf_zbee_nwk_gp_cmd_comm_switch_info_num_contacts,
2665 | { "Number of contacts", "zbee_nwk_gp.cmd.comm.switch_info.num_contacts", FT_UINT8, BASE_DEC, NULL((void*)0),
2666 | ZBEE_NWK_GP_CMD_COMMISSIONING_SWITCH_CONF_NUM_CONTACTS0x0F , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2667 |
2668 | { &hf_zbee_nwk_gp_cmd_comm_switch_info_switch_type,
2669 | { "Switch type", "zbee_nwk_gp.cmd.comm.switch_info.switch_type", FT_UINT8, BASE_HEX, VALS(zbee_nwk_gp_switch_type_names)((0 ? (const struct _value_string*)0 : ((zbee_nwk_gp_switch_type_names )))),
2670 | ZBEE_NWK_GP_CMD_COMMISSIONING_SWITCH_CONF_SWITCH_TYPE0x30 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2671 |
2672 | { &hf_zbee_nwk_gp_cmd_comm_switch_info_reserved,
2673 | { "Reserved", "zbee_nwk_gp.cmd.comm.switch_info.reserved", FT_UINT8, BASE_HEX, NULL((void*)0),
2674 | ZBEE_NWK_GP_CMD_COMMISSIONING_SWITCH_CONF_RES0xC0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2675 |
2676 | { &hf_zbee_nwk_gp_cmd_comm_switch_info_current_contact_status,
2677 | { "Current contact status", "zbee_nwk_gp.cmd.comm.switch_info.current_contact_status", FT_UINT8, BASE_HEX, NULL((void*)0),
2678 | 0x0 , NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2679 |
2680 | { &hf_zbee_nwk_gp_cmd_comm_rep_opt_key_encr,
2681 | { "GPD Key Encryption", "zbee_nwk_gp.cmd.comm_reply.opt.sec_key_encr", FT_BOOLEAN, 8, NULL((void*)0),
2682 | ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_KEY_ENCR0x04, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2683 |
2684 | { &hf_zbee_nwk_gp_cmd_comm_rep_opt,
2685 | { "Options Field", "zbee_nwk_gp.cmd.comm_reply.opt", FT_UINT8, BASE_HEX, NULL((void*)0),
2686 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2687 |
2688 | { &hf_zbee_nwk_gp_cmd_comm_rep_opt_panid_present,
2689 | { "PANID Present", "zbee_nwk_gp.cmd.comm_reply.opt.pan_id_present", FT_BOOLEAN, 8, NULL((void*)0),
2690 | ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_PAN_ID_PRESENT0x01, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2691 |
2692 | { &hf_zbee_nwk_gp_cmd_comm_rep_opt_sec_key_present,
2693 | { "GPD Security Key Present", "zbee_nwk_gp.cmd.comm_reply.opt.sec_key_present", FT_BOOLEAN, 8, NULL((void*)0),
2694 | ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_SEC_KEY_PRESENT0x02, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2695 |
2696 | { &hf_zbee_nwk_gp_cmd_comm_rep_opt_sec_level,
2697 | { "Security Level", "zbee_nwk_gp.cmd.comm_reply.opt.sec_level", FT_UINT8, BASE_HEX, NULL((void*)0),
2698 | ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_SEC_LEVEL0x18, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2699 |
2700 | { &hf_zbee_nwk_gp_cmd_comm_rep_opt_sec_type,
2701 | { "Key Type", "zbee_nwk_gp.cmd.comm_reply.opt.key_type", FT_UINT8, BASE_HEX, NULL((void*)0),
2702 | ZBEE_NWK_GP_CMD_COMMISSIONING_REP_OPT_KEY_TYPE0xE0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2703 |
2704 | { &hf_zbee_nwk_gp_cmd_comm_rep_pan_id,
2705 | { "PAN ID", "zbee_nwk_gp.cmd.comm_reply.pan_id", FT_UINT16, BASE_HEX, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2706 |
2707 | { &hf_zbee_nwk_gp_cmd_comm_rep_frame_counter,
2708 | { "Frame Counter", "zbee_nwk_gp.cmd.comm_reply.frame_counter", FT_UINT32, BASE_HEX, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2709 |
2710 | { &hf_zbee_nwk_gp_cmd_read_att_opt_multi_rec,
2711 | { "Multi-record", "zbee_nwk_gp.cmd.read_att.opt.multi_record", FT_BOOLEAN, 8, NULL((void*)0),
2712 | ZBEE_NWK_GP_CMD_READ_ATTRIBUTE_OPT_MULTI_RECORD0x01, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2713 |
2714 | { &hf_zbee_nwk_gp_cmd_read_att_opt_man_field_present,
2715 | { "Manufacturer field present", "zbee_nwk_gp.cmd.read_att.opt.man_field_present", FT_BOOLEAN, 8, NULL((void*)0),
2716 | ZBEE_NWK_GP_CMD_READ_ATTRIBUTE_OPT_MAN_FIELD_PRESENT0x02, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2717 |
2718 | { &hf_zbee_nwk_gp_cmd_read_att_opt,
2719 | { "Option field", "zbee_nwk_gp.cmd.read_att.opt", FT_UINT8, BASE_HEX, NULL((void*)0),
2720 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2721 |
2722 | { &hf_zbee_nwk_gp_cmd_zcl_tunnel_opt_frame_type,
2723 | { "Frame type", "zbee_nwk_gp.cmd.zcl_tunnel.opt.frame_type", FT_UINT8, BASE_HEX, NULL((void*)0),
2724 | ZBEE_NWK_GP_CMD_ZCL_TUNNEL_OPT_FRAME_TYPE0x03, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2725 |
2726 | { &hf_zbee_nwk_gp_cmd_zcl_tunnel_opt_man_field_present,
2727 | { "Manufacturer field present", "zbee_nwk_gp.cmd.zcl_tunnel.opt.man_field_present", FT_BOOLEAN, 8, NULL((void*)0),
2728 | ZBEE_NWK_GP_CMD_ZCL_TUNNEL_OPT_MAN_FIELD_PRESENT0x04, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2729 |
2730 | { &hf_zbee_nwk_gp_cmd_zcl_tunnel_opt_direction,
2731 | { "Direction", "zbee_nwk_gp.cmd.zcl_tunnel.opt.direction", FT_UINT8, BASE_HEX, NULL((void*)0),
2732 | ZBEE_NWK_GP_CMD_ZCL_TUNNEL_OPT_DIRECTION0x08, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2733 |
2734 | { &hf_zbee_nwk_gp_cmd_zcl_tunnel_opt,
2735 | { "Option field", "zbee_nwk_gp.cmd.zcl_tunnel.opt", FT_UINT8, BASE_HEX, NULL((void*)0),
2736 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2737 |
2738 | { &hf_zbee_nwk_gp_cmd_zcl_tunnel_command_id,
2739 | { "Zigbee Command ID", "zbee_nwk_gp.cmd.zcl_tunnel.command_id", FT_UINT8, BASE_HEX, NULL((void*)0), 0x0,
2740 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2741 |
2742 | { &hf_zbee_nwk_gp_cmd_zcl_tunnel_payload_len,
2743 | { "Length of Payload", "zbee_nwk_gp.cmd.zcl_tunnel.payload_len", FT_UINT8, BASE_DEC, NULL((void*)0), 0x0,
2744 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2745 |
2746 | { &hf_zbee_nwk_gp_cmd_compact_attr_report_report_id,
2747 | { "Report Identifier", "zbee_nwk_gp.cmd.compact_attr_report.report_id", FT_UINT8, BASE_HEX, NULL((void*)0),
2748 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2749 |
2750 | { &hf_zbee_nwk_gp_cmd_compact_attr_report_data_points,
2751 | { "Data Points", "zbee_nwk_gp.cmd.compact_attr_report.data_points", FT_BYTES, BASE_NONE, NULL((void*)0),
2752 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2753 |
2754 | { &hf_zbee_nwk_gp_cmd_app_desc_total_report,
2755 | { "Total Number of Reports", "zbee_nwk_gp.app_desc.total_report", FT_UINT8, BASE_DEC, NULL((void*)0),
2756 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2757 |
2758 | { &hf_zbee_nwk_gp_cmd_app_desc_num_report,
2759 | { "Number of Reports", "zbee_nwk_gp.app_desc.num_report", FT_UINT8, BASE_DEC, NULL((void*)0),
2760 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2761 |
2762 | { &hf_zbee_nwk_gp_cmd_app_desc_report_desc_id,
2763 | { "Report Identifier", "zbee_nwk_gp.app_desc.report_desc.id", FT_UINT8, BASE_HEX, NULL((void*)0),
2764 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2765 |
2766 | { &hf_zbee_nwk_gp_cmd_app_desc_report_desc_opt,
2767 | { "Report Options", "zbee_nwk_gp.app_desc.report_desc.opt", FT_UINT8, BASE_HEX, NULL((void*)0),
2768 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2769 |
2770 | { &hf_zbee_nwk_gp_cmd_app_desc_report_desc_opt_timeout_present,
2771 | { "Timeout Present", "zbee_nwk_gp.app_desc.report_desc.opt.timeout_present", FT_BOOLEAN, 8, NULL((void*)0),
2772 | ZBEE_NWK_GP_CMD_APP_DESC_REPORT_DESC_OPT_TIMEOUT_PRESENT0x01, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2773 |
2774 | { &hf_zbee_nwk_gp_cmd_app_desc_report_desc_timeout,
2775 | { "Timeout Period", "zbee_nwk_gp.app_desc.report_desc.timeout", FT_UINT16, BASE_DEC, NULL((void*)0),
2776 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2777 |
2778 | { &hf_zbee_nwk_gp_cmd_app_desc_report_desc_len_remain,
2779 | { "Remaining Length", "zbee_nwk_gp.app_desc.report_desc.len_remain", FT_UINT8, BASE_DEC, NULL((void*)0),
2780 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2781 |
2782 | { &hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt,
2783 | { "Data Point Options", "zbee_nwk_gp.app_desc.data_pt_desc.opt", FT_UINT8, BASE_HEX, NULL((void*)0),
2784 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2785 |
2786 | { &hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt_num_recs,
2787 | { "Number of Attribute Records", "zbee_nwk_gp.app_desc.data_pt_desc.opt.num_recs", FT_UINT8, BASE_DEC, NULL((void*)0),
2788 | ZBEE_NWK_GP_CMD_APP_DESC_DATA_PT_DESC_OPT_ATTR_NUM0x07, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2789 |
2790 | { &hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt_server,
2791 | { "Server", "zbee_nwk_gp.app_desc.data_pt_desc.opt.server", FT_BOOLEAN, 8, NULL((void*)0),
2792 | ZBEE_NWK_GP_CMD_APP_DESC_DATA_PT_DESC_OPT_SERVER0x08, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2793 |
2794 | { &hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_opt_manu_id_present,
2795 | { "Manufacturer ID Present", "zbee_nwk_gp.app_desc.data_pt_desc.opt.manu_id_present", FT_BOOLEAN, 8, NULL((void*)0),
2796 | ZBEE_NWK_GP_CMD_APP_DESC_DATA_PT_DESC_OPT_MANU_ID_PRESENT0x10, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2797 |
2798 | { &hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_cluster_id,
2799 | { "Cluster ID", "zbee_nwk_gp.app_desc.data_pt_desc.cluster_id", FT_UINT16, BASE_HEX | BASE_RANGE_STRING0x00000100, RVALS(zbee_aps_cid_names)((0 ? (const struct _range_string*)0 : ((zbee_aps_cid_names)) )),
2800 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2801 |
2802 | { &hf_zbee_nwk_gp_cmd_app_desc_data_pt_desc_manu_id,
2803 | { "Manufacturer ID", "zbee_nwk_gp.app_desc.data_pt_desc.manu_id", FT_UINT16, BASE_HEX, VALS(zbee_mfr_code_names)((0 ? (const struct _value_string*)0 : ((zbee_mfr_code_names) ))),
2804 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2805 |
2806 | { &hf_zbee_nwk_gp_cmd_app_desc_attr_rec_id,
2807 | { "Attribute ID", "zbee_nwk_gp.app_desc.attr_rec.id", FT_UINT16, BASE_HEX, NULL((void*)0),
2808 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2809 |
2810 | { &hf_zbee_nwk_gp_cmd_app_desc_attr_rec_data_type,
2811 | { "Attribute Data Type", "zbee_nwk_gp.app_desc.attr_rec.data_type", FT_UINT8, BASE_HEX, VALS(zbee_zcl_short_data_type_names)((0 ? (const struct _value_string*)0 : ((zbee_zcl_short_data_type_names )))),
2812 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2813 |
2814 | { &hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt,
2815 | { "Attribute Options", "zbee_nwk_gp.app_desc.attr_rec.opt", FT_UINT8, BASE_HEX, NULL((void*)0),
2816 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2817 |
2818 | { &hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt_len_remain,
2819 | { "Remaining Attribute Record Length", "zbee_nwk_gp.app_desc.attr_rec.opt.len_remain", FT_UINT8, BASE_DEC, NULL((void*)0),
2820 | ZBEE_NWK_GP_CMD_APP_DESC_ATTR_REC_OPT_LEN_REMAIN0x0F, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2821 |
2822 | { &hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt_reported,
2823 | { "Reported", "zbee_nwk_gp.app_desc.attr_rec.opt.reported", FT_BOOLEAN, 8, NULL((void*)0),
2824 | ZBEE_NWK_GP_CMD_APP_DESC_ATTR_REC_OPT_REPORTED0x10, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2825 |
2826 | { &hf_zbee_nwk_gp_cmd_app_desc_attr_rec_opt_val_present,
2827 | { "Attribute Value Present", "zbee_nwk_gp.app_desc.attr_rec.opt.val_present", FT_BOOLEAN, 8, NULL((void*)0),
2828 | ZBEE_NWK_GP_CMD_APP_DESC_ATTR_REC_OPT_VAL_PRESENT0x20, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2829 |
2830 | { &hf_zbee_nwk_gp_cmd_app_desc_attr_rec_offset,
2831 | { "Attribute Offset within Report", "zbee_nwk_gp.app_desc.attr_rec.offset", FT_UINT8, BASE_DEC, NULL((void*)0),
2832 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2833 |
2834 | { &hf_zbee_nwk_gp_cmd_app_desc_attr_rec_val,
2835 | { "Attribute Value", "zbee_nwk_gp.app_desc.attr_rec.val", FT_BYTES, BASE_NONE, NULL((void*)0),
2836 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2837 |
2838 | { &hf_zbee_zcl_gp_cmd_ms_manufacturer_code,
2839 | { "Manufacturer Code", "zbee_nwk_gp.cmd.manufacturer_code", FT_UINT16, BASE_HEX, VALS(zbee_mfr_code_names)((0 ? (const struct _value_string*)0 : ((zbee_mfr_code_names) ))),
2840 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2841 |
2842 | { &hf_zbee_nwk_gp_cmd_read_att_record_len,
2843 | { "Length of Record List", "zbee_nwk_gp.cmd.read_att.record_len", FT_UINT8, BASE_DEC, NULL((void*)0), 0x0,
2844 | NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2845 |
2846 | { &hf_zbee_nwk_gp_zcl_attr_status,
2847 | { "Status", "zbee_nwk_gp.zcl.attr.status", FT_UINT8, BASE_HEX, VALS(zbee_zcl_status_names)((0 ? (const struct _value_string*)0 : ((zbee_zcl_status_names )))),
2848 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2849 |
2850 | { &hf_zbee_nwk_gp_zcl_attr_data_type,
2851 | { "Data Type", "zbee_nwk_gp.zcl.attr.datatype", FT_UINT8, BASE_HEX, VALS(zbee_zcl_short_data_type_names)((0 ? (const struct _value_string*)0 : ((zbee_zcl_short_data_type_names )))),
2852 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) } },
2853 |
2854 | { &hf_zbee_nwk_gp_zcl_attr_cluster_id,
2855 | { "ZigBee Cluster ID", "zbee_nwk_gp.zcl.attr.cluster_id", FT_UINT16, BASE_HEX | BASE_RANGE_STRING0x00000100, RVALS(zbee_aps_cid_names)((0 ? (const struct _range_string*)0 : ((zbee_aps_cid_names)) )),
2856 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2857 |
2858 | { &hf_zbee_nwk_gp_cmd_channel_request_toggling_behaviour,
2859 | { "Channel Toggling Behaviour", "zbee_nwk_gp.cmd.ch_req", FT_UINT8, BASE_HEX, NULL((void*)0),
2860 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2861 |
2862 | { &hf_zbee_nwk_gp_cmd_channel_request_toggling_behaviour_1st,
2863 | { "Rx channel in the next attempt", "zbee_nwk_gp.cmd.ch_req.1st", FT_UINT8, BASE_HEX, NULL((void*)0),
2864 | ZBEE_NWK_GP_CMD_CHANNEL_REQUEST_1ST0x0F, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2865 |
2866 | { &hf_zbee_nwk_gp_cmd_channel_request_toggling_behaviour_2nd,
2867 | { "Rx channel in the second next attempt", "zbee_nwk_gp.ch_req.2nd", FT_UINT8, BASE_HEX, NULL((void*)0),
2868 | ZBEE_NWK_GP_CMD_CHANNEL_REQUEST_2ND0xF0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2869 |
2870 | { &hf_zbee_nwk_gp_cmd_operational_channel,
2871 | { "Operational Channel", "zbee_nwk_gp.cmd.configuration_ch", FT_UINT8, BASE_HEX, NULL((void*)0),
2872 | 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2873 |
2874 | { &hf_zbee_nwk_gp_cmd_channel_configuration,
2875 | { "Operation channel", "zbee_nwk_gp.cmd.configuration_ch.operation_ch", FT_UINT8, BASE_HEX, NULL((void*)0),
2876 | ZBEE_NWK_GP_CMD_CHANNEL_CONFIGURATION_OPERATION_CH0x0F, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2877 |
2878 | { &hf_zbee_nwk_gp_cmd_move_color_ratex,
2879 | { "RateX", "zbee_nwk_gp.cmd.move_color.ratex", FT_UINT16, BASE_DEC, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2880 |
2881 | { &hf_zbee_nwk_gp_cmd_move_color_ratey,
2882 | { "RateY", "zbee_nwk_gp.cmd.move_color.ratey", FT_UINT16, BASE_DEC, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2883 |
2884 | { &hf_zbee_nwk_gp_cmd_move_up_down_rate,
2885 | { "Rate", "zbee_nwk_gp.cmd.move_up_down.rate", FT_UINT8, BASE_DEC, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2886 |
2887 | { &hf_zbee_nwk_gp_cmd_step_color_stepx,
2888 | { "StepX", "zbee_nwk_gp.cmd.step_color.stepx", FT_UINT16, BASE_DEC, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2889 |
2890 | { &hf_zbee_nwk_gp_cmd_step_color_stepy,
2891 | { "StepY", "zbee_nwk_gp.cmd.step_color.stepy", FT_UINT16, BASE_DEC, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2892 |
2893 | { &hf_zbee_nwk_gp_cmd_step_color_transition_time,
2894 | { "Transition Time", "zbee_nwk_gp.cmd.step_color.transition_time", FT_UINT16, BASE_DEC, NULL((void*)0), 0x0, NULL((void*)0),
2895 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2896 |
2897 | { &hf_zbee_nwk_gp_cmd_step_up_down_step_size,
2898 | { "Step Size", "zbee_nwk_gp.cmd.step_up_down.step_size", FT_UINT8, BASE_DEC, NULL((void*)0), 0x0, NULL((void*)0), HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }},
2899 |
2900 | { &hf_zbee_nwk_gp_cmd_step_up_down_transition_time,
2901 | { "Transition Time", "zbee_nwk_gp.cmd.step_up_down.transition_time", FT_UINT16, BASE_DEC, NULL((void*)0), 0x0, NULL((void*)0),
2902 | HFILL-1, 0, HF_REF_TYPE_NONE, -1, ((void*)0) }}
2903 | };
2904 |
2905 | static ei_register_info ei[] = {
2906 | { &ei_zbee_nwk_gp_no_payload,
2907 | { "zbee_nwk_gp.no_payload", PI_MALFORMED0x07000000, PI_ERROR0x00800000,
2908 | "Payload is missing", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
2909 | { &ei_zbee_nwk_gp_inval_residual_data,
2910 | { "zbee_nwk_gp.inval_residual_data", PI_MALFORMED0x07000000, PI_ERROR0x00800000,
2911 | "Invalid residual data", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }},
2912 | { &ei_zbee_nwk_gp_com_rep_no_out_cnt,
2913 | { "zbee_nwk_gp.com_rep_no_out_cnt", PI_DEBUG0x08000000, PI_WARN0x00600000,
2914 | "Missing outgoing frame counter", EXPFILL0, ((void*)0), 0, ((void*)0), {0, {((void*)0), ((void*)0), FT_NONE , BASE_NONE, ((void*)0), 0, ((void*)0), -1, 0, HF_REF_TYPE_NONE , -1, ((void*)0)}} }}
2915 | };
2916 |
2917 | static int *ett[] = {
2918 | &ett_zbee_nwk,
2919 | &ett_zbee_nwk_cmd,
2920 | &ett_zbee_nwk_cmd_cinfo,
2921 | &ett_zbee_nwk_cmd_appli_info,
2922 | &ett_zbee_nwk_cmd_options,
2923 | &ett_zbee_nwk_fcf,
2924 | &ett_zbee_nwk_fcf_ext,
2925 | &ett_zbee_nwk_clu_rec,
2926 | &ett_zbee_nwk_att_rec,
2927 | &ett_zbee_nwk_cmd_app_desc_report_desc,
2928 | &ett_zbee_nwk_cmd_app_desc_data_pt_desc,
2929 | &ett_zbee_nwk_cmd_app_desc_data_pt_options,
2930 | &ett_zbee_nwk_cmd_app_desc_att_rec,
2931 | &ett_zbee_nwk_cmd_comm_gpd_cmd_id_list,
2932 | &ett_zbee_nwk_cmd_comm_length_of_clid_list,
2933 | &ett_zbee_nwk_cmd_comm_clid_list_server,
2934 | &ett_zbee_nwk_cmd_comm_clid_list_client,
2935 | &ett_zbee_nwk_cmd_comm_switch_info,
2936 | &ett_zbee_nwk_cmd_comm_switch_info_generic_switch_config
2937 | };
2938 |
2939 | static uat_field_t key_uat_fields[] = {
2940 | UAT_FLD_CSTRING(gp_uat_key_records, string, "Key", "A 16-byte key."){"string", "Key", PT_TXTMOD_STRING,{uat_fld_chk_str,gp_uat_key_records_string_set_cb ,gp_uat_key_records_string_tostr_cb},{0,0,0},0,"A 16-byte key." ,((void*)0)},
2941 | UAT_FLD_VS(gp_uat_key_records, byte_order, "Byte Order", byte_order_vals, "Byte order of a key."){"byte_order", "Byte Order", PT_TXTMOD_ENUM,{uat_fld_chk_enum ,gp_uat_key_records_byte_order_set_cb,gp_uat_key_records_byte_order_tostr_cb },{&(byte_order_vals),&(byte_order_vals),&(byte_order_vals )},&(byte_order_vals),"Byte order of a key.",((void*)0)},
2942 | UAT_FLD_LSTRING(gp_uat_key_records, label, "Label", "User label for a key."){"label", "Label", PT_TXTMOD_STRING,{0,gp_uat_key_records_label_set_cb ,gp_uat_key_records_label_tostr_cb},{0,0,0},0,"User label for a key." ,((void*)0)},
2943 | UAT_END_FIELDS{((void*)0),((void*)0),PT_TXTMOD_NONE,{0,0,0},{0,0,0},0,0,((void *)0)}
2944 | };
2945 |
2946 | proto_zbee_nwk_gp = proto_register_protocol("ZigBee Green Power Profile", "ZigBee Green Power",
2947 | ZBEE_PROTOABBREV_NWK_GP"zbee_nwk_gp");
2948 |
2949 | gp_zbee_prefs = prefs_register_protocol(proto_zbee_nwk_gp, NULL((void*)0));
2950 |
2951 | zbee_gp_sec_key_table_uat = uat_new("ZigBee GP Security Keys", sizeof(uat_key_record_t), "zigbee_gp_keys", true1,
2952 | &gp_uat_key_records, &num_uat_key_records, UAT_AFFECTS_DISSECTION0x00000001, NULL((void*)0), uat_key_record_copy_cb,
2953 | uat_key_record_update_cb, uat_key_record_free_cb, uat_key_record_post_update_cb, NULL((void*)0), key_uat_fields);
2954 |
2955 | prefs_register_uat_preference(gp_zbee_prefs, "gp_key_table", "Pre-configured GP Security Keys",
2956 | "Pre-configured GP Security Keys.", zbee_gp_sec_key_table_uat);
2957 |
2958 | register_init_routine(gp_init_zbee_security);
2959 | register_cleanup_routine(gp_cleanup_zbee_security);
2960 |
2961 | /* Register the Wireshark protocol. */
2962 | proto_register_field_array(proto_zbee_nwk_gp, hf, array_length(hf)(sizeof (hf) / sizeof (hf)[0]));
2963 | proto_register_subtree_array(ett, array_length(ett)(sizeof (ett) / sizeof (ett)[0]));
2964 |
2965 | expert_zbee_nwk_gp = expert_register_protocol(proto_zbee_nwk_gp);
2966 | expert_register_field_array(expert_zbee_nwk_gp, ei, array_length(ei)(sizeof (ei) / sizeof (ei)[0]));
2967 |
2968 | /* Register the dissectors. */
2969 | register_dissector(ZBEE_PROTOABBREV_NWK_GP"zbee_nwk_gp", dissect_zbee_nwk_gp, proto_zbee_nwk_gp);
2970 | register_dissector(ZBEE_PROTOABBREV_NWK_GP_CMD"zbee_nwk_gp_cmd", dissect_zbee_nwk_gp_cmd, proto_zbee_nwk_gp);
2971 | } /* proto_register_zbee_nwk_gp */
2972 |
2973 | /**
2974 | *Registers the ZigBee dissector with Wireshark.
2975 | *
2976 | */
2977 | void
2978 | proto_reg_handoff_zbee_nwk_gp(void)
2979 | {
2980 | /* Register our dissector with IEEE 802.15.4. */
2981 | dissector_add_for_decode_as(IEEE802154_PROTOABBREV_WPAN_PANID"wpan.panid", find_dissector(ZBEE_PROTOABBREV_NWK_GP"zbee_nwk_gp"));
2982 | heur_dissector_add(IEEE802154_PROTOABBREV_WPAN"wpan", dissect_zbee_nwk_heur_gp, "ZigBee Green Power over IEEE 802.15.4", "zbee_nwk_gp_wlan", proto_zbee_nwk_gp, HEURISTIC_ENABLE);
2983 | } /* proto_reg_handoff_zbee */
2984 |
2985 | /*
2986 | * Editor modelines
2987 | *
2988 | * Local Variables:
2989 | * c-basic-offset: 4
2990 | * tab-width: 8
2991 | * indent-tabs-mode: nil
2992 | * End:
2993 | *
2994 | * ex: set shiftwidth=4 tabstop=8 expandtab:
2995 | * :indentSize=4:tabSize=8:noTabs=true:
2996 | */