### Bug Summary

File: | builds/wireshark/wireshark/capinfos.c
Warning: | line 1081, column 33 Read function called when stream is in EOF state. Function has no effect

### Annotated Source Code

Press '?' to see keyboard shortcuts

Show analyzer invocation
clang -cc1 -cc1 -triple x86_64-pc-linux-gnu -analyze -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name capinfos.c -analyzer-checker=core -analyzer-checker=apiModeling -analyzer-checker=unix -analyzer-checker=deadcode -analyzer-checker=security.insecureAPI.UncheckedReturn -analyzer-checker=security.insecureAPI.getpw -analyzer-checker=security.insecureAPI.gets -analyzer-checker=security.insecureAPI.mktemp -analyzer-checker=security.insecureAPI.mkstemp -analyzer-checker=security.insecureAPI.vfork -analyzer-checker=nullability.NullPassedToNonnull -analyzer-checker=nullability.NullReturnedFromNonnull -analyzer-output plist -w -setup-static-analyzer -mrelocation-model pic -pic-level 2 -pic-is-pie -fno-delete-null-pointer-checks -mframe-pointer=all -relaxed-aliasing -fmath-errno -ffp-contract=on -fno-rounding-math -ffloat16-excess-precision=fast -fbfloat16-excess-precision=fast -mconstructor-aliases -funwind-tables=2 -target-cpu x86-64 -tune-cpu generic -debugger-tuning=gdb -fdebug-compilation-dir=/builds/wireshark/wireshark/build -fcoverage-compilation-dir=/builds/wireshark/wireshark/build -resource-dir /usr/lib/llvm-22/lib/clang/22 -isystem /usr/include/glib-2.0 -isystem /usr/lib/x86_64-linux-gnu/glib-2.0/include -D CARES_NO_DEPRECATED -D G_DISABLE_DEPRECATED -D G_DISABLE_SINGLE_INCLUDES -D WS_DEBUG -D WS_DEBUG_UTF_8 -I /builds/wireshark/wireshark/build -I /builds/wireshark/wireshark -I /builds/wireshark/wireshark/include -I /builds/wireshark/wireshark/wiretap -D _GLIBCXX_ASSERTIONS -internal-isystem /usr/lib/llvm-22/lib/clang/22/include -internal-isystem /usr/local/include -internal-isystem /usr/lib/gcc/x86_64-linux-gnu/16/../../../../x86_64-linux-gnu/include -internal-externc-isystem /usr/include/x86_64-linux-gnu -internal-externc-isystem /include -internal-externc-isystem /usr/include -fmacro-prefix-map=/builds/wireshark/wireshark/= -fmacro-prefix-map=/builds/wireshark/wireshark/build/= -fmacro-prefix-map=../= -Wno-format-nonliteral -std=gnu17 -ferror-limit 19 -fvisibility=hidden -fwrapv -fwrapv-pointer -fstrict-flex-arrays=3 -stack-protector 2 -fstack-clash-protection -fcf-protection=full -fgnuc-version=4.2.1 -fskip-odr-check-in-gmf -fexceptions -fcolor-diagnostics -analyzer-output=html -faddrsig -fdwarf2-cfi-asm -o /builds/wireshark/wireshark/sbout/2026-08-26-100403-3659-1 -x c /builds/wireshark/wireshark/capinfos.c

Keyboard shortcuts:

- Use 'j/k' keys for keyboard navigation
- Use 'Shift+S' to show/hide relevant lines
- Use '?' to toggle this window

Close
Show only relevant lines Show control flow arrows

1 | /* capinfos.c
2 | * Reports capture file information including # of packets, duration, others
3 | *
4 | * Copyright 2004 Ian Schorr
5 | *
6 | * Wireshark - Network traffic analyzer
7 | * By Gerald Combs <gerald@wireshark.org>
8 | * Copyright 1998 Gerald Combs
9 | *
10 | * SPDX-License-Identifier: GPL-2.0-or-later
11 | */
12 |
13 | /*
14 | * 2009-09-19: jyoung
15 | *
16 | * New capinfos features
17 | *
18 | * Continue processing additional files after
19 | * a wiretap open failure. The new -C option
20 | * reverts to capinfos' original behavior which
21 | * is to cancel any further file processing at
22 | * first file open failure.
23 | *
24 | * Change the behavior of how the default display
25 | * of all infos is initiated. This gets rid of a
26 | * special post getopt() argument count test.
27 | *
28 | * Add new table output format (with related options)
29 | * This feature allows outputting the various infos
30 | * into a tab delimited text file, or to a comma
31 | * separated variables file (*.csv) instead of the
32 | * original "long" format.
33 | *
34 | * 2011-04-05: wmeier
35 | * behaviour changed: Upon exit capinfos will return
36 | * an error status if an error occurred at any
37 | * point during "continuous" file processing.
38 | * (Previously a success status was always
39 | * returned if the -C option was not used).
40 | *
41 | */
42 |
43 |
44 | #include <config.h>
45 | #define WS_LOG_DOMAIN"Main" LOG_DOMAIN_MAIN"Main"
46 |
47 | #include <stdio.h>
48 | #include <stdlib.h>
49 | #include <string.h>
50 | #include <stdarg.h>
51 | #include <locale.h>
52 |
53 | #include <ws_exit_codes.h>
54 | #include <wsutil/clopts_common.h>
55 | #include <wsutil/ws_getopt.h>
56 |
57 | #include <glib.h>
58 |
59 | #include <wiretap/wtap.h>
60 |
61 | #include <wsutil/cmdarg_err.h>
62 | #include <wsutil/filesystem.h>
63 | #include <app/application_flavor.h>
64 | #include <wsutil/file_compressed.h>
65 | #include <wsutil/privileges.h>
66 | #include <wsutil/version_info.h>
67 | #include <wsutil/report_message.h>
68 | #include <wiretap/wtap_opttypes.h>
69 |
70 | #ifdef HAVE_PLUGINS1
71 | #include <wsutil/plugins.h>
72 | #endif
73 |
74 | #include <wsutil/str_util.h>
75 | #include <wsutil/to_str.h>
76 | #include <wsutil/file_util.h>
77 | #include <wsutil/ws_assert.h>
78 | #include <wsutil/wslog.h>
79 |
80 | #include <gcrypt.h>
81 |
82 | #include "ui/failure_message.h"
83 |
84 | /*
85 | * By default capinfos now continues processing
86 | * the next filename if and when wiretap detects
87 | * a problem opening or reading a file.
88 | * Use the '-C' option to revert back to original
89 | * capinfos behavior which is to abort any
90 | * additional file processing at the first file
91 | * open or read failure.
92 | */
93 |
94 | static bool_Bool stop_after_failure;
95 |
96 | /*
97 | * table report variables
98 | */
99 |
100 | static bool_Bool long_report = true1; /* By default generate long report */
101 | static bool_Bool table_report_header = true1; /* Generate column header by default */
102 | static char field_separator = '\t'; /* Use TAB as field separator by default */
103 | static char quote_char = '\0'; /* Do NOT quote fields by default */
104 | static bool_Bool machine_readable; /* Display machine-readable numbers */
105 |
106 | /*
107 | * capinfos has the ability to report on a number of
108 | * various characteristics ("infos") for each input file.
109 | *
110 | * By default reporting of all info fields is enabled.
111 | *
112 | * Optionally the reporting of any specific info field
113 | * or combination of info fields can be enabled with
114 | * individual options.
115 | */
116 |
117 | static bool_Bool report_all_infos = true1; /* Report all infos */
118 |
119 | static bool_Bool cap_file_type = true1; /* Report capture type */
120 | static bool_Bool cap_file_encap = true1; /* Report encapsulation */
121 | static bool_Bool cap_snaplen = true1; /* Packet size limit (snaplen)*/
122 | static bool_Bool cap_packet_count = true1; /* Report packet count */
123 | static bool_Bool cap_file_size = true1; /* Report file size */
124 | static bool_Bool cap_comment = true1; /* Display the capture comment */
125 | static bool_Bool cap_file_more_info = true1; /* Report more file info */
126 | static bool_Bool cap_file_idb = true1; /* Report Interface info */
127 | static bool_Bool cap_file_nrb = true1; /* Report Name Resolution Block info */
128 | static bool_Bool cap_file_dsb = true1; /* Report Decryption Secrets Block info */
129 |
130 | static bool_Bool cap_data_size = true1; /* Report packet byte size */
131 | static bool_Bool cap_duration = true1; /* Report capture duration */
132 | static bool_Bool cap_earliest_packet_time = true1; /* Report timestamp of earliest packet */
133 | static bool_Bool cap_latest_packet_time = true1; /* Report timestamp of latest packet */
134 | static bool_Bool time_as_secs; /* Report time values as raw seconds */
135 |
136 | static bool_Bool cap_data_rate_byte = true1; /* Report data rate bytes/sec */
137 | static bool_Bool cap_data_rate_bit = true1; /* Report data rate bites/sec */
138 | static bool_Bool cap_packet_size = true1; /* Report average packet size */
139 | static bool_Bool cap_packet_rate = true1; /* Report average packet rate */
140 | static bool_Bool cap_order = true1; /* Report if packets are in chronological order (True/False) */
141 | static bool_Bool pkt_comments = true1; /* Report individual packet comments */
142 |
143 | static bool_Bool cap_file_hashes = true1; /* Calculate file hashes */
144 |
145 | // Strongest to weakest
146 | #define HASH_SIZE_SHA25632 32
147 | #define HASH_SIZE_SHA120 20
148 |
149 | #define HASH_STR_SIZE(65) (65) /* Max hash size * 2 + '\0' */
150 | #define HASH_BUF_SIZE(1024 * 1024) (1024 * 1024)
151 |
152 |
153 | static char file_sha256[HASH_STR_SIZE(65)];
154 | static char file_sha1[HASH_STR_SIZE(65)];
155 |
156 | static char *hash_buf;
157 | static gcry_md_hd_t hd;
158 |
159 | static unsigned int num_ipv4_addresses;
160 | static unsigned int num_ipv6_addresses;
161 | static unsigned int num_decryption_secrets;
162 |
163 | /*
164 | * If we have at least two packets with time stamps, and they're not in
165 | * order - i.e., the later packet has a time stamp older than the earlier
166 | * packet - the time stamps are known not to be in order.
167 | *
168 | * If every packet has a time stamp, and they're all in order, the time
169 | * stamp is known to be in order.
170 | *
171 | * Otherwise, we have no idea.
172 | */
173 | typedef enum {
174 | IN_ORDER,
175 | NOT_IN_ORDER,
176 | ORDER_UNKNOWN
177 | } order_t;
178 |
179 | typedef struct _pkt_cmt {
180 | uint32_t recno;
181 | char *cmt;
182 | struct _pkt_cmt *next;
183 | } pkt_cmt;
184 |
185 | typedef struct _capture_info {
186 | const char *filename;
187 | uint16_t file_type;
188 | ws_compression_type compression_type;
189 | int file_encap;
190 | int file_tsprec;
191 | wtap *wth;
192 | int64_t filesize;
193 | uint64_t packet_bytes;
194 | bool_Bool times_known;
195 | nstime_t earliest_packet_time;
196 | int earliest_packet_time_tsprec;
197 | nstime_t latest_packet_time;
198 | int latest_packet_time_tsprec;
199 | uint32_t packet_count;
200 | bool_Bool snap_set; /* If set in capture file header */
201 | uint32_t snaplen; /* value from the capture file header */
202 | uint32_t snaplen_min_inferred; /* If caplen < len for 1 or more rcds */
203 | uint32_t snaplen_max_inferred; /* ... */
204 | bool_Bool drops_known;
205 | uint32_t drop_count;
206 |
207 | nstime_t duration;
208 | int duration_tsprec;
209 | double packet_rate;
210 | double packet_size;
211 | double data_rate; /* in bytes/s */
212 | bool_Bool know_order;
213 | order_t order;
214 |
215 | int *encap_counts; /* array of per_packet encap counts; array has one entry per wtap_encap type */
216 | pkt_cmt *pkt_cmts; /* list of packet comments */
217 |
218 | unsigned int num_interfaces; /* number of IDBs, and thus size of interface_packet_counts array */
219 | GArray *interface_packet_counts; /* array of per_packet interface_id counts; one entry per file IDB */
220 | uint32_t pkt_interface_id_unknown; /* counts if packet interface_id didn't match a known one */
221 | GArray *idb_info_strings; /* array of IDB info strings */
222 | } capture_info;
223 |
224 | static char *decimal_point;
225 |
226 | static void
227 | enable_all_infos(void)
228 | {
229 | report_all_infos = true1;
230 |
231 | cap_file_type = true1;
232 | cap_file_encap = true1;
233 | cap_snaplen = true1;
234 | cap_packet_count = true1;
235 | cap_file_size = true1;
236 | cap_comment = true1;
237 | pkt_comments = true1;
238 | cap_file_more_info = true1;
239 | cap_file_idb = true1;
240 | cap_file_nrb = true1;
241 | cap_file_dsb = true1;
242 |
243 | cap_data_size = true1;
244 | cap_duration = true1;
245 | cap_earliest_packet_time = true1;
246 | cap_latest_packet_time = true1;
247 | cap_order = true1;
248 |
249 | cap_data_rate_byte = true1;
250 | cap_data_rate_bit = true1;
251 | cap_packet_size = true1;
252 | cap_packet_rate = true1;
253 |
254 | cap_file_hashes = true1;
255 | }
256 |
257 | static void
258 | disable_all_infos(void)
259 | {
260 | report_all_infos = false0;
261 |
262 | cap_file_type = false0;
263 | cap_file_encap = false0;
264 | cap_snaplen = false0;
265 | cap_packet_count = false0;
266 | cap_file_size = false0;
267 | cap_comment = false0;
268 | pkt_comments = false0;
269 | cap_file_more_info = false0;
270 | cap_file_idb = false0;
271 | cap_file_nrb = false0;
272 | cap_file_dsb = false0;
273 |
274 | cap_data_size = false0;
275 | cap_duration = false0;
276 | cap_earliest_packet_time = false0;
277 | cap_latest_packet_time = false0;
278 | cap_order = false0;
279 |
280 | cap_data_rate_byte = false0;
281 | cap_data_rate_bit = false0;
282 | cap_packet_size = false0;
283 | cap_packet_rate = false0;
284 |
285 | cap_file_hashes = false0;
286 | }
287 |
288 | static const char *
289 | order_string(order_t order)
290 | {
291 | switch (order) {
292 |
293 | case IN_ORDER:
294 | return "True";
295 |
296 | case NOT_IN_ORDER:
297 | return "False";
298 |
299 | case ORDER_UNKNOWN:
300 | return "Unknown";
301 |
302 | default:
303 | return "???"; /* "cannot happen" (the next step is "Profit!") */
304 | }
305 | }
306 |
307 | static char *
308 | absolute_time_string(nstime_t *timer, int tsprecision, capture_info *cf_info)
309 | {
310 | /*
311 | * https://web.archive.org/web/20120513133703/http://www.idrbt.ac.in/publications/workingpapers/Working%20Paper%20No.%209.pdf
312 | *
313 | * says:
314 | *
315 | * A 64-bit Unix time would be safe for the indefinite future, as
316 | * this variable would not overflow until 2**63 or
317 | * 9,223,372,036,854,775,808 (over nine quintillion) seconds
318 | * after the beginning of the Unix epoch - corresponding to
319 | * GMT 15:30:08, Sunday, 4th December, 292,277,026,596.
320 | *
321 | * So, if we're displaying the time as YYYY-MM-DD HH:MM:SS.SSSSSSSSS,
322 | * we'll have the buffer be large enough for a date of the format
323 | * 292277026596-MM-DD HH:MM:SS.SSSSSSSSS, which is the biggest value
324 | * you'll get with a 64-bit time_t and a nanosecond-resolution
325 | * fraction-of-a-second.
326 | *
327 | * That's 12+1+2+1+2+1+2+1+2+2+2+1+9+1, including the terminating
328 | * \0, or 39.
329 | *
330 | * If we're displaying the time as epoch time, and the time is
331 | * unsigned, 2^64-1 is 18446744073709551615, so the buffer has
332 | * to be big enough for 18446744073709551615.999999999. That's
333 | * 20+1+9+1, including the terminating '\0', or 31. If it's
334 | * signed, 2^63 is 9223372036854775808, so the buffer has to
335 | * be big enough for -9223372036854775808.999999999, which is
336 | * again 20+1+9+1, or 31.
337 | *
338 | * So we go with 39.
339 | */
340 | static char time_string_buf[39];
341 |
342 | if (cf_info->times_known && cf_info->packet_count > 0) {
343 | if (time_as_secs) {
344 | display_epoch_time(time_string_buf, sizeof time_string_buf, timer, tsprecision);
345 | } else {
346 | format_nstime_as_iso8601(time_string_buf, sizeof time_string_buf, timer, decimal_point, true1, tsprecision);
347 | }
348 | } else {
349 | snprintf(time_string_buf, sizeof time_string_buf, "n/a");
350 | }
351 | return time_string_buf;
352 | }
353 |
354 | static char *
355 | relative_time_string(nstime_t *timer, int tsprecision, capture_info *cf_info, bool_Bool want_seconds)
356 | {
357 | const char *second = want_seconds ? " second" : "";
358 | const char *plural = want_seconds ? "s" : "";
359 | /*
360 | * If we're displaying the time as epoch time, and the time is
361 | * unsigned, 2^64-1 is 18446744073709551615, so the buffer has
362 | * to be big enough for "18446744073709551615.999999999 seconds".
363 | * That's 20+1+9+1+7+1, including the terminating '\0', or 39.
364 | * If it's signed, 2^63 is 9223372036854775808, so the buffer has to
365 | * be big enough for "-9223372036854775808.999999999 seconds",
366 | * which is again 20+1+9+1+7+1, or 39.
367 | */
368 | static char time_string_buf[39];
369 |
370 | if (cf_info->times_known && cf_info->packet_count > 0) {
371 | char *ptr;
372 | size_t remaining;
373 | int num_bytes;
374 |
375 | ptr = time_string_buf;
376 | remaining = sizeof time_string_buf;
377 | num_bytes = snprintf(ptr, remaining,
378 | "%"PRId64"l" "d",
379 | (int64_t)timer->secs);
380 | if (num_bytes < 0) {
381 | /*
382 | * That got an error.
383 | * Not much else we can do.
384 | */
385 | snprintf(ptr, remaining, "snprintf() failed");
386 | return time_string_buf;
387 | }
388 | if ((unsigned int)num_bytes >= remaining) {
389 | /*
390 | * That filled up or would have overflowed the buffer.
391 | * Nothing more we can do.
392 | */
393 | return time_string_buf;
394 | }
395 | ptr += num_bytes;
396 | remaining -= num_bytes;
397 |
398 | if (tsprecision != 0) {
399 | /*
400 | * Append the fractional part.
401 | */
402 | num_bytes = format_fractional_part_nsecs(ptr, remaining, timer->nsecs, decimal_point, tsprecision);
403 | if ((unsigned int)num_bytes >= remaining) {
404 | /*
405 | * That filled up or would have overflowed the buffer.
406 | * Nothing more we can do.
407 | */
408 | return time_string_buf;
409 | }
410 | ptr += num_bytes;
411 | remaining -= num_bytes;
412 | }
413 |
414 | /*
415 | * Append the units.
416 | */
417 | snprintf(ptr, remaining, "%s%s",
418 | second,
419 | timer->secs == 1 ? "" : plural);
420 |
421 | return time_string_buf;
422 | }
423 |
424 | snprintf(time_string_buf, sizeof time_string_buf, "n/a");
425 | return time_string_buf;
426 | }
427 |
428 | static void print_value(const char *text_p1, int width, const char *text_p2, double value)
429 | {
430 | if (value > 0.0)
431 | printf("%s%.*f%s\n", text_p1, width, value, text_p2);
432 | else
433 | printf("%sn/a\n", text_p1);
434 | }
435 |
436 | /* multi-line comments would conflict with the formatting that capinfos uses
437 | we replace linefeeds with spaces */
438 | static void
439 | string_replace_newlines(char *str)
440 | {
441 | char *p;
442 |
443 | if (str) {
444 | p = str;
445 | while (*p != '\0') {
446 | if (*p == '\n')
447 | *p = ' ';
448 | if (*p == '\r')
449 | *p = ' ';
450 | p++;
451 | }
452 | }
453 | }
454 |
455 | static void
456 | show_option_string(const char *prefix, const char *option_str)
457 | {
458 | char *str;
459 |
460 | if (option_str != NULL((void*)0) && option_str[0] != '\0') {
461 | str = g_strdup(option_str)g_strdup_inline (option_str);
462 | string_replace_newlines(str);
463 | printf("%s%s\n", prefix, str);
464 | g_free(str)(__builtin_object_size ((str), 0) != ((size_t) - 1)) ? g_free_sized (str, __builtin_object_size ((str), 0)) : (g_free) (str);
465 | }
466 | }
467 |
468 | static void
469 | print_stats(const char *filename, capture_info *cf_info)
470 | {
471 | const char *file_type_string, *file_encap_string;
472 | char *size_string;
473 | pkt_cmt *p, *prev;
474 |
475 | /* Build printable strings for various stats */
476 | if (machine_readable) {
477 | file_type_string = wtap_file_type_subtype_name(cf_info->file_type);
478 | file_encap_string = wtap_encap_name(cf_info->file_encap);
479 | }
480 | else {
481 | file_type_string = wtap_file_type_subtype_description(cf_info->file_type);
482 | file_encap_string = wtap_encap_description(cf_info->file_encap);
483 | }
484 |
485 | if (filename) printf ("File name: %s\n", filename);
486 | if (cap_file_type) {
487 | const char *compression_type_description;
488 | compression_type_description = ws_compression_type_description(cf_info->compression_type);
489 | if (compression_type_description == NULL((void*)0))
490 | printf ("File type: %s\n",
491 | file_type_string);
492 | else
493 | printf ("File type: %s (%s)\n",
494 | file_type_string, compression_type_description);
495 | }
496 | if (cap_file_encap) {
497 | printf ("File encapsulation: %s\n", file_encap_string);
498 | if (cf_info->file_encap == WTAP_ENCAP_PER_PACKET-1) {
499 | int i;
500 | printf ("Encapsulation in use by packets (# of pkts):\n");
501 | for (i=0; i<WTAP_NUM_ENCAP_TYPESwtap_get_num_encap_types(); i++) {
502 | if (cf_info->encap_counts[i] > 0)
503 | printf(" %s (%d)\n",
504 | wtap_encap_description(i), cf_info->encap_counts[i]);
505 | }
506 | }
507 | }
508 | if (cap_file_more_info) {
509 | printf ("File timestamp precision: %s (%d)\n",
510 | wtap_tsprec_string(cf_info->file_tsprec), cf_info->file_tsprec);
511 | }
512 |
513 | if (cap_snaplen && cf_info->snap_set)
514 | printf ("Packet size limit: file hdr: %u bytes\n", cf_info->snaplen);
515 | else if (cap_snaplen && !cf_info->snap_set)
516 | printf ("Packet size limit: file hdr: (not set)\n");
517 | if (cf_info->snaplen_max_inferred > 0) {
518 | if (cf_info->snaplen_min_inferred == cf_info->snaplen_max_inferred)
519 | printf ("Packet size limit: inferred: %u bytes\n", cf_info->snaplen_min_inferred);
520 | else
521 | printf ("Packet size limit: inferred: %u bytes - %u bytes (range)\n",
522 | cf_info->snaplen_min_inferred, cf_info->snaplen_max_inferred);
523 | }
524 | if (cap_packet_count) {
525 | printf ("Number of packets: ");
526 | if (machine_readable) {
527 | printf ("%u\n", cf_info->packet_count);
528 | } else {
529 | size_string = format_size(cf_info->packet_count, FORMAT_SIZE_UNIT_NONE, 0)format_size_wmem(((void*)0), cf_info->packet_count, FORMAT_SIZE_UNIT_NONE , 0);
530 | printf ("%s\n", size_string);
531 | g_free(size_string)(__builtin_object_size ((size_string), 0) != ((size_t) - 1)) ? g_free_sized (size_string, __builtin_object_size ((size_string ), 0)) : (g_free) (size_string);
532 | }
533 | }
534 | if (cap_file_size) {
535 | printf ("File size: ");
536 | if (machine_readable) {
537 | printf ("%" PRId64"l" "d" " bytes\n", cf_info->filesize);
538 | } else {
539 | size_string = format_size(cf_info->filesize, FORMAT_SIZE_UNIT_BYTES, 0)format_size_wmem(((void*)0), cf_info->filesize, FORMAT_SIZE_UNIT_BYTES , 0);
540 | printf ("%s\n", size_string);
541 | g_free(size_string)(__builtin_object_size ((size_string), 0) != ((size_t) - 1)) ? g_free_sized (size_string, __builtin_object_size ((size_string ), 0)) : (g_free) (size_string);
542 | }
543 | }
544 | if (cap_data_size) {
545 | printf ("Data size: ");
546 | if (machine_readable) {
547 | printf ("%" PRIu64"l" "u" " bytes\n", cf_info->packet_bytes);
548 | } else {
549 | size_string = format_size(cf_info->packet_bytes, FORMAT_SIZE_UNIT_BYTES, 0)format_size_wmem(((void*)0), cf_info->packet_bytes, FORMAT_SIZE_UNIT_BYTES , 0);
550 | printf ("%s\n", size_string);
551 | g_free(size_string)(__builtin_object_size ((size_string), 0) != ((size_t) - 1)) ? g_free_sized (size_string, __builtin_object_size ((size_string ), 0)) : (g_free) (size_string);
552 | }
553 | }
554 | if (cf_info->times_known) {
555 | if (cap_duration) /* XXX - shorten to hh:mm:ss */
556 | printf("Capture duration: %s\n", relative_time_string(&cf_info->duration, cf_info->duration_tsprec, cf_info, true1));
557 | if (cap_earliest_packet_time)
558 | printf("Earliest packet time: %s\n", absolute_time_string(&cf_info->earliest_packet_time, cf_info->earliest_packet_time_tsprec, cf_info));
559 | if (cap_latest_packet_time)
560 | printf("Latest packet time: %s\n", absolute_time_string(&cf_info->latest_packet_time, cf_info->latest_packet_time_tsprec, cf_info));
561 | if (cap_data_rate_byte) {
562 | printf("Data byte rate: ");
563 | if (machine_readable) {
564 | print_value("", 2, " bytes/sec", cf_info->data_rate);
565 | } else {
566 | size_string = format_size((int64_t)cf_info->data_rate, FORMAT_SIZE_UNIT_BYTES_S, 0)format_size_wmem(((void*)0), (int64_t)cf_info->data_rate, FORMAT_SIZE_UNIT_BYTES_S , 0);
567 | printf ("%s\n", size_string);
568 | g_free(size_string)(__builtin_object_size ((size_string), 0) != ((size_t) - 1)) ? g_free_sized (size_string, __builtin_object_size ((size_string ), 0)) : (g_free) (size_string);
569 | }
570 | }
571 | if (cap_data_rate_bit) {
572 | printf("Data bit rate: ");
573 | if (machine_readable) {
574 | print_value("", 2, " bits/sec", cf_info->data_rate*8);
575 | } else {
576 | size_string = format_size((int64_t)(cf_info->data_rate*8), FORMAT_SIZE_UNIT_BITS_S, 0)format_size_wmem(((void*)0), (int64_t)(cf_info->data_rate* 8), FORMAT_SIZE_UNIT_BITS_S, 0);
577 | printf ("%s\n", size_string);
578 | g_free(size_string)(__builtin_object_size ((size_string), 0) != ((size_t) - 1)) ? g_free_sized (size_string, __builtin_object_size ((size_string ), 0)) : (g_free) (size_string);
579 | }
580 | }
581 | }
582 | if (cap_packet_size) printf("Average packet size: %.2f bytes\n", cf_info->packet_size);
583 | if (cf_info->times_known) {
584 | if (cap_packet_rate) {
585 | printf("Average packet rate: ");
586 | if (machine_readable) {
587 | print_value("", 2, " packets/sec", cf_info->packet_rate);
588 | } else {
589 | size_string = format_size((int64_t)cf_info->packet_rate, FORMAT_SIZE_UNIT_PACKETS_S, 0)format_size_wmem(((void*)0), (int64_t)cf_info->packet_rate , FORMAT_SIZE_UNIT_PACKETS_S, 0);
590 | printf ("%s\n", size_string);
591 | g_free(size_string)(__builtin_object_size ((size_string), 0) != ((size_t) - 1)) ? g_free_sized (size_string, __builtin_object_size ((size_string ), 0)) : (g_free) (size_string);
592 | }
593 | }
594 | }
595 | if (cap_file_hashes) {
596 | printf ("SHA256: %s\n", file_sha256);
597 | printf ("SHA1: %s\n", file_sha1);
598 | }
599 | if (cap_order) printf ("Strict time order: %s\n", order_string(cf_info->order));
600 |
601 | bool_Bool has_multiple_sections = (wtap_file_get_num_shbs(cf_info->wth) > 1);
602 |
603 | for (unsigned int section_number = 0;
604 | section_number < wtap_file_get_num_shbs(cf_info->wth);
605 | section_number++) {
606 | wtap_block_t shb;
607 |
608 | // If we have more than one section, add headers for each section.
609 | if (has_multiple_sections)
610 | printf("Section %u:\n\n", section_number);
611 |
612 | shb = wtap_file_get_shb(cf_info->wth, section_number);
613 | if (shb != NULL((void*)0)) {
614 | if (cap_file_more_info) {
615 | char *str;
616 |
617 | if (wtap_block_get_string_option_value(shb, OPT_SHB_HARDWARE2, &str) == WTAP_OPTTYPE_SUCCESS)
618 | show_option_string("Capture hardware: ", str);
619 | if (wtap_block_get_string_option_value(shb, OPT_SHB_OS3, &str) == WTAP_OPTTYPE_SUCCESS)
620 | show_option_string("Capture oper-sys: ", str);
621 | if (wtap_block_get_string_option_value(shb, OPT_SHB_USERAPPL4, &str) == WTAP_OPTTYPE_SUCCESS)
622 | show_option_string("Capture application: ", str);
623 | }
624 | if (cap_comment) {
625 | unsigned int i;
626 | char *str;
627 |
628 | for (i = 0; wtap_block_get_nth_string_option_value(shb, OPT_COMMENT1, i, &str) == WTAP_OPTTYPE_SUCCESS; i++) {
629 | show_option_string("Capture comment: ", str);
630 | }
631 | }
632 | }
633 | }
634 |
635 | if (pkt_comments && cf_info->pkt_cmts != NULL((void*)0)) {
636 | for (p = cf_info->pkt_cmts; p != NULL((void*)0); prev = p, p = p->next, g_free(prev)(__builtin_object_size ((prev), 0) != ((size_t) - 1)) ? g_free_sized (prev, __builtin_object_size ((prev), 0)) : (g_free) (prev)) {
637 | if (machine_readable){
638 | char *escaped_cmt = g_strescape(p->cmt, NULL((void*)0));
639 | printf("Packet %u Comment: %s\n", p->recno, escaped_cmt);
640 | g_free(escaped_cmt)(__builtin_object_size ((escaped_cmt), 0) != ((size_t) - 1)) ? g_free_sized (escaped_cmt, __builtin_object_size ((escaped_cmt ), 0)) : (g_free) (escaped_cmt);
641 | } else {
642 | printf("Packet %u Comment: %s\n", p->recno, p->cmt);
643 | }
644 | g_free(p->cmt)(__builtin_object_size ((p->cmt), 0) != ((size_t) - 1)) ? g_free_sized (p->cmt, __builtin_object_size ((p->cmt), 0)) : (g_free ) (p->cmt);
645 | }
646 | cf_info->pkt_cmts = NULL((void*)0);
647 | }
648 |
649 | if (cap_file_idb && cf_info->num_interfaces != 0) {
650 | unsigned int i;
651 | ws_assert(cf_info->num_interfaces == cf_info->idb_info_strings->len)do { if ((1) && !(cf_info->num_interfaces == cf_info ->idb_info_strings->len)) ws_log_fatal_full("Main", LOG_LEVEL_ERROR , "capinfos.c", 651, __func__, "assertion failed: %s", "cf_info->num_interfaces == cf_info->idb_info_strings->len" ); } while (0);
652 | printf ("Number of interfaces in file: %u\n", cf_info->num_interfaces);
653 | for (i = 0; i < cf_info->idb_info_strings->len; i++) {
654 | char *s = g_array_index(cf_info->idb_info_strings, char*, i)(((char**) (void *) (cf_info->idb_info_strings)->data) [ (i)]);
655 | uint32_t packet_count = 0;
656 | if (i < cf_info->interface_packet_counts->len)
657 | packet_count = g_array_index(cf_info->interface_packet_counts, uint32_t, i)(((uint32_t*) (void *) (cf_info->interface_packet_counts)-> data) [(i)]);
658 | printf ("Interface #%u info:\n", i);
659 | printf ("%s", s);
660 | printf (" Number of packets = %u\n", packet_count);
661 | }
662 | }
663 |
664 | if (cap_file_nrb) {
665 | if (num_ipv4_addresses != 0)
666 | printf ("Number of resolved IPv4 addresses in file: %u\n", num_ipv4_addresses);
667 | if (num_ipv6_addresses != 0)
668 | printf ("Number of resolved IPv6 addresses in file: %u\n", num_ipv6_addresses);
669 | }
670 | if (cap_file_dsb) {
671 | if (num_decryption_secrets != 0)
672 | printf ("Number of decryption secrets in file: %u\n", num_decryption_secrets);
673 | }
674 | }
675 |
676 | static void
677 | putsep(void)
678 | {
679 | if (field_separator) putchar(field_separator);
680 | }
681 |
682 | static void
683 | putquote(void)
684 | {
685 | if (quote_char) putchar(quote_char);
686 | }
687 |
688 | static void G_GNUC_PRINTF(1, 2)__attribute__((__format__ (__printf__, 1, 2)))
689 | print_stats_table_header_label(const char *fmt, ...)
690 | {
691 | va_list ap;
692 |
693 | putsep();
694 | putquote();
695 | va_start(ap, fmt)__builtin_va_start(ap, fmt);
696 | vprintf(fmt, ap);
697 | va_end(ap)__builtin_va_end(ap);
698 | putquote();
699 | }
700 |
701 | static void
702 | print_stats_table_header(capture_info *cf_info)
703 | {
704 | pkt_cmt *p;
705 |
706 | putquote();
707 | printf("File name");
708 | putquote();
709 |
710 | if (cap_file_type) print_stats_table_header_label("File type");
711 | if (cap_file_encap) print_stats_table_header_label("File encapsulation");
712 | if (cap_file_more_info) print_stats_table_header_label("File time precision");
713 | if (cap_snaplen) {
714 | print_stats_table_header_label("Packet size limit");
715 | print_stats_table_header_label("Packet size limit min (inferred)");
716 | print_stats_table_header_label("Packet size limit max (inferred)");
717 | }
718 | if (cap_packet_count) print_stats_table_header_label("Number of packets");
719 | if (cap_file_size) print_stats_table_header_label("File size (bytes)");
720 | if (cap_data_size) print_stats_table_header_label("Data size (bytes)");
721 | if (cap_duration) print_stats_table_header_label("Capture duration (seconds)");
722 | if (cap_earliest_packet_time) print_stats_table_header_label("Start time");
723 | if (cap_latest_packet_time) print_stats_table_header_label("End time");
724 | if (cap_data_rate_byte) print_stats_table_header_label("Data byte rate (bytes/sec)");
725 | if (cap_data_rate_bit) print_stats_table_header_label("Data bit rate (bits/sec)");
726 | if (cap_packet_size) print_stats_table_header_label("Average packet size (bytes)");
727 | if (cap_packet_rate) print_stats_table_header_label("Average packet rate (packets/sec)");
728 | if (cap_file_hashes) {
729 | print_stats_table_header_label("SHA256");
730 | print_stats_table_header_label("SHA1");
731 | }
732 | if (cap_order) print_stats_table_header_label("Strict time order");
733 | if (cap_file_more_info) {
734 | print_stats_table_header_label("Capture hardware");
735 | print_stats_table_header_label("Capture oper-sys");
736 | print_stats_table_header_label("Capture application");
737 | }
738 | if (cap_comment) print_stats_table_header_label("Capture comment");
739 |
740 | if (pkt_comments && cf_info->pkt_cmts != NULL((void*)0)) {
741 | for (p = cf_info->pkt_cmts; p != NULL((void*)0); p = p->next) {
742 | print_stats_table_header_label("Packet %u Comment", p->recno);
743 | }
744 | }
745 |
746 | printf("\n");
747 | }
748 |
749 | static void
750 | print_stats_table(const char *filename, capture_info *cf_info)
751 | {
752 | const char *file_type_string, *file_encap_string;
753 | pkt_cmt *p, *prev;
754 |
755 | /* Build printable strings for various stats */
756 | file_type_string = wtap_file_type_subtype_name(cf_info->file_type);
757 | file_encap_string = wtap_encap_name(cf_info->file_encap);
758 |
759 | if (filename) {
760 | putquote();
761 | printf("%s", filename);
762 | putquote();
763 | }
764 |
765 | if (cap_file_type) {
766 | putsep();
767 | putquote();
768 | printf("%s", file_type_string);
769 | putquote();
770 | }
771 |
772 | /* ToDo: If WTAP_ENCAP_PER_PACKET, show the list of encapsulations encountered;
773 | * Output a line for each different encap with all fields repeated except
774 | * the encapsulation field which has "Per Packet: ..." for each
775 | * encapsulation type seen ?
776 | */
777 | if (cap_file_encap) {
778 | putsep();
779 | putquote();
780 | printf("%s", file_encap_string);
781 | putquote();
782 | }
783 |
784 | if (cap_file_more_info) {
785 | putsep();
786 | putquote();
787 | printf("%s", wtap_tsprec_string(cf_info->file_tsprec));
788 | putquote();
789 | }
790 |
791 | if (cap_snaplen) {
792 | putsep();
793 | putquote();
794 | if (cf_info->snap_set)
795 | printf("%u", cf_info->snaplen);
796 | else
797 | printf("(not set)");
798 | putquote();
799 | if (cf_info->snaplen_max_inferred > 0) {
800 | putsep();
801 | putquote();
802 | printf("%u", cf_info->snaplen_min_inferred);
803 | putquote();
804 | putsep();
805 | putquote();
806 | printf("%u", cf_info->snaplen_max_inferred);
807 | putquote();
808 | }
809 | else {
810 | putsep();
811 | putquote();
812 | printf("n/a");
813 | putquote();
814 | putsep();
815 | putquote();
816 | printf("n/a");
817 | putquote();
818 | }
819 | }
820 |
821 | if (cap_packet_count) {
822 | putsep();
823 | putquote();
824 | printf("%u", cf_info->packet_count);
825 | putquote();
826 | }
827 |
828 | if (cap_file_size) {
829 | putsep();
830 | putquote();
831 | printf("%" PRId64"l" "d", cf_info->filesize);
832 | putquote();
833 | }
834 |
835 | if (cap_data_size) {
836 | putsep();
837 | putquote();
838 | printf("%" PRIu64"l" "u", cf_info->packet_bytes);
839 | putquote();
840 | }
841 |
842 | if (cap_duration) {
843 | putsep();
844 | putquote();
845 | printf("%s", relative_time_string(&cf_info->duration, cf_info->duration_tsprec, cf_info, false0));
846 | putquote();
847 | }
848 |
849 | if (cap_earliest_packet_time) {
850 | putsep();
851 | putquote();
852 | printf("%s", absolute_time_string(&cf_info->earliest_packet_time, cf_info->earliest_packet_time_tsprec, cf_info));
853 | putquote();
854 | }
855 |
856 | if (cap_latest_packet_time) {
857 | putsep();
858 | putquote();
859 | printf("%s", absolute_time_string(&cf_info->latest_packet_time, cf_info->latest_packet_time_tsprec, cf_info));
860 | putquote();
861 | }
862 |
863 | if (cap_data_rate_byte) {
864 | putsep();
865 | putquote();
866 | if (cf_info->times_known)
867 | printf("%.2f", cf_info->data_rate);
868 | else
869 | printf("n/a");
870 | putquote();
871 | }
872 |
873 | if (cap_data_rate_bit) {
874 | putsep();
875 | putquote();
876 | if (cf_info->times_known)
877 | printf("%.2f", cf_info->data_rate*8);
878 | else
879 | printf("n/a");
880 | putquote();
881 | }
882 |
883 | if (cap_packet_size) {
884 | putsep();
885 | putquote();
886 | printf("%.2f", cf_info->packet_size);
887 | putquote();
888 | }
889 |
890 | if (cap_packet_rate) {
891 | putsep();
892 | putquote();
893 | if (cf_info->times_known)
894 | printf("%.2f", cf_info->packet_rate);
895 | else
896 | printf("n/a");
897 | putquote();
898 | }
899 |
900 | if (cap_file_hashes) {
901 | putsep();
902 | putquote();
903 | printf("%s", file_sha256);
904 | putquote();
905 |
906 | putsep();
907 | putquote();
908 | printf("%s", file_sha1);
909 | putquote();
910 | }
911 |
912 | if (cap_order) {
913 | putsep();
914 | putquote();
915 | printf("%s", order_string(cf_info->order));
916 | putquote();
917 | }
918 |
919 | for (unsigned section_number = 0;
920 | section_number < wtap_file_get_num_shbs(cf_info->wth);
921 | section_number++) {
922 | wtap_block_t shb;
923 |
924 | shb = wtap_file_get_shb(cf_info->wth, section_number);
925 | if (cap_file_more_info) {
926 | char *str;
927 |
928 | putsep();
929 | putquote();
930 | if (wtap_block_get_string_option_value(shb, OPT_SHB_HARDWARE2, &str) == WTAP_OPTTYPE_SUCCESS) {
931 | printf("%s", str);
932 | }
933 | putquote();
934 |
935 | putsep();
936 | putquote();
937 | if (wtap_block_get_string_option_value(shb, OPT_SHB_OS3, &str) == WTAP_OPTTYPE_SUCCESS) {
938 | printf("%s", str);
939 | }
940 | putquote();
941 |
942 | putsep();
943 | putquote();
944 | if (wtap_block_get_string_option_value(shb, OPT_SHB_USERAPPL4, &str) == WTAP_OPTTYPE_SUCCESS) {
945 | printf("%s", str);
946 | }
947 | putquote();
948 | }
949 |
950 | /*
951 | * One might argue that the following is silly to put into a table format,
952 | * but oh well note that there may be *more than one* of each of these types
953 | * of options. To mitigate some of the potential silliness the if(cap_comment)
954 | * block is moved AFTER the if(cap_file_more_info) block. This will make any
955 | * comments the last item(s) in each row. We now have a new -K option to
956 | * disable cap_comment to more easily manage the potential silliness.
957 | * Potential silliness includes multiple comments (therefore resulting in
958 | * more than one additional column and/or comments with embedded newlines
959 | * and/or possible delimiters).
960 | *
961 | * To mitigate embedded newlines and other special characters, use -M
962 | */
963 | if (cap_comment) {
964 | unsigned int i;
965 | char *opt_comment;
966 | bool_Bool have_cap = false0;
967 |
968 | for (i = 0; wtap_block_get_nth_string_option_value(shb, OPT_COMMENT1, i, &opt_comment) == WTAP_OPTTYPE_SUCCESS; i++) {
969 | have_cap = true1;
970 | putsep();
971 | putquote();
972 | if (machine_readable){
973 | opt_comment = g_strescape(opt_comment, NULL((void*)0));
974 | printf("%s", opt_comment);
975 | g_free(opt_comment)(__builtin_object_size ((opt_comment), 0) != ((size_t) - 1)) ? g_free_sized (opt_comment, __builtin_object_size ((opt_comment ), 0)) : (g_free) (opt_comment);
976 | } else {
977 | printf("%s", opt_comment);
978 | }
979 | putquote();
980 | }
981 | if(!have_cap) {
982 | /* Maintain column alignment when we have no OPT_COMMENT */
983 | putsep();
984 | putquote();
985 | putquote();
986 | }
987 | }
988 |
989 | }
990 |
991 | if (pkt_comments && cf_info->pkt_cmts != NULL((void*)0)) {
992 | for(p = cf_info->pkt_cmts; p != NULL((void*)0); prev = p, p = p->next, g_free(prev)(__builtin_object_size ((prev), 0) != ((size_t) - 1)) ? g_free_sized (prev, __builtin_object_size ((prev), 0)) : (g_free) (prev)) {
993 | putsep();
994 | putquote();
995 | if (machine_readable) {
996 | char *escaped_cmt = g_strescape(p->cmt, NULL((void*)0));
997 | printf("%s", escaped_cmt);
998 | g_free(escaped_cmt)(__builtin_object_size ((escaped_cmt), 0) != ((size_t) - 1)) ? g_free_sized (escaped_cmt, __builtin_object_size ((escaped_cmt ), 0)) : (g_free) (escaped_cmt);
999 | } else {
1000 | printf("%s", p->cmt);
1001 | }
1002 | g_free(p->cmt)(__builtin_object_size ((p->cmt), 0) != ((size_t) - 1)) ? g_free_sized (p->cmt, __builtin_object_size ((p->cmt), 0)) : (g_free ) (p->cmt);
1003 | putquote();
1004 | }
1005 | cf_info->pkt_cmts = NULL((void*)0);
1006 | }
1007 |
1008 | printf("\n");
1009 | }
1010 |
1011 | static void
1012 | cleanup_capture_info(capture_info *cf_info)
1013 | {
1014 | pkt_cmt *p, *prev;
1015 | unsigned int i;
1016 | ws_assert(cf_info != NULL)do { if ((1) && !(cf_info != ((void*)0))) ws_log_fatal_full ("Main", LOG_LEVEL_ERROR, "capinfos.c", 1016, __func__, "assertion failed: %s" , "cf_info != ((void*)0)"); } while (0);
1017 |
1018 | g_free(cf_info->encap_counts)(__builtin_object_size ((cf_info->encap_counts), 0) != ((size_t ) - 1)) ? g_free_sized (cf_info->encap_counts, __builtin_object_size ((cf_info->encap_counts), 0)) : (g_free) (cf_info->encap_counts );
1019 | cf_info->encap_counts = NULL((void*)0);
1020 |
1021 | g_array_free(cf_info->interface_packet_counts, true1);
1022 | cf_info->interface_packet_counts = NULL((void*)0);
1023 |
1024 | if (cf_info->idb_info_strings) {
1025 | for (i = 0; i < cf_info->idb_info_strings->len; i++) {
1026 | char *s = g_array_index(cf_info->idb_info_strings, char*, i)(((char**) (void *) (cf_info->idb_info_strings)->data) [ (i)]);
1027 | g_free(s)(__builtin_object_size ((s), 0) != ((size_t) - 1)) ? g_free_sized (s, __builtin_object_size ((s), 0)) : (g_free) (s);
1028 | }
1029 | g_array_free(cf_info->idb_info_strings, true1);
1030 | }
1031 | cf_info->idb_info_strings = NULL((void*)0);
1032 |
1033 | for(p = cf_info->pkt_cmts; p != NULL((void*)0); prev = p, p = p->next, g_free(prev)(__builtin_object_size ((prev), 0) != ((size_t) - 1)) ? g_free_sized (prev, __builtin_object_size ((prev), 0)) : (g_free) (prev)) {
1034 | g_free(p->cmt)(__builtin_object_size ((p->cmt), 0) != ((size_t) - 1)) ? g_free_sized (p->cmt, __builtin_object_size ((p->cmt), 0)) : (g_free ) (p->cmt);
1035 | }
1036 | cf_info->pkt_cmts = NULL((void*)0);
1037 | }
1038 |
1039 | static void
1040 | count_ipv4_address(const unsigned int addr _U___attribute__((unused)), const char *name _U___attribute__((unused)), const bool_Bool static_entry _U___attribute__((unused)))
1041 | {
1042 | num_ipv4_addresses++;
1043 | }
1044 |
1045 | static void
1046 | count_ipv6_address(const ws_in6_addr *addrp _U___attribute__((unused)), const char *name _U___attribute__((unused)), const bool_Bool static_entry _U___attribute__((unused)))
1047 | {
1048 | num_ipv6_addresses++;
1049 | }
1050 |
1051 | static void
1052 | count_decryption_secret(uint32_t secrets_type _U___attribute__((unused)), const void *secrets _U___attribute__((unused)), unsigned int size _U___attribute__((unused)))
1053 | {
1054 | /* XXX - count them based on the secrets type (which is an opaque code,
1055 | not a small integer)? */
1056 | num_decryption_secrets++;
1057 | }
1058 |
1059 | static void
1060 | hash_to_str(const unsigned char *hash, size_t length, char *str)
1061 | {
1062 | int i;
1063 |
1064 | for (i = 0; i < (int) length; i++) {
1065 | snprintf(str+(i*2), 3, "%02x", hash[i]);
1066 | }
1067 | }
1068 |
1069 | static void
1070 | calculate_hashes(const char *filename)
1071 | {
1072 | FILE *fh;
1073 | size_t hash_bytes;
1074 |
1075 | (void) g_strlcpy(file_sha256, "<unknown>", HASH_STR_SIZE(65));
1076 | (void) g_strlcpy(file_sha1, "<unknown>", HASH_STR_SIZE(65));
1077 |
1078 | if (cap_file_hashes) {
18 | ← | Assuming 'cap_file_hashes' is true | →
19 | ← | Taking true branch | →
1079 | fh = ws_fopenfopen(filename, "rb");
1080 | if (fh
19.1 | 'fh' is non-null
&& hd) {
20 | ← | Assuming 'hd' is non-null | →
21 | ← | Taking true branch | →
1081 | while((hash_bytes = fread(hash_buf, 1, HASH_BUF_SIZE(1024 * 1024), fh)) > 0) {
22 | ← | Assuming stream reaches end-of-file here | →
23 | ← | Assuming the condition is true | →
24 | ← | Loop condition is true. Entering loop body | →
25 | ← | Read function called when stream is in EOF state. Function has no effect
1082 | gcry_md_write(hd, hash_buf, hash_bytes);
1083 | }
1084 | gcry_md_final(hd)gcry_md_ctl ((hd), GCRYCTL_FINALIZE, ((void*)0), 0);
1085 | hash_to_str(gcry_md_read(hd, GCRY_MD_SHA256), HASH_SIZE_SHA25632, file_sha256);
1086 | hash_to_str(gcry_md_read(hd, GCRY_MD_SHA1), HASH_SIZE_SHA120, file_sha1);
1087 | }
1088 | if (fh) fclose(fh);
1089 | if (hd) gcry_md_reset(hd);
1090 | }
1091 | }
1092 |
1093 | static int
1094 | process_cap_file(const char *filename, bool_Bool need_separator)
1095 | {
1096 | int status = 0;
1097 | int err;
1098 | char *err_info;
1099 | int64_t size;
1100 | int64_t data_offset;
1101 |
1102 | uint32_t packet = 0;
1103 | int64_t bytes = 0;
1104 | uint32_t snaplen_min_inferred = 0xffffffff;
1105 | uint32_t snaplen_max_inferred = 0;
1106 | wtap_rec rec;
1107 | capture_info cf_info;
1108 | bool_Bool have_times = true1;
1109 | nstime_t earliest_packet_time;
1110 | int earliest_packet_time_tsprec;
1111 | nstime_t latest_packet_time;
1112 | int latest_packet_time_tsprec;
1113 | nstime_t cur_time;
1114 | nstime_t prev_time;
1115 | bool_Bool know_order = false0;
1116 | order_t order = IN_ORDER;
1117 | unsigned int i;
1118 | wtapng_iface_descriptions_t *idb_info;
1119 |
1120 | pkt_cmt *pc = NULL((void*)0), *prev = NULL((void*)0);
1121 |
1122 | cf_info.wth = wtap_open_offline(filename, WTAP_TYPE_AUTO0, &err, &err_info, false0, application_configuration_environment_prefix());
1123 | if (!cf_info.wth) {
15 | ← | Assuming field 'wth' is non-null | →
16 | ← | Taking false branch | →
1124 | report_cfile_open_failure(filename, err, err_info);
1125 | return 2;
1126 | }
1127 |
1128 | /*
1129 | * Calculate the checksums. Do this after wtap_open_offline, so we don't
1130 | * bother calculating them for files that are not known capture types
1131 | * where we wouldn't print them anyway.
1132 | */
1133 | calculate_hashes(filename);
17 | ← | Calling 'calculate_hashes' | →
1134 |
1135 | if (need_separator && long_report) {
1136 | printf("\n");
1137 | }
1138 |
1139 | nstime_set_zero(&earliest_packet_time);
1140 | earliest_packet_time_tsprec = WTAP_TSPREC_UNKNOWN-2;
1141 | nstime_set_zero(&latest_packet_time);
1142 | latest_packet_time_tsprec = WTAP_TSPREC_UNKNOWN-2;
1143 | nstime_set_zero(&cur_time);
1144 | nstime_set_zero(&prev_time);
1145 |
1146 | cf_info.encap_counts = g_new0(int,WTAP_NUM_ENCAP_TYPES)((int *) g_malloc0_n ((wtap_get_num_encap_types()), sizeof (int )));
1147 |
1148 | idb_info = wtap_file_get_idb_info(cf_info.wth);
1149 |
1150 | ws_assert(idb_info->interface_data != NULL)do { if ((1) && !(idb_info->interface_data != ((void *)0))) ws_log_fatal_full("Main", LOG_LEVEL_ERROR, "capinfos.c" , 1150, __func__, "assertion failed: %s", "idb_info->interface_data != ((void*)0)" ); } while (0);
1151 |
1152 | cf_info.pkt_cmts = NULL((void*)0);
1153 | cf_info.num_interfaces = idb_info->interface_data->len;
1154 | cf_info.interface_packet_counts = g_array_sized_new(false0, true1, sizeof(uint32_t), cf_info.num_interfaces);
1155 | g_array_set_size(cf_info.interface_packet_counts, cf_info.num_interfaces);
1156 | cf_info.pkt_interface_id_unknown = 0;
1157 |
1158 | g_free(idb_info)(__builtin_object_size ((idb_info), 0) != ((size_t) - 1)) ? g_free_sized (idb_info, __builtin_object_size ((idb_info), 0)) : (g_free) (idb_info);
1159 | idb_info = NULL((void*)0);
1160 |
1161 | /* Zero out the counters for the callbacks. */
1162 | num_ipv4_addresses = 0;
1163 | num_ipv6_addresses = 0;
1164 | num_decryption_secrets = 0;
1165 |
1166 | /* Register callbacks for new name<->address maps from the file and
1167 | decryption secrets from the file. */
1168 | wtap_set_cb_new_ipv4(cf_info.wth, count_ipv4_address);
1169 | wtap_set_cb_new_ipv6(cf_info.wth, count_ipv6_address);
1170 | wtap_set_cb_new_secrets(cf_info.wth, count_decryption_secret);
1171 |
1172 | /* Tally up data that we need to parse through the file to find */
1173 | wtap_rec_init(&rec, DEFAULT_INIT_BUFFER_SIZE_2048(2 * 1024));
1174 | while (wtap_read(cf_info.wth, &rec, &err, &err_info, &data_offset)) {
1175 | if (rec.presence_flags & WTAP_HAS_TS0x00000001) {
1176 | prev_time = cur_time;
1177 | cur_time = rec.ts;
1178 | if (packet == 0) {
1179 | earliest_packet_time = rec.ts;
1180 | earliest_packet_time_tsprec = rec.tsprec;
1181 | latest_packet_time = rec.ts;
1182 | latest_packet_time_tsprec = rec.tsprec;
1183 | prev_time = rec.ts;
1184 | }
1185 | if (nstime_cmp(&cur_time, &prev_time) < 0) {
1186 | order = NOT_IN_ORDER;
1187 | }
1188 | if (nstime_cmp(&cur_time, &earliest_packet_time) < 0) {
1189 | earliest_packet_time = cur_time;
1190 | earliest_packet_time_tsprec = rec.tsprec;
1191 | }
1192 | if (nstime_cmp(&cur_time, &latest_packet_time) > 0) {
1193 | latest_packet_time = cur_time;
1194 | latest_packet_time_tsprec = rec.tsprec;
1195 | }
1196 | } else {
1197 | have_times = false0; /* at least one packet has no time stamp */
1198 | if (order != NOT_IN_ORDER)
1199 | order = ORDER_UNKNOWN;
1200 | }
1201 |
1202 | if (rec.rec_type == REC_TYPE_PACKET0) {
1203 | bytes += rec.rec_header.packet_header.len;
1204 | packet++;
1205 | /* packet comments */
1206 | if (pkt_comments && wtap_block_count_option(rec.block, OPT_COMMENT1) > 0) {
1207 | char *cmt_buff;
1208 | for (i = 0; wtap_block_get_nth_string_option_value(rec.block, OPT_COMMENT1, i, &cmt_buff) == WTAP_OPTTYPE_SUCCESS; i++) {
1209 | pc = g_new0(pkt_cmt, 1)((pkt_cmt *) g_malloc0_n ((1), sizeof (pkt_cmt)));
1210 |
1211 | pc->recno = packet;
1212 | pc->cmt = g_strdup(cmt_buff)g_strdup_inline (cmt_buff);
1213 | pc->next = NULL((void*)0);
1214 |
1215 | if (prev == NULL((void*)0))
1216 | cf_info.pkt_cmts = pc;
1217 | else
1218 | prev->next = pc;
1219 |
1220 | prev = pc;
1221 | }
1222 | }
1223 |
1224 | /* If caplen < len for a rcd, then presumably */
1225 | /* 'Limit packet capture length' was done for this rcd. */
1226 | /* Keep track as to the min/max actual snapshot lengths */
1227 | /* seen for this file. */
1228 | if (rec.rec_header.packet_header.caplen < rec.rec_header.packet_header.len) {
1229 | if (rec.rec_header.packet_header.caplen < snaplen_min_inferred)
1230 | snaplen_min_inferred = rec.rec_header.packet_header.caplen;
1231 | if (rec.rec_header.packet_header.caplen > snaplen_max_inferred)
1232 | snaplen_max_inferred = rec.rec_header.packet_header.caplen;
1233 | }
1234 |
1235 | if ((rec.rec_header.packet_header.pkt_encap > 0) &&
1236 | (rec.rec_header.packet_header.pkt_encap < WTAP_NUM_ENCAP_TYPESwtap_get_num_encap_types())) {
1237 | cf_info.encap_counts[rec.rec_header.packet_header.pkt_encap] += 1;
1238 | } else {
1239 | fprintf(stderrstderr, "capinfos: Unknown packet encapsulation %d in frame %u of file \"%s\"\n",
1240 | rec.rec_header.packet_header.pkt_encap, packet, filename);
1241 | }
1242 |
1243 | /* Packet interface_id info */
1244 | if (rec.presence_flags & WTAP_HAS_INTERFACE_ID0x00000004) {
1245 | /* cf_info.num_interfaces is size, not index, so it's one more than max index */
1246 | if (rec.rec_header.packet_header.interface_id >= cf_info.num_interfaces) {
1247 | /*
1248 | * OK, re-fetch the number of interfaces, as there might have
1249 | * been an interface that was in the middle of packets, and
1250 | * grow the array to be big enough for the new number of
1251 | * interfaces.
1252 | */
1253 | idb_info = wtap_file_get_idb_info(cf_info.wth);
1254 |
1255 | cf_info.num_interfaces = idb_info->interface_data->len;
1256 | g_array_set_size(cf_info.interface_packet_counts, cf_info.num_interfaces);
1257 |
1258 | g_free(idb_info)(__builtin_object_size ((idb_info), 0) != ((size_t) - 1)) ? g_free_sized (idb_info, __builtin_object_size ((idb_info), 0)) : (g_free) (idb_info);
1259 | idb_info = NULL((void*)0);
1260 | }
1261 | if (rec.rec_header.packet_header.interface_id < cf_info.num_interfaces) {
1262 | g_array_index(cf_info.interface_packet_counts, uint32_t,(((uint32_t*) (void *) (cf_info.interface_packet_counts)-> data) [(rec.rec_header.packet_header.interface_id)])
1263 | rec.rec_header.packet_header.interface_id)(((uint32_t*) (void *) (cf_info.interface_packet_counts)-> data) [(rec.rec_header.packet_header.interface_id)]) += 1;
1264 | }
1265 | else {
1266 | cf_info.pkt_interface_id_unknown += 1;
1267 | }
1268 | }
1269 | else {
1270 | /* it's for interface_id 0 */
1271 | if (cf_info.num_interfaces != 0) {
1272 | g_array_index(cf_info.interface_packet_counts, uint32_t, 0)(((uint32_t*) (void *) (cf_info.interface_packet_counts)-> data) [(0)]) += 1;
1273 | }
1274 | else {
1275 | cf_info.pkt_interface_id_unknown += 1;
1276 | }
1277 | }
1278 | }
1279 |
1280 | wtap_rec_reset(&rec);
1281 | } /* while */
1282 | wtap_rec_cleanup(&rec);
1283 |
1284 | /*
1285 | * Get IDB info strings.
1286 | * We do this at the end, so we can get information for all IDBs in
1287 | * the file, even those that come after packet records, and so that
1288 | * we get, for example, a count of the number of statistics entries
1289 | * for each interface as of the *end* of the file.
1290 | */
1291 | idb_info = wtap_file_get_idb_info(cf_info.wth);
1292 |
1293 | cf_info.idb_info_strings = g_array_sized_new(false0, false0, sizeof(char*), cf_info.num_interfaces);
1294 | cf_info.num_interfaces = idb_info->interface_data->len;
1295 | for (i = 0; i < cf_info.num_interfaces; i++) {
1296 | const wtap_block_t if_descr = g_array_index(idb_info->interface_data, wtap_block_t, i)(((wtap_block_t*) (void *) (idb_info->interface_data)-> data) [(i)]);
1297 | char *s = wtap_get_debug_if_descr(if_descr, 21, "\n");
1298 | g_array_append_val(cf_info.idb_info_strings, s)g_array_append_vals (cf_info.idb_info_strings, &(s), 1);
1299 | }
1300 |
1301 | g_free(idb_info)(__builtin_object_size ((idb_info), 0) != ((size_t) - 1)) ? g_free_sized (idb_info, __builtin_object_size ((idb_info), 0)) : (g_free) (idb_info);
1302 | idb_info = NULL((void*)0);
1303 |
1304 | if (err != 0) {
1305 | fprintf(stderrstderr,
1306 | "capinfos: An error occurred after reading %u packets from \"%s\".\n",
1307 | packet, filename);
1308 | report_cfile_read_failure(filename, err, err_info);
1309 | if (err == WTAP_ERR_SHORT_READ-12) {
1310 | /* Don't give up completely with this one. */
1311 | status = 1;
1312 | fprintf(stderrstderr,
1313 | " (will continue anyway, checksums might be incorrect)\n");
1314 | } else {
1315 | cleanup_capture_info(&cf_info);
1316 | wtap_close(cf_info.wth);
1317 | return 2;
1318 | }
1319 | }
1320 |
1321 | /* File size */
1322 | size = wtap_file_size(cf_info.wth, &err);
1323 | if (size == -1) {
1324 | fprintf(stderrstderr,
1325 | "capinfos: Can't get size of \"%s\": %s.\n",
1326 | filename, g_strerror(err));
1327 | cleanup_capture_info(&cf_info);
1328 | wtap_close(cf_info.wth);
1329 | return 2;
1330 | }
1331 |
1332 | cf_info.filesize = size;
1333 |
1334 | /* File Type */
1335 | cf_info.file_type = wtap_file_type_subtype(cf_info.wth);
1336 | cf_info.compression_type = wtap_get_compression_type(cf_info.wth);
1337 |
1338 | /* File Encapsulation */
1339 | cf_info.file_encap = wtap_file_encap(cf_info.wth);
1340 |
1341 | cf_info.file_tsprec = wtap_file_tsprec(cf_info.wth);
1342 |
1343 | /* Packet size limit (snaplen) */
1344 | cf_info.snaplen = wtap_snapshot_length(cf_info.wth);
1345 | if (cf_info.snaplen > 0)
1346 | cf_info.snap_set = true1;
1347 | else
1348 | cf_info.snap_set = false0;
1349 |
1350 | cf_info.snaplen_min_inferred = snaplen_min_inferred;
1351 | cf_info.snaplen_max_inferred = snaplen_max_inferred;
1352 |
1353 | /* # of packets */
1354 | cf_info.packet_count = packet;
1355 |
1356 | /* File Times */
1357 | cf_info.times_known = have_times;
1358 | cf_info.earliest_packet_time = earliest_packet_time;
1359 | cf_info.earliest_packet_time_tsprec = earliest_packet_time_tsprec;
1360 | cf_info.latest_packet_time = latest_packet_time;
1361 | cf_info.latest_packet_time_tsprec = latest_packet_time_tsprec;
1362 | nstime_delta(&cf_info.duration, &latest_packet_time, &earliest_packet_time);
1363 | /* Duration precision is the higher of the earliest and latest packet timestamp precisions. */
1364 | if (cf_info.latest_packet_time_tsprec > cf_info.earliest_packet_time_tsprec)
1365 | cf_info.duration_tsprec = cf_info.latest_packet_time_tsprec;
1366 | else
1367 | cf_info.duration_tsprec = cf_info.earliest_packet_time_tsprec;
1368 | cf_info.know_order = know_order;
1369 | cf_info.order = order;
1370 |
1371 | /* Number of packet bytes */
1372 | cf_info.packet_bytes = bytes;
1373 |
1374 | cf_info.data_rate = 0.0;
1375 | cf_info.packet_rate = 0.0;
1376 | cf_info.packet_size = 0.0;
1377 |
1378 | if (packet > 0) {
1379 | double delta_time = nstime_to_sec(&latest_packet_time) - nstime_to_sec(&earliest_packet_time);
1380 | if (delta_time > 0.0) {
1381 | cf_info.data_rate = (double)bytes / delta_time; /* Data rate per second */
1382 | cf_info.packet_rate = (double)packet / delta_time; /* packet rate per second */
1383 | }
1384 | cf_info.packet_size = (double)bytes / packet; /* Avg packet size */
1385 | }
1386 |
1387 | if (!long_report && table_report_header) {
1388 | print_stats_table_header(&cf_info);
1389 | }
1390 |
1391 | if (long_report) {
1392 | print_stats(filename, &cf_info);
1393 | } else {
1394 | print_stats_table(filename, &cf_info);
1395 | }
1396 |
1397 | cleanup_capture_info(&cf_info);
1398 | wtap_close(cf_info.wth);
1399 |
1400 | return status;
1401 | }
1402 |
1403 | static void
1404 | print_usage(FILE *output)
1405 | {
1406 | fprintf(output, "\n");
1407 | fprintf(output, "Usage: capinfos [options] <infile> ...\n");
1408 | fprintf(output, "\n");
1409 | fprintf(output, "General infos:\n");
1410 | fprintf(output, " -t display the capture file type\n");
1411 | fprintf(output, " -E display the capture file encapsulation\n");
1412 | fprintf(output, " -I display the capture file interface information\n");
1413 | fprintf(output, " -F display additional capture file information\n");
1414 | fprintf(output, " -H display the SHA256 and SHA1 hashes of the file\n");
1415 | fprintf(output, " -k display the capture comment\n");
1416 | fprintf(output, " -p display individual packet comments\n");
1417 | fprintf(output, "\n");
1418 | fprintf(output, "Size infos:\n");
1419 | fprintf(output, " -c display the number of packets\n");
1420 | fprintf(output, " -s display the size of the file (in bytes)\n");
1421 | fprintf(output, " -d display the total length of all packets (in bytes)\n");
1422 | fprintf(output, " -l display the packet size limit (snapshot length)\n");
1423 | fprintf(output, "\n");
1424 | fprintf(output, "Time infos:\n");
1425 | fprintf(output, " -u display the capture duration (in seconds)\n");
1426 | fprintf(output, " -a display the timestamp of the earliest packet\n");
1427 | fprintf(output, " -e display the timestamp of the latest packet\n");
1428 | fprintf(output, " -o display the capture file chronological status (True/False)\n");
1429 | fprintf(output, " -S display earliest and latest packet timestamps as seconds\n");
1430 | fprintf(output, "\n");
1431 | fprintf(output, "Statistic infos:\n");
1432 | fprintf(output, " -y display average data rate (in bytes/sec)\n");
1433 | fprintf(output, " -i display average data rate (in bits/sec)\n");
1434 | fprintf(output, " -z display average packet size (in bytes)\n");
1435 | fprintf(output, " -x display average packet rate (in packets/sec)\n");
1436 | fprintf(output, "\n");
1437 | fprintf(output, "Metadata infos:\n");
1438 | fprintf(output, " -n display number of resolved IPv4 and IPv6 addresses\n");
1439 | fprintf(output, " -D display number of decryption secrets\n");
1440 | fprintf(output, "\n");
1441 | fprintf(output, "Output format:\n");
1442 | fprintf(output, " -L generate long report (default)\n");
1443 | fprintf(output, " -T generate table report\n");
1444 | fprintf(output, " -M display machine-readable values in long reports\n");
1445 | fprintf(output, "\n");
1446 | fprintf(output, "Table report options:\n");
1447 | fprintf(output, " -R generate header record (default)\n");
1448 | fprintf(output, " -r do not generate header record\n");
1449 | fprintf(output, "\n");
1450 | fprintf(output, " -B separate infos with TAB character (default)\n");
1451 | fprintf(output, " -m separate infos with comma (,) character\n");
1452 | fprintf(output, " -b separate infos with SPACE character\n");
1453 | fprintf(output, "\n");
1454 | fprintf(output, " -N do not quote infos (default)\n");
1455 | fprintf(output, " -q quote infos with single quotes (')\n");
1456 | fprintf(output, " -Q quote infos with double quotes (\")\n");
1457 | fprintf(output, "\n");
1458 | fprintf(output, "Miscellaneous:\n");
1459 | fprintf(output, " -h, --help display this help and exit\n");
1460 | fprintf(output, " -v, --version display version info and exit\n");
1461 | fprintf(output, " -C cancel processing if file open fails (default is to continue)\n");
1462 | fprintf(output, " -A generate all infos (default)\n");
1463 | fprintf(output, " -K disable displaying the capture comment\n");
1464 | fprintf(output, " -P disable displaying individual packet comments\n");
1465 | fprintf(output, "\n");
1466 | fprintf(output, "Options are processed from left to right order with later options superseding\n");
1467 | fprintf(output, "or adding to earlier options.\n");
1468 | fprintf(output, "\n");
1469 | fprintf(output, "If no options are given the default is to display all infos in long report\n");
1470 | fprintf(output, "output format.\n");
1471 | }
1472 |
1473 | int
1474 | main(int argc, char *argv[])
1475 | {
1476 | char *configuration_init_error;
1477 | bool_Bool need_separator = false0;
1478 | int opt;
1479 | int overall_error_status = EXIT_SUCCESS0;
1480 | static const struct ws_option long_options[] = {
1481 | {"help", ws_no_argument0, NULL((void*)0), 'h'},
1482 | {"version", ws_no_argument0, NULL((void*)0), 'v'},
1483 | LONGOPT_WSLOG{"log-level", 1, ((void*)0), 5000 +1}, {"log-domain", 1, ((void *)0), 5000 +2}, {"log-domains", 1, ((void*)0), 5000 +2}, {"log-file" , 1, ((void*)0), 5000 +3}, {"log-fatal", 1, ((void*)0), 5000 + 4}, {"log-fatal-count", 1, ((void*)0), 5000 +5}, {"log-fatal-domain" , 1, ((void*)0), 5000 +6}, {"log-fatal-domains", 1, ((void*)0 ), 5000 +6}, {"log-debug", 1, ((void*)0), 5000 +7}, {"log-noisy" , 1, ((void*)0), 5000 +8},
1484 | {0, 0, 0, 0 }
1485 | };
1486 | const struct file_extension_info* file_extensions;
1487 | unsigned num_extensions;
1488 |
1489 | #define OPTSTRING"abcdehiklmnopqrstuvxyzABCDEFHIKLMNPQRST" "abcdehiklmnopqrstuvxyzABCDEFHIKLMNPQRST"
1490 | static const char optstring[] = OPTSTRING"abcdehiklmnopqrstuvxyzABCDEFHIKLMNPQRST";
1491 |
1492 | int status = 0;
1493 |
1494 | /* Set the program name. */
1495 | g_set_prgname("capinfos");
1496 |
1497 | /*
1498 | * Set the C-language locale to the native environment and set the
1499 | * code page to UTF-8 on Windows.
1500 | */
1501 | #ifdef _WIN32
1502 | setlocale(LC_ALL6, ".UTF-8");
1503 | #else
1504 | setlocale(LC_ALL6, "");
1505 | #endif
1506 |
1507 | cmdarg_err_init(stderr_cmdarg_err, stderr_cmdarg_err_cont);
1508 |
1509 | /* Initialize log handler early so we can have proper logging during startup. */
1510 | ws_log_init(vcmdarg_err, "Capinfos Debug Console");
1511 |
1512 | /* Early logging command-line initialization. */
1513 | ws_log_parse_args(&argc, argv, optstring, long_options, vcmdarg_err, WS_EXIT_INVALID_OPTION1);
1514 |
1515 | ws_noisy("Finished log init and parsing command line log arguments")do { if (1) { ws_log_full("Main", LOG_LEVEL_NOISY, "capinfos.c" , 1515, __func__, "Finished log init and parsing command line log arguments" ); } } while (0);
1 | Taking true branch | →
2 | ← | Loop condition is false. Exiting loop | →
1516 |
1517 | /* Get the decimal point. */
1518 | decimal_point = g_strdup(localeconv()->decimal_point)g_strdup_inline (localeconv()->decimal_point);
1519 |
1520 | #ifdef _WIN32
1521 | create_app_running_mutex();
1522 | #endif /* _WIN32 */
1523 |
1524 | /*
1525 | * Get credential information for later use.
1526 | */
1527 | init_process_policies();
1528 |
1529 | /*
1530 | * Attempt to get the pathname of the directory containing the
1531 | * executable file.
1532 | */
1533 | configuration_init_error = configuration_init(argv[0], "wireshark");
1534 | if (configuration_init_error != NULL((void*)0)) {
3 | ← | Assuming 'configuration_init_error' is equal to NULL | →
4 | ← | Taking false branch | →
1535 | fprintf(stderrstderr,
1536 | "capinfos: Can't get pathname of directory containing the capinfos program: %s.\n",
1537 | configuration_init_error);
1538 | g_free(configuration_init_error)(__builtin_object_size ((configuration_init_error), 0) != ((size_t ) - 1)) ? g_free_sized (configuration_init_error, __builtin_object_size ((configuration_init_error), 0)) : (g_free) (configuration_init_error );
1539 | }
1540 |
1541 | /* Initialize the version information. */
1542 | ws_init_version_info("Capinfos", NULL((void*)0), application_get_vcs_version_info, NULL((void*)0), NULL((void*)0));
1543 |
1544 | init_report_failure_message("capinfos");
1545 |
1546 | application_file_extensions(&file_extensions, &num_extensions);
1547 | wtap_init(true1, application_configuration_environment_prefix(), file_extensions, num_extensions);
1548 |
1549 | /* Process the options */
1550 | while ((opt = ws_getopt_long(argc, argv, optstring, long_options, NULL((void*)0))) !=-1) {
5 | ← | Assuming the condition is false | →
6 | ← | Loop condition is false. Execution continues on line 1742 | →
1551 |
1552 | switch (opt) {
1553 |
1554 | case 't':
1555 | if (report_all_infos) disable_all_infos();
1556 | cap_file_type = true1;
1557 | break;
1558 |
1559 | case 'E':
1560 | if (report_all_infos) disable_all_infos();
1561 | cap_file_encap = true1;
1562 | break;
1563 |
1564 | case 'l':
1565 | if (report_all_infos) disable_all_infos();
1566 | cap_snaplen = true1;
1567 | break;
1568 |
1569 | case 'c':
1570 | if (report_all_infos) disable_all_infos();
1571 | cap_packet_count = true1;
1572 | break;
1573 |
1574 | case 's':
1575 | if (report_all_infos) disable_all_infos();
1576 | cap_file_size = true1;
1577 | break;
1578 |
1579 | case 'd':
1580 | if (report_all_infos) disable_all_infos();
1581 | cap_data_size = true1;
1582 | break;
1583 |
1584 | case 'u':
1585 | if (report_all_infos) disable_all_infos();
1586 | cap_duration = true1;
1587 | break;
1588 |
1589 | case 'a':
1590 | if (report_all_infos) disable_all_infos();
1591 | cap_earliest_packet_time = true1;
1592 | break;
1593 |
1594 | case 'e':
1595 | if (report_all_infos) disable_all_infos();
1596 | cap_latest_packet_time = true1;
1597 | break;
1598 |
1599 | case 'S':
1600 | time_as_secs = true1;
1601 | break;
1602 |
1603 | case 'y':
1604 | if (report_all_infos) disable_all_infos();
1605 | cap_data_rate_byte = true1;
1606 | break;
1607 |
1608 | case 'i':
1609 | if (report_all_infos) disable_all_infos();
1610 | cap_data_rate_bit = true1;
1611 | break;
1612 |
1613 | case 'z':
1614 | if (report_all_infos) disable_all_infos();
1615 | cap_packet_size = true1;
1616 | break;
1617 |
1618 | case 'x':
1619 | if (report_all_infos) disable_all_infos();
1620 | cap_packet_rate = true1;
1621 | break;
1622 |
1623 | case 'H':
1624 | if (report_all_infos) disable_all_infos();
1625 | cap_file_hashes = true1;
1626 | break;
1627 |
1628 | case 'o':
1629 | if (report_all_infos) disable_all_infos();
1630 | cap_order = true1;
1631 | break;
1632 |
1633 | case 'k':
1634 | if (report_all_infos) disable_all_infos();
1635 | cap_comment = true1;
1636 | break;
1637 |
1638 | case 'p':
1639 | if (report_all_infos) disable_all_infos();
1640 | pkt_comments = true1;
1641 | break;
1642 |
1643 | case 'K':
1644 | cap_comment = false0;
1645 | break;
1646 |
1647 | case 'P':
1648 | pkt_comments = false0;
1649 | break;
1650 |
1651 | case 'F':
1652 | if (report_all_infos) disable_all_infos();
1653 | cap_file_more_info = true1;
1654 | break;
1655 |
1656 | case 'I':
1657 | if (report_all_infos) disable_all_infos();
1658 | cap_file_idb = true1;
1659 | break;
1660 |
1661 | case 'n':
1662 | if (report_all_infos) disable_all_infos();
1663 | cap_file_nrb = true1;
1664 | break;
1665 |
1666 | case 'D':
1667 | if (report_all_infos) disable_all_infos();
1668 | cap_file_dsb = true1;
1669 | break;
1670 |
1671 | case 'C':
1672 | stop_after_failure = true1;
1673 | break;
1674 |
1675 | case 'A':
1676 | enable_all_infos();
1677 | break;
1678 |
1679 | case 'L':
1680 | long_report = true1;
1681 | break;
1682 |
1683 | case 'T':
1684 | long_report = false0;
1685 | break;
1686 |
1687 | case 'M':
1688 | machine_readable = true1;
1689 | break;
1690 |
1691 | case 'R':
1692 | table_report_header = true1;
1693 | break;
1694 |
1695 | case 'r':
1696 | table_report_header = false0;
1697 | break;
1698 |
1699 | case 'N':
1700 | quote_char = '\0';
1701 | break;
1702 |
1703 | case 'q':
1704 | quote_char = '\'';
1705 | break;
1706 |
1707 | case 'Q':
1708 | quote_char = '"';
1709 | break;
1710 |
1711 | case 'B':
1712 | field_separator = '\t';
1713 | break;
1714 |
1715 | case 'm':
1716 | field_separator = ',';
1717 | break;
1718 |
1719 | case 'b':
1720 | field_separator = ' ';
1721 | break;
1722 |
1723 | case 'h':
1724 | show_help_header("Print various information (infos) about capture files.");
1725 | print_usage(stdoutstdout);
1726 | goto exit;
1727 | break;
1728 |
1729 | case 'v':
1730 | show_version();
1731 | goto exit;
1732 | break;
1733 |
1734 | case '?': /* Bad flag - print usage message */
1735 | print_usage(stderrstderr);
1736 | overall_error_status = WS_EXIT_INVALID_OPTION1;
1737 | goto exit;
1738 | break;
1739 | }
1740 | }
1741 |
1742 | if ((argc - ws_optind) < 1) {
7 | ← | Assuming the condition is false | →
8 | ← | Taking false branch | →
1743 | print_usage(stderrstderr);
1744 | overall_error_status = WS_EXIT_INVALID_OPTION1;
1745 | goto exit;
1746 | }
1747 |
1748 | if (cap_file_hashes
8.1 | 'cap_file_hashes' is true
) {
9 | ← | Taking true branch | →
1749 | gcry_check_version(NULL((void*)0));
1750 | gcry_md_open(&hd, GCRY_MD_SHA256, 0);
1751 | if (hd)
10 | ← | Assuming 'hd' is null | →
11 | ← | Taking false branch | →
1752 | gcry_md_enable(hd, GCRY_MD_SHA1);
1753 |
1754 | hash_buf = (char *)g_malloc(HASH_BUF_SIZE(1024 * 1024));
1755 | }
1756 |
1757 | overall_error_status = 0;
1758 |
1759 | for (opt = ws_optind; opt < argc; opt++) {
12 | ← | Assuming 'opt' is < 'argc' | →
13 | ← | Loop condition is true. Entering loop body | →
1760 |
1761 | status = process_cap_file(argv[opt], need_separator);
14 | ← | Calling 'process_cap_file' | →
1762 | if (status) {
1763 | /* Something failed. It's been reported; remember that processing
1764 | one file failed and, if -C was specified, stop. */
1765 | overall_error_status = status;
1766 | if (stop_after_failure)
1767 | goto exit;
1768 | }
1769 | if (status != 2) {
1770 | /* Either it succeeded or it got a "short read" but printed
1771 | information anyway. Note that we need a blank line before
1772 | the next file's information, to separate it from the
1773 | previous file. */
1774 | need_separator = true1;
1775 | }
1776 | }
1777 |
1778 | exit:
1779 | g_free(hash_buf)(__builtin_object_size ((hash_buf), 0) != ((size_t) - 1)) ? g_free_sized (hash_buf, __builtin_object_size ((hash_buf), 0)) : (g_free) (hash_buf);
1780 | gcry_md_close(hd);
1781 | wtap_cleanup();
1782 | free_progdirs();
1783 | return overall_error_status;
1784 | }